# SoftEther VPN String Table


# Copyright (c) all contributors on SoftEther VPN project in GitHub.


# Copyright (c) Daiyuu Nobori, SoftEther Project at University of Tsukuba, and SoftEther Corporation.


#


# https://www.softether.org/


###########################################################################
#                                                                         #
# String data such as messages in software                                #
# (Excludes dialog box resource strings)                                  #
#                                                                         #
###########################################################################


# Environment parameters
DEFAULT_FONT			Tahoma
DEFAULT_FONT_WIN7		Segoe UI
DEFAULT_FONT_2			Tahoma
DEFAULT_FONT_SIZE		8
DEFAULT_LOCALE	- - $ : : $ Dom Seg Ter Qua Qui Sex Sáb : : : $ (Nenhum)


# 言語


# (0: 日本語, 1: 英語)
LANG					6
LANGSTR					Portuguese-Brazil
STRTABLE_ID				SE_VPN_20121007


# Strings for Japanese version only (not required for other language versions.)
CM_JAPANESE_ONLY_OLD_STARTUP	%s\\SoftEther VPN Client 2.0 タスクトレイ.lnk


# Software information
PRODUCT_NAME_VPN_CLI	Edição de desenvolvedor do SoftEther VPN Cliente
PRODUCT_NAME_VPN_CMGR	Edição de desenvolvedor do gerenciador SoftEther VPN Cliente
PRODUCT_NAME_VPN_SVR	Edição de desenvolvedor do SoftEther VPN Servidor
PRODUCT_NAME_VPN_BRIDGE	Edição de desenvolvedor do SoftEther VPN Bridge
PRODUCT_NAME_VPN_SMGR	Edição de desenvolvedor do gerenciador SoftEther VPN Servidor
PRODUCT_NAME_ELOGSVC	Edição de desenvolvedor do SoftEther EtherLogger
PRODUCT_NAME_ELOGMGR	Edição de desenvolvedor do SoftEther EtherLogger


# Branding String for Limited Connection


# BRANDED_C_TO_S	Branded_VPN


# BRANDED_C_FROM_S	Branded_VPN


# Client ID (sample)


# CLIENT_ID	123


# Family Name for Software Update Check
PRODUCT_FAMILY_NAME	SoftEtherDev


# Product information
SE_COMPANY_URL	https://selinks.org/?se
SE_VPNAZURE_URL	https://selinks.org/?vpnazure


# Common strings
COMMON_UNKNOWN	(Desconhecido)


# Protocol error strings
ERR_UNKNOWN	Ocorreu um erro desconhecido.
ERR_0	Sem erro.
ERR_1	Falha na conexão com o servidor. Verifique a conexão de rede e se o endereço e o número da porta do servidor de destino estão corretos.
ERR_2	Ocorreu um erro no protocolo. Erro foi retornado do servidor de destino.
ERR_3	A conexão foi desconectada.
ERR_4	Ocorreu um erro de protocolo.
ERR_5	Um cliente que não é um software VPN SoftEther se conectou à porta.
ERR_6	O comando foi cancelado pelo usuário.
ERR_7	O servidor negou o tipo de autenticação especificado.
ERR_8	O Hub Virtual especificado não existe no servidor.
ERR_9	Falha na autenticação do usuário.
ERR_10	O Hub Virtual especificado está atualmente parado. Aguarde um pouco e reconecte-se.
ERR_11	A sessão da VPN foi excluída. É possível que o administrador tenha desconectado a sessão ou a conexão do cliente com o servidor VPN tenha sido desconectada.
ERR_12	O acesso foi negado.
ERR_13	Tempo-limite esgotado durante a comunicação da sessão VPN. É possível que a conexão do cliente com o servidor VPN tenha sido desconectada.
ERR_14	O número do protocolo é inválido.
ERR_15	Existem muitas conexões TCP/IP.
ERR_16	Existem muitas sessões conectadas ao servidor de destino ou ao Hub Virtual.
ERR_17	Connection to proxy server failed.
ERR_18	An error occurred on the proxy server.
ERR_19	User authentication failed on the proxy server.
ERR_20	There are too many sessions by the same user. Other person might be connected to the Virtual Hub as the same user.
ERR_21	A license error occurred on the VPN Server. Contact the VPN Server's administrator.
ERR_22	Cannot access the Virtual Network Adapter device driver. Check the Virtual Network Adapter is installed and make sure that it has not been disabled.
ERR_23	An internal error occurred.
ERR_24	Access to either the smart card or USB hardware token device failed.
ERR_25	The PIN code is incorrect.
ERR_26	The specified certificate is not stored on either the smart card or the USB hardware token device.
ERR_27	The specified private key is not stored on either the smart card or the USB hardware token device.
ERR_28	Write operation to the smart card or USB hardware token device failed.
ERR_29	Object not found.
ERR_30	A Virtual Network Adapter with the specified name already exists. Specify a different name.
ERR_31	Installation of the Virtual Network Adapter device driver failed.
ERR_32	Você não pode usar o nome especificado para um dispositivo de adaptador de rede virtual.
ERR_33	Não suportado.
ERR_34	VPN Connection Setting with the specified name already exists.
ERR_35	The specified VPN Connection Setting is currently connected.
ERR_36	The specified VPN Connection Setting does not exist.
ERR_37	The specified VPN Connection Setting is not connected.
ERR_38	Invalid parameter.
ERR_39	Error occurred on smart card or USB hardware token.
ERR_40	Although authentication of smart card or USB hardware token was selected, but the device to be used has not been selected. Select from the Smart Card menu of Connection Manager.
ERR_41	The specified Virtual Network Adapter is being used by at least one VPN Connection Setting. \r\nEither delete the VPN Connection Setting that is using this Virtual Network Adapter or change Virtual Network Adapter that this VPN Connection Setting is using.
ERR_42	Cannot find the Virtual Network Adapter that the specified VPN Connection Setting is using. \r\nMake sure this Virtual Network Adapter exists. Also make sure the Virtual Network Adapter device has not been disabled. \r\n\r\nIf you cannot resolve the problem, either change the Virtual Network Adapter being used by this VPN Connection Setting or create a new Virtual Network Adapter with the same name.
ERR_43	The Virtual Network Adapter used by the specified VPN Connection Setting is already being used by another VPN Connection Setting. \r\nIf there is another VPN Connection Setting that is using the same Virtual Network Adapter, disconnect that VPN Connection Setting.
ERR_44	The Virtual Network Adapter being used by the specified VPN Connection Setting has been disabled. \r\nBefore using this VPN Connection Setting, enable the Virtual Network Adapter.
ERR_45	The specified value is invalid.
ERR_46	The connection destination is not a cluster controller.
ERR_47	Trying to connect.
ERR_48	Connection to the cluster controller failed.
ERR_49	The cluster controller was unable to assign a new session on a cluster.
ERR_50	Unable to manage the Virtual Hub of the cluster member server.
ERR_51	The user's password used to connect was blank so the connection from remote is prohibited. Blank password can be allowed only to connections from the VPN Server's localhost (127.0.0.1).
ERR_52	Not enough privileges.
ERR_53	Specified listener not found.
ERR_54	The listener of the specified port number already exists.
ERR_55	This is not a cluster member server.
ERR_56	The specified encryption algorithm name is not supported.
ERR_57	The Virtual Hub with the specified name already exists on the server.
ERR_58	There are too many registered Virtual Hubs. No more can be created. Delete the old Virtual Hubs.
ERR_59	The Cascade Connection with the specified name already exists.
ERR_60	A Cascade Connection cannot be created on a server on a cluster.
ERR_61	The specified Cascade Connection is offline. 
ERR_62	There are too many access lists.
ERR_63	There are too many users.
ERR_64	There are too many groups.
ERR_65	The specified group does not exist.
ERR_66	The user with the specified name already exists on the Virtual Hub.
ERR_67	The group with the specified name already exists on the Virtual Hub.
ERR_68	A user with the specified name exists on the server but the type of authentication is not password authentication. Unable to change the password.
ERR_69	The user name or old password you entered is incorrect. Note that the password is case-sensitive.
ERR_70	Saitama.
ERR_71	SoftEther has temporarily stopped the current distribution by order of the Japan Ministry of Economy Trade and Industry.
ERR_72	SoftEther has temporarily stopped the current distribution by order of the IPA.
ERR_73	Unable to disconnect the Cascade Connection's session. To delete the session, stop the Cascade Connection.
ERR_74	The VPN Connection Setting for connection with the VPN Server is incomplete. At first you have to complete the VPN Connection Setting for connection with the VPN Server.
ERR_75	VPN Connection to the VPN Server has already started.
ERR_76	Not connected to the VPN Server.
ERR_77	The specified X509 certificate file does not contain a RSA 1024 bit or 2048 bit public key. SoftEther VPN software supports only RSA 1024 bit or 2048 bit certificates.
ERR_78	Unable to disconnect the SecureNAT session. To delete the session, stop the SecureNAT function.
ERR_79	Cannot enable the SecureNAT in a clustering environment.
ERR_80	The SecureNAT is not operating.
ERR_81	This VPN Connection session to the VPN Server has been disconnected by the firewall device installed by the network administrator. Contact the network administrator.
ERR_82	Unable to disconnect the Local Bridge session. To delete the session, stop the Local Bridge.
ERR_83	The Local Bridge is not operating.
ERR_84	Local Bridge cannot be used by the destination VPN Server. Refer to online help or other documentation for the setting method when using Local Bridge on the VPN Server you are using.
ERR_85	Unable to trust the certificate provided by the destination server. The setting to always verify the server certificate is enabled in the VPN Connection Settings. Either register a root certificate that can be trusted or register a individual certificate.
ERR_86	The product code of the destination server is incorrect. It is not possible to connect from this client.
ERR_87	The client and server version is different. Update the software.
ERR_88	Failed to add a capture device. A same capture device might be already registered.
ERR_89	Unable to connect to the destination server from this client. A special client software is required.
ERR_90	The specified capture device is not registered.
ERR_91	Unable to disconnect the Virtual Layer 3 Switch session. To delete the session, stop the Virtual Layer 3 Switch.
ERR_92	A Virtual Layer 3 Switch with the specified name already exists. Specify a different name.
ERR_93	Specified Virtual Layer 3 Switch not found.
ERR_94	The specified name is invalid. Check if the name contains characters that cannot be used.
ERR_95	Failed to add the Virtual Layer 3 interface. Please check that the parameters are valid. Also please make sure that the Virtual Layer 3 switch is stopped. Adding or deleting interfaces are unable when the Virtual Layer 3 switch is running.
ERR_96	Failed to delete the Virtual Layer 3 interface. Please check that the parameters are valid. Also please make sure that the Virtual Layer 3 switch is stopped. Adding or deleting interfaces are unable when the Virtual Layer 3 switch is running.
ERR_97	The Virtual Layer 3 interface that is connecting to the destination Virtual Hub of the specified Virtual Layer 3 interface already exists in the Virtual Layer 3 Switch. No more than one Virtual Layer 3 interface that connects to the same Virtual Hub can be defined in a Virtual Layer 3 Switch.
ERR_98	Failed to add routing table entry. Please check that the parameters are valid. Also please make sure that the Virtual Layer 3 switch is stopped. Adding or deleting routing table entries are unable when the Virtual Layer 3 switch is running.
ERR_99	Failed to delete routing table entry. Please check that the parameters are valid. Also please make sure that the Virtual Layer 3 switch is stopped. Adding or deleting routing table entries are unable when the Virtual Layer 3 switch is running.
ERR_100	The specified routing table entry already exists.
ERR_101	The client clock and the server clock are not synchronized with each other. Check the time settings.
ERR_102	Unable to start this Virtual Layer 3 Switch. \r\n\r\nTo start the Virtual Layer 3 Switch, at least 1 virtual interface must be defined in the Virtual Layer 3 Switch.
ERR_103	Not enough Client Connection Licenses on the destination VPN Server. Contact the server administrator.
ERR_104	Not enough Bridge Connection Licenses on the destination VPN Server. Contact the server administrator.
ERR_105	Due to current technical difficulties, the destination VPN Server is not receiving the connection. Either wait a while, or contact the VPN Server administrator requesting that the server log file be checked.
ERR_106	The destination VPN Server's certificate has expired. Contact the VPN Server's administrator.
ERR_107	A connection has been requested in Monitoring Mode. But the security policy for the connecting user does not permit Monitoring Mode.
ERR_108	A connection has been requested in Bridge / Router Mode. But the security policy for the connecting user forbids both bridge mode and router mode.
ERR_109	A connection from a client IP address has been denied by the Source IP Restriction List of the Virtual Hub.
ERR_110	There are too many items.
ERR_111	Out of memory.
ERR_112	The specified object already exists.
ERR_113	A fatal error occurred. It is possible that the program operation is unable to continue.
ERR_114	The destination VPN Server has detected a software license violation. Connection is refused. Contact the VPN Server's administrator.
ERR_115	The destination VPN Server has connected via the Internet to an important server provided by SoftEther VPN Project and cannot validate a license. Either wait a while, or contact the VPN Server administrator requesting that the server log file and the Internet connection status of the server itself be checked.
ERR_116	A software license violation has been detected on the client side. Connection is refused.
ERR_117	The command or file name is incorrect.
ERR_118	The license key is incorrect.
ERR_119	No valid product license is registered on the VPN Server. Contact the VPN Server's administrator.
ERR_120	The product license required for the VPN Server to operate as a cluster is not registered. Contact the VPN Server's administrator.
ERR_121	This VPN Connection Setting has been installed using the "Web Installer Creation Kit" or "Simple Installer Creation Kit". The destination server is not an edition that supports the SoftEther VPN 2.0 Administration Pack. Contact the system administrator or person who created the installer.
ERR_122	With the VPN Server SDK for .NET, it is only possible to connect to the SoftEther VPN Server edition that supports the SoftEther VPN 2.0 Administration Pack. The destination VPN Server is not an edition that supports the SoftEther VPN 2.0 Administration Pack. Contact the system administrator.
ERR_123	Beta Version Software on the destination server is expired. Contact to system administrator of the server to download a new beta version or full version from http://selinks.org/.
ERR_124	The VPN connection to VPN Server is refused at server side.
ERR_125	The VPN connection to VPN Server is refused at client side.
ERR_126	The security policy enforced the VPN session to disconnect automatically because the specific time has been elapsed. If you wish to continue please re-connect.
ERR_127	The VPN Server requires the special-version VPN Client software. Consult with the administrator.
ERR_128	The number of registered user objects exceeds the maximum number which is allowed the product license applied on the VPN Server. You cannot add user objects anymore unless you delete old one, or upgrade the edition of the product.
ERR_129	The subscription contract has already expired before the release-date of this version of VPN Server. The customer has been authorized to use VPN Server's builds only in the period of the subscription contract. The customer has to extend the period of the subscription. The customer also be able to 'downgrade' the version of VPN Server to older version which has released before the end of the subscription. If you want to downgrade the version, older versions might be available on http://selinks.org/.
ERR_130	We are afraid that the trial license keys cannot be obtained frequently by the same customer. Please consider to purchase the product version.
ERR_131	Several VPN Servers on the same IP address. You can specify the destination server's private IP or hostname concretely such as "Global IP address or host name/192.168.x.x". Or if a NAT is used on the server's side, configure the NAT to open, relay or transfer appropriate ports.
ERR_132	The key for Dynamic DNS Service duplicates to others. The key will be reset automatically.
ERR_133	The specified Dynamic DNS hostname is already used. Please change the hostname.
ERR_134	The specified Dynamic DNS hostname has an invalid characters. Please change the hostname.
ERR_135	The length of the specified Dynamic DNS hostname is too long. A hostname must be equal or shorter than 31 letters.
ERR_136	O nome do host de DNS dinâmico não está especificado.
ERR_137	The length of the specified Dynamic DNS hostname is too long. A hostname must be equal of longer than 3 letters.
ERR_138	The password of the specified user in the Virtual Hub must be reset before using MS-CHAP v2 authentication. Please ask the administrator of the VPN Server to reset the password by the VPN Server Manager or vpncmd which internal version is 4.0 or greater. Or you can change the password with VPN Client by yourself.
ERR_139	The connection to the Dynamic DNS server has been disconnected.
ERR_140	Failed to initialize the ICMP (Ping) protocol. The process of the VPN Server might be running in a normal-user privileges. In such case, run the VPN Server as a system service. (in Linux / UNIX, run it in root privileges.)
ERR_141	Failed to open the DNS port 53. Make sure that there are no other DNS server program (for example, BIND or Microsoft DNS Server) on the same computer. If there are conflicting services stop them. Or run the VPN Server's process in root privileges on Linux / UNIX/
ERR_142	The OpenVPN Server function is not enabled.
ERR_143	The Certificate Authentication function and the External Server Authentication function have not been implemented on the open-source version of SoftEther VPN yet. Choose either Anonymous Authentication or Password Authentication instead.
ERR_144	Unacceptable operation. Use the VPN Gate Control Panel to change the VPN Gate Relay Server settings.
ERR_145	Unacceptable operation. Use the VPN Gate Utility to modify the connection setting for VPN Gate Public VPN Relay Servers.
ERR_146	The VPN Gate Service is running inside the VPN Client program. You cannot stop the VPN Gate Service on this screen. Use the VPN Client Manager to enable or disable the VPN Gate Service.
ERR_147	This feature is not supported. It hasn't been implemented yet on the open-source version of SoftEther VPN.
ERR_148	The VPN connection was disconnected because the system is being suspended.
ERR_149	The destination VPN Server's certificate does not match the specified hostname.
ERR_150	Failed to find the TLS version that is supported by both sides. This usually means that one side may be using an obsolete TLS version which is diabled by the other side.
ERR_151	Failed to find an available cipher that is supported by both sides, or the cipher specified is not compatible with the server certificate.
ERR_152	TLS handshake has failed.


# Concerning licenses
LICENSE_INFO_URL	https://selinks.org/?new_license
LICENSE_SUPPORT_URL	https://selinks.org/?q=license_info&id=%s
LICENSE_STATUS_OK	Válido
LICENSE_STATUS_EXPIRED	Expirado
LICENSE_STATUS_ID_DIFF	Server ID Mismatch
LICENSE_STATUS_DUP	Duplicar
LICENSE_STATUS_INSUFFICIENT	Other Licenses are Required
LICENSE_STATUS_COMPETITION	Competition with Other Licenses
LICENSE_STATUS_NONSENSE	Meaningless for Current Edition
LICENSE_STATUS_CPU	CPU Type is Incompatible
LICENSE_STATUS_OTHERERROR	Erro desconhecido 


# Concerning TCP optimization
TCPOPT_NOT_SUPPORTED	The TCP Optimization Utility cannot be used on this operating system.
TCPOPT_NOT_ADMIN	Users without administrator privileges cannot use the TCP Optimization Utility.


# Windows Vista / Windows 7 / Windows 8 Optimization
VISTA_MMCSS_MSG	Do you wish to optimize Windows Vista / Windows 7 / Windows 8 / Windows 10 for playing multimedia files with VPN? (e.g. videos, audios and streaming)
VISTA_MMCSS_MSG_2	Optimization for Windows Vista / Windows 7 / Windows 8 / Windows 10 with VPN has already done.\r\nDo you wish to remove optimized configuration?
VISTA_MMCSS_MSG_3	You cannot use optimization in currently environment.
VISTA_MMCSS_MSG_4	You must have administrator privileges for this function.\r\nPlease note that in Windows Vista / Windows 7 / Windows 8 / Windows 10 you should use "Run as Administrators" to execute program.
VISTA_MMCSS_MSG_5	Otimização está finalizada.
VISTA_MMCSS_MSG_6	Optimization configuration is removed.


# Concerning PKCS utility
PKCS_UTIL_TITLE	PKCS#12 Writing Utility
PKCS_UTIL_SAVEDLG_TITLE	Select the PKCS#12 file that you want to write to the USB token.
PKCS_UTIL_READ_ERROR	Unable to read the file: %s.
PKCS_UTIL_WRITE_OK_MSG	The file %s has been written to the USB hardware token.
PKCS_UTIL_DELETE_OK_MSG	The PKCS#12 certificate data has been deleted from the USB hardware token.
PKCS_UTIL_SECA_FILENAME	seca_p12
PKCS_MAKE_SURE	The PKCS#12 certificate data written to USB token will be deleted. \r\n Once data is deleted it cannot be restored. \r\r\n\r\r\nDo you wish to continue?
PKCS_UTIL_BAD_FILE	The specified file could not be identified as a PKCS#12 file.


# Concerning common dialogs
DLG_ALL_FILES	All Files (*.*)|*.*
DLG_CERT_FILES	X509 Certificate Files (*.CER;*.CRT)|*.cer;*.crt|All Files (*.*)|*.*
DLG_KEY_FILTER	Private Key Files (*.KEY;*.PEM)|*.key;*.pem|All Files (*.*)|*.*
DLG_PKCS12_FILTER	PKCS#12 Files (*.P12;*.PFX)|*.p12;*.pfx|All Files (*.*)|*.*
DLG_CERT_OR_P12_FILTER	X509 Certificate Files or PKCS#12 Files (*.CER;*.CRT;*.P12;*.PFX)|*.cer;*.crt;*.p12;*.pfx|X509 Certificate Files (*.CER;*.CRT)|*.cer;*.crt|PKCS#12 Files (*.P12;*.PFX)|*.p12;*.pfx|All Files (*.*)|*.*
DLG_CONFIG_FILES	Setting Files (*.CONFIG)|*.config|All Files (*.*)|*.*
DLG_KEY_OR_P12_FILTER	Private Key Files or PKCS#12 Files (*.KEY;*.PEM;*.P12;*.PFX)|*.key;*.pem;*.p12;*.pfx|Private Key Files (*.KEY;*.PEM)|*.key;*.pem|PKCS#12 Files (*.P12;*.PFX)|*.p12;*.pfx|All Files (*.*)|*.*
DLG_ZIP_FILER	Arquivos ZIP (*.ZIP)|*.zip|Todos os arquivos (*.*)|*.*
DLG_OPEN_CERT	Select the Certificate File
DLG_OPEN_KEY	Select the Private Key File
DLG_OPEN_KEY_WITH_CERT	Select the Corresponding Private Key file
DLG_OPEN_FILE_ERROR	Unable to read the specified file: %S.
DLG_OPEN_FILE_ERROR_W	Unable to read the specified file: %s.
DLG_BAD_P12	The file "%S" is not a valid PKCS#12 certificate file.
DLG_BAD_P12_W	The file "%s" is not a valid PKCS#12 certificate file.
DLG_BAD_X509	The file "%S" is not a valid X509 certificate file.
DLG_BAD_X509_W	The file "%s" is not a valid X509 certificate file.
DLG_BAD_KEY	The file "%S" is not a valid RSA private key file.
DLG_BAD_KEY_W	The file "%s" is not a valid RSA private key file.
DLG_BAD_SIGNATURE	The private key does not correctly correspond with the public key contained in the specified certificate. \r\nA private key that corresponds to the certificate public key is required.
DLG_SAVE_CERT	Specify a file name where you want to save the certificate
DLG_SAVE_KEY	Specify a file name where you want to save the private key
DLG_SAVE_P12	Specify a file name where you want to save the certificate and private key
DLG_SAVE_FILE	Specify a file name to save a file
DLG_SAVE_OPENVPN_CONFIG	Specify a file name to save the ZIP file contains OpenVPN settings
DLG_CERT_SAVE_OK	The certificate has been saved successfully.
DLG_CERT_SAVE_ERROR	Unable to save certificate.
DLG_KEY_SAVE_OK	The private key has been saved successfully.
DLG_KEY_SAVE_ERROR	Unable to save private key.
DLG_KEY_PAIR_SAVE_OK	The certificate and private key were saved successfully.
DLG_KEY_PAIR_SAVE_ERROR	Unable to save the certificate and private key.
DLG_REBOOT_INFO	The computer will restart after %u seconds.
DLG_REBOOT_INFO_2	Restarting the computer.
DLG_REBOOT_ERROR	Failed to restart the computer. \r\n\r\nPlease manually restart the computer now. 
DLG_SAVE_CONFIG	Specify a File Name for Saving the Configuration
DLG_OPEN_CONFIG	Specify the Configuration File to Import
DLG_STRING_DEFTITLE	String Input
DLG_STRING_DEFINFO	Enter strings.
DLG_ABOUT_LEGAL	Informações legais
DLG_ABOUT_AUTHORS	List of Authors
DLG_UPDATE_DATE	\ (Released on %S)
DLG_UPDATE_HINT	Press OK to view the information of the latest update on the web browser.\r\n\r\nYou have to download and install updates manually. If you want to update software on the other computer you have to log in to the computer by Remote Desktop or SSH to perform the download and update.


# Concerning competing processes
BAD_PROCESS_TITLE	Warning concerning %S
BAD_PROCESS_MESSAGE	It is possible that the software "%S" is running on this computer, which could cause problems. \r\n\r\nThere is a possibility that problems in "%S" will cause instability in VPN communication and errors. \r\n\r\nIf, by using VPN together with the software "%S" VPN becomes unstable, either stop or uninstall "%S". (Note that in some cases, because of the nature of the software, there are cases that the problems will still remain on the computer where even if you stop the software.) \r\n


# Concerning hardware tokens
SEC_SMART_CARD	Smart Card
SEC_USB_TOKEN	Token USB
SEC_INIT_MSG_1	Insert the following smart card into the smart card reader and enter the PIN code.
SEC_INIT_MSG_2	Connect the following USB token hardware to the computer's USB port and enter the PIN code.
SEC_OPENING	Opening Device...
SEC_CLOSING	Closing Device...
SEC_OPEN_SESSION	Opening Secure Session...
SEC_CLOSE_SESSION	Closing Secure Session...
SEC_LOGIN	Logging in to Token...
SEC_LOGOUT	Logging out from Token...
SEC_INIT_BATCH	Starting Batch Process...
SEC_READ_DATA	Reading Data...
SEC_WRITE_DATA	Writing Data...
SEC_READ_CERT	Reading Certificate...
SEC_WRITE_CERT	Writing Certificate...
SEC_DELETE	Deleting Object...
SEC_SIGN	Processing Digital Signature by Private Key...
SEC_WRITE_KEY	Writing Private Key...
SEC_ENUM	Enumerating Object...
SEC_FINISHED	The operation is complete.
SEC_ERROR_INVALID_ID	The specified security device (device %u) is invalid.
SEC_ERROR_OPEN_DEVICE	Unable to open the device %S. Make sure the device is connected to the computer.
SEC_ERROR_OPEN_DEVICEEX	Unable to open the device %S. Make sure the device is connected to the computer. \r\n\r\nIf using public key infrastructure (PKI) with special client software, it is necessary to select the smart card device in PKI Utility from the Start menu beforehand.
SEC_ERROR_OPEN_SESSION	Unable to start security session in device: %S. Make sure the correct device is selected.
SEC_ERROR_LOGIN	The entered PIN code is incorrect.
SEC_ERROR_NOT_FOUND_1	The specified object does not exist in smart card. Make sure the correct smart card is inserted.
SEC_ERROR_NOT_FOUND_2	The specified object does not exist in USB token hardware. Make sure the correct USB token hardware is connected.
SEC_ERROR_SIGN_1	Either private key does not exist in smart card or digital signature operation failed. Make sure the correct smart card is inserted.
SEC_ERROR_SIGN_2	Either private key does not exist in USB token hardware or digital signature operation failed. Make sure the correct USB token hardware is connected.
SEC_ERROR_WRITE_1	Unable to write object to smart card. There is a possibility that there is insufficient free memory available on smart card.
SEC_ERROR_WRITE_2	Unable to write object to USB token hardware. There is a possibility that is insufficient free memory available on the USB token.
SEC_ERROR_ENUM	Enumeration of object stored in token failed.
SEC_ERROR_DELETE	Deletion of specified object failed. It is possible the specified object does not exist in the memory.
SEC_COLUMN1	Nome do dispositivo
SEC_COLUMN2	Tipo
SEC_COLUMN3	Fabricante
SEC_COLUMN4	Nome DLL
SEC_INVALID_ID	The specified smart card device does not exist. Select the smart card type again.
SEC_MGR_COLUMN1	Nome
SEC_MGR_COLUMN2	Tipo
SEC_MGR_COLUMN3	Privado
SEC_TYPE_DATA	Dado
SEC_TYPE_CERT	Certificado
SEC_TYPE_KEY	Chave privada
SEC_TYPE_PUB	Chave pública
SEC_YES	Sim
SEC_NO	Não
SEC_NONE	Nenhum
SEC_IMPORT_DATA	Select the data you want to import.
SEC_IMPORT_CERT	Select the certificate you want to import.
SEC_IMPORT_KEY	Select the private key you want to import.
SEC_READ_FAILED	Reading from specified file failed.
SEC_DATA_TOO_BIG	The specified data size is too big. Data larger than %u bytes cannot be written to the smart card.
SEC_OBJECT_NAME_TITLE	Name of object to insert
SEC_OBJECT_NAME_INFO	Specify the name of the object to be written to the new smart card. You can specify alphanumeric characters excluding double-byte and special characters for the object name. \r\n\r\nCaution: If there is an object with the same name of the same type already written on the card, that object will be overwritten.
SEC_DELETE_MSG	The selected object will be deleted from the smart card. \r\nDo you really want to do this?
SEC_OBJECT_IMPORT_OK	Object has been written to smart card.
SEC_OBJECT_EXPORT_OK	The data read from the smart card has been saved.
SEC_NEW_CERT_IMPORT_OK	The newly created certificate has been written to the smart card.
SEC_CURRENT_DEVICE	Currently the device %S is selected.
SEC_CURRENT_NO_DEVICE	Select which smart card device to use. 
SEC_NO_SECURE_DEVICE	A SoftEther VPN-compatible smart card or hardware security token device is not installed on the system. \r\n\r\nTo use a smart card or hardware token using SoftEther VPN it is necessary to install a PKCS#11-compatible device driver on Windows. In addition, it is necessary that SoftEther VPN supports the device type. \r\n\r\nMake sure a system-compatible device driver has been installed. \r\nRefer to the SoftEther VPN Project website for the list of SoftEther VPN-compatible devices. Also, it may be possible to increase the compatible devices by updating to the most recent software version.
SEC_PIN_DEVICE_OPEN_ERR	Unable to connect the device "%S". Make sure the hardware is correctly connected.
SEC_PIN_CURRENT_BAD	Current PIN code is incorrect.
SEC_PIN_CHANGE_FAILED	Changing of PIN code failed.
SEC_PIN_OK	The PIN code has been changed.


# TCP Connection Dialog
CONNECTDLG_CAPTION	Conectando
CONNECTDLG_MESSAGE	Conectando ao servidor "%S" (Porta TPC: %u)...
CONNECTDLG_CANCELING	Aborting the connection. Please wait...


# NIC Info Dialog
NICINFO_1	Connected to the VPN Server.
NICINFO_1_1	Requesting an IP address to the DHCP server in the VPN...
NICINFO_1_2	Determining the IP address to use in the VPN...
NICINFO_2	A conexão VPN foi estabelecida.
NICINFO_2_1	O endereço de IP atribuído a você é %S.
NICINFO_3	A conexão VPN foi estabelecida.
NICINFO_3_1	Seu endereço de IP %S está pronto para o uso.


# Concerning password input dialogs during login
PW_RETRYCOUNT	Automatic reconnection will be made after %u seconds with no input.
PW_LOGIN_DLG_TITLE	Login
PW_TYPE_0	Anônima
PW_TYPE_1	Autenticação de senha padrão
PW_TYPE_2	Autenticação de Domínio RADIUS ou NT
PW_TYPE_3	Certificado do cliente
PW_TYPE_4	Autenticação Smart Card
PW_TYPE_5				OpenSSL Engine Authentication
PW_MSG_PROXY	User authentication failed on the proxy server %S. Re-enter the correct user name and password.
PW_TYPE_PROXY	Proxy Server Authentication


# Concerning VPN connection status
STATUS_1	Inicializando...
STATUS_2	Conectando ao servidor VPN "%S" via servidor proxy %S...
STATUS_3	Authenticating User on Proxy Server %S...
STATUS_4	Conectando ao servidor VPN "%S"...
STATUS_5	Verifying Server Certificate...
STATUS_6	Authenticating User...
STATUS_7	Establishing VPN Session...
STATUS_8	Connecting to VPN Server on Cluster...
STATUS_9	VPN Session has been established.


# Concerning certificate dialogs
CERT_NOT_FOUND	Unable to find the certificate of the certificate authority who issued this certificate on the list of trusted certificates.
CERT_ROOT	This certificate is a root certificate (self-signed certificate). 
CERT_LV_C1	Campo
CERT_LV_C2	Valor
CERT_SERIAL	Número serial
CERT_ISSUER	Emissor
CERT_SUBJECT	Assunto
CERT_NOT_BEFORE	Emitido em
CERT_NOT_AFTER	Expira às
CERT_BITS	Bits
CERT_PUBLIC_KEY	Chave pública
CERT_DIGEST_MD5	Resumo (MD5)
CERT_DIGEST_SHA1	Resumo (SHA-1)
CERT_NO_SERIAL	There is no serial number
CERT_BITS_FORMAT	%u bits
CERT_KEY_ALGORITHM		Public Key Algorithm
CERT_KEY_PARAMETER		Parameters


# Concerning certificate confirmation dialogs
CC_DANGEROUS_MSG	The server certificate that was saved on the previous VPN connection to this server (%S) does not match the current server certificate provided by the server. \r\n\r\nDigest Value (MD5) of Previous: %S\r\nDigest Value (SHA1) of Previous: %S\r\n\r\nDigest Value (MD5) of Current: %S\r\nDigest Value (SHA1) of Current: %S\r\n\r\nIt is possible the server administrator changed the certificate on the VPN Server side. However, it is also possible a man-in-the-middle attack such as spoofing is occurring. \r\nIt is strongly recommended that you ask for clarification from the administrator of VPN Server you want to connect to.
CC_WARNING_MSG	Do you want the certificate of the VPN Server you are currently connecting to be automatically trusted next time you connect to %s?\r\n\r\nDigest Value (SHA1): %S\r\nDigest Value (MD5): %S\r\n\r\nIf there is doubt regarding the authenticity of this server's certificate, contact the server's owner, by a sure and safe method, and quote the above digest value to confirm the facts. \r\n\r\nClick Yes to automatically trust this certificate if this server provides the same certificate next time you connect to it. \r\nClick No to trust the certificate for this time only and to display this warning again next time you connect to this server. \r\nClick Cancel to return to the Security Warnings window. \r\n\r\nNote: This setting can be changed on an account-by-account basis. You can make this setting in Account Properties of VPN Client Manager.


# Errors about Windows Versions
WINVER_TITLE	Warning about Windows versions
WINVER_ERROR_FORMAT	The version and Service Pack of Windows on %s is "%S".\r\n\r\nThe latest supported version and Service Pack of Windows by %s is as follows:\r\n%S\r\nBecause of the version of Windows on %s is newer than the version of Windows which %s supports, unexpected troubles or compatible issues might occur.\r\nIn order to avoid problems, we will recommend you to obtain and install the latest update of %s.\r\n(It is possible to continue using the current version without updates although that is not what we recommend.)\r\n\r\nIf you are the administrator, you can download the latest update-patch of %s from the web site http://selinks.org/?se for free.\r\n\r\nIf you are not the administrator you should notify the VPN Server's administrator of this message.\r\n\r\n----- MSG%04u%02u -----\r\n\r\n
WINVER_ERROR_VPNSERVER	the VPN Server on the destination computer
WINVER_ERROR_VPNBRIDGE	the VPN Bridge on the destination computer
WINVER_ERROR_VPNCLIENT	the VPN Client on this local computer
WINVER_ERROR_PC_LOCAL	this local computer
WINVER_ERROR_PC_REMOTE	the remote server


# Warning for Open-source Version
OSS_MSG	Welcome to the SoftEther VPN Server Academic Version!\r\n\r\n\r\nThis VPN Server is open-source free software developed as academic research at University of Tsukuba, Japan, and distributed from the SoftEther VPN Project (http://www.softether.org/), for free of charge for the public interests.\r\n\r\nSoftEther VPN software is distributed to public as a part of the joint-research contract between University of Tsukuba and SoftEther VPN Project. SoftEther VPN software is developed and published for JUST AN ACADEMIC RESEARCH PURPOSE. Therefore no support service are provided about SoftEther VPN software even if it contains bugs or vulnerabilities. A user will be liable for the result of use SoftEther VPN. The developers and publishers of SoftEther VPN will never be liable for either any consequences or damages.\r\n\r\nEnjoy using VPN with SoftEther VPN Server.\r\n\r\nFor more details of SoftEther VPN, visit http://www.softether.org/.\r\n\r\n
NATT_MSG	** Connected with NAT traversal - might be unstable **\r\n\r\nThis VPN Client is connected to the VPN Server '%S' by using the NAT Traversal (UDP Hole Punching) technology.\r\n\r\nNAT Traversal allows the VPN Server behind the NAT-box to accept VPN connections from VPN Client without any port-forwarding setting on the NAT-box.\r\n\r\nHowever, NAT Traversal-based VPN sessions sometimes become unstable, because NAT Traversal uses UDP-based protocol. For example, the VPN tunnel disconnects every 5 minutes if there is a poor NAT-box between the VPN Server and the VPN Client. Some large-scale NAT gateways in cheap ISPs sometimes cause the same problem on NAT Traversal. This is a problem of routers or ISPs. This is not a problem of SoftEther VPN software.\r\n\r\nTo solve the unstable tunnel problem, you should connect to the VPN Server's TCP listener port directly, instead of using NAT Traversal. To connect to the VPN Server directly by using TCP, a listener port of the VPN Server must be exposed to the Internet by a port-forward setting on the NAT-box. Ask the administrator of the NAT-box, or refer to the manual of the NAT-box to add a port-forwarding setting on the NAT-box.\r\n\r\nIf this message still remains despite the VPN Server is exposing a TCP port to the Internet, check the "Disable NAT-T" checkbox on the VPN Client connection setting screen.\r\n\r\n


# Virtual HUB Admin Options
HUB_AO_CLICK	Select an item to view the description here.
HUB_AO_UNKNOWN	The description of the item was not found. Refer to the documents, or speculate the meaning and purpose of the item from the name of the item.
HUB_AO_allow_hub_admin_change_option	This is a special item. If you are enable (set to 1) this option, then not only the VPN Server's global administrator but also the Virtual Hub's administrator will be granted to modify the Virtual Hub Admin Options by himself.
HUB_AO_deny_hub_admin_change_ext_option	If you are enable (set to 1) this option, the Virtual Hub's administrator will be forbidden to modify any values on the Virtual Hub Extended Options, then only the VPN Server's global administrator can modify them.
HUB_AO_no_delay_jitter_packet_loss	If you set this option to non-zero value, then all parameters of delay, jitter and packet-loss on the access-list entry will be ignored even if these parameters are set when the administrator adds a new access list entry. Therefore, delay, jitter and packet-loss generating function will be virtually disabled. Because of the delay generating function sometimes make a high volume of load on the CPU and RAM, a Virtual Hub which is shared by several users should have this option enabled.
HUB_AO_max_users	If you set this option to non-zero value, the maximum number of user objects registered on the Virtual Hub will be limited to this value, then greater number of user objects than this value cannot be added.
HUB_AO_max_multilogins_per_user	If you set this option to non-zero value, the maximum number of VPN Sessions per an individual user object will be limited to this value, then greater number of VPN Sessions of individual user object than this value cannot be established.
HUB_AO_max_groups	If you set this option to non-zero value, then the maximum number of group objects on the Virtual Hub will be limited to this value and any more groups will not be allowed to be registered.
HUB_AO_max_accesslists	If you set this option to non-zero value, then the maximum number of access list entries on the Virtual Hub will be limited to this value and any more entries will not be allowed to be registered.
HUB_AO_max_sessions_client_bridge_apply	Only when this value is set to non-zero value, the values max_sessions_client and max_sessions_bridge will be applied.
HUB_AO_max_sessions	If you set this option to non-zero value, then the maximum number of VPN Sessions will be limited to this value.
HUB_AO_max_sessions_client	If you set this option to non-zero value, then the maximum number of VPN Client sessions will be limited to this value. No more VPN Client sessions will be allowed to establish. This option is valid only when the max_sessions_client_bridge_apply option is set to non-zero value.
HUB_AO_max_sessions_bridge	If you set this option to non-zero value, then the maximum number of VPN Bridge sessions will be limited to this value. No more VPN Bridge sessions will be allowed to establish. This option is valid only when the max_sessions_client_bridge_apply option is set to non-zero value.
HUB_AO_max_bitrates_download	If you set this option to non-zero value, then all VPN Sessions on the Virtual Hub will be mandated to have a security policy setting which the "Download Bandwidth" value is set to this value. It will limit the downloading traffic speed of each VPN Session. For example, if this value is set to 1000000, then a downloading bandwidth of each VPN Session on the Virtual Hub will be limited to 1Mbps.
HUB_AO_max_bitrates_upload	If you set this option to non-zero value, then all VPN Sessions on the Virtual Hub will be mandated to have a security policy setting which the "Download Bandwidth" value is set to this value. It will limit the uploading traffic speed of each VPN Session. For example, if this value is set to 1000000, then a uploading bandwidth of each VPN Session on the Virtual Hub will be limited to 1Mbps.
HUB_AO_deny_empty_password	If you set this option to non-zero value, no user objects will be able to have an empty password. A user who has an empty password will be forbidden to connect a VPN Session. (Exception: a VPN connection from localhost will be permitted even if the password is empty.)
HUB_AO_deny_bridge	If you set this option to non-zero value, then any VPN Sessions in Bridge Mode will not be granted to establish, regardless of the setting of existing security policy of the user. No one will be able to connect to the Virtual Hub for bridging purpose.
HUB_AO_deny_routing	If you set this option to non-zero value, then any VPN Sessions in Routing Mode will not be granted to establish, regardless of the setting of existing security policy of the user. No one will be able to connect to the Virtual Hub for routing purpose.
HUB_AO_deny_qos	If you set this option to non-zero value, then every VPN Sessions will be enforced to disable the QoS function regardless of the setting of existing security policy of the user.
HUB_AO_deny_change_user_password	If you set this option to non-zero value, then any users on the Virtual Hub will be forbidden to change its password by VPN Client's password-changing function.
HUB_AO_no_change_users	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to add, edit or remove a user.
HUB_AO_no_change_groups	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to add, edit or remove a group.
HUB_AO_no_securenat	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to enable or disable the SecureNAT function.
HUB_AO_no_securenat_enablenat	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to enable or disable the Virtual NAT function in the SecureNAT function.
HUB_AO_no_securenat_enabledhcp	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to enable or disable the Virtual DHCP Server function in the SecureNAT function.
HUB_AO_no_cascade	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to add, edit, remove or change the online status of a cascade connection.
HUB_AO_no_online	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to change the offline Virtual Hub to the online state.
HUB_AO_no_offline	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to change the online Virtual Hub to the offline state.
HUB_AO_no_change_log_config	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to change the settings of logging function.
HUB_AO_no_disconnect_session	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to disconnect a specific VPN Session.
HUB_AO_no_delete_iptable	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to delete a specific IP address entry from the IP address table database.
HUB_AO_no_delete_mactable	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to delete a specific MAC address entry from the MAC address table database.
HUB_AO_no_enum_session	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to enumerate the sessions on the Virtual Hub.
HUB_AO_no_query_session	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to specify a session and get the information of the session.
HUB_AO_no_change_admin_password	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to change the administrator's password of the Virtual Hub.
HUB_AO_no_change_log_switch_type	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to change the Log Switching settings on the logging function settings of the Virtual Hub.
HUB_AO_no_change_access_list	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to modify the access list of the Virtual Hub.
HUB_AO_no_change_access_control_list	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to modify the source IP address limit list of the Virtual Hub.
HUB_AO_no_change_cert_list	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to modify the trusted certificate authority list of the Virtual Hub.
HUB_AO_no_change_crl_list	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to modify the certificate revoked list of the Virtual Hub.
HUB_AO_no_read_log_file	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to enumerate or download the log files of the Virtual Hub remotely.
HUB_AO_no_change_msg	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to change the message which should be displayed when a VPN Client connects to the Virtual Hub.
HUB_AO_no_access_list_include_file	If you set this option to non-zero value, then the administrator of the Virtual HUB will be forbidden to specify "include:" or "exclude:" instruction as a source or a destination user field on a access list entry of the Virtual Hub.


# Virtual Hub Extended Options
HUB_AO_NoAddressPollingIPv4	If you set this option to non-zero value, then the Virtual Hub will not perform the maintenance of the IPv4 address table and the MAC address table on the hub with using sending ARP packets per 5 seconds in order to check keep-alive IPv4 devices. As a result, IPv4 devices might be deleted on the IPv4 address table and MAC address table after a particular period (from 1 to 10 minutes) will be elapsed in the case of no-communication activities via the Virtual Hub, even if it is still alive. This option can eliminate the amount of broadcast packets, however some IPv4-related security policies will not work effectively.
HUB_AO_NoAddressPollingIPv6	If you set this option to non-zero value, then the Virtual Hub will not perform the maintenance of the IPv6 address table and the MAC address table on the hub with using sending ICMPv6 packets per 5 seconds in order to check keep-alive IPv6 devices. As a result, IPv6 devices might be deleted on the IPv6 address table and MAC address table after a particular period (from 1 to 10 minutes) will be elapsed in the case of no-communication activities via the Virtual Hub, even if it is still alive. This option can eliminate the amount of broadcast packets, however some IPv6-related security policies will not work effectively.
HUB_AO_NoIpTable	If you set this option to non-zero value, then the Virtual Hub will not construct and maintain the internal IP address table. This option can eliminate the amount of CPU and RAM usages, however some IP-related security policies will not work effectively.
HUB_AO_NoMacAddressLog	If you set this option to non-zero value, then any logs which indicate the registration of a new MAC address to the MAC address table on the Virtual Hub will not be logged to the security log.
HUB_AO_ManageOnlyPrivateIP	If you set this option to non-zero value, then the IPv4 address table of the Virtual Hub will contain only private IPv4 addresses. In this context, the private IPv4 addresses are: 10.0.0.0/8, 172.16.0.0/12, 192.168.0.0/16 and 169.254.0.0/16. Any other IPv4 addresses will not added on the table.
HUB_AO_ManageOnlyLocalUnicastIPv6	If you set this option to non-zero value, then the IPv6 address table of the Virtual Hub will contain only local unicast IPv6 addresses. In this context, the private IPv6 addresses are: fe80::/10. Any other IPv6 addresses will not added on the table.
HUB_AO_DisableIPParsing	If you set this option to non-zero value, then the Virtual Hub will disable the internal parsing function of IP headers in all Ethernet packets. This option can eliminate the amount of CPU and RAM usages, however the Vitual Hub will not perform building and maintenance of the IP address table internally, and some IP-related security policies will not work effectively.
HUB_AO_YieldAfterStorePacket	If you set this option to non-zero value, then the Virtual Hub sets the CPU to idle state after store-forward processing of a packet. This might results good effects to make the delay of packets shorter, however the counts of thread context switch will be increased and the performance might decline.
HUB_AO_FilterPPPoE	If you set this option to non-zero value, then the Virtual Hub discards all PPPoE (PPP over Ethernet) packets. It is convenient to split each site's PPPoE segment when making a bridge between two or more local area networks.
HUB_AO_FilterOSPF	If you set this option to non-zero value, then the Virtual Hub discards all OSPF (Open Shortest Path First) packets.
HUB_AO_FilterIPv4	If you set this option to non-zero value, then the Virtual Hub discards all IPv4 and ARP packets.
HUB_AO_FilterIPv6	If you set this option to non-zero value, then the Virtual Hub discards all IPv6 packets.
HUB_AO_FilterNonIP	If you set this option to non-zero value, then the Virtual Hub discards all non-IP packets (non-IPv4, ARP or IPv6 packets). Incidentally, any tagged-VLAN packets via the Virtual Hub will be regarded as non-IP packets.
HUB_AO_FilterBPDU	If you set this option to non-zero value, then the Virtual Hub discards all BPDU (Bridge Protocol Data Unit) packets.
HUB_AO_NoIPv6DefaultRouterInRAWhenIPv6	If you set this option to non-zero value, then all VPN Sessions on the Virtual Hub will have the enabled "No Default-Router on IPv6 RA (physical IPv6)" security policy. When the physical communication protocol between VPN Client / VPN Bridge and VPN Server is IPv6, any IPv6 RA (Router Advertisement) packet with non-zero value in the router-lifetime will set to zero-value. This is effective to avoid the horrible behavior from the IPv6 routing confusion which is caused by the VPN client's attempts to use the remote-side IPv6 router as its local IPv6 router.
HUB_AO_NoLookBPDUBridgeId	If you set this option to non-zero value, then the Virtual Hub will ignore the source MAC field in a BPDU (Bridge Protocol Data Unit) packet. This value will be much more advanced. Do not modify it unless you are very ultra special expert of computer networking.
HUB_AO_NoManageVlanId	If you set this option to non-zero value, then the Virtual Hub will not use VLAN ID on the MAC address table. Any VLAN ID in tagged-VLAN packets will be ignored.
HUB_AO_VlanTypeId	Specify the Ethernet Type ID (TPID) of VLAN tags in decimal. The default value is 33024 (0x8100 in hex). This value will be much more advanced. Do not modify it unless you are very ultra special expert of computer networking.
HUB_AO_FixForDLinkBPDU	If you set this option to non-zero value, then the FixForDLinkBPDU option will be enabled. This value will be much more advanced. Do not modify it unless you are very ultra special expert of computer networking.
HUB_AO_NoIPv4PacketLog	If you set this option to non-zero value, then IPv4 packets via the Virtual Hub will not be logged.
HUB_AO_NoIPv6PacketLog	If you set this option to non-zero value, then IPv6 packets via the Virtual Hub will not be logged.
HUB_AO_NoSpinLockForPacketDelay	If you set this option to non-zero value, then the VPN Server will not use spin-lock mechanisms to simulate the delay of packets when the packet-delay generating function is applied to the packet. Instead, the timer interrupt by the operating system will be adopted. It will reduce the CPU time, however the resolution of generating delays will deteriorate.
HUB_AO_BroadcastStormDetectionThreshold	Specify the threshold to detect the broadcast storm per a second. When the number of broadcast packets from a particular VPN Session exceeded this threshold, packets will be regarded as broadcast storm and become subjects to be filtered. The default value (zero-value) is 32.
HUB_AO_ClientMinimumRequiredBuild	If you set this option to non-zero value, then the Virtual Hub will deny any access from VPN Client which has less build number than this value.
HUB_AO_RequiredClientId	If you set this option to non-zero value, then the Virtual Hub will deny any access from VPN Client which doesn't have the embedded "Client ID" value in the software.
HUB_AO_AdjustTcpMssValue	If you set this option to non-zero value, then the Virtual Hub will adjust MSS (Max Segment Size) values of headers of all TCP/IP packets not to exceed this value.
HUB_AO_DisableAdjustTcpMss	If you set this option to non-zero value, then any MSS (Max Segment Size) options on the Virtual Hub will be disabled. Even if the AdjustTcpMssValue option is specified, or a VPN Session is made by IPsec / L2TP / EtherIP / L2TPv3 Server Function, the adjustment of MSS will be disabled.
HUB_AO_NoDhcpPacketLogOutsideHub	If you set this option to non-zero value, then the Virtual Hub will not record non-related DHCP packets to the packet log. "Non-related DHCP packets" are DHCP packets which are not bound to any VPN Session on the Virtual Hub.
HUB_AO_DisableHttpParsing	If you set this option to non-zero value, then the Virtual Hub will not perform parsing HTTP headers in all HTTP packets. It will reduce the usage of CPU and RAM, however the HTTP access logs will not be recorded.
HUB_AO_DisableUdpAcceleration	If you set this option to non-zero value, then all UDP Acceleration Function will be disabled on the all VPN Sessions of the Virtual Hub.
HUB_AO_DisableUdpFilterForLocalBridgeNic	If you set this option to non-zero value, then the Virtual Hub disables the trouble-preventing filtering function to filter DHCP packets which might causes of network unstable. By default, a local bridge interface sometimes try to acquire an IP address from remote-side DHCP server, however such a behavior should infinite loop in the routing table. The filtering function can avoid such problems. This option can disable the filtering function.
HUB_AO_ApplyIPv4AccessListOnArpPacket	If you set this option to non-zero value, then the IPv4 access list entries will be applied on not only IPv4 packets but also ARP packets. It is convenient to filter unnecessary ARP packets which might cause troubles.
HUB_AO_RemoveDefGwOnDhcpForLocalhost	If you set this option to non-zero value, when a VPN Client on the localhost connects to the Virtual Hub and try to acquire an IP address from the DHCP Server in the segment of the Virtual Hub, corresponding DHCP reply packets will be discarded. It can prevent unexpected infinite loop of packets routing.
HUB_AO_SecureNAT_MaxTcpSessionsPerIp	If you set this option to non-zero value, then the number of TCP connections (which is not SYN_SENT) per IP state will be limited to this value.
HUB_AO_SecureNAT_MaxTcpSynSentPerIp	If you set this option to non-zero value, then the number of TCP connections (which is SYN_SENT) per IP state will be limited to this value.
HUB_AO_SecureNAT_MaxUdpSessionsPerIp	If you set this option to non-zero value, then the number of UDP sessions per IP state will be limited to this value.
HUB_AO_SecureNAT_MaxDnsSessionsPerIp	If you set this option to non-zero value, then the number of DNS sessions per IP which is not SYN_SENT state will be limited to this value.
HUB_AO_SecureNAT_MaxIcmpSessionsPerIp	If you set this option to non-zero value, then the number of ICMP sessions per IP which is not SYN_SENT state will be limited to this value.
HUB_AO_AccessListIncludeFileCacheLifetime	Specify a period in seconds to hold the cache of external user-list files which is for an access list entry which has "include:" or "exclude:" formats as its username.
HUB_AO_DisableKernelModeSecureNAT	If you set this option to non-zero value, then the Kernel-mode NAT function on the SecureNAT function will be disabled. Kernel-mode NAT is a function to accelerate the performance of the Virtual NAT function on SecureNAT. Kernel-mode NAT can work only when the VPN Server process is running with system privileges (i.e. root, SYSTEM or Administrators contexts.). If the Kernel-mode NAT causes something wrong operations, use this option to disable it.
HUB_AO_DisableUserModeSecureNAT	If you set this option to non-zero value, then the User-mode NAT function on the SecureNAT function will be disabled. User-mode NAT is a function to make the NAT possible to run as normal-user privileges.
HUB_AO_DisableCheckMacOnLocalBridge	If you set this option to non-zero value, the MAC address duplication check will be disabled on the Local Bridge function. There might be a case when some network adapters has a problem that reflects outgoing packets towards the Virtual Hub. A Virtual HUB detects such duplications automatically, and discards them. Enable this flag to disable the detection and discarding.
HUB_AO_DisableCorrectIpOffloadChecksum	If you set this option to non-zero value, then the checking and correction of IP check-sum value on the Local Bridge function. Some network adapters, which have IP, TCP or UDP header check-sum offloading engines, transmit packets with incomplete check-sum values. Such packets cannot be treated correctly by receiver-side. So the Local Bridge detects such packets and corrects its check-sum fields. Enable this flag to disable such correction.
HUB_AO_BroadcastLimiterStrictMode	If you set this option to non-zero value, then the broadcast-storm detection algorithm will compare either source or destination IP address of each packet. If any of the two fields matches, the packet will be recorded on the short-term history of broadcast-storm detection state machine.
HUB_AO_MaxLoggedPacketsPerMinute	Maximum number of logging target packets per minute.
HUB_AO_DoNotSaveHeavySecurityLogs	Do not take heavy security log.
HUB_AO_DropBroadcastsInPrivacyFilterMode	Drop broadcasting packets if the both source and destination session is PrivacyFilter mode.
HUB_AO_DropArpInPrivacyFilterMode	Drop ARP packets if the both source and destination session is PrivacyFilter mode.
HUB_AO_AllowSameUserInPrivacyFilterMode			Allow packets if both the source and destination session users are the same, even in PrivacyFilter mode.
HUB_AO_SuppressClientUpdateNotification	Suppress the update notification screen on the VPN Client.
HUB_AO_FloodingSendQueueBufferQuota	Specify the quota limitation value (in bytes) of the sending queue buffer size which the flooding operation on the Virtual Hub can consume. The quota value is applied on the total length of sending queues of all active VPN sessions. Specify '0' to disable the quota. This option is effective to solve the out-of-memory problem on the network where there are many flooding packets.
HUB_AO_AssignVLanIdByRadiusAttribute	Enable the VLAN ID dynamic assignment function. Each VPN session will be assigned its own VLAN ID by the RADIUS attribute value when the user is authenticated by the external RADIUS server unless the user object has a VLAN ID security policy. The RADIUS attribute with the name "Tunnel-Pvt-Group-ID" (ID = 81) will be used as the VLAN ID. The data type must be STRING.
HUB_AO_DenyAllRadiusLoginWithNoVlanAssign	If you set this option to non-zero value, then all users, which RADIUS server returns no "Tunnel-Pvt-Group-ID" (ID = 81) value, will be denied to connect to the Virtual Hub. (Only if the values of AssignVLanIdByRadiusAttribute is non-zero value.)
HUB_AO_SecureNAT_RandomizeAssignIp	If you set this option to non-zero value, then the Virtual DHCP Server of the SecureNAT function will choose an unused IP address randomly from the DHCP pool while the default behavior is to choose the first unused IP address.
HUB_AO_DetectDormantSessionInterval	If you set this option to non-zero value, then the Virtual Hub will treat the VPN sessions, which have transmitted no packets for the last specified intervals (in seconds), as Dormant Sessions. The Virtual Hub will not flood packets, which should be flood, to any Dormant Sessions.
HUB_AO_NoPhysicalIPOnPacketLog	If you set this option to non-zero value, then the physical IP addresses of VPN clients of either the source VPN session or the destination VPN session will not be recorded on the packet log file.
HUB_AO_UseHubNameAsDhcpUserClassOption	If you set this option to non-zero value, then the Virtual Hub Name will be added to a DHCP request to an external DHCP server as the "User-Class" option. This allows to use separate pools of IP addresses for each Virtual Hub. (For only L2TP/IPsec and OpenVPN sessions.)
HUB_AO_UseHubNameAsRadiusNasId	If you set this option to non-zero value, then the NAS-Identifier RADIUS attribute will be set to a name of the Virtual Hub. This allows to determine on RADIUS server whether access to the Virtual Hub should be granted or denied.
HUB_AO_AllowEapMatchUserByCert	If you enable (set to 1) this option, the Virtual Hub will attempt to match the EAP Identity not only with usernames, but also with user certificates during the PPP EAP authentication flow.


# Concerning failed connection dialogs
ERRDLG_ERRMSG	Erro (Código de erro %u):\r\n%s\r\n
ERRDLG_RETRYCOUNT	Uma reconexão automática será feita após %u segundos...
ERRDLG_INFORMATION	Click Retry to start connecting again.
ERRDLG_RETRY_INFO_1	Você quer tentar novamente? (%u tentativa / %u tentativas)
ERRDLG_RETRY_INFO_2	Você quer tentar novamente? (%u tentativa / infinitas)
ERRDLG_DISCONNECTED_MSG	Connection to VPN Server "%S" has been disconnected.
ERRDLG_DEVICE_ERROR	The connection with the VPN Server has been disconnected because the Virtual Network Adapter (device name: %S) has been stopped. \r\n\r\nError code %u: %s


# Concerning protocols
PROTO_DIRECT_TCP	Conexão TPC/IP direta
PROTO_HTTP_PROXY	Conectar via proxy HTTP
PROTO_SOCKS_PROXY	Conectar via proxy SOCKS4 Proxy
PROTO_SOCKS5_PROXY	Conectar via proxy SOCKS5 Proxy
PROTO_SSH	Connection via SSH Server
PROTO_UNKNOWN	Unknown Protocol


# Concerning caps


# (Control characters)
CAPS_YES	Sim
CAPS_NO	Não


# (Title)
CT_i_max_packet_size	Maximum Ethernet Packet Size
CT_i_max_hubs	Maximum Virtual Hubs
CT_i_max_user_creation	Máximo de usuários em todo o servidor VPN
CT_i_max_sessions	Maximum Total Sessions
CT_i_max_clients	Maximum Client Sessions
CT_i_max_bridges	Maximum Bridge Sessions
CT_i_max_users_per_hub	Maximum Users per Virtual Hub
CT_i_max_groups_per_hub	Maximum Groups per Virtual Hub
CT_i_max_access_lists	Maximum Access Lists per Virtual Hub
CT_i_max_mac_tables	Maximum MAC Address Entries per Virtual Hub
CT_i_max_ip_tables	Maximum IP Address Entries per Virtual Hub
CT_i_max_secnat_tables	Maximum SecureNAT Entries per Virtual Hub
CT_i_max_l3_sw	Maximum Virtual Layer 3 Switches
CT_i_max_l3_if	Maximum Virtual Interfaces per Layer 3 Switch
CT_i_max_l3_table	Maximum Routing Tables per Layer 3 Switch
CT_b_bridge	Works as VPN Bridge Software
CT_b_standalone	Standalone Mode
CT_b_cluster_controller	Cluster Controller Mode
CT_b_cluster_member	Cluster Member Mode
CT_b_vpn_client_connect	Accepting Connection from VPN Client / Bridge
CT_b_local_bridge	Local Bridge is Supported
CT_b_must_install_pcap	Packet Capture Driver is Not Installed
CT_b_tap_supported	Tun/Tap Device is Supported (only in Linux)
CT_b_support_config_hub	Changing Virtual Hub Settings is Supported
CT_b_support_securenat	SecureNAT is Supported
CT_b_virtual_nat_disabled	Virtual NAT is Disabled (only DHCP Enabled)
CT_b_support_cascade	Cascade Connection is Supported
CT_b_support_cascade_cert	Server Authentication for Cascade Connection is Supported
CT_b_support_config_log	Changing Settings for Saving Log is Supported
CT_b_support_autodelete	Automatic Deletion of Log Files is Supported
CT_b_support_radius	External Authentication Server is Supported
CT_b_support_config_rw	Remote Reading and Writing of Config File is Supported
CT_b_support_hub_admin_option	Virtual Hub Administration Options is Supported
CT_b_support_cascade_client_cert	Client Certificates for Cascade Connection is Supported
CT_b_support_hide_hub	Virtual Hub Enumeration Setting is Supported
CT_b_support_cluster_admin	Integrated Administration for All Cluster Nodes is Supported
CT_b_support_cluster	Operation as Part of a Cluster is Supported
CT_b_support_cluster_controller	Operating as a Cluster Controller
CT_b_support_layer3	The Virtual Layer 3 Switch is Supported
CT_b_support_crl	Virtual Hub-Specific Certificate Revocation Lists is Supported
CT_b_support_ac	Virtual Hub-Specific Source IP Address Limit Lists is Supported
CT_b_support_read_log	Downloading of Log Files is Supported
CT_b_support_rename_cascade	Renaming of Cascade Connection is Supported
CT_b_support_license	Management of Licenses is Supported
CT_b_support_limit_multilogin	Limits for Multiple Login by Same User is Supported
CT_b_support_qos	VoIP / QoS Functions is Supported
CT_b_support_syslog	Syslog Sending Functions is Supported
CT_b_cluster_hub_type_fixed	The Virtual Hub Types in a Cluster are Fixed
CT_b_beta_version	Beta Version (Pre-release build)
CT_b_support_check_mac	Specifing MAC Address in Access Lists is Supported
CT_b_support_check_tcp_state	Checking TCP Connection State Filtering is Supported
CT_b_support_network_connection_name	Getting Network Friendly Name is Supported
CT_b_support_radius_retry_interval_and_several_servers	Retry Interval and Multi server is Supported in RADIUS Auth
CT_b_support_vlan	Tagged VLAN ID is Supported in MAC Address Table
CT_b_support_hub_ext_options	Virtual Hub Extended Option is Supported
CT_b_support_policy_ver_3	Security Policy version 3 is Supported
CT_b_support_ipv6_acl	IPv6 Access List is Supported
CT_b_support_ex_acl	Delay, Jitter and Packet Loss is Supported in Access List
CT_b_support_acl_group	Conditioning by Group name is Supported in Access List
CT_b_support_ipv6_ac	IPv6 IP Access Control Lists is Supported
CT_b_support_eth_vlan	Tagged VLAN Packet Transparency Support tool is Supported
CT_b_support_msg	Message of Today function is Supported
CT_b_vpn3	Internal Version 3.0 functions are Supported
CT_b_vpn4	Internal Version 4.0 functions are Supported
CT_b_support_ipsec	Funções de servidor IPsec / L2TP / EtherIP / L2TPv3 são suportadas
CT_b_support_sstp	MS-SSTP VPN Server Function is Supported
CT_b_support_udp_acceleration	UDP Acceleration Function is Supported
CT_b_support_openvpn	OpenVPN Server Function is Supported
CT_b_support_ddns	Dynamic DNS Client Function is Supported
CT_b_support_ddns_proxy	DDNS via Proxy Server is Supported
CT_b_support_special_listener	VPN over ICMP and VPN over DNS is Supported
CT_b_support_redirect_url_acl	HTTP URL Redirection in Access List is Supported
CT_b_is_in_vm	Running on VM (Virtual Machine)
CT_b_support_azure	VPN Azure is Supported
CT_b_support_aes_ni	CPU AES Acceleration (AES-NI) is Active
CT_b_using_selow_driver	SoftEther Lightweight Kernel-mode Ethernet Driver is Active
CT_b_support_vgs	VPN Gate Service Server Functions are Supported
CT_b_support_vgs_in_client	VPN Gate Service Server Functions (VPN Client integrated)
CT_b_is_softether	Either Free or Open-Source Version of SoftEther VPN
CT_b_suppport_push_route	Static Routing Table Pushing Function
CT_b_suppport_push_route_config	Static Routing Table Pushing Function (Configurable)


# Concerning policies
POL_TITLE_STR	Nome da política
POL_VALUE_STR	Valor atual
POL_TYPE_BOOL	ON / OFF
POL_TYPE_INT	Inteiro
POL_BOOL_ENABLE	Ativado
POL_BOOL_DISABLE	-
POL_BOOL_DISABLE_EX	-
POL_INT_ZERO	-
POL_INT_COUNT	%u 
POL_INT_SEC	%u segundos
POL_INT_BPS	%u bps
POL_INT_VLAN	%u


# Ver 2.0
POL_0	Permitir acesso
POL_EX_0	The users defined this policy have permission to make VPN connection to VPN Server.
POL_1	Filter DHCP Packets (IPv4)
POL_EX_1	All IPv4 DHCP packets in sessions defined this policy will be filtered.
POL_2	Disallow DHCP Server Operation (IPv4)
POL_EX_2	Computers connected to sessions that have this policy setting will not be allowed to become a DHCP server and distribute IPv4 addresses to DHCP clients.
POL_3	Enforce DHCP Allocated IP Addresses (IPv4)
POL_EX_3	Computers in sessions that have this policy setting will only be able to use IPv4 addresses allocated by a DHCP server on the virtual network side.
POL_4	Deny Bridge Operation
POL_EX_4	Bridge-mode connections are denied for user sessions that have this policy setting. Even in cases when the Ethernet Bridge is configured in the client side, communication will not be possible.
POL_5	Deny Routing Operation (IPv4)
POL_EX_5	IPv4 routing will be denied for sessions that have this policy setting. Even in the case where the IP router is operating on the user client side, communication will not be possible.
POL_6	Deny MAC Addresses Duplication
POL_EX_6	The use of duplicating MAC addresses that are in use by computers of different sessions cannot be used by sessions with this policy setting.
POL_7	Deny IP Address Duplication (IPv4)
POL_EX_7	The use of duplicating IPv4 addresses that are in use by computers of different sessions cannot be used by sessions with this policy setting.
POL_8	Deny Non-ARP / Non-DHCP / Non-ICMPv6 broadcasts
POL_EX_8	The sending or receiving of broadcast packets that are not ARP protocol, DHCP protocol, nor ICMPv6 on the virtual network will not be allowed for sessions with this policy setting.
POL_9	Privacy Filter Mode
POL_EX_9	All direct communication between sessions with the privacy filter mode policy setting will be filtered.
POL_10	Deny Operation as TCP/IP Server (IPv4)
POL_EX_10	Computers of sessions with this policy setting can't listen and accept TCP/IP connections in IPv4.
POL_11	Unlimited Number of Broadcasts
POL_EX_11	If a computer of a session with this policy setting sends broadcast packets of a number unusually larger than what would be considered normal on the virtual network, there will be no automatic limiting.
POL_12	Allow Monitoring Mode
POL_EX_12	Users with this policy setting will be granted to connect to the Virtual Hub in Monitoring Mode. Sessions in Monitoring Mode are able to monitor (tap) all packets flowing through the Virtual Hub.
POL_13	Número máximo de conexões TCP
POL_EX_13	For sessions with this policy setting, this sets the maximum number of physical TCP connections consists in a physical VPN session. 
POL_14	Time-out Period
POL_EX_14	For sessions with this policy setting, this sets, in seconds, the time-out period to wait before disconnecting a session when communication trouble occurs between the VPN Client / VPN Server.
POL_15	Maximum Number of MAC Addresses
POL_EX_15	For sessions with this policy setting, this limits the number of MAC addresses per session.
POL_16	Maximum Number of IP Addresses (IPv4)
POL_EX_16	For sessions with this policy setting, this specifies the number of IPv4 addresses that can be registered for a single session.
POL_17	Upload Bandwidth
POL_EX_17	For sessions with this policy setting, this limits the traffic bandwidth that is in the inwards direction from outside to inside the Virtual Hub.
POL_18	Download Bandwidth
POL_EX_18	For sessions with this policy setting, this limits the traffic bandwidth that is in the outwards direction from inside the Virtual Hub to outside the Virtual Hub.
POL_19	Deny Changing Password
POL_EX_19	The users which use password authentication with this policy setting are not allowed to change their own password from the VPN Client Manager or similar.
POL_20	Maximum Number of Multiple Logins
POL_EX_20	Users with this policy setting are unable to have more than this number of concurrent logins. Bridge Mode sessions are not subjects to this policy. This security policy is only available on VPN Server 3.0 or greater, or VPN Server 2.0 with the multi-login restriction function.
POL_21	Deny VoIP / QoS Function
POL_EX_21	Users with this security policy are unable to use VoIP / QoS functions in VPN connection sessions. This security policy is only available on VPN Server 3.0 or greater, or VPN Server 2.0 with the VoIP / QoS functions.


# Ver 3.0
POL_22	Filter RS / RA Packets (IPv6)
POL_EX_22	All ICMPv6 packets which the message-type is 133 (Router Solicitation) or 134 (Router Advertisement) in sessions defined this policy will be filtered. As a result, an IPv6 client will be unable to use IPv6 address prefix auto detection and IPv6 default gateway auto detection.
POL_23	Filter RA Packets (IPv6)
POL_EX_23	All ICMPv6 packets which the message-type is 134 (Router Advertisement) in sessions defined this policy will be filtered. As a result, a malicious users will be unable to spread illegal IPv6 prefix or default gateway advertisements on the network.
POL_24	Filter DHCP Packets (IPv6)
POL_EX_24	All IPv6 DHCP packets in sessions defined this policy will be filtered.
POL_25	Disallow DHCP Server Operation (IPv6)
POL_EX_25	Computers connected to sessions that have this policy setting will not be allowed to become a DHCP server and distribute IPv6 addresses to DHCP clients.
POL_26	Deny Routing Operation (IPv6)
POL_EX_26	IPv6 routing will be denied for sessions that have this policy setting. Even in the case where the IP router is operating on the user client side, communication will not be possible.
POL_27	Deny IP Address Duplication (IPv6)
POL_EX_27	The use of duplicating IPv6 addresses that are in use by computers of different sessions cannot be used by sessions with this policy setting.
POL_28	Deny Operation as TCP/IP Server (IPv6)
POL_EX_28	Computers of sessions with this policy setting can't listen and accept TCP/IP connections in IPv6.
POL_29	Maximum Number of IP Addresses (IPv6)
POL_EX_29	For sessions with this policy setting, this specifies the number of IPv6 addresses that can be registered for a single session.
POL_30	Disallow Password Save in VPN Client
POL_EX_30	For users with this policy setting, when the user is using *standard* password authentication, the user will be unable to save the password in VPN Client. The user will be required to input passwords for every time to connect a VPN. This will improve the security. If this policy is enabled, VPN Client Version 2.0 will be denied to access.
POL_31	VPN Client Automatic Disconnect
POL_EX_31	For users with this policy setting, a user's VPN session will be disconnected automatically after the specific period will elapse. In this case no automatic re-connection will be performed. This can prevent a lot of inactive VPN Sessions. If this policy is enabled, VPN Client Version 2.0 will be denied to access.
POL_32	Filter All IPv4 Packets
POL_EX_32	All IPv4 and ARP packets in sessions defined this policy will be filtered.
POL_33	Filter All IPv6 Packets
POL_EX_33	All IPv6 packets in sessions defined this policy will be filtered.
POL_34	Filter All Non-IP Packets
POL_EX_34	All non-IP packets in sessions defined this policy will be filtered. "Non-IP packet" mean a packet which is not IPv4, ARP nor IPv6. Any tagged-VLAN packets via the Virtual Hub will be regarded as non-IP packets.
POL_35	No Default-Router on IPv6 RA
POL_EX_35	In all VPN Sessions defines this policy, any IPv6 RA (Router Advertisement) packet with non-zero value in the router-lifetime will set to zero-value. This is effective to avoid the horrible behavior from the IPv6 routing confusion which is caused by the VPN client's attempts to use the remote-side IPv6 router as its local IPv6 router.
POL_36	No Default-Router on IPv6 RA (physical IPv6)
POL_EX_36	In all VPN Sessions defines this policy (only when the physical communication protocol between VPN Client / VPN Bridge and VPN Server is IPv6), any IPv6 RA (Router Advertisement) packet with non-zero value in the router-lifetime will set to zero-value. This is effective to avoid the horrible behavior from the IPv6 routing confusion which is caused by the VPN client's attempts to use the remote-side IPv6 router as its local IPv6 router.
POL_37	VLAN ID (IEEE802.1Q)
POL_EX_37	You can specify the VLAN ID on the security policy. All VPN Sessions defines this policy, all Ethernet packets toward the Virtual Hub from the user will be inserted a VLAN tag (IEEE 802.1Q) with the VLAN ID. The user can also receive only packets with a VLAN tag which has the same VLAN ID. (Receiving process removes the VLAN tag automatically.) Any Ethernet packets with any other VLAN IDs or non-VLAN packets will not be received. All VPN Sessions without this policy definition can send / receive any kinds of Ethernet packets regardless of VLAN tags, and VLAN tags are not inserted or removed automatically. Any tagged-VLAN packets via the Virtual Hub will be regarded as non-IP packets. Therefore, tagged-VLAN packets are not subjects for IPv4 / IPv6 security policies, access lists nor other IPv4 / IPv6 specific deep processing.


# Concerning remote connection dialog
REMOTE_DEF_CAPTION	Remote Connection
REMOTE_DEF_TITLE	Specify the computer you want to remotely connect to.


# Concerning client notification service
CN_TITLE	Edição de desenvolvedor do SoftEther VPN Cliente


# Concerning Connection Manager
CM_TITLE	Edição de desenvolvedor do gerenciador SoftEther VPN Cliente
CM_PW_LOCALMACHINE	Computador local
CM_NO_REMOTE	The VPN Client service running on %s disallows remote connections.
CM_CONNECT_FAILED	Unable to connect to the VPN Client service operating on %s. \r\nMake sure the VPN Client service has started and is running normally.
CM_BAD_PASSWORD	The password is incorrect. Re-enter password. The password is case-sensitive so be sure to discern between upper and lower case letters.
CM_NUM_CONN_COUNT	%u Sessões VPN
CM_CONN_NO	Não conectado
CM_PRODUCT_NAME	SoftEther VPN Client Build %u
CM_ACCOUNT_COLUMN_1	Nome da configuração da conexão VPN
CM_ACCOUNT_COLUMN_2	Status
CM_ACCOUNT_COLUMN_3	Nome do host do servidor VPN
CM_ACCOUNT_COLUMN_3_2	Hub Virtual
CM_ACCOUNT_COLUMN_4	Nome do adaptador de rede virtual
CM_VLAN_COLUMN_1	Nome do adaptador de rede virtual
CM_VLAN_COLUMN_2	Status
CM_VLAN_COLUMN_3	Endereço MAC
CM_VLAN_COLUMN_4	Versão
CM_ACCOUNT_OFFLINE	Offline
CM_ACCOUNT_ONLINE	Conectado
CM_ACCOUNT_CONNECTING	Conectando
CM_VLAN_ENABLED	Ativado
CM_VLAN_DISABLED	Desativado
CM_DELETE_ACCOUNT_MSG	This will delete the VPN Connection Setting "%s". Do you really want to do this?
CM_ST_ACCOUNT_NAME	Nome da configuração da conexão VPN
CM_ST_CONNECTED	Session Status
CM_ST_CONNECTED_TRUE	Connection Completed (Session Established)
CM_ST_CONNECTED_FALSE	Trying to Connect
CM_ST_CONNECTING	Connection to VPN Server Started
CM_ST_NEGOTIATION	Negociando
CM_ST_AUTH	Authenticating User
CM_ST_ESTABLISHED	Connection is Established
CM_ST_RETRY	Repetindo
CM_ST_IDLE	Ocioso
CM_ST_SERVER_NAME	Nome do servidor
CM_ST_SERVER_PORT	Número da porta
CM_ST_PORT_TCP	Porta TCP %u
CM_ST_SERVER_P_NAME	Nome do produto do servidor
CM_ST_SERVER_P_VER	Server Version
CM_ST_SERVER_P_BUILD	Build do servidor
CM_ST_START_TIME	Conexão iniciada às
CM_ST_FIRST_ESTAB_TIME	First Session has been Established since
CM_ST_NONE	-
CM_ST_CURR_ESTAB_TIME	Current Session has been Established since
CM_ST_NUM_ESTABLISHED	Number of Established Sessions
CM_ST_NUM_STR	%u vezes
CM_ST_HALF_CONNECTION	Half Duplex TCP Connection Mode
CM_ST_HALF_TRUE	Yes (Half Duplex Mode)
CM_ST_HALF_FALSE	No (Full Duplex Mode)
CM_ST_QOS	VoIP / QoS Function
CM_ST_QOS_TRUE	Ativado
CM_ST_QOS_FALSE	Desativado
CM_ST_NUM_TCP	Número de conexões TCP
CM_ST_NUM_TCP_UPLOAD	Número de conexões TCP Uplink
CM_ST_NUM_TCP_DOWNLOAD	Number of Downlink TCP Connections
CM_ST_MAX_TCP	Número máximo de conexões TCP
CM_ST_VLAN_ID	ID VLAN
CM_ST_NO_VLAN	-
CM_ST_USE_ENCRYPT	Criptografia
CM_ST_USE_ENCRYPT_TRUE	Enabled (Algorithm: %S)
CM_ST_USE_ENCRYPT_TRUE2	Ativado
CM_ST_USE_ENCRYPT_TRUE3 Enabled (%S Algorithm: %S)
CM_ST_USE_ENCRYPT_FALSE	Disabled (No Encryption)
CM_ST_USE_COMPRESS	Use of Compression
CM_ST_UDP_ACCEL_ENABLED	UDP Acceleration is Supported
CM_ST_UDP_ACCEL_USING	UDP Acceleration is Active
CM_ST_RUDP	TCP over UDP (NAT Traversal)
CM_ST_UNDERLAY_PROTOCOL	Physical Underlay Protocol
CM_ST_PROTOCOL_DETAILS	Protocol Details
CM_ST_COMPRESS_TRUE	Sim (%u %%)
CM_ST_COMPRESS_FALSE	No (No Compression)
CM_ST_SESSION_NAME	Nome da sessão
CM_ST_CONNECTION_NAME	Nome da conexão
CM_ST_SESSION_KEY	Session Key (160 bit)
CM_ST_BRIDGE_MODE	Bridge / Router Mode
CM_ST_MONITOR_MODE	Modo de monitoramento
CM_ST_YES	Sim
CM_ST_NO	Não
CM_ST_SEND_SIZE	Outgoing Data Size
CM_ST_RECV_SIZE	Incoming Data Size
CM_ST_SEND_UCAST_NUM	Pacotes unicast de saída
CM_ST_SEND_UCAST_SIZE	Tamanho total unicast de saída
CM_ST_SEND_BCAST_NUM	Pacotes broadcast de saída
CM_ST_SEND_BCAST_SIZE	Tamanho total broadcast de saída
CM_ST_RECV_UCAST_NUM	Pacotes unicast de entrada
CM_ST_RECV_UCAST_SIZE	Tamanho total unicast de entrada
CM_ST_RECV_BCAST_NUM	Pacotes broadcast de entrada
CM_ST_RECV_BCAST_SIZE	Tamanho total broadcast de entrada
CM_ST_NUM_PACKET_STR	%S pacotes
CM_ST_SIZE_BYTE_STR	%S bytes
CM_NEW_ICON	Adicionar conexão VPN
CM_VGC_ICON	VPN Gate Public VPN Relay Servers
CM_VGC_LINK	VPN Gate Academic Web Site
CM_ST_TITLE	Connection Status of %s
CM_ST_COLUMN_1	Item
CM_ST_COLUMN_2	Status
CM_NEW_ACCOUNT_NAME_1	Nova conexão VPN
CM_NEW_ACCOUNT_NAME_2	Nova conexão VPN (%u)
CM_ACCOUNT_TITLE_1	Propriedades da nova configuração de conexão VPN...
CM_ACCOUNT_TITLE_2	Propriedade de %s
CM_SERVER_CERT_1	Certificado &individual
CM_SERVER_CERT_2	&Excluir certificado
CM_CLIENT_CERT_1	&Certificado do cliente
CM_CLIENT_CERT_2	Delete &Client Certificate
CM_CERT_INFO	Issued to: %s\r\nIssuer: %s\r\nExpiration: %s
CM_NO_CERT	Você deve especificar um certificado do cliente a ser usado para autenticação do usuário.
CM_NO_SECURE	Specify the client certificate and private key inside the smart card to be used for user authentication.
CM_CERT_SECURE_INFO	Certificate: "%S"\r\nPrivate Key: "%S"
CM_SELECT_SECURE_DEVICE	Selecionar Smart Card
CM_SELECT_CERT_INCARD	Specify Cert and Pri&vate Key
CM_VIEW_CLIENT_CERT	&View Client Certificate
CM_NO_VLAN	Antes de criar uma nova configuração de conexão VPN, você precisa criar um adaptador de rede virtual.\r\n\r\n Deseja criar um adaptador de rede virtual?
CM_NO_VLAN_2	Before connecting to VPN Server you need to create a Virtual Network Adapter. \r\n\r\nDo you want to create a Virtual Network Adapter?
CM_VLAN_REMOTE_ERROR	Unable to create a Virtual Network Adapter from a remote location. \r\n\rStart the VPN Client Manager on the local computer on which the VPN Client service is running and install a Virtual Network Adapter.
CM_9X_VLAN_INSTALL	A new Virtual Network Adapter will now be created. \r\n\r\nAfter a Virtual Network Adapter is created, it is necessary to restart Windows directly afterwards. \r\nWhile the Virtual Network Adapter is being installed, you may be asked to insert the Windows installation CD-ROM. \r\n\r\nClose all currently running applications except the VPN Client Manager, have your Windows installation CD-ROM ready at hand, and click OK. \r\nClicking OK will start the installation of the Virtual Network Adapter. When this is finished, Windows will automatically restart.
CM_9X_VLAN_ME_MESSAGE	A Virtual Network Adapter has been created. After you click OK, the computer will automatically restart. \r\n\r\nAfter the computer restarts, the Install New Device wizard might appear. \r\nIf the wizard does appear, click Next for each screen until the installation is completed.
CM_9X_VLAN_UNINSTALL	To delete a Virtual Network Adapter, delete it from Network Properties. \r\n\r\nDo you want to display the Network Properties window?
CM_PORT_1	8888 (Porta PX-VPN)
CM_PORT_2	443 (Porta HTTPS)
CM_PORT_3	992 (Porta TELNETS)
CM_PORT_4	5555 (Porta SE-VPN)
CM_RETRY_INTERVAL_ERROR	Set a re-connection interval (at least 5 seconds) when VPN connection has been disconnected.
CM_DELETE_CLIENT_CERT	This will delete the client certificate that has been set. Do you really want to do this?
CM_DELETE_SERVER_CERT	This will delete the server individual certificate that has been set. Do you really want to do this?
CM_SET_STARTUP	The VPN Connection Setting "%s" is now set as a startup connection.\r\n\r\nThis account will be connected automatically next time the computer restarts.\r\n(If you are using Windows, the automatic connection will be started in the background mode before a user logs on to Windows.)
CM_REMOVE_STARTUP	Do you wish to delete the startup connection property of VPN Connection Setting "%s"?
CM_NO_DISCONNECT_SPAN	Please set the life of the TCP connection.
CM_HALF_MSG	When using half-duplex mode, set at least 2 for the number of TCP connections.
CM_TOO_SMALL_INTERVAL	Set at least 1 second for the interval to establish a TCP connection.
CM_DELETE_VLAN	This will delete the Virtual Network Adapter "%s". Do you really want to do this?
CM_COPY_NAME_1	Copia de %s
CM_COPY_NAME_2	Copy (%u) of %s
CM_IMPORT_NAME_1	%s
CM_IMPORT_NAME_2	%s (%u)
CM_CERT_COLUMN_1	Emitido para
CM_CERT_COLUMN_2	Emissor
CM_CERT_COLUMN_3	Expiração
CM_CERT_DELETE_MSG	Delete this certificate from the list?
CM_PASSWORD_SET	The password has been set.
CM_PASSWORD_REMOVE	The password setting has been deleted.
CM_UNDER_CONSTRUCTION	Incompleto.
CM_CURRENT_ACTIVE	The settings of VPN Connection Setting "%s" were saved. But this VPN Connection Setting is currently online and the new settings will apply in the next connection.
CM_DISCONNECT_ALL	This will disconnect all %u VPN Connection Settings that are currently connected. \r\nDo you really want to do this?
CM_HTTPS_MSG	You have chosen to connect via an HTTP proxy server. \r\n\r\nUsual HTTP proxy servers do not allow access to a TCP port of your choice. \r\nWhen a VPN Client connects to a VPN Server via a HTTP proxy server, it is possible to connect by using HTTPS (HTTP over SSL) communication. \r\nIn this case it is recommended that you specify 443 (HTTPS Port) as the destination VPN Server port number. \r\n(If you specify a different port number, there are cases where it will not be possible to connect via an HTTP proxy server. \r\n Make sure that port 443 is enabled on the destination VPN Server.)\r\n\r\nFor detailed information contact either the system administrator or network administrator of the HTTP proxy server you plan to connect via. \r\n\r\nDo you want to change the port number specification of the destination VPN Server to 443 (HTTPS Port)?
CM_REMOTE_WARNING	You are making changes to the remote management setting that will disallow remote management. \r\n\r\nCurrently the VPN Client Manager is connected to remote computer "%S" and is controlling the VPN Client service on that computer. \r\nIf remote connection is disabled, it will no longer be possible to remotely connect to and control the VPN Client service on computer "%S" using the VPN Client Manager. \r\n\r\nDo you want to disable remote management?
CM_KEEP_INTERVAL_MSG	Set a period between %u and %u seconds in the Packet Send Interval.
CM_REMOTE_TITLE	Using the VPN Client Manager, it is possible to connect to, and remotely manage a VPN Client service operating on another computer. \r\n(Note that the VPN Client service on the remote computer must allow remote management.)
CM_DESKTOP_LOCAL_PC	Computador local
CM_DESKTOP_REMOTE_PC	Computador %S 
CM_DESKTOP_MSG_LOCAL_TS	Terminal Service (Remote Desktop) Function
CM_DESKTOP_MSG_LOCAL_SW	Switch User Function
CM_DESKTOP_MSG_LOCAL_1	Currently %s is installed on this computer, providing an environment that permits multiple users to log on concurrently. In this case, the messages regarding progress status, error messages and other messages displayed by VPN Client will be displayed on a session called the "Console Session".
CM_DESKTOP_MSG_LOCAL_21	Currently "Session ID: 0, User %s" is assigned as the Console Session of this computer, however because you have started VPN Client Manager on session %u, it is not possible to display the message windows such as the progress status or errors that VPN Client displays.
CM_DESKTOP_MSG_LOCAL_22	Currently no one is logged into the Console Session "Session ID: 0" of this computer and because you have started VPN Client Manager on session %u, it is not possible to display the message windows such as the progress status or errors that VPN Client displays.
CM_DESKTOP_MSG_LOCAL_31	It is recommended that when this computer's Console Session (Session ID: 0, User %s) is displayed, start the VPN Client Manager in that session and start the connection to the VPN Connection Setting "%s". You will be able to start a connection process by doing what you are doing now. But it will be at the risk of being unable to check the progress status and error messages that may be displayed during the process.
CM_DESKTOP_MSG_LOCAL_32	It is recommended that you first log off and then after logging in locally, start the VPN Client Manager in that session and start the connection to VPN Connection Setting "%s". Although you will be able to start a connection process by doing what you are doing now, this will be at the risk of being unable to check the progress status and error messages that may be displayed during the process.
CM_DESKTOP_MSG_REMOTE_1	Because you are currently performing operation while remotely connected to VPN Client on computer %S, if the VPN Client displays any progress status or error messages during the VPN connection process to the VPN Connection Setting, you will not be able to check these messages from your current screen display.
CM_DESKTOP_MSG_REMOTE_2	To check all the progress status, error and other message windows that VPN Client displays, you must log in locally to computer %S and display the Control Session (desktop). 
CM_DESKTOP_MSG_REMOTE_3	It is recommended that you first log in directly and locally to computer %S, and then start the VPN Client Manager in that session and start the connection to VPN Connection Setting "%s". Although you will be able to start a connection process by doing what you are doing now, this will be at the risk of being unable to check the progress status and error messages that may be displayed during the process.
CM_STOP_INST_VLAN_1	To install a Virtual Network Adapter on this computer you must start the VPN Client Manager within a "Console Session". \r\n\r\nCurrently, %s is installed on this computer and the current user is not logged into the Console Session but rather is logged in as the remote session (session ID: %u).\r\nTo install a Virtual Network Adapter, VPN Client Manager must be started in the Console Session (session ID: %u, user %s is logged on). \r\n\r\nFirst log on to the computer locally by using the user switching function, or the /console switch function that is on the remote desktop, or alternatively the computer's local console device and then start the VPN Client Manager and install the Virtual Network Adapter.
CM_STOP_INST_VLAN_2	To install a Virtual Network Adapter on this computer you must start the VPN Client Manager within a "Console Session". \r\n\r\nCurrently, %s is installed on this computer and the current user is not logged into the Console Session but rather is logged in as the remote session (session ID: %u).\r\nTo install a Virtual Network Adapter you must start the VPN Client Manager within a "Console Session". \r\n(Currently the user is not logged on to the Console Session (Session ID: 0).) \r\n\r\nFirst log on to the computer locally by using the user switching function, or the /console switch function that is on the remote desktop, or alternatively the computer's local console device and then start the VPN Client Manager and install the Virtual Network Adapter.
CM_SHORTCUT_DESKTOP_MSG	To start a connection using the shortcut to the VPN Connection Setting, you must launch the shortcut file within the "Console Session". \r\n\r\nCurrently the user is logged on as the remote session (session ID: %u) and not as the Console Session.
CM_HTTP_PROXY_WARNING	Connect via HTTP Proxy Server is selected. \r\n\r\nIn many cases, the HTTP proxy server will only allow 2 kinds of TCP port to be used for the connection to the destination server port number, HTTP protocol (TCP port number 80) and HTTPS protocol (TCP port number 443). \r\n(There are also cases when the proxy server does allow a wider choice of TCP port for connection.) \r\n\r\nWhen making a VPN connection via an HTTP proxy server that denies connections to server ports other than HTTP ports or HTTPS ports, you must specify 443 (HTTPS protocol) as the destination VPN Server port number. \r\n\r\nTo check whether the HTTP proxy server you are connecting via allows connection to ports other than port numbers 80 or 443, contact the administrator of the HTTP proxy server. \r\n\r\nCurrently, %d is specified as the destination VPN Server port number. Do you want to change the port number to 443 (HTTPS protocol)?\r\n(The port 443 of the VPN Servers you connect to must be set to listening status and ready for connection.) \r\nIf you are unsure, then contact the system administrator or the network administrator.
CM_HTTP_HEADER_COLUMN_0	Nome
CM_HTTP_HEADER_COLUMN_1	Valor
CM_PASSWORD_CHANGED	A senha foi alterada.
CM_ACCOUNT_SETTING_FILE	VPN Connection Setting Files (*.VPN)|*.vpn|All Files (*.*)|*.*
CM_ACCOUNT_SAVE_TITLE	Enter a VPN Connection Setting File's File Name for the Export Destination
CM_ACCOUNT_OPEN_TITLE	Select the VPN Connection Setting File to Import
CM_ACCOUNT_FILE_BANNER	# VPN Client VPN Connection Setting File\r\n# \r\n# This file is exported using the VPN Client Manager.\r\n# The contents of this file can be edited using a text editor.\r\n# \r\n# When this file is imported to the Client Connection Manager\r\n#  it can be used immediately.\r\n\r\n
CM_FAILED_TO_OPEN_FILE	Unable to open file.
CM_FAILED_TO_SAVE_FILE	Unable to save file.
CM_ACCOUNT_PARSE_FAILED	Unable to load the VPN Connection Setting from the specified file. \r\nCheck the contents of the file.
CM_ACCOUNT_MSG_SENSITIVE	This VPN Connection Setting has the username and the password.\r\nDo you want to remove these sensitive information from the exported setting file?\r\n\r\nClick Yes to remove sensitive information.\r\nIn that case a user will be required to input the username and the password when he is trying to connect to the VPN Server.\r\n\r\nClick No to stay the sensitive information remaining on the file.
CM_SHORTCUT_FILE	Shortcut Files|*.lnk
CM_SHORTCUT_SAVE_TITLE	Enter the Shortcut File Name.
CM_SHORTCUT_UNSUPPORTED	The connection shortcut function is not supported by this version of VPN Client. \r\nUpdate to a new version.
CM_SHORTCUT_COMMENT	Using the VPN Connection Setting "%s" to connect to the VPN Server.
CM_SHORTCUT_ERROR	Failed to create a shortcut.
CM_VPN_FILE_CLICKED	Do you want to import the VPN Connection File?
CM_VPN_FILE_IMPORT_NG	Unable to import the VPN Connection Setting File. Because the VPN Client setting has been locked.
CM_VLAN_INSTALLING	Please Wait a While
CM_SECURE_MUST_LOCAL	It is currently not possible to configure smart card settings because you are connected to and managing a VPN Client on a remote computer.
CM_DETAIL_MODE_LINK_STR	With a Cascade Connection, Connect by Bridge / Router mode is always enabled.
CM_TRAY_INITING			SoftEther VPN
CM_TRAY_NOT_CONNECTED	\r\nNot connected
CM_TRAY_CONNECTING		\r\nConnecting
CM_TRAY_CONNECTED		\r\nConnected
CM_TRAY_MENU_1_SHOW	&Mostra gerenciador de clientes VPN
CM_TRAY_MENU_1_HIDE	&Fechar o gerenciador de clientes VPN
CM_TRAY_MENU_2_QUIT	Sair doGerenciador de clientes VPN
CM_TRAY_MENU_CONNECT	&Iniciar conexão VPN
CM_TRAY_MENU_DISCONNECT	&Disconnect VPN Connection
CM_TRAY_MENU_STATUS	Show VPN Connec&tion Status
CM_TRAY_MENU_DISCONNECT_ALL	Disconnect &All VPN Connections
CM_TRAY_MENU_NEW	&Nova configuração de conexão VPN...
CM_TRAY_MENU_RECENT	Servidores VPN recentes...
CM_TRAY_MENU_TRAFFIC	Network &Traffic Speed Test Tool...
CM_TRAY_MENU_NETIF	Show Network &Device Status...
CM_TRAY_MENU_ABOUT	&Sobre o gerenciador de clientes VPN...
CM_TRAY_MENU_SETTING	Alterar &modo de operação...
CM_TRAY_MENU_CANCEL	Close this menu
CM_EXIT_MESSAGE	This will exit the VPN Client Manager program. \r\nDo you really want to do this?
CM_IMPORT_MESSAGE	From file "%S", VPN Connection Setting "%s" has been installed.
CM_VLAN_CREATING	Criando um novo adaptador de rede virtual para o Windows.\r\n\r\nEste processo pode levar alguns segundos ou mais de um minuto.\r\nPor favor, aguarde...\r\n\r\n (Por favor, não execute outras operações enquanto o adaptador de rede virtual estiver sendo instalado)
CM_SETTING_PASSWORD	The setting is locked. To remove the setting-locker, you must enter a password.
CM_EASY_MODE_NOT_ON_REMOTE	Unable to connect because of the VPN Client on the remote computer is running in Easy Mode.
CM_EASY_CONNECT_BUTTON_1	&Iniciar conexão VPN
CM_EASY_CONNECT_BUTTON_2	&Desconectar
CM_EASY_ACCOUNT_WARNING	You can only modify Proxy Server Setting, User Authentication and Virtual Network Adapter Used because the setting has been locked.
CM_EASY_INFO_1	Select a VPN connection.
CM_EASY_INFO_2	Click Start VPN Connection to start a VPN connection.
CM_EASY_INFO_3	VPN connection is active. You can disconnect by clicking Disconnect.
CM_EXT_VOICE_MSG	It is possible that some of the voice message contents of the Extension Voice Guide has not been played normally. \r\nIs the Extension Voice Guide enabled?
CM_EASY_TITLE	VPN Client Easy Connection Manager
CM_EASY_CONNECTED	VPN connection is active.
CM_EASY_CONNECTING	Establishing VPN connection...
CM_PROXY_FROM_IE	Currently proxy setting from Internet Explorer has been loaded.
CM_TRAY_ICON_RESTORE	The icon in the task tray has been deleted.\r\n\r\nTo restore the icon, run the VPN Client Manager and click Show Task-tray Icon in the View menu.
CM_WOULDYOULOAD_IE_PROXY	Currently the Internet Explorer on this computer is configured to use the proxy server "%S".\r\nDo you want to apply the current proxy settings on the new VPN connection setting?\r\n\r\nClick Yes to use the proxy settings of Internet Explorer.\r\nClick No to use direct connection to the VPN Server (does not a proxy server.)\r\nThis setting can be modified in the property screen of the connection settings any time later.
CM_MSG_TITLE	VPN Server "%S" (Virtual Hub: "%S")
CM_JUMPLIST_RCCONNECT	Servidores VPN recentes
CM_VPNGATE_MESSAGE	There is the list of Public VPN Relay Servers on the VPN Gate Academic Project Web Site.\r\nAnyone on the Internet can connect a VPN connection to any VPN servers on the list.\r\n\r\nVPN Gate Academic Project is not a part of SoftEther VPN.\r\nThis icon provides just a link to http://www.vpngate.net/.\r\nYou need to install VPN Gate Plugin to connect VPN Gate.\r\n\r\nDo you want to visit http://www.vpngate.net/ (provided by University of Tsukuba) ?
CM_VLAN_REINSTALL_MSG	After reinstalling the Virtual Network Adapter driver, the current Virtual Network Adapter's MAC address will change. Also, all TCP/IP settings within the Virtual Network Adapter will reset.\r\n\r\nIn case the reinstalled Virtual Network Adapter fails to work, delete it and create a new one. If it still doesn't work properly, please create a new Virtual Network Adapter with a different name.
VGC_COLUMN_0	DDNS Hostname
VGC_COLUMN_1	IP Address (Hostname)
VGC_COLUMN_2	Região
VGC_COLUMN_3	Tempo de atividade
VGC_COLUMN_4	Sessões VPN
VGC_COLUMN_5	Velocidade da linha
VGC_COLUMN_6	Ping (Google, SE)
VGC_COLUMN_7	SSL-VPN (TCP)
VGC_COLUMN_8	Suporte UDP
VGC_COLUMN_9	Logging Policy
VGC_COLUMN_10	Cumulative Transfers
VGC_COLUMN_11	Cumulative Users
VGC_COLUMN_12	Operator's Name
VGC_COLUMN_13	Operator's Message
VGC_COLUMN_14	Pontuação total
VGC_LOG_PERMANENT	Permanente
VGC_LOG_2WEEKS	2 semanas
VGC_LOG_NONE	Sem Logs
VGC_UPTIME_MIN	%u min
VGC_UPTIME_HOUR	%u horas
VGC_UPTIME_DAY	%u dias
VGC_NUM_VPN	%u Sessões
VGC_NUM_LOGIN	%S logins
VGC_UDP_AVAILABLE	UDP OK
VGC_TITLE	VPN Gate Plug-in Message
VGC_VER_DIFF	The version of VPN Gate Client Plug-in is different from SoftEther VPN Client.\r\n\r\n- Current VPN Gate Plug-in: Build %u\r\n- Current SoftEther VPN Client: Build %u\r\n\r\nIt is recommended to download and install VPN Gate Plug-in Build %u. Otherwise, communication errors or list-update errors might be occur. If the VPN Server List updating fails many times, update the VPN Gate Plug-in version.\r\n\r\nThe latest VPN Gate Plug-in is available at http://www.vpngate.net/.\r\n(Use a mirror-site if you cannot visit the above web-site directly.)\r\n\r\n
VGC_LIST_STR_OK	%S Public VPN Relay Servers on the Earth! (Updated at %S)
VGC_LIST_STR_OK_2	%S Servers (at %S) - List update failed. Try again. If fails again, download the latest VPN Gate Client.
VGC_LIST_STR_NG	List update failed. Try again. If fails again, download the latest VPN Gate Client.
VGC_PROXY_MSG	If you are using a proxy server, you might not be able to use VPN Relay Servers which don't support the TCP port 443 as "SSL-VPN Connection" from such a proxy-mandated network.
VGC_PROXY_TITLE	Notice for Proxy Server Users
VGS_NO_HUB_YET	In order to set the message, first you have to commit enabling the VPN Gate service. After the service will be enabled, re-open this window and set the message.
VGS_STOP	VPN Gate Service will stop after you click the OK button.\r\n\r\nAfter VPN Gate Service will be stopped, this computer will never accept new VPN connection requests, however, still-alive VPN Sessions might remain.\r\n (Such VPN sessions sometimes hidden from the enumeration.) \r\n\r\nTo terminate all of still-alive VPN Sessions completely, restart SoftEther VPN Server or SoftEther VPN Client service, or reboot the computer.
VGS_START	This will activate the VPN Gate Relay Service function.\r\n\r\nVPN Gate Relay Service function must be activated by your own risk.\r\nSome countries prohibit using of encrypted VPN by laws.\r\nFor more details about VPN Gate Relay Service please visit http://www.vpngate.net/en/join.aspx.\r\n\r\nThe VPN Gate Academic Experiment Service is operated as a research project at the graduate school on University of Tsukuba, Japan. The service is governed under the Japanese laws. Other countries' laws are none of our concerns nor responsibilities.\r\n\r\nBy nature, there are almost 200 countries in the World, with different laws. It is impossible to verify every countries' laws and regulations and make the software comply with all countries' laws in advance to release the software. If a user uses VPN Gate service in a specific country, and damaged by public servants of the authority, the developer of either the service or software will never be liable to recover or compensate such damages or criminal responsibilities.\r\nBy using this software and service, the user must observe all concerned laws and rules with user's own responsibility. The user will be completely liable to any damages and responsibilities which are results of using this software and service, regardless of either inside or outside of Japan's territory.\r\nIf you don't agree nor understand the above warnings, do not use any of VPN Gate Academic Experiment Service functions.


# Concerning services (Win32)
SVC_HELP	*** Command Line Arguments of %s (%S) ***\r\n\r\nThis program (%s) is a process runs as a background task. Start the program by specifying the following arguments on the command line. \r\n\r\n\r\n/install : Installs %s service (service name: %S) in Windows. After this, the service will automatically start. \r\n\r\n/uninstall... Uninstalls %s service (service name: %S) from Windows. \r\n\r\n/start : Starts %s service (service name: %S). \r\n\r\n/stop : Stops %s service (service name: %S). \r\n\r\n/test : Starts %s program in test mode. (For debug)\r\n\r\n/usermode : Starts %s program in the user mode. (When possible)\r\n\r\n/usermode_showtray : When starting in the user mode, this is used to display task tray icons when they were set to be hidden on a previous occasion. \r\n\r\n/usermode_hidetray : When starting in the user mode, this sets the task tray icons to be hidden. \r\n\r\n\r\nNote: Commands related to service operation other than /test and /usermode can only be operated on Windows NT / XP / Server 2003 / Vista / Server 2008.
SVC_NT_ONLY	The service related operation commands can only operate on Windows NT / 2000 / XP / Server 2003 / Vista / Server 2008. \r\nThey do not operate on Windows 98 / Me.
SVC_ALREADY_INSTALLED	The "%s" service (service name: %S) is already installed on this computer. Do you want to uninstall it and then re-install?
SVC_INSTALL_OK	The "%s" service (Service name: %S) has been installed successfully. \r\n\r\n(Execution path: %s)\r\n\r\nThe service has started.
SVC_INSTALL_FAILED	The installation of the "%s" service (service name: %S) failed.
SVC_INSTALL_FAILED_2	The "%s" service (Service name: %S) has been successfully installed. \r\n\r\n(Execution path: %s)\r\n\r\nAn attempt to start the service, however, failed.
SVC_NOT_INSTALLED	The "%s" service (service name: %S) is not yet installed on this computer. Use the /install command line argument to install it.
SVC_START_OK	The "%s" service (service name: %S) started successfully.
SVC_START_FAILED	The "%s" service (service name: %S) failed to start.
SVR_ALREADY_START	The "%s" service (service name: %S) has already started.
SVC_STOP_OK	The "%s" service (Service name: %S) has been stopped.
SVC_STOP_FAILED	The "%s" service (service name: %S) failed to stop.
SVC_ALREADY_STOP	The "%s" service (service name: %S) is already stopped.
SVC_UNINSTALL_OK	The "%s" service (Service name: %S) has been uninstalled successfully.
SVC_UNINSTALL_FAILED	The uninstallation of the "%s" service (service name: %S) failed.
SVC_NOT_FOUND	Unable to find information related to service %S from the string table.
SVC_NOT_ADMIN	To install, uninstall, start or stop the service you must have administrator privileges for this computer. \r\n\r\nIf you have an administrators account for this computer, log out and log on as an administrator. \r\nIf you are unclear about administrators accounts, contact your system administrator.
SVC_TEST_MSG	The "%s" service is started in test mode. \r\n\r\nClick OK to exit the service.
SVC_TRAY_TOOLTIP	%S (Modo usuário)
SVC_TEST_MUTEX	The executable file %s is already started.
SVC_USERMODE_MUTEX	Another process of %s is already started.
SVC_SERVICE_MUTEX	Because service %S has process %s that is already started, the service cannot start.
SVC_USERMODE_MENU_1	&Ocultar ícone da bandeja de tarefas
SVC_USERMODE_MENU_2	S&air %s
SVC_HIDE_TRAY_MSG	This will hide the tasktray icons when starting %S in user mode. \r\nBeginning from next time %S is started in user mode, icons will not be displayed in the tasktray. \r\nThe menu to exit the process will also be hidden. \r\n\r\nTo exit the process in the case of Windows 98 / Me, use the Ctrl + Alt + Del key combination and select to end the process. \r\nWhen using other operating systems, use Task Manager. \r\n\r\nTo redisplay the tasktray icons, use the /usermode_showtray option when starting in user mode next time.


# Concerning services (UNIX)
UNIX_SVC_HELP	%S service program\nCopyright (c) all contributors on SoftEther VPN project in GitHub.\nCopyright (c) Daiyuu Nobori, SoftEther Project at University of Tsukuba, and SoftEther Corporation.\nAll Rights Reserved.\n\n%S command usage:\n %S start  - Start the %S service.\n %S stop   - Stop the %S service if the service has been already started.\n\n
UNIX_SVC_STARTED	The %S service has been started.\n
UNIX_SVC_STOPPING	Stopping the %S service ...\n
UNIX_SVC_STOPPED	%S service has been stopped.\n
UNIX_SVC_STOP_FAILED	Stopping %S service was failed.\n
UNIX_SVC_ALREADY_START	%S service has been already started.\nRun the "%S stop" command to stop this service.\n
UNIX_SVC_NOT_STARTED	%S service has not yet been started.\nRun the "%S start" to start this service.\n
UNIX_SVC_ERROR_FORK	Failed to create child process for the %S service.\n
UNIX_SVC_NONROOT	\nWarning: The current user context is non-root. It is recommended to run the VPN service by the root user. Although the VPN service may run under non-root users, some privilege-required functions (e.g. the local bridge function) need the root privilege.\n


# Service definition (SoftEther VPN Client)
SVC_VPNCLIENT_NAME	vpnclient
SVC_VPNCLIENT_TITLE	SoftEther VPN Cliente
SVC_VPNCLIENT_DESCRIPT	This manages the Virtual Network Adapter device driver and connection service for the SoftEther VPN Client. When this service is stopped, it will not be possible to use SoftEther VPN Client on this computer to connect to a SoftEther VPN Server.


# Service Definition (SoftEther VPN Server)
SVC_VPNSERVER_NAME	vpnserver
SVC_VPNSERVER_TITLE	SoftEther VPN Servidor
SVC_VPNSERVER_DESCRIPT	This manages the server processes of SoftEther VPN Server. SoftEther VPN Server provides high-performance SoftEther VPN Server functions via TCP/IP protocol. When this service is stopped, SoftEther VPN Server on this computer will stop and SoftEther VPN Client will be unable to establish a VPN connection with this computer.


# Service Definition (SoftEther VPN Bridge)
SVC_VPNBRIDGE_NAME	vpnbridge
SVC_VPNBRIDGE_TITLE	SoftEther VPN Bridge
SVC_VPNBRIDGE_DESCRIPT	This manages the processes of SoftEther VPN Bridge. SoftEther VPN Bridge provides a bridging connection between the network this computer is connected to and a SoftEther VPN Server that is remotely located. When this service is stopped, SoftEther VPN Bridge on this computer will stop and it will no longer be possible to communicate via the bridge connection.


# Service definition (SoftEther VPN Client)
SVC_SEVPNCLIENTDEV_NAME	sevpnclientdev
SVC_SEVPNCLIENTDEV_TITLE	Edição de desenvolvedor do SoftEther VPN Cliente
SVC_SEVPNCLIENTDEV_DESCRIPT	This manages the Virtual Network Adapter device driver and connection service for the SoftEther VPN Client. When this service is stopped, it will not be possible to use SoftEther VPN Client on this computer to connect to a SoftEther VPN Server.


# Service Definition (SoftEther VPN Server)
SVC_SEVPNSERVERDEV_NAME	sevpnserverdev
SVC_SEVPNSERVERDEV_TITLE	Edição de desenvolvedor do SoftEther VPN Servidor
SVC_SEVPNSERVERDEV_DESCRIPT	This manages the server processes of SoftEther VPN Server. SoftEther VPN Server provides high-performance SoftEther VPN Server functions via TCP/IP protocol. When this service is stopped, SoftEther VPN Server on this computer will stop and SoftEther VPN Client will be unable to establish a VPN connection with this computer.


# Service Definition (SoftEther VPN Bridge)
SVC_SEVPNBRIDGEDEV_NAME	sevpnbridgedev
SVC_SEVPNBRIDGEDEV_TITLE	Edição de desenvolvedor do SoftEther VPN Bridge
SVC_SEVPNBRIDGEDEV_DESCRIPT	This manages the processes of SoftEther VPN Bridge. SoftEther VPN Bridge provides a bridging connection between the network this computer is connected to and a SoftEther VPN Server that is remotely located. When this service is stopped, SoftEther VPN Bridge on this computer will stop and it will no longer be possible to communicate via the bridge connection.


# Service definition (SoftEther VPN User-mode Router)
SVC_VPNROUTER_NAME	vpnrouter
SVC_VPNROUTER_TITLE	Edição de desenvolvedor do SoftEther VPN Router
SVC_VPNROUTER_DESCRIPT	This manages the server processes of SoftEther VPN Router (service mode). SoftEther VPN Router is a program that provides a virtual NAT and DHCP server that operates in user mode and by using simple operations it is possible to establish a safe connection between a virtual IP network and a physical IP network. When this service is stopped, SoftEther VPN Router on this computer will stop and SoftEther VPN Client will be unable to use the routing service on this computer.


# Service Definition (EtherLogger)
SVC_ELOGSVC_NAME	elogsvc
SVC_ELOGSVC_TITLE	Edição de desenvolvedor do SoftEther EtherLogger
SVC_ELOGSVC_DESCRIPT	SoftEther EtherLogger is a service that captures data flowing through LAN cards connected to the computer and keeps a log of the headers of the packet types specified by the administrator and all data in text file format.


# Concerning SoftEther VPN Server Manager
SM_TITLE	Edição de desenvolvedor do gerenciador SoftEther VPN Servidor
SM_LOCALHOST	localhost (Este servidor)
SM_SERVER_BRIDGE_TITLE	Manage VPN Bridge "%S"
SM_S_VHUB_BRIDGE	When using VPN Bridge, you manage Virtual Hub "BRIDGE" to operate management of VPN Bridge.
SM_DISCONNECTED	The management connection has been disconnected.
SM_MIKAN	Under Construction.
SM_MAIN_COLUMN_1	Nome da configuração
SM_MAIN_COLUMN_2	Nome do host do servidor VPN
SM_MAIN_COLUMN_3	Modo de operação
SM_MODE_SERVER	Todo o servidor VPN
SM_MODE_HUB	Apenas o hub '%S'
SM_EDIT_CAPTION_1	Nova configuração de conexão
SM_EDIT_CAPTION_2	Editar %s
SM_SETTING_EXISTS	A Connection Setting with the same name as Connection Setting "%s" is already registered. Specify a different name.
SM_SETTING_DELETE_MSG	This will delete the Connection Setting "%s". Do you really want to do this?
SM_PASSWORD_TYPE_STR	Password for Administration Connection
SM_HUB_COLUMN_1	Nome do Hub Virtual
SM_HUB_COLUMN_2	Status
SM_HUB_COLUMN_3	Tipo
SM_HUB_COLUMN_4	Usuários
SM_HUB_COLUMN_5	Grupos
SM_HUB_COLUMN_6	Sessões
SM_HUB_COLUMN_7	Tabelas MAC
SM_HUB_COLUMN_8	Tabelas IP
SM_HUB_COLUMN_9	Número de logins
SM_HUB_COLUMN_10	Último login
SM_HUB_COLUMN_11	Última comunicação
SM_HUB_ONLINE	Online
SM_HUB_OFFLINE	Offline
SM_HUB_STANDALONE	Autônomo
SM_HUB_STATIC	Hub estático
SM_HUB_DYNAMIC	Hub dinâmico
SM_SERVER_STANDALONE	Standalone Server
SM_FARM_CONTROLLER	Cluster Controller
SM_FARM_MEMBER	Cluster Member Server
SM_INFORMATION	Latest Information
SM_HUB_STATUS_CAPTION	Status of Virtual Hub "%s"
SM_HUB_STATUS_HUBNAME	Nome do Hub Virtual
SM_HUB_STATUS_ONLINE	Status
SM_HUB_TYPE	Tipo
SM_HUB_NUM_SESSIONS	Sessões
SM_HUB_NUM_SESSIONS_CLIENT	Sessions (Client)
SM_HUB_NUM_SESSIONS_BRIDGE	Sessions (Bridge)
SM_HUB_NUM_ACCESSES	Listas de acesso
SM_HUB_NUM_USERS	Usuários
SM_HUB_NUM_GROUPS	Grupos
SM_HUB_NUM_MAC_TABLES	Tabelas MAC
SM_HUB_NUM_IP_TABLES	Tabelas IP
SM_HUB_SECURE_NAT	SecureNAT
SM_HUB_SECURE_NAT_YES	Ativado
SM_HUB_SECURE_NAT_NO	Desativado
SM_HUB_NUM_LOGIN	Número de logins
SM_HUB_LAST_LOGIN_TIME	Último login
SM_HUB_LAST_COMM_TIME	Última comunicação
SM_HUB_CREATED_TIME	Criado em
SM_STATUS_COLUMN_1	Item
SM_STATUS_COLUMN_2	Valor
SM_ST_SEND_UCAST_NUM	Pacotes unicast de saída
SM_ST_SEND_UCAST_SIZE	Tamanho total unicast de saída
SM_ST_SEND_BCAST_NUM	Pacotes broadcast de saída
SM_ST_SEND_BCAST_SIZE	Tamanho total broadcast de saída
SM_ST_RECV_UCAST_NUM	Pacotes Unicast de entrada
SM_ST_RECV_UCAST_SIZE	Tamanho total unicast de entrada
SM_ST_RECV_BCAST_NUM	Pacotes broadcast de entrada
SM_ST_RECV_BCAST_SIZE	Tamanho total broadcast de entrada
SM_ST_NUM_PACKET_STR	%S pacotes
SM_ST_SIZE_BYTE_STR	%S bytes
CM_EDIT_HUB_1	New Virtual Hub
CM_EDIT_HUB_2	Propriedade de %S
CM_EDIT_HUB_STANDALONE	Currently the server is operating in Standalone Mode. This Virtual Hub is operating as a Standalone Hub.
CM_EDIT_HUB_TYPE_FIXED	Currently the server is operating in Cluster Mode. This Virtual Hub is of the following type, which means it is not possible to make dynamic changes.
CM_EDIT_HUB_CREATED	A new Virtual Hub '%S' has been created.
CM_OFFLINE_MSG	Do you want to switch %s to offline?\r\n\r\nIf you switch the Virtual Hub to offline all sessions currently connected to the Virtual Hub will be disconnected and new sessions will be unable to connect.
CM_DELETE_HUB_MSG	Do you want to delete %S?\r\n\r\nIf you delete the Virtual Hub, all sessions currently connected to the Virtual Hub will be disconnected and new sessions will be unable to connect. \r\nThis will also delete all the Hub settings, user objects, group objects, certificates and Cascade Connections. \r\n\r\nOnce you delete the Virtual Hub, it cannot be recovered. \r\nAre you sure you want to delete it?
CM_HUB_DELETED_MSG	Hub Virtual %S foi excluído.
CM_LISTENER_COLUMN_1	Número da porta
CM_LISTENER_COLUMN_2	Status
CM_LISTENER_TCP_PORT	TCP %u
CM_LISTENER_ONLINE	Ouvindo
CM_LISTENER_OFFLINE	Parado
CM_LISTENER_ERROR	Erro
CM_DELETE_LISTENER_MSG	This will delete the Listener (TCP port %u). From now on, it will not be possible to connect to this port. \r\nDo you really want to do this?
CM_STOP_LISTENER_MSG	This will stop the Listener (TCP port %u). Until Listener is restarted it will not be possible to connect to this port. \r\n\r\nDo you really want to do this?
CM_CLOSE_BUTTON	Fechar
CM_CERT_SET_MSG	A new server certificate has been set.\r\n\r\nIf you are using OpenVPN protocols, please mind that you may have to update the inline certificate data in the OpenVPN configuration file.
CM_SHORTCUT_DISCONNECT	There is already an active connection to the specified connection destination. \r\n\r\nDo you want to disconnect?
SM_SERVER_STATUS	Status do servidor
SM_ST_SERVER_TYPE	Tipo de servidor
SM_ST_NUM_TCP	Number of Active Sockets
SM_ST_NUM_TCP_LOCAL	Number of Active Sockets (This Server)
SM_ST_NUM_TCP_REMOTE	Number of Active Sockets (Other Member Servers)
SM_ST_NUM_HUB_TOTAL	Number of Virtual Hubs
SM_ST_NUM_HUB_STATIC	Number of Static Virtual Hubs
SM_ST_NUM_HUB_DYNAMIC	Number of Dynamic Virtual Hubs
SM_ST_NUM_SESSION_TOTAL	Número de sessões
SM_ST_NUM_SESSION_LOCAL	Number of Sessions (This Server)
SM_ST_NUM_SESSION_REMOTE	Number of Sessions (Other Member Servers)
SM_ST_NUM_MAC_TABLE	Number of MAC Address Tables
SM_ST_NUM_IP_TABLE	Número de tabelas de endereços IP
SM_ST_NUM_USERS	Number of Users
SM_ST_NUM_GROUPS	Number of Groups
SM_ST_CLIENT_LICENSE	Using Client Connection Licenses (This Server)
SM_ST_BRIDGE_LICENSE	Using Bridge Connection Licenses (This Server)
SM_ST_CLIENT_LICENSE_EX	Using Client Connection Licenses (Entire Cluster)
SM_ST_BRIDGE_LICENSE_EX	Using Bridge Connection Licenses (Entire Cluster)
SM_ST_START_TIME	Server Started at
SM_ST_CURRENT_TIME	Data atual
SM_ST_CURRENT_TICK	64 bit High-Precision Logical System Clock
SM_ST_TOTAL_MEMORY	Total Logical Memory Size
SM_ST_USED_MEMORY	Used Logical Memory Size
SM_ST_FREE_MEMORY	Free Logical Memory Size
SM_ST_TOTAL_PHYS	Total Physical Memory Size
SM_ST_USED_PHYS	Used Physical Memory Size
SM_ST_FREE_PHYS	Free Physical Memory Size
SM_ST_RAM_SIZE_KB	%S bytes
SM_INFO_TITLE	VPN Server Version Information
SM_INFO_PRODUCT_NAME	Nome do produto
SM_INFO_VERSION	Versão
SM_INFO_BUILD	Build
SM_INFO_HOSTNAME	Nome do host
SM_OS_SYSTEM_NAME	Type of Operating System
SM_OS_PRODUCT_NAME	Product Name of Operating System
SM_OS_SERVICE_PACK	Service Pack
SM_OS_SP_TAG	Service Pack %u
SM_OS_VENDER_NAME	Operating System Vendor
SM_OS_VERSION	Operating System Version
SM_OS_KERNEL_NAME	Type of OS Kernel
SM_OS_KERNEL_VERSION	Version of OS Kernel
SM_CONNECTION_TYPE_0	Cliente
SM_CONNECTION_TYPE_1	Inicializando...
SM_CONNECTION_TYPE_2	Login
SM_CONNECTION_TYPE_3	Additional Connection
SM_CONNECTION_TYPE_4	Clustering RPC
SM_CONNECTION_TYPE_5	RPC de gerenciamento
SM_CONNECTION_TYPE_6	Hub Enumeration RPC
SM_CONNECTION_TYPE_7	Changing Password
SM_CONNECTION_TYPE_8	MS-SSTP Connection
SM_CONNECTION_TYPE_9	OpenVPN Connection
SM_CONN_COLUMN_1	Nome da conexão
SM_CONN_COLUMN_2	Origem da conexão
SM_CONN_COLUMN_3	Início da conexão
SM_CONN_COLUMN_4	Tipo
SM_HOSTNAME_AND_PORT	%S: %u
SM_CONN_DISCONNECT_MSG	This will disconnect connection %s. \r\nDo you really want to do this?
SM_CONNINFO_CAPTION	Connection %s Information
SM_CONNINFO_NAME	Nome da conexão
SM_CONNINFO_TYPE	Connection Type
SM_CONNINFO_HOSTNAME	Nome do host de origem
SM_CONNINFO_IP	Endereço IP do cliente
SM_CONNINFO_PORT	Client Port Number (TCP)
SM_CONNINFO_TIME	Início da conexão
SM_CONNINFO_SERVER_STR	Nome do produto do servidor
SM_CONNINFO_SERVER_VER	Versão sever
SM_CONNINFO_SERVER_BUILD	Server Build Number
SM_CONNINFO_CLIENT_STR	Client Product Name
SM_CONNINFO_CLIENT_VER	Versão do cliente
SM_CONNINFO_CLIENT_BUILD	Build do cliente
SM_FARM_REBOOT_MSG	You are about to change the clustering configuration. \r\n\r\nWhen you change the clustering configuration, all currently connected sessions and connections for management purposes (including this management connection) will be disconnected and the server program will restart. \r\nWhen there are many server users, it could take over a minute to restart. \r\n\r\nClick OK to automatically disconnect the connection with the server. To continue management, you will need to reconnect to the server.
SM_FM_COLUMN_1	Tipo
SM_FM_COLUMN_2	Conexão iniciada às
SM_FM_COLUMN_3	Nome do host
SM_FM_COLUMN_4	Ponto
SM_FM_COLUMN_5	Número de sessões
SM_FM_COLUMN_6	Número de conexões TCP
SM_FM_COLUMN_7	Number of Operating Hubs
SM_FM_COLUMN_8	Using Client Connection Licenses
SM_FM_COLUMN_9	Using Bridge Connection Licenses
SM_FM_CONTROLLER	Controle
SM_FM_MEMBER	Membro
SM_FMINFO_TYPE	Tipo de servidor
SM_FMINFO_CONNECT_TIME	Connection Established at
SM_FMINFO_IP	Endereço IP
SM_FMINFO_HOSTNAME	Nome do host
SM_FMINFO_POINT	Ponto
SM_FMINFO_WEIGHT	Performance Standard Ratio
SM_FMINFO_NUM_PORT	Number of Public Ports
SM_FMINFO_PORT	Public Port #%u (TCP/IP)
SM_FMINFO_NUM_HUB	Number of Running Virtual Hubs
SM_FMINFO_HUB	Hub Virtual #%u
SM_FMINFO_HUB_TAG_1	%S (Dinâmico)
SM_FMINFO_HUB_TAG_2	%S (Estático)
SM_FMINFO_NUM_SESSION	Número de sessões
SM_FMINFO_NUN_CONNECTION	Número de conexões TCP
SM_FMINFO_CAPTION	Cluster Member Server Status
SM_FC_STATUS_CAPTION	Connection to Cluster Controller Status
SM_FC_IP	Controller IP Address
SM_FC_PORT	Controller TCP/IP Port
SM_FC_STATUS	Status da conexão
SM_FC_ONLINE	Online
SM_FC_OFFLINE	Offline
SM_FC_LAST_ERROR	Último erro
SM_FC_ERROR_TAG	%s (Código de erro: %u)
SM_FC_START_TIME	Conexão iniciada às
SM_FC_FIRST_TIME	First Connection Established at
SM_FC_CURRENT_TIME	Current Connection Established at
SM_FC_NUM_TRY	Number of Connection Attempts
SM_FC_NUM_CONNECTED	Number of Successful Connections
SM_FC_NUM_FAILED	Number of Failed Connections
SM_FC_NOT_CONNECTED	(Not Connected)
SM_CHANGE_PASSWORD_1	The passwords you entered did not match. Enter the same password in Confirm as you enter in Password.
SM_CHANGE_PASSWORD_2	You have entered an empty password. Continue anyway?
SM_CHANGE_PASSWORD_3	A senha foi alterada.
SM_USER_COLUMN_1	Nome de usuário
SM_USER_COLUMN_2	Nome completo
SM_USER_COLUMN_3	Nome do grupo
SM_USER_COLUMN_4	Descrição
SM_USER_COLUMN_5	Método de autenticação
SM_USER_COLUMN_6	Número de logins
SM_USER_COLUMN_7	Último login
SM_AUTHTYPE_0	Anônima
SM_AUTHTYPE_1	Senha
SM_AUTHTYPE_2	Certificado individual
SM_AUTHTYPE_3	Certificado assinado
SM_AUTHTYPE_4	RADIUS
SM_AUTHTYPE_5	Domínio NT
SM_NO_GROUP	-
SM_USER_DELETE_MSG	Isso excluirá o usuário "%s". Você realmente quer fazer isso?
SM_EDIT_USER_CAPTION_1	Criar novo usuário
SM_EDIT_USER_CAPTION_2	Propriedades do usário %S
SM_EDIT_USER_CERT_INFO	Os usuários que usam 'Autenticação de certificado individual' serão permitidos ou negados, dependendo de o certificado do cliente SSL corresponder completamente o certificado que foi definido anteriormente para o usuário.
SM_EDIT_USER_POL_DLG	Security Policy of User %S
SM_POLICY_DEF_CAPTION	Política de segurança
SM_LIMIT_STR	Specify an integer that is within the range %u to %u.
SM_POLICY_INIT_TITLE	Select a policy item from the list on the left.
SM_USER_CREATE_OK	User %S has been created.
SM_USERINFO_CAPTION	User "%S" Information
SM_USERINFO_NAME	Nome de usuário
SM_USERINFO_GROUP	Nome do grupo
SM_USERINFO_CREATE	Criado em
SM_USERINFO_UPDATE	Atualizado em
SM_USERINFO_EXPIRE	Data de validade
SM_USERINFO_NUMLOGIN	Number of Logins
SM_GROUPLIST_NAME	Nome do grupo
SM_GROUPLIST_REALNAME	Nome completo
SM_GROUPLIST_NOTE	Descrição
SM_GROUPLIST_NUMUSERS	Num Usuários
SM_EDIT_GROUP_CAPTION_1	Creation of New Group
SM_EDIT_GROUP_CAPTION_2	Propriedades do grupo %S
SM_GROUP_CREATED	Group %S has been created.
SM_GROUP_DELETE_MSG	Group %S has been deleted. Do you really want to do this?
SM_GROUP_POLICY_CAPTION	Security Policy of Group %S
SM_GROUP_MEMBER_STR	\ (Display only users belonging to group %S)
SM_SELECT_GROUP	&Selecionar
SM_SELECT_NO_GROUP	&Nenhum
SM_SELECT_ALT_GROUP	Select a &Group...
SM_ACCESS_COLUMN_0	ID
SM_ACCESS_COLUMN_1	Ação
SM_ACCESS_COLUMN_2	Status
SM_ACCESS_COLUMN_3	Prioridade
SM_ACCESS_COLUMN_4	Lembrete
SM_ACCESS_COLUMN_5	Conteúdo
SM_ACCESS_COLUMN_6	ID única
SM_ACCESS_PASS	Senha
SM_ACCESS_DISCARD	Descartar
SM_ACCESS_ENABLE	Ativar
SM_ACCESS_DISABLE	Desativar
SM_ACCESS_PROTO_1	All IPv4 / IPv6 Protocols
SM_ACCESS_PROTO_2	6 (TCP/IP Protocol)
SM_ACCESS_PROTO_3	17 (UDP/IP Protocol)
SM_ACCESS_PROTO_4	1 (ICMPv4 Protocol)
SM_ACCESS_PROTO_5	58 (ICMPv6 Protocol)
SM_ACCESS_PROTO_6	Specify the IP Protocol Number
SM_SELECT_USER	&Selecionar
SM_SELECT_NO	&Não selecionar
SM_PLEASE_SELECT	Selecinar usuário.
SM_LINK_COLUMN_1	Nome da configuração
SM_LINK_COLUMN_2	Status
SM_LINK_COLUMN_3	Estabelecido em
SM_LINK_COLUMN_4	Destination VPN Server
SM_LINK_COLUMN_5	Hub Virtual
SM_LINK_STATUS_OFFLINE	Offline (Stopped)
SM_LINK_STATUS_ERROR	Erro %u: %s
SM_LINK_STATUS_ONLINE	Online (Established)
SM_LINK_POLICY_GROUP	Cascade Connection Setting
SM_LINK_POLICY_CAPTION	Security policy settings applicable to Cascade sessions
SM_LINK_CONNECTING	Conectando
SM_LINK_SAVE_ONLINE	Although the Cascade Connection Setting "%s" has been changed, this Cascade Connection is currently online. The setting will not be applied until next time the connection is established.
SM_LINK_DELETE_MSG	This will delete the settings for Cascade Connection "%s". Do you really want to do this?
SM_LINK_OFFLINE_MSG	Currently Cascade Connection "%s" is active. Do you want to disconnect this connection?
SM_LINK_STATUS_CAPTION	Connection status of Cascade Connection "%s"
SM_LOG_SWITCH_0	No Switching
SM_LOG_SWITCH_1	Switch in Every Second
SM_LOG_SWITCH_2	Switch in Every Minute
SM_LOG_SWITCH_3	Switch in Every Hour
SM_LOG_SWITCH_4	Switch in Every Day
SM_LOG_SWITCH_5	Switch in Every Month
SM_SESS_DISCONNECT_MSG	This will disconnect session "%S". Do you really want to do this?
SM_SESS_COLUMN_1	Nome da sessão
SM_SESS_COLUMN_2	Localização
SM_SESS_COLUMN_3	Nome de usuário
SM_SESS_COLUMN_4	Nome do host de origem
SM_SESS_COLUMN_5	TCP Connections
SM_SESS_COLUMN_6	Bytes transferidos
SM_SESS_COLUMN_7	Pacote transferidos
SM_SESS_COLUMN_8	ID VLAN
SM_SESS_NORMAL	Sessão local
SM_SESS_LOCAL	Sessão local
SM_SESS_LOCAL_2	Em '%S'
SM_SESS_REMOTE	Em '%S'
SM_SESS_LINK	Cascade Connection
SM_SESS_LINK_HOSTNAME	Host virtual
SM_SESS_LINK_TCP	Nenhum
SM_SESS_SNAT	SecureNAT Session
SM_SESS_SNAT_HOSTNAME	Host virtual
SM_SESS_SNAT_TCP	Nenhum
SM_SESS_BRIDGE	Local Bridge Session
SM_SESS_BRIDGE_HOSTNAME	Ethernet Bridge
SM_SESS_LAYER3_HOSTNAME	Virtual Layer 3 Switch
SM_SESS_BRIDGE_TCP	Nenhum
SM_SESS_STATUS_CAPTION	VPN Session "%S" Status
SM_SESS_STATUS_USERNAME	User Name (Authentication)
SM_SESS_STATUS_REALUSER	User Name (Database)
SM_SESS_STATUS_GROUPNAME	Nome do grupo
SM_CLIENT_IP	Endereço IP do cliente
SM_CLIENT_HOSTNAME	Nome do Host do Cliente
SM_NODE_CLIENT_NAME	Client Product Name (Reported)
SM_NODE_CLIENT_VER	Client Version (Reported)
SM_NODE_CLIENT_BUILD	Client Build (Reported)
SM_NODE_SERVER_NAME	Server Product Name (Reported)
SM_NODE_SERVER_VER	Server Version (Reported)
SM_NODE_SERVER_BUILD	Server Build (Reported)
SM_NODE_CLIENT_OS_NAME	Client OS Name (Reported)
SM_NODE_CLIENT_OS_VER	Client OS Version (Reported)
SM_NODE_CLIENT_OS_PID	Client OS Product ID (Reported)
SM_NODE_CLIENT_HOST	Client Host Name (Reported)
SM_NODE_CLIENT_IP	Client IP Address  (Reported)
SM_NODE_CLIENT_PORT	Client Port (Reported)
SM_NODE_SERVER_HOST	Server Host Name (Reported)
SM_NODE_SERVER_IP	Server IP Address (Reported)
SM_NODE_SERVER_PORT	Server Port (Reported)
SM_NODE_PROXY_HOSTNAME	Proxy Host Name (Reported)
SM_NODE_PROXY_IP	Proxy IP Address (Reported)
SM_NODE_PROXY_PORT	Proxy Port (Reported)
SM_MAC_COLUMN_1	Nome da sessão
SM_MAC_COLUMN_2	Endereço MAC
SM_MAC_COLUMN_3	Criado em
SM_MAC_COLUMN_4	Atualizado as
SM_MAC_COLUMN_5	Localização
SM_MAC_COLUMN_1A	ID VLAN
SM_SESSION_FILTER	\ (Displays only entries of session %S)
SM_IP_COLUMN_1	Nome da sessão
SM_IP_COLUMN_2	Endereço IP
SM_IP_COLUMN_3	Criado em
SM_IP_COLUMN_4	Atualizado as
SM_IP_COLUMN_5	Localização
SM_MAC_IP_DHCP	%S (DHCP)
SM_MACIP_LOCAL	On This Server
SM_MACIP_SERVER	Em '%S'
SM_SNAT_STATUS	SecureNAT Operating Status
SM_SNAT_NUM_SESSION	%u Sessão
SM_SNAT_NUM_CLIENT	%u Cliente
SM_SNAT_IS_KERNEL	Kernel-mode NAT is Active
SM_SNAT_IS_RAW	Raw IP mode NAT is Active
SM_BRIDGE_TOO_OLD_VER	The Local Bridge function is not supported by the version of the VPN Server that is currently connected. \r\nTry update to a new version.
SM_BRIDGE_UNSUPPORTED	Unable to use the Local Bridge function with the operating system that this VPN Server is operating on. For the list of operating system that the Local Bridge function can be used on, refer to the online documentation of the VPN Server.
SM_BRIDGE_WPCAP_REMOTE	In order to use the Local Bridge function on this VPN Server, you must install the WinPcap software. The software WinPcap is currently not installed on the server computer. \r\n\r\nTo continue the installation of the WinPcap software, you must start SoftEther VPN Server Manager on the server computer that is running VPN Server and then while connected to localhost (location of your own computer), have the Local Bridge Function Setting window displayed. \r\nTo continue, first exit this management session, and then, after starting SoftEther VPN Server Manager on the server computer, connect to localhost and continue the setting process. 
SM_BRIDGE_WPCAP_ROOT	In order to use the Local Bridge function on this VPN Server, you must install the WinPcap software. \r\n\r\nTo continue the installation you must log in to this computer as a user with administrator privileges. \r\nLog on as an administrator and start the SoftEther VPN Server Manager again.
SM_BRIDGE_WPCAP_INSTALL	In order to use the Local Bridge function on this VPN Server, you must install the WinPcap software. The software WinPcap is currently not installed on the server computer. \r\n\r\nWinPcap is an easy-to-install free software that is bundled together with the VPN Server. \r\n\r\nDo you want to begin the installation of WinPcap?
SM_BRIDGE_WPCAP_REBOOT1	After WinPcap installation has completed, you must restart the computer before you use the Local Bridge function again. \r\n\r\nAfter you restart the computer manually and start VPN Server, configure the settings for the Local Bridge function.
SM_BRIDGE_WPCAP_REBOOT2	After WinPcap installation has completed, you must restart the SoftEther VPN Server service before you use the Local Bridge function again. \r\n\r\nIt only takes a short time to restart the SoftEther VPN Server service, however all sessions that are currently connected to the VPN Server will be disconnected. \r\nThis management session will also be disconnected, so you will need to reconnect to continue. \r\n\r\nDo you want to restart the SoftEther VPN Server service?
SM_BRIDGE_RESOURCE	Unable to load the WinPcap driver.
SM_BRIDGE_COLUMN_1	Número
SM_BRIDGE_COLUMN_2	Nome do Hub Virtual
SM_BRIDGE_COLUMN_3	Network Adapter or Tap Device Name
SM_BRIDGE_COLUMN_4	Status
SM_BRIDGE_OFFLINE	Offline
SM_BRIDGE_ONLINE	Operativo
SM_BRIDGE_ERROR	Erro
SM_BRIDGE_OK	The Local Bridge connection definition has been added.
SM_BRIDGE_DELETE	Do you want to delete the Local Bridge from Virtual Hub "%s" to device "%s"?
SM_BRIDGE_DELETE_OK	The Local Bridge has been deleted.
SM_BRIDGE_INTEL	While in the condition that occurs immediately after a new bridge connection is made when bridging to a physical network adapter, depending on the type of network adapter, there are cases where it will not be possible to communicate using TCP/IP to the network adapter using a bridge connection from a computer on the virtual network. \r\n(This phenomenon is known to occur for Intel and Broadcom network adapters.) \r\n\r\n\r\nIf this issue arises, remedy the situation by restarting the computer on which VPN Server / Bridge is running. Normal communication will be possible after the computer has restarted. \r\n\r\n\r\nAlso many wireless network adapters will not respond to the sending of packets in promiscuous mode and when this occurs you will be unable to use the Local Bridge. If this issue arises, try using a regular wired network adapter instead of the wireless network adapter.
SM_BRIDGE_VPN	You are attempting to make a Local Bridge to "%S".\r\n\r\nA Local Bridge is made between a Virtual Hub and a physical network adapter in usual usage. It is unusual to make a Local Bridge to a Virtual Network Adapter.\r\nPlease make sure that it is your intention.\r\n\r\nDo you really want to continue?
SM_BRIDGE_INFO_1	Selecione o dispositivo Ethernet (adaptador de rede) a ser usado como destino da bridge.
SM_BRIDGE_INFO_2	Enter a name of the new tap device to create.
SM_CONFIG_SAVED	The configuration file has been saved.
SM_CONFIG_SAVE_FAILED	Failed to save the configuration file.
SM_CONFIG_OPEN_FAILED	Unable to open the specified file.
SM_CONFIG_CONFIRM	This will apply the specified configuration file to the VPN Server. The VPN Server will automatically restart and it will start loading the new configuration file. The users who are currently connected to the VPN Server will be disconnected. This management session will also be disconnected, you will be needing to reconnect to the server. \r\n\r\nDo you want to proceed?
SM_CONFIG_WRITE_OK	The configuration file on the server side has been overwritten.
SM_AO_COLUMN_1	Item
SM_AO_COLUMN_2	Valor
SM_TRUE_OR_FALSE	Set either 0 (false) or 1 (true) for this item.
SM_AO_SET_OK	The Virtual Hub Administration Option has been set.
SM_EXT_OPTION_SET_OK	The Virtual Hub Extended Option has been set.
SM_PASSWORD_MSG	Currently an administrator password has not been set for this VPN Server. It is recommended that a password is set. \r\n\r\nDo you want to set a server administrator password?
SM_L3_SW_COLUMN1	Layer 3 Switch Name
SM_L3_SW_COLUMN2	Running Status
SM_L3_SW_COLUMN3	Interfaces
SM_L3_SW_COLUMN4	Routing Tables
SM_L3_SW_ST_F_F	Parar
SM_L3_SW_ST_T_F	Iniciar (erro) 
SM_L3_SW_ST_T_T	Iniciar (executando)
SM_L3_SW_DEL_MSG	This will delete the Virtual Layer 3 Switch "%S". \r\nDo you really want to do this?
SM_L3_SW_IF_COLUMN1	Endereço IP
SM_L3_SW_IF_COLUMN2	Máscara de sub-rede
SM_L3_SW_IF_COLUMN3	Nome do Hub Virtual
SM_L3_SW_TABLE_COLUMN1	Network Address
SM_L3_SW_TABLE_COLUMN2	Máscara de sub-rede
SM_L3_SW_TABLE_COLUMN3	Gateway Address
SM_L3_SW_TABLE_COLUMN4	Métrica
SM_SECURE_NAT_MSG	Are you sure you want to enable the SecureNAT?\r\n\r\nIf you enable the SecureNAT, a virtual router with virtual NAT function will be created that has one IP address in the Virtual Hub. This Virtual Router will interact as one computer or router with other computers that are connected to the virtual network. \r\n\r\nThe SecureNAT in the Virtual NAT enables any computers connected to the Virtual Hub to establish communication with an external network via the SecureNAT. \r\nTherefore, when SecureNAT is running on this VPN Server, there is no need to use local VPN Client to connect the self-computer's Virtual Hub.\r\n\r\n\r\nAlso, please take care about that if there is already a DHCP server in a location that can be reached from a Virtual Hub Layer 2 segment, disable the DHCP server function by clicking the SecureNAT Configuration, otherwise there will be a DHCP conflict. \r\n\r\nMoreover, you can disable the NAT function and only use the DHCP server if you wish.
SM_CRL_COLUMN_1	Certificate Summary
SM_CRL_DELETE_MSG	This will delete the selected item. Do you really want to do this?
SM_CRL_EMPTY_MSG	No items have been selected. \r\nIf you add this certificate revocation entry, all certificates will be judged as invalid and all client connections that are made in certificate authentication mode will be refused. \r\n\r\nDo you really want to do this?
SM_AC_COLUMN_1	ID
SM_AC_COLUMN_2	Prioridade
SM_AC_COLUMN_3	Ação
SM_AC_COLUMN_4	Conteúdo
SM_AC_PASS	Senha
SM_AC_DENY	Negar
SM_LOG_FILE_COLUMN_1	Nome do arquivo de log
SM_LOG_FILE_COLUMN_2	Tamanho do arquivo
SM_LOG_FILE_COLUMN_3	Atualizado em
SM_LOG_FILE_COLUMN_4	Localização
SM_READ_LOG_FILE_INFO_1	Please wait until processing is finished...
SM_READ_LOG_FILE_INFO_2	%S em prograsso, %S terminou...
SM_READ_LOG_FILE_ERROR	Failed to download file
SM_READ_SAVE_DLG_TITLE	Specify a File Name for the Log File's Save Destination
SM_READ_SAVE_DLG_FILTER	Log Files (*.LOG)|*.log|All Files (*.*)|*.*
SM_READ_SAVE_FAILED	Failed to save the log file.
SM_READ_SAVE_TMP_FAILED	Unable to write to temporary file "%S".
SM_READ_SAVE_OPEN_ERROR	Unable to open temporary file "%S". \r\n\r\nIt is possible that the .LOG file extension is not an assigned file type in Windows.
SM_LICENSE_COLUMN_1	Número
SM_LICENSE_COLUMN_2	Chave de licença
SM_LICENSE_COLUMN_3	License Type Name
SM_LICENSE_COLUMN_4	Status
SM_LICENSE_COLUMN_5	Data de validade
SM_LICENSE_COLUMN_6	ID da licença
SM_LICENSE_COLUMN_7	License Type ID
SM_LICENSE_COLUMN_8	ID servidor
SM_LICENSE_COLUMN_9	ID serial
SM_LICENSE_INFINITE	Infinito
SM_LICENSE_NO_EXPIRES	Sem expiração
SM_LICENSE_STATUS_EDITION	Product Edition
SM_LICENSE_STATUS_RELEASE	Release Date of VPN Server
SM_LICENSE_STATUS_SYSTEM_ID	Current Server ID
SM_LICENSE_STATUS_EXPIRES	Expiration of Current Product License
SM_LICENSE_STATUS_SUBSCRIPTION	Status of Subscription Contract
SM_LICENSE_STATUS_SUBSCRIPTION_NONEED	No Need (This Edition requires no subscription keys)
SM_LICENSE_STATUS_SUBSCRIPTION_NONE	No Keys (Adding a subscription key is required)
SM_LICENSE_STATUS_SUBSCRIPTION_VALID	Subscription is Active [Until %s]
SM_LICENSE_STATUS_SUBSCRIPTION_EXPIRED	Subscription is Expired [at %s]
SM_LICENSE_STATUS_SUBSCRIPTION_BUILD	Version Allowed by Current Contract
SM_LICENSE_STATUS_SUBSCRIPTION_BUILD_STR	Free Upgrade to Any Future Versions Released Until %s is Allowed
SM_LICENSE_STATUS_ENTERPRISE	Enterprise Functions Availability
SM_LICENSE_STATUS_ENTERPRISE_YES	Yes (Available)
SM_LICENSE_STATUS_ENTERPRISE_NO	No (Unavailable)
SM_LICENSE_NUM_USER	Allowed User Objects to Create
SM_LICENSE_NUM_CLIENT	Allowed Concurrent Clients
SM_LICENSE_NUM_BRIDGE	Allowed Concurrent Bridges
SM_NO_LICENSE_COLUMN	Cuidado: 
SM_NO_LICENSE	Because there are no product licenses registered, this VPN Server's communication function doesn't operate.
SM_LICENSE_DELETE_MSG	Are you sure you want to delete the selected license from the VPN Server?
SM_SYSLOG_0	Disable Syslog Send Function
SM_SYSLOG_1	Send Server Logs by Syslog
SM_SYSLOG_2	Send Server and Virtual Hub Security Logs by Syslog
SM_SYSLOG_3	Send Server, Virtual Hub Security, and Packet Logs by Syslog
SM_SETUP_INFO_1	Clique em Próximo para iniciar a instalação. Clique em Fechar se desejar sair da instalação e definir manualmente todas as configurações.
SM_SETUP_INFO_2	Click Close to configuring the settings of a VPN server manually by yourself.
SM_SETUP_BRIDGE_ONLY	You are currently connected to VPN Bridge. You can only create VPN Bridge at Each Site for Multi-site VPN.
SM_SETUP_BRIDGE_EDGE	VPN Bridge at &Each Site
SM_SETUP_WARNING	As configurações atuais deste servidor VPN ou Bridge VPN serão criadas.\r\nDeseja realmente fazer isso?
SM_SETUP_SELECT	Select the Ethernet device to establish the bridge connection.
SM_SETUP_NO_LICENSE_KEY	Currently there is no licenses registered for this SoftEther VPN Server. \r\n\r\nFor SoftEther VPN Server to operate as a VPN server, you must enter a license key. \r\nDo you want to display the License Manager?\r\n\r\n(To use the VPN Server as a Trial Version, you have to obtain a trial key from the SoftEther VPN Project web site.\r\nClick Yes and click Obtain or Extend of License button to obtain a trial key.
SM_HUBEXT_OPTION_TITLE	Virtual Hub Extended Options
SM_HUBEXT_OPTION_STATIC1	Virtual Hub Extended Options allows you to configure more detailed parameters of this Virtual Hub.
SM_HUBEXT_OPTION_STATIC2	By default, both VPN Server's global administrators and individual Virtual Hub's administrators can modify the Virtual Hub Extended Options.\nHowever, if the deny_hub_admin_change_ext_option is set to 1 on the Virtual Hub Admin Options, the individual Virtual Hub's administrators cannot modify the Virtual Hub Extended Options. (View only.)
SM_VLAN_COLUMN_0	Nome do adaptador de rede
SM_VLAN_COLUMN_1	Tipo de driver
SM_VLAN_COLUMN_2	Nome do arquivo do driver
SM_VLAN_COLUMN_3	VLAN Transparency Setting
SM_VLAN_COLUMN_4	GUID
SM_VLAN_COLUMN_5	Device Instance ID
SM_VLAN_YES	Ativado
SM_VLAN_NO	Não ativado
SM_VLAN_MSG_1	The Windows Registry has been configured to allow the network adapter "%S" to transmit / receive tagged-VLAN packets.\r\n\r\nHowever, there are some network adapters which requires additional settings on the property of the Device Manager on the local computer's Windows to set the parameters to enable Jumbo Frames. (Ethernet frames which are larger than 1,512 bytes.) Unless you enable Jumbo Frames, some large VLAN packets will be dropped. In the case if large VLAN packets always disappeared, please enable Jumbo Frames. (For example, set the maximum size to 4,088 bytes.) The Device Manager in Windows will help you to configure.\r\n\r\nThis VLAN Transparency Setting has been written to the Windows Registry, however it is not guaranteed that VLAN packets can be transmitted effectively.\r\nIf transmitting VLAN tagged packets will fail after this configuration, refer the manual of the network adapter "%S" to configure manually and adequately. Moreover, "%S" might not support the VLAN transparency setting. In that case, such a network adapter cannot be used to transmit VLAN frames. Use other products.\r\n\r\nTo apply this setting, Windows which runs VPN Server must be rebooted. Do not forget to reboot it.
SM_VLAN_MSG_2	The Windows Registry parameters which was enabling the VLAN transparency features on the network adapter "%S" are deleted from the Registry.\r\n\r\nIf you did a Jumbo Frame enable settings last time, undo such changes manually.\r\n\r\nTo apply this setting, Windows which runs VPN Server must be rebooted. Do not forget to reboot it.
SM_VLAN_NOTHING	There are no network adapters which VLAN Transparency Setting Tool supports on the computer "%S".\r\n\r\nHowever, some network adapters are capable to transmit VLAN tagged packets by default, or can be configured to perform VLAN tagged packets by specific configuration utility provided by the vendor.\r\nBy using such network adapters, you have to configure such settings by yourself manually.
SM_SERVER_ADMIN_MSG	VPN Server / Bridge "%S"
SM_ETHERIP_COLUMN_0	ISAKMP Phase 1 ID
SM_ETHERIP_COLUMN_1	Nome do Hub Virtual
SM_ETHERIP_COLUMN_2	Nome de usuário
SM_ETHERIP_ADD_OK	A new EtherIP / L2TPv3 client setting has been registered.
SM_IPSEC_SETUP_QUESTION	This VPN Server has a function to accept IPsec / L2TP / EtherIP / L2TPv3 compatible VPN clients or VPN router products.\r\n\r\nYou can allow the VPN Server to accept connections from smartphones such as iPhone, iPad, Android, or standard VPN client functions on Mac OS X or Windows.\r\n\r\nDo you want to set up the IPsec?\r\n(IPsec settings can be configured by clicking "IPsec / L2TP Settings" button any time later.)
SM_OPENVPN_CONFIG_SAVE_OK	The ZIP file '%s' which contains the setting files for OpenVPN.\r\n\r\nOpen this ZIP file to extract sample configuration files for OpenVPN which can be used immediately and easily.\r\nYou might be required to revise the configuration file a little.\r\n\r\nFor details please read the 'readme.txt' file in the ZIP file.\r\n\r\nDo you want to open this ZIP file now?
SM_OPENVPN_CONFIG_SAVE_NG	Failed to save the ZIP file '%s'.
SM_OPENVPN_CONFIG_OPEN_NG	Failed to open the ZIP file '%s'. Please open this file manually.
SM_DDNS_IPV4_ERROR	Unable to reach the IPv4 DDNS Server.
SM_DDNS_IPV6_ERROR	Unable to reach the IPv6 DDNS Server.
SM_DDNS_FQDN_EMPTY	(Nenhum)
SM_DDNS_OK_MSG	O nome do host DNS dinâmico: %S%S\r\n\r\nVocê pode acessar o endereço IP abaixo especificando o nome de host DNS acima.\r\n\r\nEndereçoIPv4: %s\r\nEndereço IPv6: %s\r\n\r\nVocê também pode usar as seguintes formas especiais de nomes de host para especificar IPv4 ou IPv6 como o tipo de conexão.\r\n\r\nHostname para IPv4: %S.v4%S\r\nHostname para IPv6: %S.v6%S\r\n
SM_DDNS_OK_TITLE	Função de DNS dinâmico
SM_DDNS_OK_MSG2	The Dynamic DNS hostname has been changed to '%S'.\r\n\r\nClick Hint to read additional information.
SM_DDNS_KEY_TITLE	Dynamic DNS Key
SM_DDNS_KEY_MSG	Sua chave privada de DNS dinâmico: %s\r\n\r\nEsta é a chave privada associada ao seu nome DDNS atual. Se o servidor VPN perder a chave, o nome DDNS atual será ocupado para sempre e outro servidor VPN não poderá usar o mesmo nome.\r\nSe você quiser continuar usando o mesmo nome, mantenha a chave em um local seguro, como um armazenamento na Internet, outro PC ou um bloco de notas.\r\nAo aplicar a chave ao novo servidor VPN, edite o arquivo de configuração do servidor VPN para substituir a chave pela string no valor a seguir para "byte Key" na diretiva "declare DDnsClient".\r\nNão use a chave em dois ou mais servidores VPN ao mesmo tempo.
SM_DDNS_KEY_ERR	Failed to read the DNS key.
SM_IPSEC_PSK_TOO_LONG	The pre-shared key (PSK) has 10 or more letters.\r\n\r\nIt is reported that several versions of Google Android has a serious bug with 10 or more letters pre-shared key.\r\nTherefore 9 or less letters are recommended for pre-shared key.\r\n\r\nDo you want to try another pre-shared key?
SM_ADVANCED_REDIRECT_URL_HINT_TITLE	How to Use Advanced HTTP Redirection Function
SM_ADVANCED_REDIRECT_URL_HINT	Advanced HTTP Redirection (For Experts)\r\n\r\nThe string "<INFO>" is a place holder. It can embedded on the URL of redirection.\r\n\r\nEmbedded URL Example:\r\nhttp://www.google.com/search?q=<INFO>|secret\r\n\r\nWhen the client is being redirected, the actual destination URL of redirection will be replaced as follows.\r\n\r\nUsername|Session ID|IP Address|Date and Time|Hash Value\r\n\r\\nAfter Replacement Example: zurukko|SID-ZURUKKO-123|219.117.219.154|20131117100354|99707160AFE7A454042B2C47B064112D652452D7\r\n\r\nThe details of each fields are described as following.\r\n\r\nUsername: The username using for the current VPN Session will be placed.\r\n\r\nSession ID: The Session ID of the VPN Session will be placed.\r\n\r\nDate and Time: 14-digits will be placed as 'YYYYMMDDHHMMSS' format (Time zone is UTC).\r\n\r\nHash Value: A 40-characters hexadecimal strings which represent 20 bytes binary data. The binary data is the result of SHA-1 hash function to the temporary string. The temporary string is the combination of the bit-array of the above fields plus the secret string after the '|' symbol in the redirection URL. (In the above example, "secret" is the secret string.) If there are no '|' symbols in the URL, no hash value will be appended.\r\n\r\nThe Purpose of Hash Value: The secret string is effective as the secret key. Thanks to the secret key, the CGI program which receives the query strings on the redirected URL can verify the integrity of the parameters included in the URL.\r\n
SM_ADVANCED_REDIRECT_URL_MSG	An URL must start with "http://" or "https://"
SM_DISABLE_DDNS_HINT_CAPTION	Disable Dynamic DNS Function
SM_DISABLE_DDNS_HINT	To disable the Dynamic DNS Function, modify the configuration file of VPN Server.\r\n\r\nThe "declare root" directive has the "declare DDnsClient" directive. In this directive, you can switch "bool Disable" from false to true, and reboot the VPN Server, then the Dynamic DNS Function will be disabled.\r\n
SM_REGENERATE_CERT_MSG	The certificate of VPN Server is being replaced to the new one.\r\n\r\nThis will affect all VPN Clients which are configured to verify the certificate of VPN Server.\r\nDo you want to continue?
SM_DDNS_SERVER_CERT_MSG	The DDNS hostname has been changed to "%S".\r\n\r\nIf you are planning to use Microsoft SSTP VPN to connect to the VPN Server from Windows Vista or greater versions of Windows with specifying the DDNS hostname as the destination of VPN Server, the destination hostname of the VPN Server must exactly match to the CN (Common Name) field on the certificate of VPN Server due to the security.\r\n\r\nDo you want to regenerate the server certificate in order to match the CN value to "%S"?\r\n(Click No to keep using the current server certificate.)
SM_DDNS_SERVER_CERT_OK	The SSL certificate of VPN Server is now regenerated.\r\n\r\nWhen you make Microsoft SSTP VPN client connects to the VPN Server, you should specify the current DDNS hostname "%S" as the destination server hostname.\r\nYou have to also prepare the "Trusted Root Certificates" list on the Windows to add the certificate of this VPN Server beforehand.\r\n(To install a root certificate to Windows, open MMC and navigate to "Local Computer" in the "Certificates" applet. After that, you can import a certificate into the trusted root certification list.\r\n For details refer Microsoft's documents.)\r\n\r\nDo you want to save the new SSL certificate as a file in the X.509 format?
SM_SETUP_STEP_SECURENAT	This VPN Server / Bridge might be running as user-more, or by other limitations, the Virtual Hub and a physical network adapter cannot be bridged together. Instead, the SecureNAT function allows VPN Clients to communicate with other computers in the physical network. The SecureNAT function was enabled by default. You can configure or disable it.
SM_SETUP_STEP_SECURENAT_TITLE	Step 3. Bridge Virtual Hub and Physical Network
SM_UPDATE_CHECK_TITLE_VPNSERVER	%S VPN Server (on the host '%S')
SM_UPDATE_CHECK_TITLE_VPNBRIDGE	%S VPN Bridge (on the host '%S')
SM_FACTORY_DEFAULT_WARNING	This will perform a factory-reset on the VPN Server / Bridge.\r\nThe current configuration of VPN Server / Bridge will be erased, and the initial settings will be applied immediately.\r\nYou are recommended to make a backup copy of the current configuration before do a factory-reset.\r\n\r\nPress OK to perform a factory-reset. The VPN Server / Bridge will be rebooted. The current management connection will be disconnected, so please re-connect to the VPN Server / Bridge.\r\n\r\nPress Cancel to cancel the operation.
SM_FACTORY_DEFAULT_PERFORMED	The factory-reset operation is performing on the server.\r\n\r\nPress OK to exit the current session of VPN Server Manager.\r\nAfter exiting, please re-start the VPN Server Manager and connect to the VPN Server again.\r\nThen you will see the VPN Server is reset.
SM_AZURE_STATUS_CONNECTED	Status: Conectado
SM_AZURE_STATUS_NOT_CONNECTED	Status: Desconectado
SM_NO_BRIDGE_NICS	No physical network adapters suitable for Local Bridge were found on the VPN server computer.\r\nIn order to create a Local Bridge, you have to install at least one physical network adapters on the computer.\r\nYou cannot use Wi-Fi adapters or 3G adapters for Local Bridge.\r\nPlease install a physical network adapter which is compatible to wired Ethernet.\r\n\r\nIf a recently-installed network adapter doesn't appear, once reboot the computer.\r\n\r\nIf the Local Bridge cannot be used anyway, you can use "SecureNAT Function" instead.\r\n\r\nIf you have a certain reason to use unusual network adapters (i.e. Wi-Fi adapters, 3G adapters or virtual adapters), set the "ShowAllInterfaces" variable on the "LocalBridgeList" directive to "true" and restart the VPN Server. Then such devices will appear on the list. (For advanced Windows users only.)\r\n\r\nIf this error occurs after you upgraded Windows, please re-install SoftEther VPN Server or SoftEther VPN Bridge>
SM_CERT_MESSAGE	The current SSL self-signed root certificate on this VPN Server is in the old format.\r\n\r\nSome versions of OpenVPN Connect for Android have a bug to misinterpret SSL certificates in the old format. It might cause the connection problem from OpenVPN Connect for Android to this VPN Server.\r\n\r\nIf you are planning to use OpenVPN Connect for Android as a VPN client, it is recommended to regenerate the SSL server certificate.\r\n\r\nDo you want to regenerate the server certificate now?
SM_CERT_MESSAGE_CLI --- Caution ---\r\n\r\nThe current SSL self-signed root certificate on this VPN Server is in the old format.\r\n\r\nSome versions of OpenVPN Connect for Android have a bug to misinterpret SSL certificates in the old format. It might cause the connection problem from OpenVPN Connect for Android to this VPN Server.\r\n\r\nIf you are planning to use OpenVPN Connect for Android as a VPN client, it is recommended to regenerate the SSL server certificate.\r\n\r\nTo regenerate and update the server certificate, execute the "ServerCertRegenerate" command after updating the VPN Server to the latest version.
SM_CERT_NEED_ROOT	The specified SSL certificate is a sub-certificate which was issued by a CA (Certificate Authority).\r\n\r\nIf you are planning to support either Microsoft SSTP or OpenVPN protocol on this VPN server, you have to install the root certificate and all intermediate certificates (if exists) on this VPN Server.\r\n\r\nTo install these certificates, copy the root certificate and all intermediate certificate files (in the X.509 format) into the "chain_certs" subdirectory on the directory which is VPN Server has been installed on.\r\n\r\nIf you don't know how to obtain root and intermediate certificate files for your certificate authority (CA), please refer to the CA's web site or contact technical support staffs of the CA.


# Concerning User-mode Router Administration Tools
NM_TITLE	excluído
NM_CONNECT_TITLE	excluído
NM_STATUS_TAG	Connection status: %s
NM_OFFLINE	You are not connected to any VPN Servers.
NM_CONNECTING	Connecting to VPN Server
NM_CONNECTED	Connected to VPN Server "%S"
NM_CONNECT_ERROR	Error number %u (%s)
NM_ACCOUNT_TITLE	excluído
NM_STATUS	User-mode Router Status
NM_STATUS_CONNECT	Status da conexão
NM_STATUS_TCP	NAT TCP/IP Sessions
NM_STATUS_UDP	NAT UDP/IP Sessions
NM_STATUS_ICMP	NAT ICMP Sessions
NM_STATUS_DNS	NAT DNS Sessions
NM_STATUS_DHCP	Allocated DHCP Clients
NM_INFO	User-mode Router information
NM_INFO_PRODUCT_NAME	Nome do produto
NM_INFO_VERSION_STR	Informações da versão
NM_INFO_BUILD_INFO	Informações da Build
NM_INFO_HOSTNAME	Nome do host
NM_NAT_ID	ID
NM_NAT_PROTOCOL	Protocolo
NM_NAT_SRC_HOST	Host de origem
NM_NAT_SRC_PORT	Porta de origem
NM_NAT_DST_HOST	Destination Host
NM_NAT_DST_PORT	Porta de destino
NM_NAT_CREATED	Session Created On
NM_NAT_LAST_COMM	Last Communication Time
NM_NAT_SIZE	Receive / Send Size
NM_NAT_TCP_STATUS	TCP Connection Status
NM_NAT_PROTO_TCP	TCP/IP
NM_NAT_PROTO_UDP	UDP/IP
NM_NAT_PROTO_DNS	DNS
NM_NAT_PROTO_ICMP	ICMP
NAT_TCP_CONNECTING	Conectando
NAT_TCP_SEND_RESET	Desconectando
NAT_TCP_CONNECTED	Conectado
NAT_TCP_ESTABLISHED	Rodando
NAT_TCP_WAIT_DISCONNECT	Desconectando
DHCP_DHCP_ID	ID
DHCP_LEASED_TIME	Alugado em
DHCP_EXPIRE_TIME	Expira às
DHCP_MAC_ADDRESS	Endereço MAC
DHCP_IP_ADDRESS	IP alocado
DHCP_HOSTNAME	Nome do Host do Cliente
NM_PASSWORD_MSG	The administration password has been set.
NM_PUSH_ROUTE_WARNING	The specified text of the static routing table may have a syntax error.


# Concerning version information
ABOUT_CAPTION	Sobre %s
BETA_EXPIRES	Because the currently installed SoftEther VPN software is a beta version, you cannot use it after the provision of a newer beta version of full version. \r\nAccess http://selinks.org/ and get the latest version of SoftEther VPN software.


# Concerning the saving of logs


# (Common log)
L_YES	Sim
L_NO	Não
L_LINE	------------------------------------------------------


# (Server log)
LS_START_UTF8	Log Messages are written with UTF-8 Encoding Format.
LS_START_1	The SoftEther VPN Server has been started.
LS_START_2	%S %S
LS_START_3	%S
LS_END_1	The SoftEther VPN Server Engine has been successfully shutdown.
LS_END_2	The Server Engine shutdown processing has started.
LS_STOP_ALL_LISTENER	All TCP listeners will be stopped.
LS_STOP_ALL_LISTENER_2	All TCP listeners have been stopped.
LS_STOP_ALL_HUB	Stopping all Virtual Hubs.
LS_STOP_ALL_HUB_2	All Virtual Hubs have been stopped.
LS_STOP_CEDAR	Shutting down the Cedar communication module.
LS_STOP_CEDAR_2	The Cedar communication module has been shut down.
LS_STOP_FARM_MEMBER	Disconnecting connection to the cluster controller.
LS_STOP_FARM_MEMBER_2	Connection with the cluster controller has been disconnected.
LS_STOP_FARM_CONTROL	Cluster controller is stopping.
LS_STOP_FARM_CONTROL_2	Cluster controller has stopped.
LS_ENUM_ETHERNET_1	Ethernet device has been enumerated.
LS_ENUM_ETHERNET_2	Device %u: "%S"
LS_LOAD_CONFIG_1	Loading the configuration file.
LS_LOAD_CONFIG_2	The configuration file has been loaded.
LS_LOAD_CONFIG_3	Configuration file does not exist. Attempting to start using initial settings.
LS_INIT_SAVE_THREAD	Starting the automatically saving background task. The interval between auto-saves is %u seconds. You can change the interval by changing the parameter AutoSaveConfigSpan in the configuration file.
LS_BAD_CONFIG	The contents of the configuration file is invalid. The loading process has been terminated.
LS_LISTENER_START_1	TCP Listener (port %u) is starting.
LS_LISTENER_START_2	TCP Listener (port %u) has started. Now listening for connection from client.
LS_LISTENER_START_3	Unable to set port to Listen status for TCP Listener (port %u). Attempting at fixed intervals until successful.
LS_LISTENER_ACCEPT	On the TCP Listener (Port %u), a Client (IP address %S, Host name "%S", Port number %u) has connected.
LS_LISTENER_DISCONNECT	The connection with the client (IP address %S, Port number %u) has been disconnected.
LS_LISTENER_DOS	A DoS attack on the TCP Listener (port %u) has been detected. The connecting source IP address is %S, port number is %u. This connection will be forcefully disconnected now.
LS_LISTENER_MAXUEC	The TCP listener is temporary suspending to accept new inward connections because of the number of pending TCP connections exceeded %u. (Current value = %u)
LS_LISTENER_STOP_1	TCP Listener (port %u) is stopping.
LS_LISTENER_STOP_2	TCP Listener (port %u) has stopped.
LS_HUB_START	Virtual Hub "%S" has been started.
LS_HUB_STOP	Virtual Hub "%S" has been stopped.
LS_HUB_MAC	The MAC address of Virtual Hub "%S" is "%S".
LS_NODE_INFO_TAG	Client product name: "%S", Client version: %u, Client build number: %u, Server product name: "%S", Server version: %u, Server build number: %u, Client OS name: "%S", Client OS version: "%S", Client product ID: "%S", Client host name: "%S", Client IP address: "%S", Client port number: %u, Server host name: "%S", Server IP address: "%S", Server port number: %u, Proxy host name: "%S", Proxy IP address: "%S", Proxy port number: %u, Virtual Hub name: "%S", Client unique ID: "%S"
LS_CONNECTION_START_1	For the client (IP address: %S, host name: "%S", port number: %u), connection "%S" has been created.
LS_SSL_START_ERROR	Failed to start SSL communication for connection "%S". Error: %s (code %u)
LS_CONNECTION_END_1	Connection "%S" has been terminated.
LS_SSL_START	SSL communication for connection "%S" has been started. The protocol version is %S. The encryption algorithm name is "%S".
LS_CONNECTION_ERROR	Connection "%S" terminated by the cause "%s" (code %u).
LS_FARMMEMBER_NOT_ADMIN	Connection "%S": Although the server is a cluster member, the client attempted that to directly connect to the Virtual Hub "%S" while not being administrator user "%S". The user name provided by the client is "%S". Access is refused.
LS_HUB_NOT_FOUND	Connection "%S": Virtual Hub "%S" that the client is trying to connect to does not exist on the server.
LS_WG_KEY_NOT_FOUND	Connection "%S": The WireGuard key is not associated with a user on the server.
LS_IP_DENIED	Connection "%S": The source IP address "%S" of the client has refused based on the Source IP Address Limit List defined for the Virtual Hub.
LS_LICENSE_ERROR	Connection "%S": Because a license-related error has been occurred, the client is unable to connect to the server.
LS_BETA_EXPIRES	This beta version of SoftEther VPN Server is expired. The beta version period of use has expired. Download a new beta version or full version from http://selinks.org/.
LS_TICKET_1	A new client authentication ticket has been issued for cluster member "%S". Virtual Hub "%S", User name "%S" ("%S"), Session name "%S", Ticket "%S"
LS_TICKET_2	A new client authentication ticket has been received from the cluster controller. Virtual Hub "%S", User name "%S" ("%S"), Session name "%S", Ticket "%S", Expiration %u seconds
LS_ENUM_HUB	Connection "%S": %u Virtual Hub servers have been enumerated on this server.
LS_FARM_ACCEPT_1	Connection "%S": Although this server received a cluster control connection request, this server is not a cluster controller.
LS_FARM_ACCEPT_2	Connection "%S":Although this server received a cluster control connection request, the authentication password is incorrect and connection has been refused.
LS_FARM_ACCEPT_3	Connection "%S": This server received a cluster control connection request. Authentication has been successful.
LS_FARM_SERV_START	Connection with a cluster member has been established. IP address: %S, Host name: "%S"
LS_FARM_SERV_END	Connection with cluster member "%S" has been deleted.
LS_FARM_CONNECT_1	Connection to cluster controller "%S" has started.
LS_FARM_CONNECT_2	Connection to cluster controller "%S" has been refused. Error: %s (code %u)
LS_FARM_CONNECT_3	TCP connection to cluster controller "%S" failed. Continuing to attempt connection in intervals of %u seconds until connection is successful.
LS_FARM_DISCONNECT	Connection to the cluster controller has stopped.
LS_FARM_START	Connected to cluster controller. Operation as cluster member is starting.
LS_LICENSE_NOT_VPNSERVER	Connection "%S": License error occurred. The VPN Client attempted to connect while the VPN Server product license is not yet registered.
LS_LICENSE_NOT_VPNCLUSTER	Connection "%S": License error occurred. The license registered on this VPN Server is of a type that prevents the use of the current clustering function and a VPN Client has attempted connection while operating in Cluster mode. You must restart the VPN Server.
LS_LICENSE_VIOLATION	Connection "%S": A license violation has occurred on the VPN Server and connections are not being received.
LS_LICENSE_VIOLATION_DETECTED	A license violation has been detected. A different VPN Server is operating with the same server ID "%I64u" as this VPN Server. It is possible that there are two or more VPN Servers in the cluster that are using the same license. Check the license information of each VPN Server.
LS_API_AUTH_OK	HTTPS API client "%r:%u" (%S): Administration mode: "%S": The embedded HTTPS web server accepted the successful login. Username: "%S", Method: "%S", Path: "%S"
LS_API_AUTH_ERROR	HTTPS API client "%r:%u" (%S): The embedded HTTPS web server refused a login attempt. Username: "%S", Method: "%S", Path: "%S"
LS_API_RPC_CALL	HTTPS API client "%r:%u" (%S): The client called a JSON-API. Method: "%S", Returned error code: %u (0 = success), Returned error message: "%s"
LS_AZURE_START			Received VPN Azure connection request from the client (IP address: %S, port number: %u).
LS_AZURE_SSL_ERROR		Failed to start SSL communication with VPN Azure relay server. Error: %s (code %u)


# (Proto log)
LP_PREFIX_SESSION		[%s] %r:%u -> %r:%u (%s): 
LP_SESSION_CREATED		Session created.
LP_SESSION_DELETED		Session deleted.


# (WireGuard log)
LW_PREFIX_SESSION	[WireGuard] %r:%u -> %r:%u: 
LW_KEYPAIR_EXPIRED	Current keypair (%x -> %x) is expired!
LW_KEYPAIR_UNKNOWN	The packet was encrypted with an unknown keypair!
LW_DECRYPT_FAIL		Decryption failure!
LW_REPLAY_ATTACK	Replay attack detected!
LW_FLOOD_ATTACK		Flood attack detected!
LW_HUB_DISCONNECT	The administrator of the Virtual Hub has disconnected this session.


# (OpenVPN Logs)
LO_PREFIX_RAW	OpenVPN Module: 
LO_PREFIX_SESSION	OpenVPN Session %u (%r:%u -> %r:%u): 
LO_PREFIX_CHANNEL	OpenVPN Session %u (%r:%u -> %r:%u) Channel %u: 
LO_NEW_CHANNEL	A new channel is created.
LO_CHANNEL_ESTABLISHED_NEWKEY	The channel is established. (Trigger: Re-key completion.)
LO_OPTION_STR_RECV	Option Strings Received: "%S"
LO_CLIENT_CERT	Client certificate received (subject: CN="%s"), will use certificate authentication.
LO_CLIENT_UNVERIFIED_CERT	Client certificate was provided but did not pass verification (error="%S"), will use password authentication.
LO_CLIENT_NO_CERT	Client certificate is not provided, will use password authentication.
LO_OPTION_STR_SEND	Option Strings to Send: "%S"
LO_INITIATE_REKEY	The re-keying process is started.
LO_CHANNEL_ESTABLISHED	The channel becomes the established state.
LO_PUSH_REPLY	The full strings replied: "%S"
LO_CHANNEL_FAILED	Failed to connect a channel.
LO_CHANNEL_DISCONNECTED_BY_HUB	This OpenVPN channel is being terminated because the administrator of the Virtual Hub has disconnected this the VPN Session.


# (IPsec Logs)
LI_PREFIX_RAW	Módulo IPsec: 
LI_PREFIX_CLIENT	IPsec Client %u (%S:%u -> %S:%u): 
LI_PREFIX_IKE	IPsec IKE Session (IKE SA) %u (Client: %u) (%S:%u -> %S:%u): 
LI_PREFIX_IPSEC	IPsec ESP Session (IPsec SA) %u (Client: %u) (%S:%u -> %S:%u): 
LI_START	The IPsec ver 2.0 (ISAKMP/IKEv1) processing module is started.
LI_STOPPING	The IPsec ver 2.0 (ISAKMP/IKEv1) processing module is now terminating...
LI_STOP	The IPsec ver 2.0 (ISAKMP/IKEv1) processing module is terminated.
LI_NUM_IPSEC_SA	The number of still-alive IPsec SAs was %u.
LI_NUM_IKE_SA	The number of still-alive IKE SAs was %u.
LI_NUM_IKE_CLIENTS	The number of still-alive IPsec Clients was %u.
LI_L2TP_SERVER_STARTED	The L2TP Server Module is started.
LI_ETHERIP_SERVER_STARTED	The EtherIP Server Module is started. The Session ID of the EtherIP Session: %u
LI_DELETE_IKE_CLIENT	This IPsec Client is deleted.
LI_DELETE_IKE_SA	This IKE SA is deleted.
LI_DELETE_IPSEC_SA	This IPsec SA is deleted.
LI_START_QM_FROM_SERVER	The server initiates a QuickMode negotiation.
LI_START_QM_FROM_CLIENT	The client initiates a QuickMode negotiation.
LI_QM_DH_ERROR	Failed to calculate a Diffie-Hellman algorithm.
LI_NEW_IKE_CLIENT	A new IPsec client is created.
LI_NEW_IKE_SA	A new IKE SA (%s) is created. Initiator Cookie: 0x%I64X, Responder Cookie: 0x%I64X, DH Group: %S, Hash Algorithm: %S, Cipher Algorithm: %S, Cipher Key Size: %u bits, Lifetime: %u Kbytes or %u seconds
LI_TAG_MAINMODE	Modo principal
LI_TAG_AGGRESSIVE	Aggressive Mode
LI_NEW_IPSEC_SA	A new IPsec SA (Direction: %s) is created. SPI: 0x%X, DH Group: %S, Hash Algorithm: %S, Cipher Algorithm: %S, Cipher Key Size: %u bits, Lifetime: %u Kbytes or %u seconds
LI_TAG_SERVER_TO_CLIENT	Servidor -> Cliente
LI_TAG_CLIENT_TO_SERVER	Client -> Server
LI_IPSEC_SA_SPI_SET	The SPI which has been pending is now set. New SPI: 0x%X
LI_IPSEC_SA_ESTABLISHED	This IPsec SA is established between the server and the client.
LI_IKE_SA_ESTABLISHED	This IKE SA is established between the server and the client.
LI_IPSEC_NO_TRANSFORM	There are no acceptable transform proposals from the client for establishing an IPsec SA.
LI_IKE_NO_TRANSFORM	There are no acceptable transform proposals from the client for establishing an IKE SA.
LI_IKE_NO_NAT_T	The connection cannot be accepted because this VPN client is not compatible with IPsec NAT Traversal (RFC 3947 Negotiation of NAT-Traversal in the IKE or draft-ietf-ipsec-nat-t-ike).
LI_SET_CLIENT_ID	The client ID which this client presented in the establishing phase is "%S".
LI_CLIENT_MERGE	This client (Client %u) and the other client (Client %u) is the same client. So they are merged to the client %u.
LI_CLIENT_UPDATE	The port number information of this client is updated.


# (EtherIP Log)
LE_PREFIX	EtherIP / L2TPv3 Session %u (%S:%u -> %S:%u): 
LE_START_MODULE	The EtherIP / L2TPv3 Module is started.
LE_STOP	The EtherIP / L2TPv3 Module is stopped.
LE_NO_SETTING	Error: No EtherIP / L2TPv3 setting entries for the Client ID "%S" is registered on the VPN Server. Please register an entry of a EtherIP / L2TPv3 setting on the VPN Server beforehand.
LE_START_IPC	The internal pipe was created between the EtherIP / L2TPv3 module to the Virtual Hub "%S". The using username is "%S". The IPv4 TCP MSS (Max Segment Size) to be set is %u bytes.
LE_IPC_CONNECT_ERROR	The connection from the EtherIP / L2TPv3 module to the Virtual Hub "%S" failed. Error: %u : %s
LE_IPC_CONNECT_OK	The connection from the EtherIP / L2TPv3 module to the Virtual Hub "%S" succeeded.
LE_RECONNECT	Settings of EtherIP / L2TPv3 has been changed. Internal pipes is now being deleted and auto-reconnecting.


# (PPP Log)
LP_PREFIX	%S%SPPP Session [%S:%u]: 
LP_CONNECTED	A new PPP session (Upper protocol: %S) is started. IP Address of PPP Client: %S (Hostname: "%S"), Port Number of PPP Client: %u, IP Address of PPP Server: %S, Port Number of PPP Server: %u, Client Software Name: "%S", IPv4 TCP MSS (Max Segment Size): %u bytes
LP_DISCONNECTED	The PPP session is disconnected.
LP_PAP_REJECTED	The client denied to accept the authentication protocol "PAP" (Password Authentication Protocol, a clear-text password authentication protocol). Enable PAP on the client-side and retry.
LP_PAP_MSCHAPV2_REJECTED	The client denied to accept both the "PAP" (Password Authentication Protocol, a clear-text password authentication protocol) and MS-CHAP v2 Protocol. Enable either PAP or MS-CHAP v2 on the client-side and retry.
LP_DISCONNECTED_ABNORMAL	A PPP protocol error occurred, or the PPP session has been disconnected.
LP_NEXT_PROTOCOL_IS_NOT_PAP	An invalid protocol (Protocol Number: 0x%x) with non-PAP (Password Authentication Protocol) control packet.
LP_PAP_FAILED	"PAP" (Password Authentication Protocol, a clear-text password authentication protocol) user authentication failed.
LP_MSCHAPV2_FAILED	"MS-CHAP v2" (Microsoft Challenge and Response Protocol Version 2.0) user authentication failed.
LP_NEXT_PROTOCOL_IS_NOT_IPCP	An invalid protocol (Protocol Number: 0x%x) with non-IPCP (IP Configuration Protocol) control packet.
LP_DATA_TIMEOUT	A timeout on the PPP data transmitting occurred. The PPP client might be disconnected from the network.
LP_CONTROL_TIMEOUT	A timeout on the PPP control transmitting occurred. No responses from the PPP client.
LP_VPN_SESSION_TERMINATED	The PPP session is disconnected because the VPN Session has been disconnected by the administrator.
LP_UPPER_PROTOCOL_DISCONNECTED	The PPP session is disconnected because the upper-layer protocol "%S" has been disconnected.
LP_NORMAL_TERMINATE	The PPP session is disconnected by the VPN Client's disconnecting request.
LP_IP_ADDRESS_NOT_DETERMIND	The VPN Client sent a packet though an IP address of the VPN Client hasn't been determined.
LP_DHCP_REQUEST_TRYING	Trying to request an IP address from the DHCP server.
LP_DHCP_REQUEST_OK	An IP address is assigned. IP Address of Client: %S, Subnet Mask: %S, Default Gateway: %S, Domain Name: "%S", DNS Server 1: %S, DNS Server 2: %S, WINS Server 1: %S, WINS Server 2: %S, IP Address of DHCP Server: %S, Lease Lifetime: %u seconds
LP_DHCP_REQUEST_NG	Acquiring an IP address from the DHCP server failed. To accept a PPP session, you need to have a DHCP server. Make sure that a DHCP server is working normally in the Ethernet segment which the Virtual Hub belongs to. If you do not have a DHCP server, you can use the Virtual DHCP function of the SecureNAT on the Virtual Hub instead.
LP_DHCP_INFORM_TRYING	Acquiring the IP networking information such as subnet mask and the default gateway information from the DHCP server.
LP_DHCP_INFORM_OK	The networking information has been acquired. Subnet Mask: %S, Default Gateway: %S, Domain Name: "%S", DNS Server 1: %S, DNS Server 2: %S, WINS Server 1: %S, WINS Server 2: %S, IP Address of DHCP Server: %S
LP_DHCP_INFORM_NG	Acquiring the networking information from the DHCP server failed. To accept a PPP session, you need to have a DHCP server. Make sure that a DHCP server is working normally in the Ethernet segment which the Virtual Hub belongs to. If you do not have a DHCP server, you can use the Virtual DHCP function of the SecureNAT on the Virtual Hub instead.
LP_SET_IPV4_PARAM	The IP address and other network information parameters are set successfully. IP Address of Client: %S, Subnet Mask: %S, Default Gateway: %S, DNS Server 1: %S, DNS Server 2: %S, WINS Server 1: %S, WINS Server 2: %S


# (Virtual Hub log)
LH_ONLINE	O hub virtual está online agora.
LH_OFFLINE	O hub virtual está offline agora.
LH_CONNECT_CLIENT	The connection "%S" (IP address: %S, Host name: %S, Port number: %u, Client name: "%S", Version: %S, Build: %u) is attempting to connect to the Virtual Hub. The auth type provided is "%s" and the user name is "%S".
LH_AUTH_UNKNOWN	Unknown auth type.
LH_AUTH_ANONYMOUS	Anonymous authentication
LH_AUTH_PASSWORD	Senha
LH_AUTH_PLAIN_PASSWORD	External server authentication
LH_AUTH_CERT	Certificate authentication
LH_AUTH_TICKET	Ticket authentication
LH_AUTH_EXTERNAL		External server authentication
LH_AUTH_WIREGUARD_KEY	WireGuard public key authentication
LH_AUTH_OPENVPN_CERT	OpenVPN certificate authentication
LH_AUTH_RADIUS_NOT_SUPPORT	Connection "%S": The authentication method of the user "%S" has been specified as RADIUS Authentication or Active Directory Authentication (NT Domain Authentication). However, the edition of the VPN Server is "%S". This edition does not support RADIUS Authentication nor Active Directory Authentication (NT Domain Authentication). The connection will be denied.
LH_AUTH_RADIUS_NOT_SUPPORT_ON_OPEN_SOURCE	Connection "%S": The authentication method of the user "%S" has been specified as RADIUS Authentication or Active Directory Authentication (NT Domain Authentication). However, such an external user-authentication function hasn't been implemented on the Open-Source version of SoftEther VPN yet. The connection will be denied.
LH_AUTH_CERT_NOT_SUPPORT_ON_OPEN_SOURCE	Connection "%S": The authentication method of the user "%S" has been specified as Certificate Authentication. However, the Certificate Authentication function hasn't been implemented on the Open-Source version of SoftEther VPN yet. The connection will be denied.
LH_AUTH_OK	Connection "%S": Successfully authenticated as user "%S".
LH_AUTH_OK_CERT	The Virtual Hub's Security Account Manager has received the following certificate from the VPN Client and accepted its contents as the certificate for when user "%S" logs in: %s
LH_AUTH_NG_CERT	Although the Virtual Hub's Security Account Manager has received the following certificate, has refused its contents as the certificate for when user "%S" logs in because this certificate's contents matches the contents that are registered in the Virtual Hub's certificates revocation list: %s
LH_AUTH_NG	Connection "%S": User authentication failed. The user name that has been provided was "%S", from %S.
LH_LOCAL_ONLY	Connection "%S": The remote login has been refused because of the password for user "%S" is blank.
LH_POLICY_ACCESS_NG	Connection "%S": Access has been refused to user "%S" based on the security policy.
LH_USER_EXPIRES	Connection "%S": Access has been refused to user "%S" because of the expiration date has been expired.
LH_CLIENT_VERSION_OLD	Connection "%S": The build number of the VPN Client is %u. Only the build %u or latest version of VPN Client is granted to access the VPN Server.
LH_CLIENT_ID_REQUIRED	Connection "%S": The Client ID which has been specified by the VPN Client is %u. However, this Virtual Hub has the RequiredClientId value set to %u.
LH_FARM_SELECT_1	Connection "%S": The cluster controller is deciding the destination cluster member of this client.
LH_FARM_SELECT_2	Connection "%S": Failed to decide the destination cluster member server.
LH_FARM_SELECT_3	Connection "%S": This current VPN Server has been decided as the destination cluster member server. Proceeding to receive connection.
LH_FARM_SELECT_4	Connection "%S": The server "%S" has been decided as a destination cluster member server. Instructing clients to redirect connection to this server.
LH_MAX_SESSION	Connection "%S": The maximum number of sessions (%u) that can be set by the Virtual Hub has been reached. Unable to create a new session.
LH_MAX_SESSION_CLIENT	Connection "%S": The maximum number of client sessions (%u) that can be set by the Virtual Hub has been reached. Unable to create a new session.
LH_MAX_SESSION_BRIDGE	Connection "%S": The maximum number of bridge sessions (%u) that can be set by the Virtual Hub has been reached. Unable to create a new session.
LH_MAX_SESSION_2	Connection "%S": The maximum number of sessions (%u) that can be managed by a VPN Server has been reached. Unable to create a new session.
LH_NEW_SESSION	Connection "%S": The new session "%S" has been created. (IP address: %S, Port number: %u, Physical underlying protocol: "%S")
LH_SET_SESSION	Session "%S": The parameter has been set. Max number of TCP connections: %u, Use of encryption: %s, Use of compression: %s, Use of Half duplex communication: %s, Timeout: %u seconds.
LH_NODE_INFO	Session "%S": VPN Client details: (%s)
LH_VLAN_ID	Session "%S": Assigned VLAN ID: %u
LH_INVALID_SIGNATURE	Session "%S": The connected client sent invalid protocol data. Unable to establish normal communication with client. First check for problems with the connections and cabling of the network connecting the client and the server and then check there is not a special transparent packet re-writing device installed.
LH_END_SESSION	Session "%S": The session has been terminated. The statistical information is as follows: Total outgoing data size: %I64u bytes, Total incoming data size: %I64u bytes.
LH_BCAST_STORM	Session "%S": A large volume of broadcast packets has been detected. There are cases where packets are discarded based on the policy. The source MAC address is %S, the source IP address is %S, the destination IP address is %S. The number of broadcast packets is equal to or larger than %u items per 1 second (note this information is the result of mechanical analysis of part of the packets and could be incorrect).
LH_DHCP_FORCE	Session "%S": The packet was discarded because it has been attempting to use the IP address %S, which is not a DHCP server allocated IP address.
LH_MAC_LIMIT	Session "%S": Although the virtual hub has attempt to assign a new MAC address "%S" was made, %u MAC addresses have already been assigned for this service. According to the security policy, this session is allowed to have a maximum of %u MAC addresses. The packet has been discarded.
LH_BRIDGE_LIMIT	Session "%S": Although the virtual hub has attempt to assign a new MAC address "%S" was made, %u MAC addresses have already been assigned for this service. According to the security policy, this session is denied bridges and is therefore allowed to hold no more than %u MAC addresses. The packet has been discarded.
LH_MAC_REGIST	Session "%S": A new MAC address "%S" has been assigned.
LH_MAC_REGIST_VLAN	Session "%S": A new MAC address "%S" (VLAN ID: %u) has been assigned.
LH_IP_LIMIT	Session "%S": Although the virtual hub has attempt to assign a new IP address %S was made, %u IP addresses have already been assigned for this service. According to the security policy, this session is allowed to have a maximum of %u IP addresses. The packet has been discarded.
LH_ROUTING_LIMIT	Session "%S": Although the virtual hub has attempt to assign a new IP address %S was made, %u IP addresses have already been assigned for this service. According to the security policy, this session is denied routing and is therefore allowed to hold no more than %u IP addresses. The packet has been discarded.
LH_IP_CONFLICT	Session "%S": Although the virtual hub has attempt to use the IP address %S was made, this IP address is already being used by another session "%S" (MAC Address: "%S"). The security policy for this session denies duplication of IP addresses that are used by other sessions. The packet has been discarded. Detailed Information: CreatedTime=%I64u, UpdatedTime=%I64u, DhcpAllocated=%u, Now=%I64u
LH_NO_SERVER	Session "%S": Although TCP/IP connection request (from %S:%u to %S:%u) was made to this session, because of the security policy denies operation as a server, the packet has been discarded.
LH_NO_DHCP	Session "%S": Although host %S on this session sent a packet that allocates an IP address as a DHCP server for host %S on another session, this session's security policy denies operation as a DHCP server. The packet has been discarded.
LH_REGIST_DHCP	Session "%S": The DHCP server of host "%S" (%S) on this session allocated, for host "%S" on another session "%S", the new IP address %S.
LH_BRIDGE_1	Session "%S": A Local Bridge connection to physical Ethernet interface "%S" was started.
LH_BRIDGE_2	Session "%S": Because communication has failed to be established with physical Ethernet interface "%S", the Local Bridge has stopped.
LH_SET_MTU	Session "%S": The physical Ethernet interface "%S" has an MTU value set to %u. It is necessary to send and receive an Ethernet packet which has %u bytes. The MTU is now changed to %u.
LH_SET_MTU_ERROR	Session "%S": The physical Ethernet interface "%S" has an MTU value set to %u. It is necessary to send and receive an Ethernet packet which has %u bytes. However, changing the MTU to %u failed. This physical Ethernet interface or device driver might be unable to process an Ethernet packet which has more 1,514 bytes (payload size: 1,500 bytes). In such case, the larger tagged-VLAN packets than 1,514 bytes cannot be transmitted. You should replace the current physical Ethernet adapter to another which supports Jumbo Frames. You can also try to update the device driver. Another possible method is to enable Jumbo Frames on the operating system or device driver settings.
LH_START_BRIDGE	The Local Bridge connection "%S" has started. The bridge session "%S" was created.
LH_STOP_BRIDGE	The Local Bridge connection "%S" has stopped.
LH_LINK_START	The Cascade Connection "%s" has been established. The Cascade session "%S" was created.
LH_LINK_STOP	The Cascade Connection "%s" has stopped.
LH_NAT_START	SecureNAT has started. The SecureNAT session "%S" was created.
LH_NAT_STOP	SecureNAT stopped.
LH_NAT_TCP_SUCCEED	The connection to TCP session %u: Host "%S (%S)", Port %u was successful.
LH_NAT_TCP_FAILED	The connection to TCP session %u: Host "%S", Port %u failed.
LH_NAT_TCP_DELETED	The TCP session %u has been deleted.
LH_NAT_TCP_CREATED	The TCP session %u has been created. Connection source %S:%u, Connection destination %S:%u
LH_NAT_UDP_DELETED	The UDP session %u has been deleted.
LH_NAT_UDP_CREATED	The UDP session %u has been created. Connection source %S:%u, Connection destination %S:%u
LH_NAT_DHCP_CREATED	The DHCP entry %u has been created. MAC address: %S, IP address: %S, host name: %S, expiration span: %u seconds
LH_CHANGE_PASSWORD_1	The connection "%S" (IP address %S) connected to Virtual Hub in change password mode.
LH_CHANGE_PASSWORD_2	Connection "%S": Changing of password failed. The specified user "%S" does not exist.
LH_CHANGE_PASSWORD_3	Connection "%S": Changing of password failed. The auth type of user "%S" is not password authentication.
LH_CHANGE_PASSWORD_4	Connection "%S": Changing of password failed. The old password of user "%S" is incorrect.
LH_CHANGE_PASSWORD_5	Connection "%S": The password of user "%S" has been changed.
LH_CONNECT_1	Starting Cascade Connection "%s": connection number %u.
LH_CONNECT_2	The Cascade Connection "%s" is connected. Session name: "%S"
LH_CONNECT_ERROR	The connection for Cascade Connection "%s" has been either disconnected or it failed. Cause: %s (code %u)
LH_POLICY_MONITOR_MODE	Connection "%S": Because of a user whose security policy denies permission for Monitoring Mode requested that Monitoring Mode be enabled and attempted to connect to a Virtual Hub, the connection has been denied.
LH_POLICY_BRIDGE_MODE	Connection "%S": Because of a user whose security policy denies both bridge connections and routing operations requested that bridge connections or routing operations be enabled and attempted to connect to the Virtual Hub, the connection has been denied.
LH_NOT_ENOUGH_CLIENT_LICENSE	Connection "%S": Although this connection attempted to connect to the VPN Server using "client connection mode", because this would have made the number of client connections on the entire server exceed the number of registered Client Connection Licenses, it is not possible to receive the connection for this connection. When the number of licenses for concurrent connections is insufficient, you must either disconnect another existing client connection or increase the number of licenses. There are currently %u registered Client Connection Licenses and the number of connections to servers was %u. 
LH_NOT_ENOUGH_BRIDGE_LICENSE	Connection "%S": Although this connection attempted to connect to the VPN Server using "bridge connection mode", because this would have made the number of bridge connections on the entire server exceed the number of registered Bridge Connection Licenses, it is not possible to receive the connection for this connection. When the number of licenses for concurrent connections is insufficient, you must either disconnect another existing client connection or increase the number of licenses. There are currently %u registered Bridge Connection Licenses and the number of connections to servers was %u. 
LH_TOO_MANY_MULTILOGINS	Connection "%S": Although the user "%S" made a login attempt, the security policy that applies to this user limits the maximum number of multiple logins to %u sessions. Currently the number of logins by this user is %u sessions and therefore the user has denied permission for a new VPN connection.
LH_TOO_MANY_MULTILOGINS2	Connection "%S": Although the user "%S" made a login attempt, this edition of the VPN Server permits the maximum number of multiple concurrent VPN sessions to %u sessions per user. Current number of the multiple concurrent VPN sessions of this users is %u, so no more concurrent VPN sessions cannot be permitted. If you want to support more number of multiple concurrent VPN sessions per user, please consider upgrading to Professional Edition or greater of the VPN Server.
LH_PACKET_LOG_NO_LOG	The edition of this VPN Server doesn't supports the packet logging function. No IP address nor TCP/UDP header data will be recorded. After you upgrade the edition of the VPN Server to Professional Edition or greater, all kinds of packet logs will be recorded in this file.
LH_PACKET_LOG_NO_LOG_OSS	The VPN Server is either Open-Source or Free version. It hasn't implemented the IP Address or TCP/UDP header data logging function. No IP address nor TCP/UDP header data are not be recorded here.
LH_NO_RADIUS_SETTING	The user "%S" is configured to use RADIUS authentication. However, there is no RADIUS authentication settings. The user cannot be authenticated.
LH_KERNEL_MODE_START	It has been detected that the Kernel-mode NAT for SecureNAT can be run on the interface "%S". The Kernel-mode NAT is starting. The TCP, UDP and ICMP NAT processings will be performed with high-performance via Kernel-Mode hereafter. The parameters of Kernel-mode NAT: IP Address = "%r", Subnet Mask = "%r", Default Gateway = "%r", Broadcast Address = "%r", Virtual MAC Address: "%S", DHCP Server Address: "%r", DNS Server Address: "%r"
LH_KERNEL_MODE_STOP	The Kernel-mode NAT on the interface "%S" for SecureNAT has been stopped.


# (Administration log)
LA_CONNECTED_1	Connection "%S" connected using server admin mode.
LA_CONNECTED_2	Connection "%S" connected using Virtual Hub Admin Mode. The name of the Virtual Hub is "%S".
LA_IP_DENIED	Connection "%S" attempted to connect using administration mode from an IP address whose permission is denied by adminip.txt. Disconnecting.
LA_ERROR	Connection "%S" was unable to log in using administration mode. %s (Error code %u)
LA_OK	Connection "%S" successfully logged in using administration mode.
LA_RPC_START	Connection "%S" created a new remote procedure call session "%S" for the purpose of administration mode.
LA_TAG_1	Administration mode [%S]: 
LA_TAG_2	Administration mode [%S] (Virtual Hub "%S"): 
LA_CREATE_LISTENER	A new TCP listener (port number %u) has been created.
LA_DELETE_LISTENER	TCP listener (port number %u) has been deleted.
LA_ENABLE_LISTENER	TCP listener (port number %u) has been enabled.
LA_DISABLE_LISTENER	TCP listener (port number %u) has been disabled.
LA_SET_PORTS_UDP	UDP ports have been set: %S.
LA_SET_PROTO_OPTIONS	%S options have been set.
LA_SET_SERVER_PASSWORD	The server administrator password has been set.
LA_SET_FARM_SETTING	The clustering setting has been changed.
LA_SET_SERVER_CERT	The server certificates have been set.
LA_REGENERATE_SERVER_CERT	The server certificate has been re-generated. The new CN: "%S"
LA_SET_SERVER_CIPHER	A new encryption algorithm name for the server has been set. The new encryption algorithm name is "%S".
LA_ADD_WGK		Added %u WireGuard key(s).
LA_DELETE_WGK	Deleted %u WireGuard key(s).
LA_CREATE_HUB	A new Virtual Hub "%S" has been created.
LA_SET_HUB	The Virtual Hub setting has been changed.
LA_DELETE_HUB	The Virtual Hub "%S" has been deleted.
LA_SET_HUB_RADIUS	The Virtual Hub's external RADIUS authentication server setting has been changed.
LA_DISCONNECT_CONN	The client connection "%S" connected to the server has been forcefully disconnected.
LA_SET_HUB_ONLINE	O hub virtual está online agora.
LA_SET_HUB_OFFLINE	O hub virtual está offline agora.
LA_SET_SNAT_OPTION	The SecureNAT option has been set.
LA_ENABLE_SNAT	The SecureNAT function has been enabled.
LA_DISABLE_SNAT	The SecureNAT function has been disabled.
LA_SET_HUB_LOG	The log save setting has been changed.
LA_ADD_CA	A registration of trusted root certificate has been added.
LA_DELETE_CA	A registration of trusted root certificate has been deleted.
LA_CREATE_LINK	The Cascade Connection "%s" has been added.
LA_SET_LINK	The setting for Cascade Connection "%s" has been changed.
LA_SET_LINK_ONLINE	The Cascade Connection "%s" is now online.
LA_SET_LINK_OFFLINE	The Cascade Connection "%s" is now offline.
LA_DELETE_LINK	The Cascade Connection "%s" has been deleted.
LA_RENAME_LINK	The name of Cascade Connection "%s" has been changed to "%s".
LA_ADD_ACCESS	An access list has been added.
LA_DELETE_ACCESS	The access list has been deleted.
LA_SET_ACCESS_LIST	The access list has been updated. An access list of %u items are set.
LA_SET_AC_LIST	The Source IP Address Limit List has been updated. Rule items for %u items are set.
LA_CREATE_USER	User "%S" has been created.
LA_SET_USER	The setting of user "%S" has been updated.
LA_DELETE_USER	User "%S" has been deleted.
LA_CREATE_GROUP	Group "%S" has been created.
LA_SET_GROUP	The setting of group "%S" has been updated.
LA_DELETE_GROUP	Group "%S" has been deleted.
LA_DELETE_SESSION	This session "%S" has been forcefully disconnected.
LA_SET_KEEP	The server's Internet keep-alive setting has been updated.
LA_SET_SYSLOG	The server's syslog send function setting has been updated.
LA_DELETE_BRIDGE	The Local Bridge connection definition "%S" --> "%S" has been deleted.
LA_ADD_BRIDGE	The Local Bridge connection definition "%S" --> "%S" has been added.
LA_REBOOT_SERVER	There has been a request to restart VPN Server.
LA_GET_CONFIG	The config file has been read.
LA_SET_CONFIG	The config file has been written. Restarting VPN Server.
LA_SET_HUB_ADMIN_OPTION	The administration option has been set for Virtual Hub "%S".
LA_SET_HUB_EXT_OPTION	The Virtual Hub Extended Option has been set for Virtual Hub "%S".
LA_ADD_L3_SW	The Virtual Layer 3 Switch "%S" has been created on the server.
LA_DEL_L3_SW	The Virtual Layer 3 Switch "%S" has been deleted from the server.
LA_START_L3_SW	The Virtual Layer 3 Switch "%S" has been started.
LA_STOP_L3_SW	The Virtual Layer 3 Switch "%S" has been stopped.
LA_ADD_L3_IF	The virtual interface for Virtual Hub "%S" has been added to Virtual Layer 3 Switch "%S".
LA_DEL_L3_IF	The virtual interface for Virtual Hub "%S" has been deleted from Virtual Layer 3 Switch "%S".
LA_ADD_L3_TABLE	The routing table for network "%S" has been added to Virtual Layer 3 Switch "%S".
LA_DEL_L3_TABLE	The routing table for network "%S" has been deleted from Virtual Layer 3 Switch "%S".
LA_ADD_CRL	A certificate has been added to Certificate Revocation List.
LA_DEL_CRL	A certificate has been edited in Certificate Revocation List.
LA_SET_CRL	A registered item in a registration of a list of invalid certificates has been edited.
LA_READ_LOG_FILE	The log file on the server "%S" (log file "%S") has been downloaded.
LA_ADD_LICENSE_KEY	A new license key "%S" has been registered.
LA_DEL_LICENSE_KEY	An existing license (No. %u) has been deleted.
LA_SET_IPSEC_CONFIG	The IPsec server setting has been updated.
LA_ADD_ETHERIP_ID	A new EtherIP / L2TPv3 server setting (ID="%S") has been added.
LA_DEL_ETHERIP_ID	The new EtherIP / L2TPv3 server setting (ID="%S") has been deleted.
LA_SET_OVPN_SSTP_CONFIG	The OpenVPN and MS-SSTP VPN Server setting has been updated.
LA_DDNS_HOSTNAME_CHANGED	The hostname of Dynamic DNS Function has been changed to "%S".
LA_SET_SPECIAL_LISTENER	Special Listener enable / disable status has been changed.


# (Client log)
LC_START_1	The SoftEther VPN Client Engine has been started.
LC_START_2	%S %S
LC_START_3	%S
LC_END	The SoftEther VPN Client Engine has been shut down.
LC_LOAD_CONFIG_1	Loading configuration file...
LC_LOAD_CONFIG_2	The configuration file has been loaded.
LC_LOAD_CONFIG_3	Configuration file does not exist. Applying the initial settings.
LC_NEW_ACCOUNT	Um nova configuração de conexão VPN "%s" foi criada.
LC_DELETE_ACCOUNT	The VPN Connection Setting "%s" has been deleted.
LC_RENAME_ACCOUNT	The name of VPN Connection Setting "%s" has been changed to "%s".
LC_CONNECT	Connection processing for VPN Connection Setting "%s" has started.
LC_CONNECT_1	VPN Connection Setting "%s": Connection operation starting (this is now %u times).
LC_SSL_CONNECTED	VPN Connection Setting "%s": SSL communication has been started. The protocol version is %S. The encryption algorithm name is "%S".
LC_CONNECT_2	VPN Connection Setting "%s": Now connected. Session name: "%S"
LC_CONNECT_ERROR	VPN Connection Setting "%s": The connection has been either disconnected or it failed. Cause: %s (code %u)
LC_DISCONNECT	Disconnecting the VPN Connection Setting "%s".
LC_CREATE_VLAN	Um adaptador de rede virtual "%S” foi criado.
LC_UPDATE_VLAN	O driver do adaptador de rede virtual "%S” foi reinstalado.
LC_DELETE_VLAN	O adaptador de rede virtual "%S” foi removido.
LC_SET_PASSWORD	The password setting for connection to a client service has been changed.
LC_TAP_NOT_FOUND	Cannot find the tun/tap driver for Mac OS X. Please install the tun/tap driver.


# (Eraser log)
LE_START	Monitoring the directory "%S". If the amount of available free disk space becomes less than %S, the backup files for log files and configurations that are saved on the sub-directories of this directory will be automatically deleted in the order of oldest first. The amount of free disk space that determines when to start deletion can be modified by changing the "AutoDeleteCheckDiskFreeSpaceMin" item in the configuration file.
LE_DELETE	The free disk space is now less then %S so the old file "%S" has been automatically deleted. The amount of free disk space that determines when to start deletion can be modified by changing the "AutoDeleteCheckDiskFreeSpaceMin" item in the configuration file.
LE_NOT_ENOUGH_FREE	<<WARNING>> If the free disk space becomes lower than %S, it will no longer be possible to automatically delete the old backup files of log files and configurations. We recommend that you immediately manually delete the unnecessary files on this computer and recover the necessary free disk space. When there is a very small amount of free disk space, computer operation can become unstable. 


# (Layer 3 Switch log)
L3_SWITCH_START	The Virtual Layer 3 Switch "%S" started. It will wait until the Virtual Hubs of all interfaces registered on this switch become online and then it will start operation.
L3_SWITCH_ONLINE	The Virtual Hubs of all interfaces of the Virtual Layer 3 Switch "%S" are online and the Virtual Layer 3 Switch has commenced Virtual Layer 3 Switch operation.
L3_SWITCH_OFFLINE	At least one Virtual Hub of an interface registered on Virtual Layer 3 Switch "%S" stopped, and Virtual Layer 3 Switch operation has been stopped.
L3_SWITCH_STOP	The Virtual Layer 3 Switch "%S" terminated.


# Concerning Microsoft.c
MS_VIRTUAL	Proprietary Virtual/Internal Interface
MS_ETHERNET	Ethernet Interface
MS_TOKENRING	Token Ring Interface
MS_FDDI	Interface FDDI
MS_PPP	PPP (Dialup or VPN)
MS_LOOPBACK	Loopback Interface
MS_SLIP	SLIP Interface
MS_WLAN	Wireless Network Interface
MS_OTHER	Unknown Other Interface
MS_NON_OPERATIONAL	Desativado
MS_UNREACHABLE	Não conectado
MS_DISCONNECTED	Não conectado
MS_CONNECTING	Conectando
MS_CONNECTED	Conectado
MS_OPERATIONAL	Conectado


# Concerning Network Utility
UT_SM_COLUMN_1	Nome do item
UT_SM_COLUMN_2	Valor
UT_SM_ST_TITLE	Nome do adaptador de rede
UT_SM_ST_GUID	GUID
UT_SM_ST_TYPE	Tipo
UT_SM_ST_TYPE2	Physical Wired Ethernet
UT_SM_ST_STATUS	Status
UT_SM_ST_MTU	MTU
UT_SM_ST_SPEED	Velocidade do link
UT_SM_ST_ADDRESS	Physical Address
UT_SM_ST_RECV_BYTES	Bytes recebidos
UT_SM_ST_RECV_BCASTS	Pacotes broadcast de entrada
UT_SM_ST_RECV_UNICASTS	Pacotes unicast de entrada
UT_SM_ST_SEND_BYTES	Outgoing Bytes
UT_SM_ST_SEND_BCASTS	Pacotes broadcast de saída
UT_SM_ST_SEND_UNICASTS	Pacotes unicast de saída
UT_SM_ST_IP	Endereço IP %u
UT_SM_ST_SUBNET	Subnet Mask %u
UT_SM_ST_GATEWAY	Gateway %u
UT_SM_ST_DHCP	Servidor DHPC
UT_SM_ST_DHCP_1	Iniciar lease
UT_SM_ST_DHCP_2	Lease Limit date and time
UT_SM_ST_WINS_1	WINS Server 1
UT_SM_ST_WINS_2	WINS Server 2


# Concerning EtherLogger Manager
EM_TITLE	SoftEther EtherLogger Gerenciador
EM_REMOTE_TITLE	You can connect to and manage the SoftEther EtherLogger service. \r\nEnter the host name and IP address of the computer on which the EtherLogger service to be managed is operating. You can also concatenate the port number by using the ":" (colon).
EM_MAIN_COLUMN_1	Nome do adaptador de rede
EM_MAIN_COLUMN_2	Status
EM_MAIN_OK	Operativo
EM_MAIN_ERROR	Erro
EM_ADD_NEW	Add new capture device
EM_ADD_EDIT	Edit capture settings
EM_DELETE_CONFIRM	Are you sure you want to delete capture setting "%S"?
EM_NO_LICENSE_COLUMN	Nota: 
EM_NO_LICENSE	Because not even one product license is registered, this SoftEther EtherLogger will not operate.
EM_UNSUPPORTED	Unable to use SoftEther EtherLogger on the operating system that this SoftEther EtherLogger is operating on. For the list of operating system that the SoftEther EtherLogger can be used on, please refer to the online documentation of the SoftEther EtherLogger.
EM_WPCAP_REMOTE	In order to use this SoftEther EtherLogger, you need to install WinPcap software. The software WinPcap is currently not installed on the server computer. \r\n\r\nTo continue the installation of the WinPcap software, you must start SoftEther EtherLogger Manager on the server computer that is running VPN Server and then while connected to localhost (location of your own computer), have the Local Bridge Function Setting window displayed. \r\nTo continue, first exit this management session, and then, after starting SoftEther EtherLogger Manager on the server computer, connect to localhost and continue the setting process. 
EM_WPCAP_ROOT	In order to use this SoftEther EtherLogger, you need to install WinPcap software. \r\n\r\nTo continue the installation you must log in to this computer as a user with administrator privileges. \r\nLog on as an administrator and start the SoftEther VPN Server Manager again.
EM_WPCAP_INSTALL	In order to use this SoftEther EtherLogger, you need to install WinPcap software. The software WinPcap is currently not installed on the server computer. \r\n\r\nWinPcap is an easy-to-install free software that is bundled together with the VPN Server. \r\n\r\nDo you want to begin the installation of WinPcap?
EM_WPCAP_REBOOT1	After WinPcap installation has completed, you must restart the computer before you use the SoftEther EtherLogger. \r\n\r\nAfter you restart the computer manually and start SoftEther EtherLogger, configure the settings again.
EM_WPCAP_REBOOT2	After WinPcap is installed, you must restart the SoftEther EtherLogger service. \r\n\r\nIt only takes a short time to restart the SoftEther EtherLogger service, however all management sessions that are currently connected to the SoftEther EtherLogger will be disconnected. \r\nThis management session will also be disconnected, so you will need to reconnect to continue. \r\n\r\nDo you want to restart the SoftEther Ether Logger service?
EM_RESOURCE	Unable to read the WinPcap driver.


###########################################################################
#                                                                         #
# String data of dialog boxes in software                                 #
#                                                                         #
###########################################################################
PREFIX	D_SECURE
CAPTION	Access to %s - %S
S_TITLE	Acesso para %S
S_DEVICE_INFO	Device Name: %S\r\nManufacturer: %S
IDS_STATIC1	Device Information
S_WARNING	Take care entering the PIN code because if you have entered it incorrectly for a few times the device will be locked.
IDOK	&OK
IDCANCEL	Cancelar
S_PIN_CODE	&Código PIN: 
PREFIX	D_PKCSUTIL
CAPTION	PKCS#12 Write Utility
S_TITLE	ePass 1000 USB token PKCS#12 Write Utility
STATIC1	By using this utility, you can write a PKCS#12 file (certificate file) of your choice to an ePass 1000 USB hardware security token. \r\n\r\nThe USB token that the certificate file is written in can be used for SoftEther VPN authentication.
STATIC2	Write to PKCS#12 file
STATIC3	To write an existing PKC#12 file to a USB token, click Write. \r\nNOTE: If a PKCS#12 certificate for SoftEther VPN is already stored in the USB token, it will be overwritten.
B_WRITE	&Gravar
STATIC4	Erase PKCS#12 certificate from USB token.
STATIC5	You can erase the certificate data from a USB token on which a PKCS#12 certificate for SoftEther VPN is already stored.
B_ERASE	&Limpar
IDCANCEL	E&xit Utilities
S_COPYRIGHT	Copyright (c) SoftEther VPN Project.\r\nAll Rights Reserved.
PREFIX	D_PASSPHRASE
CAPTION	Private Key Passphrase
STATIC1	The private key is protected by passphrase. \r\n\r\nEnter the passphrase to read the private key.
STATIC2	&Senha: 
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_NM_CONNECT
CAPTION	Connect to SoftEther VPN User-mode Router
S_TITLE	Connecting to "%S"...
PREFIX	D_PASSWORD
CAPTION	Acesso para %S
S_TITLE	Enter your user name and password to log in to server %S. Make sure you select the correct auth type.
STATIC1	Enter Use&r Info: 
STATIC2	&Autenicação: 
STATIC3	Nome de &usuário: 
STATIC4	&Senha: 
R_NO_SAVE_PASSWORD	&Do not Save Password
S_COUNTDOWN	Uma reconexão automática será feita após %u segundos...
IDOK	&OK
IDCANCEL	Cancelar conexão
PREFIX	D_STATUS
CAPTION	Connecting to "%s"...
S_STATUS	Inicializando...
IDCANCEL	Cancelar
PREFIX	D_CERT
CAPTION	Certificado
S_TITLE	The following information is available for this certificate.
STATIC1	Basic Information of this Certificate:
STATIC2	Emitido para:
STATIC3	Emissor:
STATIC4	Expira às:
STATIC5	Advanced Information of this Certificate:
STATIC6	Certificate of Authority Who Signed This Certificate:
S_PARENT	The certificate of the certificate authority who signed this certificate is registered on the list of trusted certificates.
S_PARENT_BUTTON_STR	&Ver certificado
IDCANCEL	&OK
B_SAVE	&Salvar para arquivo
PREFIX	D_CHECKCERT
CAPTION	Security Alert - %s
S_TITLE	Although the connection to the destination VPN Server "%S" that you are currently connecting to is encrypted, the trustworthiness of the server certificate provided by the server is unknown.
STATIC1	About the Server Certificate
STATIC2	Establishing encrypted tunnel (SSL session) between VPN Server and VPN Client. Checking the server certificate enables to verify the authenticity of the server.
S_MSG1	The server certificate provided by destination VPN Server "%S" is as follows.
STATIC3	Emitido para: 
STATIC4	Emissor: 
STATIC5	Expira às: 
B_SHOW	&Show Certificate
STATIC6	Resumo (MD5) 
STATIC7	Digest (SHA-1): 
IDOK	&Resume the Connection
IDCANCEL	&Cancel Connection
STATIC8	There may be a problem with this certificate, such as it has not been issued by a trusted certificate authority (CA), or cert is expired.
STATIC9	Confirm the content of this certificate and decide whether or not to connect to this VPN Server. Click Cancel Connection to abort the connection.
PREFIX	D_CONNECTERROR
CAPTION	Connect Error - %s
S_TITLE	Ocorreu um erro ao conectar-se ao servidor VPN "%S".
S_COUNTDOWN	Reconecta-se automaticamente após %u segundos...
IDOK	&Repetir
IDCANCEL	Cancelar conexão
R_HIDE	&Ocultar esta janela ao conectar na próxima vez
PREFIX	D_CM_LOGIN
CAPTION	Enter Password - VPN Client Manager
S_TITLE	You must enter a client administration password to operate the VPN Client that is operating on %s. Enter the client administration password.
STATIC1	&Senha:
STATIC2	Enter the Client Administration Password:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_CONNECTION_STATUS
S_TITLE	Status of VPN Session of %s (Real Time)
B_POLICY	Security &Policy...
B_SERVER_CERT	&Server Certificate
B_CLIENT_CERT	&Client Certificate
IDCANCEL	&Fechar
PREFIX	D_CM_POLICY
CAPTION	Security Policy List
S_TITLE	Security policies defined for the current session %s
IDCANCEL	&Fechar
PREFIX	D_CM_ACCOUNT
STATIC1	Por favor, defina a configuração de conexão VPN para o servidor VPN.
S_ACCOUNT_NAME	&Nome da configuração: 
STATIC2	Servidor VPN de destino:
STATIC3	Especifique o nome do host ou o endereço IP, o número da porta e o hub virtual do servidor VPN de destino.
STATIC4	&Nome do host:
STATIC5	&Número da porta:
STATIC6	(Porta TCP)
STATIC7	&Nome do Hub Virtual:
STATIC8	Servidor proxy como retransmissor:
STATIC9	Conectar a um servidor VPN através de um servidor proxy.
STATIC10	&Tipo de proxy:
R_DIRECT_TCP	&Conexão TCP/IP direta (sem proxy)
R_HTTPS	Conectar via servidor proxy H&TTP
R_SOCKS	Conectar via servidor proxy &SOCKS4
R_SOCKS5	Conectar via servidor proxy &SOCKS5
B_PROXY_CONFIG	Configuração do servidor &proxy
STATIC11	Opção de verificação do certificado do servidor:
R_CHECK_CERT	Sempre verificar o certificado do servidor
R_TRUST_DEFAULT	Confie no armazenamento de certificados do sistema
B_TRUST	Gerenciar lista de &certificados CA confiáveis
B_SERVER_CERT	Certificado &individual
B_VIEW_SERVER_CERT	&Mostrar individual
S_VLAN_GROUP	Adaptador de rede virtual a ser usado:
S_POLICY_1	You can configure the security policy which will be applied to the Cascade Connection on this Virtual Hub's side.
B_POLICY	Security Po&licy
STATIC12	Configuração de &autenticação do usuário:
STATIC13	&Autenicação:
S_USERNAME	&Nome de usuário:
S_PASSWORD	Senha:
S_CERT_INFO	Você deve especificar um certificado do cliente a ser usado para autenticação do usuário.
STATIC14	Configuração &avançada de comunicação: 
R_RETRY	Reconecta automaticamente após desconectar
S_RETRY_NUM_1	&Contagem de reconexões:
S_RETRY_NUM_2	vezes
S_RETRY_SPAN_1	Intervalo de reconexão:
S_RETRY_SPAN_2	segundos
R_INFINITE	&Reconexões infinitas (mantem a VPN sempre online)
B_DETAIL	C&onfigurações avançadas...
IDOK	&OK
IDCANCEL	Cancelar
B_CHANGE_PASSWORD	Mudar &senha
S_CHANGE_PASSWORD	Você pode alterar a senha do usuário no servidor VPN.
R_HIDE	Ocultar telas de status e erros
R_HIDE2	Ocultar telas de endereços IP
STATIC15	Defina as informações de autenticação do usuário necessárias ao conectar-se ao servidor VPN.
B_REGIST_CLIENT_CERT	&Certificado do cliente
B_IE	Importar configurações proxy do IE
R_DISABLE_NATT	Desativar NAT-T
PREFIX	D_CM_PROXY
CAPTION	Proxy Server Connection Setting
STATIC1	Enter the host name of the proxy server for relaying (HTTP proxy or SOCKS proxy), and the IP address, port, and when necessary, the user name and password.
STATIC2	&Nome do host:
STATIC3	Porta:
STATIC4	&Nome de usuário:
STATIC5	&Senha:
B_HTTP_HEADER	Custom HTTP header values
IDOK	&OK
IDCANCEL	Cancelar
STATIC6	(opcional)
STATIC7	(opcional)
PREFIX	D_CM_PROXY_HTTP_HEADER
CAPTION	Custom Proxy HTTP Header Values
B_NEW	Novo
B_DELETE	Excluir
B_CLEAR	Limpar
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_CM_DETAIL
CAPTION	Configurações avançadas
STATIC1	Configurações opcionais para administradores de sistema e especialistas em rede, protocolo de comunicação e segurança. Personalize as configurações de comunicação do protocolo VPN.
STATIC2	Otimização da comunicação VPN:
STATIC3	Use várias conexões TCP físicas em uma conexão VPN lógica para aumentar o rendimento da comunicação.
STATIC4	&Número de conexões TCP:
STATIC5	conexões
STATIC6	Nota: recomenda-se cerca de 8 conexões para banda larga e 1 conexão para conexões lentas (por exemplo, discada).
STATIC7	Configurações avançadas: 
STATIC8	&Estabelecendo intervalo:
STATIC9	segundos
R_USE_DISCONNECT	Definir a &vida útil de cada conexão TCP
STATIC10	Tempo de vida:
STATIC11	segundos
STATIC12	Ao usar duas ou mais conexões TCP, o Modo Half Duplex está disponível. O modo half-duplex fixa a direção dos dados como metade e metade para cada conexão TCP. Por exemplo, quando uma VPN usando 8 conexões TCP é estabelecida, o túnel da VPN será corrigido para que 4 conexões TCP sejam dedicadas ao upload e as outras 4 conexões sejam dedicadas ao download. 
R_USE_HALF_CONNECTION	Usar modo &Half-Duplex
STATIC13	Criptografia e &compactação:
STATIC14	Normalmente, a sessão da VPN é criptografada para segurança. Você pode desativar a criptografia para melhorar a taxa de transferência. Observe que os dados fluem em texto simples pela rede quando desabilitado.
R_USE_ENCRYPT	&Criptografar sessão VPN com SSL
STATIC15	Você pode usar a compactação de dados para economizar largura de banda da VPN. Ative esta opção ao usar uma conexão lenta, como conexão discada ou móvel.
R_DISABLE_UDP	Disable UD&P Acceleration
R_USE_COMPRESS	&Usar compressão de dados
STATIC16	&Modo de conexão da VPN:
S_MODE	Você pode especificar os seguintes modos de conexão. (opções para administradores de rede)
R_BRIDGE	&Bridge / Router Mode
R_MONITOR	Mo&do de monitoramento
STATIC17	Outras confi&gurações:
R_NO_ROUTING	Sem ajustes na tabela de &roteamento
STATIC18	Mantenha as configurações padrão nesta caixa de diálogo, a menos que seja solicitado por um administrador do sistema ou se você possui experiência em redes e segurança.
STATIC19	As funções VoIP/QoS lidam com pacotes de alta prioridade, para serem transmitidos mais rapidamente.
STATIC20				Source IP Address:
STATIC21				Source Port Number:
R_DISABLE_QOS	Desativar função VoIP / &QoS
IDOK	&OK
IDCANCEL	Cancelar
S_UDPACCEL	Você pode usar a compactação de dados para economizar largura de banda da VPN. Ative esta opção ao usar uma conexão lenta, como conexão discada ou móvel.
PREFIX	D_CM_NEW_VLAN
CAPTION	Criar um novo adapatador de rede virtual
S_INFO	Um novo adaptador de rede virtual será criado no sistema.\r\nVocê pode especificar um nome para o adaptador de rede virtual, que pode ter no máximo %u caracteres alfanuméricos.
STATIC1	&Nome do adaptador de rede virtual: 
IDOK	&OK
IDCANCEL	Cancelar
S_WIN8	The name of a Virtual Network Adapter must be 'VPN' or 'VPN2' to 'VPN127'. (Maximum 127 adapters can be created.)
PREFIX	D_CM_TRUST
CAPTION	Gerenciar lista de certificados CA confiáveis
STATIC1	Aqui, você pode gerenciar a lista de certificados de autoridade de certificação (CA) confiáveis.\r\n\r\nVocê pode usar a lista de certificados de CA registrada aqui para verificar os certificados do servidor ao se conectar aos servidores VPN.
B_IMPORT	&Adicionar
B_EXPORT	&Exportar
IDOK	&Ver certificado
IDCANCEL	&Fechar
B_DELETE	&Excluir
PREFIX	D_CM_PASSWORD
CAPTION	Set Password - VPN Client Manager
S_TITLE	You can set the password to limit the SoftEther VPN Client Service.\r\nAfter setting a password, you will be asked to enter a password the next time you use the VPN Client Connect Manager to connect to the SoftEther VPN Client service.
STATIC1	Set Client Administration Password: 
R_USE_PASSWORD	&Usar senha
R_REMOTE_ONLY	Only &Request Password for Remote Operation
IDC_STATIC1	&Senha:
IDC_STATIC2	&Confirmar:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_CM_CONFIG
CAPTION	Configurações opcionais
STATIC1	You can modify the settings for VPN Client.
STATIC2	R&emote Management:
STATIC3	You can remotely manage the VPN Client Service Program from another computer by using VPN Client Manager Remote Mode.
R_ALLOW_REMOTE_CONFIG	Allow &Remote Management of VPN Client Service
S_WARNING	It is recommended to set a password if you allow remote management. From the menu bar, choose Tools -> Set Password to set the password.
STATIC4	For environments where Internet connections will automatically be disconnected when idle, you can keep alive the Internet connection by sending dummy packets to any host on the Internet.
R_USE_KEEP_CONNECT	Use &Keep Alive Internet Connection Function
S_HOSTNAME	&Nome do host:
S_PORT	&Número da porta:
S_INTERVAL	Packet Send &Interval:
S_INTERVAL2	segundos
S_PROTOCOL	Pr&otocolo:
R_TCP	&Protocolo TCP/IP
R_UDP	&Protocolo UDP/IP
S_INFO	Packets sent to keep alive the Internet connection have random bits. No personal information is sent.
IDOK	&OK
IDCANCEL	Cancelar
STATIC5	&Outras configurações:
R_ALPHA	Transparency of UI:
STATIC6	Note: The transparency setting will be applied after the connection manager is restarted.
STATIC7	&Keep Alive Internet Connection Function:
PREFIX	D_ABOUT
S_INFO1	SoftEther VPN %u.0 Developer Edition (Ver %u.%02u, Build %u)
S_INFO2	Licensed under the Apache License, Version 2.0.\r\nCopyright (c) 2012-%u all contributors on SoftEther VPN project in GitHub. All Rights Reserved.\r\nWeb Site: http://www.softether.org/\r\n%S
S_INFO3	This product includes the following software components:\r\nBitVisor: Copyright (c) 2007, 2008 University of Tsukuba. Copyright (C) 2007, 2008 National Institute of Information and Communications Technology. All rights reserved. / Microsoft(R) C Runtime Library: (c) 2007 Microsoft Corporation. All Rights Reserved. / PKCS #11 Cryptographic Token Interface (Cryptoki): Copyright (c) RSA Security Inc. / WinPcap: Copyright (c) 2001 - 2003 NetGroup, Politecnico di Torino (Italy). All rights reserved. / libedit: Copyright (c) 1992, 1993 The Regents of the University of California. All rights reserved. / libiconv: Copyright (C) 2007 Free Software Foundation, Inc. / ncurses: Copyright (c) 1998-2005, 2006 Free Software Foundation, Inc. / OpenSSL: Copyright (c) 1998-2011 The OpenSSL Project. All rights reserved. This product includes software developed by the OpenSSL Project for use in the OpenSSL Toolkit (http://www.openssl.org/). This product includes cryptographic software written by Eric Young (eay@cryptsoft.com). / zlib: (C) 1995-2004 Jean-loup Gailly and Mark Adler. / Special Thanks to: Software Laboratory, Academic Computing Communication Center, Industrial Liaison and Cooperative Research Center and Professor Yasushi Shinjo in University of Tsukuba, Japan.
S_INFO4	THIS SOFTWARE IS FREEWARE DEVELOPED UNDER THE SOFTETHER VPN PROJECT AT UNIVERSITY OF TSUKUBA, WITHOUT WARRANTY OF ANY KIND. IN NO EVENT SHALL THE DEVELOPERS, COPYRIGHT OWNERS OR DISTRIBUTORS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY IN ANY WAY OUT OF THE USE OF THIS SOFTWARE.\r\n\r\nSoftEther VPN is a work of the research and development project of Japanese Government, subsidized by Ministry of Economy, Trade and Industry of Japan, administrated by Information Promotion Agency.
IDCANCEL	&OK
B_WEB	Visite o &site da SoftEther VPN...
B_EULA	&Licença de usuário final
B_IMPORTANT	&Avisos importantes
B_LEGAL	Informações &legais
B_UPDATE_CONFIG	&Configurar atualizações
B_AUTHORS	Lista de &autores
PREFIX	D_REMOTE
STATIC1	&Specify the Host Name of the Destination Computer, or IP Address:
R_LOCAL	Conectar ao &computador local (computador exibindo esta janela)
S_HOSTNAME	&Nome do computador: 
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_CM_DESKTOP
CAPTION	Connection - %s
S_TITLE	Starting connect process for VPN Connection Setting "%s".
S_WARNING	VPN Client will output to the "Console Session" window of %s, the progress status and error messages related to the process of connecting to VPN Server 
S_INFO	Do you want to proceed with the connection?
IDOK	&ContinuAR
IDCANCEL	Cancelar
PREFIX	D_CM_CHANGE_PASSWORD
CAPTION	Change Password
S_TITLE	You can change the password of the user registered on server %S.
STATIC1	Mudar &senha
STATIC2	Virtual &Hub Name:
STATIC3	&Nome de usuário:
STATIC4	&Senha antiga:
STATIC5	&Nova senha:
STATIC6	&Confirm of New Password:
IDOK	&OK
IDCANCEL	Cancelar
S_STATIC	Note: If authentication type is RADIUS or NT Domain Authentication, you cannot change the user's password here.
PREFIX	D_SM_MAIN
CAPTION	Edição de desenvolvedor do gerenciador SoftEther VPN Servidor
STATIC1	Con&figurações de conexão para o servidor VPN:
STATIC2	As configurações de conexão do servidor VPN ou da Bridge VPN são definidas da seguinte maneira. Clique duas vezes no item para se conectar ao servidor.\r\nPara adicionar uma nova conexão, clique em Nova configuração.
B_NEW_SETTING	&Nova configuração
B_EDIT_SETTING	&Editar configuração
B_DELETE	&Excluir configuração
IDOK	&Conectar
B_SECURE_MANAGER	&Gerenciador de Smart Card...
B_SELECT_SECURE	Selecionar S&mart Car...
B_ABOUT	&Sobre o SoftEhter VPN...
IDCANCEL	Sair do gerencidor de servidores SoftEther VPN
B_CERT_TOOL	Cria um certificado
PREFIX	D_SM_EDIT_SETTING
STATIC1	Por favor, defina a configuração de conexão para o servidor VPN ou a Bridge VPN gerenciar.
STATIC2	&Nome da configuração:
STATIC3	Servidor VPN de destino:
STATIC4	Especifique o nome do host ou o endereço IP, o número da porta e o hub virtual do servidor VPN de destino.
STATIC5	&Nome do host:
R_LOCALHOST	Conectar ao &localhost
STATIC6	&Número da porta:
STATIC7	(Porta TCP)
STATIC8	Servidor pro&xy como retransmissão:
STATIC9	Conectar a um servidor VPN através de um servidor proxy.
STATIC10	&Tipo de proxy:
R_DIRECT_TCP	&Conexão TCP/IP direta (sem proxy)
R_HTTPS	Conectar via servidor proxy H&TTP
R_SOCKS	Conectar via servidor proxy S&OCKS4
R_SOCKS5	Conectar via servidor proxy S&OCKS5
B_PROXY_CONFIG	Configuração do servidor &proxy
STATIC11	Selecione o  &modo de administração e digite a senha
STATIC12	Você pode se conectar ao servidor VPN usando o modo de administrador do servidor ou o modo de administrador do hub virtual.\r\n\r\nO modo de administrador do servidor permite gerenciar todo o servidor VPN e todos os hubs virtuais.\r\n\r\nO modo de administrador do hub virtual permite gerenciar apenas um hub virtual para o qual você possui privilégios.
R_SERVER_ADMIN	Admin do &servidor
R_HUB_ADMIN	Admin do H&UB Virtual
S_HUBNAME	&Nome do Hub Virtual:
STATIC13	Digite a senha para conectar ao modo de administrador.
S_PASSWORD	&Senha: 
R_NO_SAVE	&Não salvar a senha do administrador.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_SERVER
CAPTION	%s - Gerencidor SoftEther VPN Servidor
S_TITLE	Gerenciar servidor VPN "%S"
S_VHUB_BRIDGE	Hubs virtuais hospedados neste servidor VPN:
IDOK	&Gerenciar hub virtual
B_ONLINE	&Online
B_OFFLINE	O&ffline
B_HUB_STATUS	Ver &Status
B_CREATE	&Criar um hub virtual
B_EDIT	Propri&edade
B_DELETE	&Excluir
STATIC1	Gerenciamento de portas:
STATIC2	Portas de escuta (TCP/IP):
B_CREATE_LISTENER	C&riar
B_DELETE_LISTENER	Exclui&r
B_START	Iniciar
B_STOP	Para&r
S_UDP	Multiple UDP ports can be specified by splitting them with a space or a comma. Leave empty to disable the UDP listener.
B_APPLY	Apply
STATIC3	Informações e configurações do servidor VPN e da rede:
B_SSL	Criptografia e &rede
B_STATUS	&Ver status do servidor
B_INFO	Sobre esse servidor VPN
B_LICENSE	Add / Delete &Licenses
B_FARM	Configuração de cluster
B_FARM_STATUS	Status do cluster
B_CONNECTION	Mostrar lista de\r\nconexões TCP/IP
B_BRIDGE	Bridge local
B_L3	Switch Layer &3 
B_CONFIG	E&ditar configurações
B_REFRESH	A&tualizar
IDCANCEL	S&air
S_BETA	Versão beta (pré-lançamento)
B_IPSEC	IPsec / L&2TP
B_DDNS	DNS dinâmico
S_DDNS	DDNS Hostname atual:
B_OPENVPN	OpenVPN / MS-SSTP
B_AZURE	Configuração VPN Azure
S_AZURE	VPN Azure Hostname:
B_VPNGATE	VPN Gate
PREFIX	D_SM_STATUS
IDOK	A&tualizar
IDCANCEL	S&air
PREFIX	D_SM_EDIT_HUB
STATIC1	&Nome do Hub Virtual:
STATIC2	Configurações de &segurança:
S_BOLD	Administration password for this Virtual Hub.
STATIC3	&Senha:
STATIC4	&Confirmar:
R_NO_ENUM	No En&umerate to Anonymous Users
STATIC5	V&irtual Hub Options: 
R_LIMIT_MAX_SESSION	&Limit Max VPN Sessions
S_MAX_SESSION_1	Ma&x Number of Sessions:
S_MAX_SESSION_2	sessões
STATIC6	(Will not count sessions on server side that are generated by Local Bridge, Virtual NAT or Cascade Connection.)
STATIC7	Virtual Hub Status:
STATIC8	Set the Virtual Hub status.
R_ONLINE	Onlin&e
R_OFFLINE	O&ffline
STATIC9	Set Clustering:
S_FARM_INFO	Select the Virtual Hub type in the cluster.
R_STATIC	St&atic Virtual Hub
R_DYNAMIC	&Dynamic Virtual Hub
S_AO_1	Virtual Hub Admin Option:
S_AO_3	Display and edit the Virtual Hub administration options.
B_ADMINOPTION	Virtual Hub Admin Option
S_ACL_3	Sou&rce IP Address Limit List
S_ACL	Allow or deny VPN connections to this Virtual Hub according to the client computer's IP address.
B_ACL	IP Access Con&trol List 
IDOK	&OK
IDCANCEL	Cancelar
STATIC10	You can configure more advanced settings on the Virtual Hub Extended Option List.
B_EXTOPTION	Edit Virtual Hub Extended Option List
S_MSG_1	Show Message when Client Connects
S_MSG_2	Shows a message on the screen of a user when a VPN Client connects to this Virtual Hub.
B_MSG	Set the Messa&ge
PREFIX	D_SM_CREATE_LISTENER
CAPTION	Create Listener
STATIC1	You can add a TCP/IP port number for the VPN Server to accept connections from clients. \r\n\r\nSpecify the port number to add.
STATIC2	If the port number is already being used by another server program, the status of the new listener will be error. \r\n\r\nIn this case, stop the other program that is opening the same port.
STATIC3	&Número da porta:
IDOK	&OK
IDCANCEL	Cancelar
STATIC4	(Porta TCP/IP)
PREFIX	D_SM_SSL
CAPTION	Encryption and Network Settings
STATIC1	You can view or change settings related to encryption, communication and security for this VPN Server.
STATIC2	Encryption &Algorithm Settings:
STATIC3	Specify the encryption algorithm for SSL applied to the connection between this VPN Server and VPN Clients. The encryption algorithm must be compatible with SSL Version 3.
STATIC4	En&cryption Algorithm Name:
STATIC6	Server &Certificate Settings:
STATIC7	Specify the X509 certificate and private key to be presented to clients by this server.
B_IMPORT	&Importar
B_EXPORT	E&xportar
B_VIEW	&Ver
B_REGENERATE	Novo
STATIC8	&Keep Alive Internet Connection:
STATIC9	For environments where Internet connections will automatically be disconnected when idle, you can keep alive the Internet connection by sending dummy packets to any host on the Internet.
STATIC10	Server Certificate:
R_USE_KEEP_CONNECT	Use &Keep Alive Internet Connection
S_HOSTNAME	&Nome do host:
S_PORT	&Porta:
S_INTERVAL	Send &Interval:
S_INTERVAL2	segundos
S_PROTOCOL	Pr&otocolo:
R_TCP	&Protocolo TCP/IP
R_UDP	&Protocolo UDP/IP
S_INFO	Packets sent to keep alive the Internet connection have random bits. No personal information is sent.
STATIC11	Administrator Pass&word: 
S_INFO4	You can modify an administrator password of the administrator for all Virtual Hubs and this entire VPN Server.
B_PASSWORD	Change Admin &Password
IDOK	&OK
IDCANCEL	Cancelar
IDCANCEL2	Cancelar
STATIC12	Syslog Send Function:
STATIC13	You can transfer the entire VPN Server / Bridge Logs, Virtual Hub Administration Logs, or Virtual Hub Packet Logs by using syslog protocol instead of writing to a local disk. 
STATIC14	Syslog &Server Host Name:
STATIC15	P&orta:
S_OVER_FUNCS	VPN over ICMP / DNS Server Function
S_INFO5	You can establish a VPN only with ICMP or DNS packets even if there is a firewall or routers which blocks TCP/IP communications.
B_SPECIALLISTENER	VPN over ICMP / DNS Settings
B_UPDATE_CONFIG	&Update Notify Setting...
PREFIX	D_SM_SAVE_KEY_PAIR
CAPTION	Save Certificate and Private Key
STATIC1	Select the method to save the certificate and private key.
STATIC2	Sa&ve Method:
R_X509_AND_KEY	Save as &X509 Certificate (.CER) and Private Key File (.KEY)
R_PKCS12	Save as &PKCA#12 File (.P12)
R_SECURE	Write to &Smart Card
STATIC3	Saving by splitting into two files: a standard Base 64-encoded certificate file and a private key file.
STATIC4	Saving as a PKCS#12 (Public Key Cryptography Standard #12) file. \r\nYou can store both certificate and private key in a single PKCS#12 file.
STATIC5	When a smart card is connected to this computer, you can write the certificate and private key to a smart card.
B_SELECT	&Selecionar qual Smart Card usar...
S_PASS3	Private Key P&rotection:
S_PASS4	When saving the private key, you can set a passphrase to encrypt. You will be required to enter the passphrase when loading it.
R_USE_PASS	Set P&assphrase
S_PASS1	S&enha:
S_PASS2	Con&firmar:
IDOK	&OK
IDCANCEL	Cancelar
B_SECURE_MANAGER	Gerenciador de Smart Card...
PREFIX	D_SM_CONNECTION
CAPTION	Connection List
S_TITLE	O servidor %S possui as seguintes conexões ativas. Conexões que foram estabelecidas como uma sessão VPN não estão incluídas.
IDOK	Mostrar &informações de conexão
B_DISCONNECT	&Desconectar
B_REFRESH	A&tualizar
IDCANCEL	S&air
PREFIX	D_SM_FARM
CAPTION	Configuração de cluster
S_TITLE	You can change configuration for clustering function of VPN Server "%S". 
STATIC1	Clustering can realize load balancing and fault balance protection to bundle multiple VPN Servers.
STATIC2	Modo atual:
STATIC3	Clustering Se&ttings:
R_STANDALONE	&Standalone Server (No Clustering)
R_CONTROLLER	&Cluster Controller
R_MEMBER	Cluster &Member Server
STATIC4	C&onfigurable Parameters as a Member Server:
S_IP_1	Public &IP Address:
S_IP_2	(When a public IP address is omitted, the IP address of the network interface used when connecting to the cluster controller will be used.)
S_PORT_1	Lista de &portas públicas:
S_PORT_2	(Separate multiple port numbers by a space or a comma.)
S_CONTROLLER	Controller &Host Name or IP Address:
S_CONTROLLER_PORT	Port Number of\r\nControlle&r:
S_PORT_3	(Porta TCP)
S_PASSWORD	Administration &Password: 
STATIC5	When you modify a clustering configuration, the VPN Server service restarts automatically. When this happens, all the currently connected sessions and administration-related connections will be disconnected.
IDOK	&OK
IDCANCEL	Cancelar
S_1	Standard Ratio in Cluster:
S_2	(Padrão: 100)
R_CONTROLLER_ONLY	Controller Functions Only (No VPN session in itself)
PREFIX	D_SM_FARM_MEMBER
CAPTION	Cluster Member List
S_TITLE	Currently the following Cluster Member Servers are connected to the Cluster Controller %S.
IDOK	Cluster Member Server &Information
B_REFRESH	A&tualizar
IDCANCEL	S&air
B_CERT	View Server &Certificate
PREFIX	D_SM_CHANGE_PASSWORD
CAPTION	Alterar senha do administrador de %S
S_TITLE	Altere a senha do administrador do servidor %S. Digite a nova senha e clique em OK.
STATIC1	Nova &senha:
STATIC2	&Confirmar senha:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_HUB
CAPTION	Gerenciamento do hub virtual - '%S'
S_TITLE	Hub Virtual '%S'
STATIC1	Gerenciamento do banco de &dados de segurança:
B_USER	Gerenciar &usuários
S_USER	Adicione, exclua ou edite contas de usuário.
B_GROUP	Gerenciar &grupos
S_GROUP	Adicione, exclua ou edite grupos.
B_ACCESS	Gerenciar listas de &acesso
S_ACCESS	Add or delete access lists (Packet filtering rules).
STATIC2	Virtual Hub Settings:
B_PROPERTY	&Propriedades do Hub Virtual
S_PROPERTY	Configure this Hub.
B_RADIUS	Configuração do servidor de &autenticação
S_RADIUS	Use o servidor de autenticação RADIUS externo para autenticação do usuário.
B_LINK	Gerenciar conexões em &cascata
S_LINK	Estabeleça a conexão em cascata com os hubs em servidores VPN locais ou remotos.
STATIC3	Status atual deste hub vi&rtual:
B_REFRESH	A&tualizar
STATIC4	&Outras configurações:
B_LOG	Configurações do &log
B_LOG_FILE	Arquivos de log
S_LOG	Defina as configurações da função de log.
B_CA	Certificados de CA confiáveis
B_CRL	Certs &revogados
S_CA	Gerenciar lista de certificados CA confiáveis.
B_SNAT	&NAT virutal e servidor DHCP (SecureNAT)
S_SNAT	NAT seguro está disponível neste hub virtual. Você pode executar o NAT virtual e o DHCP virtual.
STATIC5	Gerenc&iamento de sessões VPN:
B_SESSION	Gerenciar &sessões
IDCANCEL	S&air
PREFIX	D_SM_USER
CAPTION	Gerenciar usuários
S_TITLE	O hub virtual "%S" tem os seguints usuários.
IDOK	&Editar
B_CREATE	&Novo
B_DELETE	&Remover
B_REFRESH	&Atualizar
IDCANCEL	S&air
B_STATUS	&Ver inf usuário
PREFIX	D_SM_EDIT_USER
IDC_STATIC1	&Nome de usuário:
IDC_STATIC3	&Nome completo:
IDC_STATIC4	&Nota:
IDC_STATIC5	Nome do grupo\r\n(Opcional):
B_GROUP	Pesquisar grupos...
R_EXPIRES	&Defina a data de validade desta conta
IDC_STATIC6	Tipo de &autenticação:
S_RADIUS_3	Configurações de autenticação de domínio RADIUS ou NT:
S_RADIUS_1	As tentativas de login por senha serão verificadas pelo servidor RADIUS externo, pelo controlador de domínio do Windows NT ou pelo controlador do Active Directory.
R_SET_RADIUS_USERNAME	Especifique o nome de usuário no servidor de autenticação
S_RADIUS_2	Nome de usuário no servidor de autenticação:
S_POLICY_1	Política de segurança
R_POLICY	Definir diretiva de &segurança
B_POLICY	Política de segurança
S_PASSWORD_1	Configurações de autenticação de senha:
S_PASSWORD_2	&Senha:
S_PASSWORD_3	&Confirmar senha:
S_USER_CERT_1	Configurações individuais de autenticação de certificado:
B_LOAD_CERT	Certificado
B_VIEW_CERT	&Ver certificado
B_CREATE	Criar certificado
S_ROOT_CERT_1	Configurações de autenticação de certificado assinado:
S_ROOT_CERT_2	Verifica se o certificado do cliente  é um certificado de uma CA que é confiável por este Hub Virtual.
R_CN	Limita o nome comum (CN) a
R_SERIAL	Limita o número de série do certificado a
S_ROOT_CERT_3	Nota: Valores hexadeciis. (Exemplo: 0155ABCDEF)
S_HINT	Dica: Defina um objeto de usuário com o nome de usuário '*' (asterisco) para aceitar uma tentativa de login de um usuário que não corresponda a nenhum dos objetos explícitos registrados. Tal usuário usará o servidor de autenticação de usuário externo para verificar o logon.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_POLICY
STATIC1	Selected &Policy:
S_BOLD	Des&cription of the policy:
S_BOLD2	Current &Value:
R_ENABLE	&Enable the Policy
R_DISABLE	&Desatiar a política
R_DEFINE	De&fine the Policy
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_GROUP
CAPTION	Gerenciar grupos
S_TITLE	O hub virtual "%S" tem os seguints grupos.
B_CREATE	&Novo
IDOK	&Editar
B_DELETE	&Remover
B_REFRESH	&Atualizar
B_USER	&Membro da lista
IDCANCEL	S&air
PREFIX	D_SM_EDIT_GROUP
IDC_STATIC1	&Nome do grupo:
IDC_STATIC3	&Nome completo:
IDC_STATIC4	&Nota:
S_POLICY_1	Security Policy:
R_POLICY	Defina a política de segurança deste &grupo
B_POLICY	Política de segurança
S_POLICY_2	Statistical Information of the Group:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_ACCESS_LIST
CAPTION	Listas de acesso
S_TITLE	The Virtual Hub "%S" has the following access lists (packet filtering rules).
B_ADD	&Novo (IPv&4)
B_ADD_V6	&Novo (IPv&6)
IDOK	&Editar
B_DELETE	&Excluir
B_SAVE	&Salvar
IDCANCEL	&Cancelar
STATIC1	Items with higher priority appear higher in the list.
STATIC2	Note: IP packets that did not match any access list items can pass.
B_CLONE	Cl&onar
B_ENABLE	A&tivar
B_DISABLE	D&esativar
PREFIX	D_SM_EDIT_ACCESS
CAPTION	Edit Access List Item
STATIC1	Configure the access list settings. The access list that is defined here will be applied to all IP packets passing through the Virtual Hub.
STATIC2	Configurações básicas
STATIC3	&Lembrete:
STATIC4	&Ação:
R_PASS	&Senha
R_DISCARD	&Descartar
STATIC5	P&rioridade:
STATIC6	(Smaller number has higher priority.)
STATIC7	Filtering Options for IP Headers
S_ACCESS_SRC_ALL	Source IP Address:
R_SRC_ALL	Applies to All Source Addresses
S_SRC_IP_1	Endereço IPv4:
S_SRC_IP_2	Máscara de sub-rede:
S_SRC_IP_3	(255.255.255.255 means a single host)
S_SRC_IP_1_V6	Endereço IPv6:
S_SRC_IP_3_V6	(Por exemplo: "ffff:ff00::" ou "/24". "/128" significa um único host.)
S_ACCESS_DST_ALL	Destination IP Address:
R_DST_ALL	Applies to All Destination Addresses
S_IP_DST_1	Endereço IPv4:
S_IP_DST_2	Máscara de sub-rede:
S_IP_DST_3	(255.255.255.255 means Specified host only)
S_IP_DST_1_V6	Endereço IPv6:
S_IP_DST_3_V6	(Por exemplo: "ffff:ff00::" ou "/24". "/128" significa um único host.)
STATIC9	Protocol Type:
STATIC10	Filtering Options for TCP Headers and UDP Headers
S_TCP_1	Mínimo
S_TCP_2	Máximo
S_TCP_3	Porta de origem:
S_TCP_5	Porta de destino:
S_TCP_7	The blank port number field matches any ports.\r\nIt will apply to packets that match only the minimum value when the minimum value is specified but the maximum value is not.
STATIC11	Filtering Options for Users or Groups
STATIC11_OLD	Filtering Options for Users
STATIC12	This access list will be applied only to the packets that for specific users, groups send or receive.
STATIC12_OLD	This access list will be applied only to packets that for specific users send or receive.
STATIC13	Nome da origem:
B_USER1	Pesquisar...
STATIC14	Destination Name:
B_USER2	Pesquisar...
STATIC15	Leave these fields blank if you don't specify user name nor group name.
STATIC15_OLD	Leave these fields blank if you don't specify user name.
IDOK	&OK
IDCANCEL	Cancelar
S_PROTOID	Specify IP Protocol:
STATIC16	Filtering Options for MAC Headers
S_CHECK_SRC_MAC	Source MAC Address:
R_CHECK_SRC_MAC	Applies to any Source Addresses
S_SRC_MAC	Endereço MAC:
S_SRC_MAC_MASK	Máscara:
S_CHECK_DST_MAC	Destination MAC Address:
R_CHECK_DST_MAC	Applies to any Destination Addresses
B_SIMULATION	De&lay and Packet Loss...
S_DST_MAC	Endereço MAC:
S_DST_MAC_MASK	Máscara:
S_MAC_NOTE	You can use hexadecimal number with two separators, "-" or ":", and without the separators.\r\n(FF-FF-FF-FF-FF-FF means a specified host) 
R_CHECK_TCP_STATE	Verify TCP Connection State (Only TCP Packets)
R_ESTABLISHED	Established Packet
R_UNESTABLISHED	Unestablished Packet
R_REDIRECT	Redirect HTTP Request to Specific URL
B_REDIRECT	Set URL Redirect to...
PREFIX	D_SM_RADIUS
CAPTION	Authentication Server Settings
S_TITLE	Para usar um servidor RADIUS externo para verificar as tentativas de login no Hub Virtual "%S", especifique um servidor RADIUS externo que verifique o nome de usuário e a senha.
STATIC1	RADIUS Server Settings:
R_USE_RADIUS	Usar autenticação &RADIUS
S_RADIUS_1	RADIUS &Server Host Name or IP:
S_RADIUS_2	&Porta:
S_RADIUS3	(Porta UDP)
S_RADIUS_4	Shared S&ecret:
S_RADIUS_5	&Confirm Shared Secret:
S_RADIUS_6	The RADIUS server must accept requests from IP addresses of this VPN Server. Also, authentication by Password Authentication Protocol (PAP) must be enabled.
S_RADIUS_7	milliseconds (above %u, below %u)
S_RADIUS_8	&Retry Interval
S_RADIUS_9	(use ',' or ';' to split multiple hostnames.)
STATIC2	When using Windows NT Domain Controller or Windows Server Active Directory Controller as an external authentication server, you must setup the VPN Server computer to join the domain. To use NT Domain Authentication, there are no items to configure here.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_LINK
CAPTION	Cascade Connections on %S
STATIC1	Cascade Connection can make a layer-2 Ethernet-level links between this Virtual Hub and other Virtual Hub which is located on either local or remote VPN Server.
STATIC2	Before Using Cascade Connection
STATIC3	Cascade Connection realizes a Layer 2 Bridge between multiple Virtual Hubs. But if the connection is incorrectly configured, an infinity loop could inadvertently be created. When using a Cascade Connection function please design the network topology with care.
B_CREATE	&Novo
B_EDIT	&Editar
B_ONLINE	O&nline
B_OFFLINE	O&ffline
IDOK	&Status
B_DELETE	&Excluir
B_RENAME	Reno&mear
B_REFRESH	&Atualizar
IDCANCEL	S&air
PREFIX	D_SM_LOG
CAPTION	Log Save Settings
S_TITLE	Você pode salvar os logs de segurança (como o histórico de logins do usuário) do Hub Virtual "%S" e os logs de todos os pacotes que passam pelo Hub Virtual.
STATIC1	&Log de segurança:
B_SEC	Salve log de &segurança
S_SEC	Log File S&witch Cycle:
STATIC2	&Log de pacotes:
B_PACKET	Salvar log de &pacotes
S_PACKET	Log File S&witch Cycle:
S_PACKET_0	Conexão TCP:
B_PACKET_0_0	Não salvar
B_PACKET_0_1	Apenas cabeçalhos
B_PACKET_0_2	Headers && Payloads
S_PACKET_1	Pacote TCP:
B_PACKET_1_0	Não salvar
B_PACKET_1_1	Apenas cabeçalhos
B_PACKET_1_2	Headers && Payloads
S_PACKET_2	Pacote DHCP:
B_PACKET_2_0	Não salvar
B_PACKET_2_1	Apenas cabeçalhos
B_PACKET_2_2	Headers && Payloads
S_PACKET_3	Pacote UDP:
B_PACKET_3_0	Não salvar
B_PACKET_3_1	Apenas cabeçalhos
B_PACKET_3_2	Headers && Payloads
S_PACKET_4	Pacote ICMP:
B_PACKET_4_0	Não salvar
B_PACKET_4_1	Apenas cabeçalhos
B_PACKET_4_2	Headers && Payloads
S_PACKET_5	Pacote IP:
B_PACKET_5_0	Não salvar
B_PACKET_5_1	Apenas cabeçalhos
B_PACKET_5_2	Headers && Payloads
S_PACKET_6	Pacote ARP:
B_PACKET_6_0	Não salvar
B_PACKET_6_1	Apenas cabeçalhos
B_PACKET_6_2	Headers && Payloads
S_PACKET_7	Pacote\r\nethernet:
B_PACKET_7_0	Não salvar
B_PACKET_7_1	Apenas cabeçalhos
B_PACKET_7_2	Headers && Payloads
IDOK	&OK
IDCANCEL	Cancelar
STATIC3	Salvar grandes quantidades de logs de pacotes pode sobrecarregar a CPU e o disco rígido, além de causar um desempenho mais baixo do Hub e de todo o servidor VPN. Habilite o log apenas de pacotes necessário.
PREFIX	D_SM_CA
CAPTION	Gerenciar lista de certificados CA confiáveis
STATIC1	You can manage the list of certificate authority (CA) certificates that are trusted by this Virtual Hub.\r\n\r\nThe list of CA certificates that is listed here is used to verify certificates when a VPN Client is connected in signed certificate authentication mode.
B_IMPORT	&Adicionar
IDOK	&Ver certificado
IDCANCEL	&Fechar
B_DELETE	&Excluir
PREFIX	D_SM_SESSION
CAPTION	Manage Sessions - %S
S_TITLE	Virtual Hub "%S" has the following VPN sessions currently.
STATIC1	Operations for Sessions
IDOK	Session &Information
B_DISCONNECT	&Desconectar
B_REFRESH	A&tualizar
B_SESSION_MAC_TABLE	&MAC Table of Selected Session
B_SESSION_IP_TABLE	I&P Table of Selected Session
STATIC2	&Other Administration Tasks
B_MAC_TABLE	MAC &Address Table List
B_IP_TABLE	IP Address Ta&ble List
IDCANCEL	S&air
S_FARM_INFO_2	The sessions displayed here are all sessions on the current cluster. To manage sessions on other cluster member servers you must connect as an administrator to those servers.
PREFIX	D_SM_MAC
CAPTION	MAC Address Table
S_TITLE	The MAC address table database on the Virtual Hub "%S" has the following entries.
B_DELETE	&Excluir entrada selecionada
B_REFRESH	A&tualizar
IDCANCEL	S&air
PREFIX	D_SM_IP
CAPTION	Tabela de endereços IP
S_TITLE	The IP address table database on the Virtual Hub "%S" has the following entries.
B_DELETE	&Excluir entrada selecionada
B_REFRESH	A&tualizar
IDCANCEL	S&air
PREFIX	D_SM_CREATE_CERT
CAPTION	Cria novo certificado
STATIC1	Você pode criar facilmente certificados assinados por si ou por outros certificados.
STATIC2	&Tipo de certificado:
R_ROOT_CERT	Certificado &raiz (certificado autoassinado)
R_SIGNED_CERT	Certificado &assinado por outro certificado
S_LOAD_1	&Certificado e chave privada para assinatura:
B_LOAD	Carregar certificado e chave &privada
S_LOAD_2	Clique em 'Carregar certificado e chave privada' para especificar o certificado X509 e a chave privada RSA que usarão uma nova assinatura de certificado.
S_LOAD_3	Nome comum (CN):
S_LOAD_4	Organização (O):
S_LOAD_5	Unidade organizacional (OU):
S_LOAD_6	País (C): 
S_LOAD_7	Estado (ST):
S_LOAD_8	Local (L):
S_LOAD_11	Número de série:\r\n(hexadecimal) 
S_LOAD_9	&Expira em:
S_LOAD_10	Dias
STATIC3	Para gerenciar certificados e autoridades de certificação em larga escala, você deve usar software livre como o OpenSSL ou software comercial de CA (autoridade de certificação).
IDOK	&OK
IDCANCEL	Cancelar
S_LOAD_12	&Força:
PREFIX	D_NM_LOGIN
CAPTION	excluído
S_TITLE	excluído
STATIC1	excluído
STATIC2	excluído
IDOK	excluído
IDCANCEL	excluído
PREFIX	D_SPEEDMETER
CAPTION	Network Device Status
STATIC1	Selecionar adaptador de rede virtual:
STATIC2	Real-time Status
STATIC3	&Atualizar
PREFIX	D_NM_MAIN
CAPTION	excluído
STATIC1	excluído
STATIC2	excluído
B_SETTING	Configuração de &conexão para o servidor VPN
B_CONNECT	&Conectar
B_DISCONNECT	&Desconectar
STATIC3	Operation Settings of User-mode Router
STATIC4	You can set the operations in a virtual network of a SoftEther VPN User-mode Router.
B_OPTION	&Operation Settings of User-mode Router
STATIC5	Operating Status of User-mode Router
STATIC6	Displays the current operating status of the SoftEther VPN User-mode Router.
B_NAT	Virtual &NAT Status
B_DHCP	Status do servidor D&HCP virtual
B_STATUS	User-mode &Router Status
B_INFO	User-mode Router &Information
B_PASSWORD	Configuração da &senha de administração
B_REFRESH	Atuali&zar
B_ABOUT	&Sobre...
IDCANCEL	S&air
PREFIX	D_NM_OPTION
CAPTION	SecureNAT Configuration
S_TITLE	Set how SecureNAT virtual host performs operation on the virtual network of Virtual Hub "%S".
STATIC1	Virtual Host's Network Interface Settings:
STATIC2	&Endereço MAC:
STATIC3	Endereço I&P:
STATIC4	&Máscara de sub-rede:
STATIC5	Virtual NAT Settings:
R_USE_NAT	Use Virtual N&AT Function
STATIC6	Valor M&TU:
STATIC7	bytes
STATIC8	T&CP Session Timeout:
STATIC9	segundos
STATIC10	&UDP Session Timeout:
STATIC11	segundos
R_SAVE_LOG	Salvar operações de NAT ou DHCP do servidor em um arquivo de &log
STATIC12	Virtual DHCP Server Settings:
R_USE_DHCP	Use Virtual DHCP Server Fu&nctions
STATIC13	&Distributes IP Address:
STATIC14	para
STATIC15	.
STATIC16	Máscara de su&b-rede:
STATIC17	Limite l&ease:
STATIC18	segundos
STATIC19	Options Applied to Clients (optional):
STATIC20	De&fault Gateway\r\nAddress:
STATIC21	DNS &Server Address 1:
STATIC22	Nome do domínio:
STATIC23	DNS &Server Address 2:
IDOK	&OK
IDCANCEL	Cancelar
S_1	Static routing table pushing function (for split tunneling)
S_2	Push the static routing table to VPN clients.
B_PUSH	Edit the static routing table to push
PREFIX	D_NM_NAT
CAPTION	NAT Session Table on Virtual NAT Router
S_TITLE	There are the following TCP or UDP NAT table entries on the virtual NAT router of SecureNAT.
B_REFRESH	A&tualizar
IDCANCEL	S&air
PREFIX	D_NM_DHCP
CAPTION	IP Lease Table on Virtual DHCP Server
S_TITLE	The SecureNAT Virtual DHCP Server has allocated the following IP addresses to clients.
B_REFRESH	A&tualizar
IDCANCEL	S&air
PREFIX	D_NM_CHANGE_PASSWORD
CAPTION	Alterar senha do administrador de %S
S_TITLE	You can change the administrator password of SoftEther VPN User-mode Router (%S). Click OK after entering the new password.
STATIC1	Nova &senha: 
STATIC2	&Confirm Your Input: 
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_SNAT
CAPTION	Virtual NAT and Virtual DHCP Function (SecureNAT) Setting
S_TITLE	SecureNAT enables you to operate a virtual NAT router (IP Masquerade) and DHCP Server function on a virtual network of Virtual Hub "%S".
STATIC1	Warning about SecureNAT
S_WARNING	The SecureNAT function is recommended only for system administrators or people with a detailed knowledge of networking.
S_WARNING2	If you use the SecureNAT correctly, it is possible to realize a safety remote access via a VPN. However when you use this as incorrectly, it can put the entire network in danger. Anyone who does not have a thorough knowledge of networks and anyone who does not have the network administrator's permission must not enable the SecureNAT. For a detailed explanation of the SecureNAT function, please refer to the VPN Server's manual or online documentation.
STATIC2	Enabling / Disabling and Changing the Setting of the SecureNAT
STATIC3	You can enable, disable or change the settings of the SecureNAT on this Virtual Hub.
B_ENABLE	&Enable SecureNAT
B_DISABLE	&Desativar SecureNAT
B_CONFIG	SecureNAT &Configuration
STATIC4	Note: When a running SecureNAT is disabled, all active TCP and UDP sessions that are connected via SecureNAT will be terminated.
STATIC5	View Current SecureNAT Status
STATIC6	You can view the current SecureNAT operating status.
B_NAT	Virtual &NAT Router Status
B_DHCP	Status do servidor D&HCP virtual
B_STATUS	View &SecureNAT Operating Status
S_TSUKUBA2	SecureNAT uses technology that Daiyuu Nobori developed in 2004 at "Special Seminar on Information I" at the College of Information Science of the Third Cluster of Colleges, Tsukuba University.
IDCANCEL	S&air
PREFIX	D_SM_BRIDGE
CAPTION	Local Bridge Settings
STATIC1	Local Bridge can establish a Layer 2 bridge connection between a Virtual Hub on this VPN server and a physical Ethernet Device (Network Adapter). \r\nIt is also possible to create a tap device (virtual network interface) and establish a bridge connection with a Virtual Hub. (Tap is supported on Linux versions only)
B_DELETE	&Excluir bridge local
STATIC2	New &New Local Bridge Definition:
STATIC3	Select the Virtual Hub to bridge.
STATIC4	&Hub Virtual: 
STATIC5	&Type to Create:
R_BRIDGE	Bridge with &Physical Existing Network Adapter
R_TAP	Bridge with New &Tap Device
S_ETH_1	Adaptardor LAN:
S_TAP_1	New Tap &Device Name:
S_TAP_2	(Maximum 11 Characters)
STATIC6	Note: Although it is possible to establish a bridge using any operating network adapter, in high load environments, you should prepare a network adapter dedicated for bridging.
IDOK	Cre&ate Local Bridge
STATIC7	If a network adapter doesn't appear which is recently added on the system, reboot the computer and re-open this screen.
IDCANCEL	S&air
B_VLAN	Ferramenta de configuração de transparência da VLAN
PREFIX	D_WIN9X_REBOOT
CAPTION	Cliente VPN - Instalar adaptador de rede virtual
STATIC1	The VPN Client Virtual Network Adapter has been installed. \r\nIt is necessary to shutdown Windows now and restart the computer. \r\n\r\nThe computer will restart automatically. If the computer does not restart, please restart the computer manually.
PREFIX	D_EM_MAIN
CAPTION	SoftEther EtherLogger Gerenciador
STATIC1	SoftEther EtherLogger is a service that captures data flowing through LAN cards connected to the computer and keeps a log of the headers of the packet types specified by the administrator and all data in text file format. \r\n\r\nCurrently, the following capture devices are performing capture logging.
B_PASSWORD	Administration &Password
B_LICENSE	&Licença
B_ADD	&Adicionar
IDOK	&Editar
B_DELETE	&Excluir
IDCANCEL	S&air
PREFIX	D_EM_ADD
STATIC1	Nome do adaptador de rede usado paa captura:
R_PROMISCUOUS	Do&n't Use Promiscuous Mode During Capture
STATIC2	&Log de pacotes: 
S_PACKET	Log File S&witch Cycle: 
S_PACKET_0	TCP Connection Log: 
B_PACKET_0_0	Não salvar nada
B_PACKET_0_1	Somente informações de cabeçalho
B_PACKET_0_2	Conteúdo do pacote inteiro
S_PACKET_1	TCP Packet Log: 
B_PACKET_1_0	Não salvar nada
B_PACKET_1_1	Somente informações de cabeçalho
B_PACKET_1_2	Conteúdo do pacote inteiro
S_PACKET_2	DHCP Packet Log: 
B_PACKET_2_0	Não salvar nada
B_PACKET_2_1	Somente informações de cabeçalho
B_PACKET_2_2	Conteúdo do pacote inteiro
S_PACKET_3	UDP Packet Log: 
B_PACKET_3_0	Não salvar nada
B_PACKET_3_1	Somente informações de cabeçalho
B_PACKET_3_2	Conteúdo do pacote inteiro
S_PACKET_4	ICMP Packet Log: 
B_PACKET_4_0	Não salvar nada
B_PACKET_4_1	Somente informações de cabeçalho
B_PACKET_4_2	Conteúdo do pacote inteiro
S_PACKET_5	IP Packet Log: 
B_PACKET_5_0	Não salvar nada
B_PACKET_5_1	Somente informações de cabeçalho
B_PACKET_5_2	Conteúdo do pacote inteiro
S_PACKET_6	Log de pacotes ARP: 
B_PACKET_6_0	Não salvar nada
B_PACKET_6_1	Somente informações de cabeçalho
B_PACKET_6_2	Conteúdo do pacote inteiro
S_PACKET_7	Ethernet\r\nPacket Log: 
B_PACKET_7_0	Não salvar nada
B_PACKET_7_1	Somente informações de cabeçalho
B_PACKET_7_2	Conteúdo do pacote inteiro
IDOK	&OK
IDCANCEL	Cancelar
STATIC3	Saving large volume packet logs can place a large burden on the CPU and the hard disk and it can cause lower performance of the entire system. Please configure settings so that only the necessary packet log information is saved.
PREFIX	D_EM_PASSWORD
CAPTION	Change Administrator Password
S_TITLE	You can change the administrator password. Click OK after entering the new password.
STATIC1	Nova &senha:
STATIC2	&Confirmar:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_EM_LICENSE
CAPTION	Add or Delete License
STATIC1	To use SoftEther EtherLogger you must acquire a valid license and register the license key. Using this window, you can register a new license key, delete a registered license key and display the current license list and the license mode of the SoftEther EtherLogger.
S_BOLD	&List of Currently Registered Licenses: 
B_OBTAIN	&Obtain License
STATIC2	Click Obtain License to display the website that will provide instructions on how to obtain a license.
B_ADD	&Add License Key Registration
B_DEL	&Excluir
IDOK	&Informações sobre licença
STATIC3	Select a license and click Information About License to connect to SoftEther VPN Project's website (softether.com) and view the registered information relating to the selected license.
S_BOLD2	Current License &Mode of SoftEther EtherLogger: 
IDCANCEL	S&air
PREFIX	D_EM_LICENSE_ADD
CAPTION	Adicionar registro de chave de licença
S_INFO	You can register a license key of a SoftEther EtherLogger product license.
STATIC1	The license keys are 36 alphanumeric characters in length plus hyphens. They are key codes that certify the ownership of a license. \r\n\r\nWhen a license certificate is received together with this software, the license key is printed on this license certificate. If the license for this software has been purchased online, the license key is provided by email and on the website window at the time the license is purchased. The license key may also be written down by some other method. If you don't know where the license key is written down, ask the vendor who sold you the license.
STATIC2	&Input the License Key Correctly: 
STATIC3	Enter the license key by separating the input into 6-digit groups. You don't need to input the hyphens. It is also possible to copy && paste the license key.
B_INFO2	This software has world-wide copyright protection. Customers can only make copies and use this software in accordance with the license conditions. Warning: Use of illegitimately obtained license keys, use of a single license on multiple servers, or unauthorized distribution of licenses is a breach of the license agreement and such action may result in civil or legal proceedings.
IDOK	&Registrar
IDCANCEL	Cancelar
PREFIX	D_EM_REMOTE
STATIC1	&Specify the Host Name of the Destination Computer, or IP Address: 
R_LOCAL	Conectar ao &computador local (computador exibindo esta janela)
S_HOSTNAME	&Nome do computador: 
IDOK	&OK
IDCANCEL	Cancelar
B_ABOUT	Informações da versão
PREFIX	D_SM_CONFIG
CAPTION	Edit Config File
IDC_INFO	The current configuration of the VPN Server "%S" is as follows.\r\nYou can edit the contents of this configuration file and apply it to the VPN Server.
B_EXPORT	&Salvar para arquivo
B_IMPORT	&Import File and Apply
IDCANCEL	&Fechar
STATIC1	You can edit the configuration file by using any text editors. When applying the edited configuration file to the VPN Server, the VPN Server will automatically restart and launch according to the new configuration file. If an invalid configuration file is applied, errors will occur and the current setting contents will get lost, so be careful when editing the configuration file.
B_FACTORY	&Restore to Factory Default
PREFIX	D_SM_ADMIN_OPTION
CAPTION	Virtual Hub Administration Option
S_INFO	Currently the following administration options are set for the Virtual Hub "%S".
B_ADD	&Adicionar valor
B_EDIT	&Editar valor
B_DELETE	&Excluir valor
STATIC1	The purpose of the Virtual Hub administration options is to set limitations to administrators who are in Virtual Hub Admin Mode.
IDOK	&Salvar
IDCANCEL	Cancelar
STATIC2	Only an administrator for this entire VPN Server may edit the Virtual Hub administration options. The individual Virtual Hub administrators are unable to change the administration options, however they are able to view them.\r\nHowever, if allow_hub_admin_change_option is set to "1", then Virtual Hub administrators are able to edit the administration options.
S_BOLD	Descrição:
PREFIX	D_SM_MSG
CAPTION	Set the Message
S_MSG_2	You can set a message to display on the screen of a user when a VPN Client connects to the Virtual Hub "%S". To show a message, input the message that you want to show.
C_USEMSG	Mostrar &mensagem
STATIC1	About the Message Display Function
S_INFO	The VPN Client must be Version 3.0 or later.\r\n\r\nSpecify a single line starts with "http://" as the message to open the default Web browser on the client instead to showing a message.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_NICINFO
CAPTION	Status do adaptador de rede virtual "%S"
IDCANCEL	&Fechar
PREFIX	D_SM_VLAN
CAPTION	Ferramenta de configuração de transparência da VLAN
STATIC1	Some network adapters are unable to transmit tagged-VLAN packets (IEEE802.1Q) transparency. by default\r\n\r\nIf you use such a network adapter to bridge to the Virtual Hub and need to exchange Ethernet packets with VLAN tags, you have to configure the network adapter to enable processing packets for VLAN transparency.
B_ENABLE	Configure the Selected Network Adapters to VLAN Transparency
B_DISABLE	&Unset the Configuration
STATIC2	About the VLAN Transparency Setting Tool
S_WARNING	This tool can enable or disable the transparency for tagged VLAN packets on Intel, Broadcom or Marvell's network adapters. (Only using the vendor provided drivers for Windows.)
S_WARNING2	The above network adapters in the list means supported by this tool. No other network adapters can be configured by this tool. However, other network adapters which is not on the list might be able to support tagged VLAN packets by default or by using some configuration.\r\n\r\nSuch network adapters must be configured by the system administrator with logged on Windows.
IDCANCEL	S&air
PREFIX	D_SM_SIMULATION
CAPTION	Delay and Packet Loss Generating Function
STATIC1	This function can generate delays, jitters and packet losses on packets which match the condition of this access list entry when transmitted via this Virtual Hub.\r\n\r\nThis function is convenient to simulate a low-quality and slow Internet, WAN or wireless connections on the desk or laboratory. For example, you can use it to evaluate and test IP telephonies (VoIP).
STATIC2	Generate Delays, Jitters and Packet Losses as follow:
C_DELAY	Generate &Delays
S_DELAY	The Period of Delay (0 - 10000) :
S_DELAY2	milissegundos
C_JITTER	Generate &Jitters (Fluctuation)
S_JITTER	The Ratio of Jitter (0 - 100) :
S_JITTER2	Porcentagem (%)
C_LOSS	Generate Packet &Losses
S_LOSS	The Ratio of Packet Losses (0 - 100) :
S_LOSS2	Porcentagem (%)
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_AO_VALUE
CAPTION	Name and Value
STATIC1	&Nome:
STATIC2	&Valor:
STATIC3	(Inteiro)
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_L3
CAPTION	Virtual Layer 3 Switch Setting
STATIC1	You can define Virtual Layer 3 Switches between two or more Virtual Hubs operating on this VPN Server to achieve routing between different IP networks.
STATIC2	The Virtual Layer 3 Switch functions are provided for network administrators or people who know a lot about networking and IP routing. If you are using the regular VPN functions, you do not need to use the Virtual Layer 3 Switch functions.\r\n\r\nIf the Virtual Layer 3 Switch functions are to be used, the person who configures them must have sufficient knowledge of IP routing.
STATIC3	Cautions about Virtual Layer 3 Switch Function
S_BOLD	Defined Virtual &Layer 3 &Switches:
B_ADD	&Novo
B_START	&Iniciar
B_STOP	P&arar
IDOK	&Editar
B_DELETE	&Excluir
IDCANCEL	&Fechar
PREFIX	D_SM_L3_ADD
CAPTION	New Virtual Layer 3 Switch
STATIC1	To create a new Virtual Layer 3 Switch, enter a name for the switch. \r\n\r\nThe Virtual Layer 3 Switch cannot have the duplicated name as another Virtual Layer 3 Switch on this VPN Server.
STATIC2	&Nome:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_L3_SW
CAPTION	Edit Virtual Layer 3 Switch "%S"
STATIC1	You can define multiple virtual interfaces and routing tables on a Virtual Layer 3 Switch.
STATIC2	A virtual interface is associated to a Virtual Hub and operates as a single IP host on the Virtual Hub when the Virtual Hub is running. When multiple virtual interfaces that respectively belong to a different IP network of a different Virtual Hub are defined, IP routing will be automatically performed between these interfaces. \r\nIt is possible to manually set the routing table and more detailed settings.
S_BOLD1	Virtual &Interfaces:
B_ADD_IF	&New Virtual Interface
B_DEL_IF	D&elete Virtual Interface
S_BOLD2	Routing &Table:
B_ADD_TABLE	A&dd Routing Table Entry
B_DEL_TABLE	De&lete Routing Table Entry
B_START	&Iniciar
B_STOP	P&arar
IDCANCEL	&Fechar
PREFIX	D_SM_L3_SW_IF
CAPTION	Add Virtual Interface
STATIC1	Adds a new virtual interface to the Virtual Layer 3 Switch. \r\n\r\nYou must define the IP network that the virtual interface belongs to and the IP address of the interface itself. \r\nPlease select or enter the name of the virtual Hub that the interface will attach to.
STATIC2	Virtual Hub to &Attach
STATIC3	Select or enter the name of the Virtual Hub that this interface will attach to.
STATIC4	&Hub Virtual:
STATIC5	IP A&ddress and Subnet Mask of Virtual Interface:
STATIC6	The virtual interface must have one IP address in the Virtual Hub. You also must specify the subnet mask of an IP network that the IP address belongs to. \r\n\r\nRouting via the Virtual Layer 3 Switches attaching to multiple virtual Hubs operates based on the IP address is specified here.
S_SRC_IP_1	&Endereço IP:
S_SRC_IP_2	&Máscara de sub-rede:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_L3_SW_TABLE
CAPTION	New Routing Table Entry
STATIC1	Adds a new routing table entry to the routing table of the Virtual Layer 3 Switch. \r\n\r\nIf the destination IP address of the IP packet does not belong to any IP network that belongs to a virtual interface, the IP routing engine of the Virtual Layer 3 Switch will reference the routing table and execute the routing.
STATIC2	Definitions of Routing Table &Entry: 
STATIC3	The virtual interface must have one IP address in the Virtual Hub. You also must specify the subnet mask of an IP network that the IP address belongs to. \r\n\r\nRouting via the Virtual Layer 3 Switches of IP spaces of multiple virtual Hubs operates based on the IP address is specified here.
S_SRC_IP_1	&Network Address:
S_SRC_IP_2	&Máscara de sub-rede:
S_SRC_IP_3	&Gateway Address:
S_SRC_IP_4	&Valor métrica:
STATIC4	Note: To specify the default gateway, specify '0.0.0.0' for both the network address and the subnet mask.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_CM_SELECT_SECURE
CAPTION	Selecionar Smart Card
STATIC1	Select the type of smart card device to use. \r\n\r\nThe types of smart cards listed in this list have had their drivers installed on the current computer and are supported by VPN software. \r\nIf there is a type of smart card that is currently being used that does not appear in the list, it may be possible that update of the VPN software to a newer version enable you to use it. \r\n\r\nNote: If a driver is not displayed immediately after installation, restart Windows.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_CM_SECURE_MANAGER
CAPTION	Autenticação do Smart Card
S_INFO	Current Smart Card:\r\n\r\n%S
B_BOLD	Objects stored on the smart card: 
B_REFRESH	&Atualizar lista de objetos
B_IMPORT	&Import to Card...
B_EXPORT	&Export from Card...
B_DELETE	&Excluir do cartão
B_NEW_CERT	&Write New Certificate and Private Key to Card...
B_PIN	&Change PIN Code...
IDCANCEL	Fechar
PREFIX	D_CM_SECURE_TYPE
CAPTION	Select Object Type
STATIC	Select the type of the object you want to import.
R_CERT	&Certificado
R_KEY	&Chave privada
R_DATA	&Dado
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_STRING
CAPTION	Software VPN
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_SELECT_KEYPAIR
CAPTION	Especificar o certificado no Smart Card
S_INFO	Currently selected smart card:\r\n\r\n%S
B_BOLD1	Select the certificate in the smart card.
IDOK	&OK
IDCANCEL	Cancelar
B_BOLD2	Select the corresponding private key.
PREFIX	D_CM_LOAD_X
CAPTION	Load Certificate
STATIC1	Select the method to load the certificate.
R_FROM_FILE	Load Certificate from &File
R_FROM_SECURE	Load Certificate from &Smart Card
S_FILE	You can load a certificate from a file that stores certificate data (extensions: .cer, .crt, .p12, .pfx).
S_CERT	If a smart card is connected to this computer, you can load a certificate from a smart card.
B_SELECT	&Selecionar qual Smart Card usar...
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_CM_SECURE_PIN
CAPTION	Change PIN Code
STATIC1	You can change the PIN code (secret number) of the smart card. \r\n\r\nTo change the PIN code, you are required to enter the current PIN code and the new PIN code twice.
STATIC2	&Current PIN code: 
STATIC3	&Novo código PIN: 
STATIC4	Con&firm New PIN: 
STATIC5	Nota
STATIC6	If you incorrectly input the current PIN a certain number of times, the smart card will be rendered unusable.
STATIC7	Please insert the smart card and click OK.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_CRL
CAPTION	Certificates Revocation List
STATIC1	You can manage the Certificates Revocation List on this Virtual Hub. \r\n\r\nBy adding certificates in Certificates Revocation List, the clients who provide these certificates will be denied to connect to this Virtual Hub using certificate authentication mode.
B_ADD	&Adicionar
IDOK	&Editar
IDCANCEL	&Fechar
B_DELETE	&Excluir
PREFIX	D_SM_EDIT_CRL
CAPTION	Revoked Certificate
STATIC1	You can set the contents of an entry on the revocation list. \r\n\r\nWhen a user connects to a Virtual Hub in certificate authentication mode and that certificate matches one or more of the contents defined in the Certificates Revocation List, the user will be denied to connect.
S_BOLD	The certificates that matches all the fields of the items will be disabled.
STATIC2	Contents of Certificate:
R_CN	Nome comum (CN):
R_O	Organização (O):
R_OU	Unidade organizacional (OU):
R_C	País (C):
R_ST	Estado (ST):
R_L	Local (L):
STATIC3	Certificate Attribute Value:
R_SERI	Serial Number (Hex):
R_MD5_HASH	MD5 Digest Value (Hex, 128 bit):
R_SHA1_HASH	SHA-1 Digest Value (Hex, 160 bit):
STATIC4	A digest value (hash value) can identify the particular certificate exactly. If you specify a MD5 or SHA-1 digest value, you need not to specify other items.
STATIC5	Import Values from a Certificate File
STATIC6	If there is a certificate file that you want to disable, you can correctly specify the certificate and add it to the invalid list by importing that file. Click Load Certificate and the contents of the specified certificate file will be imported automatically.
B_LOAD	&Carregar certificado...
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_AC_LIST
CAPTION	Source IP Address Limit List
S_TITLE	To allow or deny VPN connections to this VPN Server Virtual Hub "%S" according to the client computer's IP address, you can set the rules to allow or deny the connection below.
B_ADD	&Nova regra
IDOK	&Editar regra
B_DELETE	&Excluir regra
B_SAVE	&Salvar
IDCANCEL	&Cancelar
STATIC1	Items with higher priority appear higher in the list.
STATIC2	If the client's IP address does not match any item in the list, VPN connection to this Virtual Hub will be allowed.
PREFIX	D_SM_AC
CAPTION	Edit Rule Entry of Source IP Address Limit List
STATIC1	Define a rule in the IP Access Control List. The values set here will be used to decide whether to allow or deny connection from a VPN Client when this client attempts connection to the Virtual Hub.
STATIC2	Defines of a Rule
STATIC3	Apply this Rule when the client's IP address matches the following:
R_SINGLE	&Single IP Address
R_MASKED	&Multiple IP Addresses (Specify by IP Network Address and Mask)
STATIC4	&Endereço
S_MASK	&Máscara de rede:
STATIC5	Ação
R_PASS	&Permitir
R_DENY	&Negar
STATIC6	Outros
STATIC7	P&rioridade:
STATIC8	(Integer: higher priority is given to smaller numbers)
STATIC9	IP Protocol Version
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_LOG_FILE
CAPTION	Arquivos de log
STATIC1	Você pode fazer o download dos arquivos de log salvos no servidor.\r\n\r\nO administrador do servidor VPN pode para fazer o download de todos os logs do servidor. Os administradores do hub virtual têm permissão para baixar apenas o arquivo de log do hub virtual.
IDOK	&Baixar
B_REFRESH	&Atualizar
IDCANCEL	Fechar
PREFIX	D_SM_READ_LOG_FILE
CAPTION	Baixar arquivo
S_INFO2	Downloading the file "%S" from the VPN Server. \r\nPlease wait...
IDCANCEL	&Parar download
PREFIX	D_SM_SAVE_LOG
CAPTION	Downloaded Log File
S_INFO	O arquivo "%S" foi baixado. \r\n\r\nVocê pode abrir ou salvar este arquivo.
IDOK	&Abrir
B_SAVE	&Salvar
IDCANCEL	Cancelar
PREFIX	D_TCP
CAPTION	Utilitário de otimização de TCP
STATIC1	By optimizing the TCP/IP settings on Windows, it is possible to increase the network communication throughput of this computer. \r\n\r\nBy using this TCP Optimization Utility, you can easily configure the settings for optimize the parameters.
STATIC2	Current TCP/IP setting parameters of Windows is as follows. By changing these values you can optimize the TCP/IP settings. Using this utility any time later you can reset the values or restore them to the previous setting.
STATIC3	TCP/IP Communication Setting:
STATIC4	TCP &Receiving Window Size:
R_RECV_DISABLE	Usar valor &padrão do sistema
R_RECV_ENABLE	S&et the Values Below
S_RECV	bytes
B_RECV	Valor padrão
STATIC5	TCP &Sending Window Size:
R_SEND_DISABLE	Use OS Default Value
R_SEND_ENABLE	Set the Values Below
S_SEND	bytes
B_SEND	Valor padrão
IDOK	&OK
IDCANCEL	Cancelar
STATIC6	The changes above will take effect after Windows has rebooted. After changing the settings, you do not need to immediately reboot the computer, but until it is rebooted the TCP/IP optimized settings will not take effect.
B_DELETE	Do not Manage by this Utility
PREFIX	D_TCP_MSG
CAPTION	Otimização TCP
STATIC1	By optimizing the TCP/IP settings on Windows, it is possible to increase the network communication throughput of this computer. Do you want to optimize the communication settings?\r\n\r\nYou can start at any time in the future the TCP Optimization Utility and optimize the communication settings or restore them to their previous values. 
STATIC2	When the TCP/IP settings are changed, the changes will take effect after Windows has restarted. After changing the settings, you do not need to immediately restart the computer, but until it is restarted the TCP/IP optimized settings will not take effect.
R_OPTIMIZE	&Automatically Optimize Communication Settings
R_MANUAL	&Manually Optimize Using TCP Optimization Utility
R_NO	&Do not Optimize
IDOK	&Próximo >
IDOK3	< &Voltar
PREFIX	D_CM_PKCSEULA
CAPTION	Notice to Use Smart Card's Drivers
S_INFO_1	You are attempting to access the smart card with software "%S".
S_INFO_2	When using software "%S", if there are conditions of use for this software and the smart card that is to be used, you must agree to these conditions of use before using them. \r\n\r\nFor details please contact the vendor of software "%S" and of the smart card.
S_INFO_3	Do you agree to the above and want to use the software "%S" and access the specified smart card?
IDOK	&Sim
IDCANCEL	&Não
PREFIX	D_CM_TRAFFIC
CAPTION	Ferramenta de teste de velocidade do tráfego de rede
STATIC1	Network Traffic Speed Test Tool performs transmitting packets between two computers connected with TCP/IP, with large amount of throughput as possible, in order to measure the actual network traffic speed available. This tool can be used for not limited VPNs, but it is useful for physical networks.
STATIC2	Use this tool to measure the current bandwidth capacity of the network. Note that the value obtained is sometimes lower than the actual network processing capacity due to the CPU performance of both endpoints, what other programs are currently running and fluctuations in the rate of use of the network.
S_1	Configurations:
S_3	Which is the role of this computer?
R_SERVER	&Servidor de teste
R_CLIENT	&Cliente de teste
S_4	To activate the test server, specify the listening port number.\r\nTo use it as the test client, specify the host name of the destination test server or the IP address, and port number. If necessary, configure the optional settings below.
S_5	Destination Test Server &Hostname: 
S_6	&Número da porta: 
S_7	(Porta TCP)
S_8	Configure following options on the client side.
S_9	Direction of Data Communication
R_DOWNLOAD	&Download (Incoming: from Server to Client)
R_UPLOAD	&Upload (Outgoing: from Client to Server)
R_FULL	Download and Upload (&Full-Duplex Mode: In and Out Simultaneously)
S_10	Configurações avançadas
S_11	&Number of Concurrent Parallel TCP Connections:
S_12	Me&asuring Period:
S_13	segundos
R_ETHERNET	Correct L2 Throughput Assuming &Ethernet
R_DOUBLE	Relay Device Mode
S_14	conexões
IDOK	&Executar
IDCANCEL	Cancelar
S_15	You can also run this tool from the vpncmd Command-line Management Utility (also available on non-Windows OS).
PREFIX	D_CM_TRAFFIC_RUN
CAPTION	Ferramenta de teste de velocidade do tráfego de rede
S_INFO	The Network Traffic Speed Test Tool is running. The operating status is as follows.
STATIC1	To abort the Network Traffic Speed Test Tool, click Exit.
IDCANCEL	&Sair
PREFIX	D_CM_TRAFFIC_RESULT
CAPTION	Communication Traffic Measurement Results
STATIC1	Communication traffic has been measured. The results are shown below.
IDCANCEL	&Fechar
PREFIX	D_SM_LICENSE
CAPTION	Add or Remove License
STATIC1	To use SoftEther VPN Server you must acquire a valid license and register the license key. You can register a new license key, delete a registered license key and display the current license list and the license mode of the VPN Server here.
S_BOLD	Currently Registered &License Keys:
B_OBTAIN	&Obtain or Extend a License
STATIC2	Click Obtain or Extend License to visit the website that will provide instructions on how to obtain a license.
B_ADD	&Adicionar uma chave de licença
B_DEL	&Excluir
IDOK	&Informações sobre licença
STATIC3	Select a license and click Information About License to connect to SoftEther VPN Project's website (softether.com) and view the registered information relating to the selected license.
S_BOLD2	Current License &Mode of SoftEther VPN Server: 
IDCANCEL	S&air
PREFIX	D_SM_LICENSE_ADD
CAPTION	Add License Keys
S_INFO	You can register a SoftEther VPN Server product license or a connection license.
STATIC1	The license keys are 36 alphanumeric characters in length plus dashes. They are key codes that certify the ownership of a license. \r\n\r\nWhen a license certificate is received together with this software, the license key is printed on this license certificate. If the license for this software has been purchased online, the license key is provided by email and on the website window at the time the license is purchased. The license key may also be written down by some other method. If you don't know where the license key is written down, ask the vendor who sold you the license.
STATIC2	&Input the License Key Accurately:
STATIC3	Enter the license key by separating the input into 6-digit groups. You don't need to input the dashes. It is also possible to copy && paste the license key.
B_INFO2	This software is protected by world-wide copyright laws. Customers can only make copies and use this software in accordance with the license conditions. Warning: Use of illegitimately obtained license keys, use of a single license on multiple servers, or unauthorized distribution of licenses is a breach of the license agreement and such action may result in civil or legal proceedings.
IDOK	&Registrar
IDCANCEL	Cancelar
PREFIX	D_FREEINFO
CAPTION	About SoftEther VPN Server Free Edition
S_INFO_1	Thank you for trying out the SoftEther VPN Server Free Edition.
S_INFO_2	The SoftEther VPN Server operating on destination server "%S" is the Free Edition intended for personal use. \r\nWhen using the Free Edition, you can use all the SoftEther VPN Server functions but the User Agreement prohibits the following usage.
S_INFO_3	Use where communication for commercial purposes travels via the VPN Server. 
S_INFO_4	Note that if the software is used based on the above mentioned prohibited usage, it is a breach of the SoftEther VPN Server user agreement. The above restriction is lifted once you obtain a regular product license for SoftEther VPN Server. For details on the regular product version, please visit www.softether.com. \r\n\r\nIf this server is being used under the usage described above, please contact us via our website at www.softether.com. \r\n\r\nNote: This window will appear when connected to a Free Edition of VPN Server. This window does not appear when Editions other than the Free Editions of the software product are used. \r\nNote: Apart from this notification window, there are absolutely no differences between the Free Edition software and the product version.
B_HIDE	&Ocultar esta janela da próxima vez.
IDCANCEL	&OK
PREFIX	D_CM_SETTING
CAPTION	Alterar modo de operação do SoftEther VPN Cliente
STATIC1	You can use SoftEther VPN Client in either Normal Mode or Easy Mode. To switch to the other mode, check the respective checkbox below.
R_NORMAL	&Modo normal
R_EASY	&Modo fácil
STATIC2	When using Normal Mode, you can perform all the operations that the SoftEther VPN Client software provides. We recommend that general users and system administrators use this mode.
STATIC3	Easy Mode only allows the most frequently used operations such as connecting to the VPN Server. We recommend this mode to beginner users.
STATIC4	By using the Setting Locker, you can connect to a VPN Server by using a Connection Setting registered in SoftEther VPN Client, but by doing so, you are prevented from changing the parameters of Connection Settings, creating a new Connection Setting or deleting a Connection Setting.
R_LOCK	Enable Setting &Locker
S_PASSWORD1	You can specify a password. The input of that password will be required next time to disable the Setting Locker.
S_PASSWORD2	&Senha:
S_PASSWORD3	&Confirmar:
IDOK	&OK
IDCANCEL	Cancelar
S_VGS2	You can configure the VPN Gate Academic Service settings.
B_VGS	VPN &Gate Service Settings...
PREFIX	D_CM_EASY
CAPTION	Edição de desenvolvedor do gerenciador fácil do SoftEther VPN Cliente 
B_MODE	Alterar &modo de operação
IDCANCEL	&Fechar
B_STATUS	Ver &status da conexão
B_VGC	VPN Gate Academic Project
PREFIX	D_SM_SETUP
CAPTION	Configuração fácil do SoftEther VPN Server / Bridge (Edição de desenvolvedor)
S_TITLE	Configuração fácil do SoftEther VPN Server / Bridge (Edição de desenvolvedor)
IDC_STATIC_1	Ao usar esta configuração, você pode configurar facilmente um servidor VPN SoftEther ou uma Bridge VPN para os seguintes usos e finalidades. Depois de sair da instalação, você pode usar o gerenciador de servidores  VPN para definir livremente configurações mais avançadas.
S_BOLD	Selecione o tipo de servidor VPN que você deseja construir. Vários tipos podem ser selecionados juntos.
C_REMOTE	Servidor VPN de acesso &remoto
S_REMOTE_1	O servidor VPN de acesso remoto permite que computadores clientes VPN em locais remotos acessem os segmentos Ethernet existentes, por exemplo, a LAN da empresa.\r\nQualquer cliente VPN conectado ao servidor VPN poderá acessar a rede como se estivesse conectado diretamente e fisicamente a ela.
C_SITE	Servidor VPN &site-to-site ou VPN Bridge
S_SITE_1	A VPN site-to-site é uma configuração VPN para conectar-se entre dois ou mais segmentos Ethernet remotos.\r\nCada um dos locais(sites) é conectado em conjunto e se torna o mesmo segmento no nível da Camada 2. Ele permite que qualquer computador de cada local se comunique entre si como se houvesse uma única rede.
S_SITE_2	Selecione a função deste servidor VPN:
C_CENTER	Servidor VPN que aceita conexão de outros locais(sites) (&Central)
C_EDGE	Servidor VPN ou Bridge VPN em cada local(site) (&Borda)
C_OTHER	&Outra configuração avançada da VPN
S_OTHER	Selecione essa opção se estiver planejando criar um sistema VPN que ofereça funções avançadas, como uma função de cluster e uma função de swithc virtual de camada 3.
IDOK	&Próximo >
IDCANCEL	&Fechar
PREFIX	D_SM_SETUP_HUB
CAPTION	Configuração fácil - Decida o nome do hub virtual
IDC_STATIC_1	Você precisa criar um hub virtual no servidor VPN. Nomeie o novo hub virtual como preferir.
IDC_STATIC_2	&Nome do Hub Virtual:
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_SETUP_STEP
CAPTION	Tarefas de configuração fácil da VPN
IDC_STATIC_1	Para concluir a instalação deste servidor VPN / Bridge VPN, você deve concluir as seguintes tarefas.
S_1_1	Etapa 1. Crie um usuário para aceitar a conexão VPN
S_1_2	Quando este servidor VPN aceita uma VPN de acesso remoto ou se torna o servidor de VPN central site-to-site que aceita conexões de outros locais(sites0, crie usuários para aceitar a conexão VPN.
B_USER	Criar &usuários
S_2_1	Etapa 2. Defina uma conexão com o servidor VPN de destino
S_2_2	Quando este servidor VPN é instalado em um site específico (borda) de uma VPN site-to-tsite, você deve especificar o endereço do servidor VPN central que aceita as conexões e estabelecer uma conexão com esse servidor VPN central.
B_CASCADE	&Configurar as configuração de conexão
S_3_1	Passo 3: Defina a bridge local
S_3_2	Para uma VPN site-to-site, use a Função Bridge Local para conectar uma Bridge entre o segmento Ethernet virtual no lado da VPN e o segmento Ethernet físico no lado local. Selecione um dispositivo Ethernet existente (adaptador de rede) que fornecerá a conexão de Bridge à VPN.
IDCANCEL	&Fechar
IDC_STATIC_8	Depois que as configurações necessárias estiverem definidas, clique em Fechar. Uma ferramenta de gerenciamento avançado para o servidor VPN / VPN Bridge será exibida. Você pode definir as configurações avançadas conforme desejar.
B_SECURENAT	Configurar Secure&NAT
PREFIX	D_CPU64_WARNING
CAPTION	Informações sobre o SoftEther VPN Edição de 64 bits
S_BOLD	O software VPN SoftEther atualmente instalado é a edição de 32 bits, mas o sistema operacional Windows atualmente em execução é uma edição de 64 bits. 
S_INFO	Você pode executar a edição de 32 bits do software SoftEther VPN em uma edição de 64 bits do Windows, mas será executada no emulador de 32 bits do Windows e isso resulta em desempenho reduzido.r\nHá também a possibilidade de que algumas funções não sejam suportadas.\r\n\r\n Recomendamos que você instale e use a edição de 64 bits do software SoftEther VPN ao executá-lo no Windows de 64 bits.\r\nVocê pode baixar a edição de 64 bits do software SoftEther VPN em http://selinks.org/. \r\n\r\nEsta caixa de diálogo será fechada automaticamente em 30 segundos.
IDOK	&OK
PREFIX	D_ONCEMSG
CAPTION	TITLE
C_DONTSHOWAGAIN	&Não mostrar esta mensagem novamente
IDCANCEL	&OK
PREFIX	D_CONNECT
IDCANCEL	Cancelar
PREFIX	D_SM_IPSEC
CAPTION	Configurações IPsec / L2TP / EtherIP / L2TPv3
S_TITLE	Configurações do servidor IPsec / L2TP / EtherIP / L2TPv3
S_3	Os hubs virtuais no servidor VPN podem aceitar conexões VPN de acesso remoto a partir de PCs compatíveis com L2TP, Mac OS X e smartphones, e também podem aceitar conexão VPN EtherIP / L2TPv3 Site-to-Site.
S01	Servidor L2TP (função de servidor VPN de acesso remoto)
S02	Podem ser aceitas conexões VPN de smartphones, como iPhone, iPad e Android, e também de clientes VPN integrados no Mac OS X e Windows.
R_L2TP_OVER_IPSEC	Ativar função de servidor L2TP (L2TP sobre IP&sec)
S03	Permite as conexões VPN do iPhone, iPad, Android, Windows e Mac OS X.
R_L2TP_RAW	Ativar função de servidor L2TP (Raw e L2TP sem criptografia)
S04	Ele suporta clientes VPN especiais que usam L2TP sem criptografia IPsec.
S_1	&Hub virtual padrão no caso de omitir um nome de Hub no nome de usuário:
S_2	Os usuários devem especificar seu nome de usuário como "nome_de_usuário@nome_do_hub_virtual_de_destino" para conectar este servidor L2TP.\r\nSe a designação de um hub virtual for omitida, o hub abaixo será usado como destino.
S05	Função de servidor EtherIP (conexão VPN site-to-site)
S06	Roteadores compatíveis com EtherIP / L2TPv3 sobre IPsec podem se conectar ao hub virtual no servidor VPN e estabelecer a ponte de camada 2 (Ethernet).
R_ETHERIP	Ativar função de servidor &EtherIP / L2TPv3 sobre IPsec
B_DETAIL	&Detalhes de configuração EtherIP / L2TPv3
S07	IPsec &Common Settings
S_PSK	Chave &pré-compartilhada IPsec:
S_PSK2	A chave pré-compartilhada IPsec também é chamada de "PSKs" ou "Segredos(secrets)". Especifique-a com cerca de oito caracteres ASCII e informe todos os usuários da VPN.
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_ETHERIP
CAPTION	Detalhes de configuração EtherIP / L2TPv3
S_TITLE	Detalhes de configuração EtherIP / L2TPv3
S01	Os roteadores EtherIP / L2TPv3 sobre IPsec compatíveis podem se conectar aos Hubs Virtuais no Servidor VPN e estabelecer a Ponte de Camada 2 (Ethernet). Por exemplo, roteadores Cisco, NEC IX series e IIJ SEIL são recomendados como roteadores VPN compatíveis.
S02	Para aceitar o protocolo EtherIP / L2TPv3, defina as configurações apropriadas do cliente EtherIP / L2TPv3 para identificar o local(site) do cliente do roteador previamente. Uma configuração do cliente EtherIP / L2TPv3 deve ter um ID IPsec Phase 1 correspondente.
S_BOLD	Tabela de identificação de fase 1 do IPsec e do hub virtual
B_ADD	&Adicionar
IDOK	&Editar
B_DELETE	&Excluir
IDCANCEL	S&air
PREFIX	D_SM_ETHERIP_ID
CAPTION	EtherIP / L2TPv3 over IPsec Client Setting
S01	The following Virtual Hub connection settings will be applied only when an EtherIP / L2TPv3 over IPsec Client is attempting to connect this VPN Server with an ISAKMP (IKE) Phase ID which is exactly equal to the value specified below.
S02	ISAKMP Phase 1 &ID:
S03	&Hub Virtual:
S04	&Username:
S05	&Senha:
S06	Note that the username and the password must be same as a registered on the Virtual Hub. An EtherIP / L2TPv3 Client will be regarded as it connected the Virtual Hub with the identification of the above user information.
IDOK	&OK
IDCANCEL	Cancelar
S07	The ID must be exact same as an ID in the configuration of the EtherIP / L2TPv3 Client. You can specify IP address as well as characters as ID, if the EtherIP / L2TPv3 Client uses IP address as Phase 1 ID. You can specify '*' (asterisk) as a wildcard to match any other clients which don't match other explicit rules.
PREFIX	D_SM_OPENVPN
CAPTION	OpenVPN / MS-SSTP Settings
S_TITLE	OpenVPN / MS-SSTP VPN Clone Server Function Settings
S_1	This VPN Server has the clone functions of OpenVPN software products by OpenVPN Technologies, Inc.\r\n\r\nAny OpenVPN Clients can connect to this VPN Server.
R_OPENVPN	Ativar função OpenVPN Clone Server
S_TOOL	Sample File Generating Tool for OpenVPN Clients
S_TOOL2	Making a OpenVPN Client configuration file is a very difficult job. You can use this tool to generate an appropriate OpenVPN Client configuration file. The generated configuration sample can be used immediately.
B_CONFIG	Generate a Sample &Configuration File for OpenVPN Clients
S_2	Microsoft SSTP VPN Clone Server Function
S_3	This VPN Server has the clone functions of MS-SSTP VPN Server which is on Windows Server 2008 / 2012 by Microsoft Corporation.\r\nBuilt-in MS-SSTP Clients on Windows Vista / 7 / 8 / RT / 10 can connect to this VPN Server.
R_SSTP	Enable &MS-SSTP VPN Clone Server Function
S_SSTP	The value of CN (Common Name) on the SSL certificate of VPN Server must match to the hostname specified on the client, and that certificate must be in the trusted list on the client. For details refer the Microsoft's documents.
S_4	The manner to specify a username to connect to the Virtual Hub, and the selection rule of default Hub by using these clone server functions are same to the IPsec Server functions.
B_IPSEC	I&Psec Server Configuration
S_13	OpenVPN Clone Server Function
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_SM_DDNS
CAPTION	Função de DNS dinâmico
S_TITLE	Função de DNS dinâmico
S_BOLD	Este servidor VPN possui uma função de DNS dinâmico interno.
S_1	O DNS dinâmico atribui um nome de host DNS exclusivo e permanente para este servidor VPN. Você pode usar esse nome de host para especificar este servidor VPN nas configurações do cliente VPN e da Bridge VPN. Você não precisa se registrar e manter um nome de domínio.
S_22	Além disso, se o seu provedor atribuir a você um endereço IP dinâmico (não fixo), o endereço IP correspondente do seu nome de host DNS dinâmico será alterado automaticamente. Ele permite que você continue executando o servidor VPN usando apenas um endereço IP dinâmico.\r\nPortanto, você não precisa mais manter endereços IP globais estáticos com custos mensais. 
S_3	Além disso, esta versão do servidor VPN suporta a função 'NAT-Traversal'. Se o servidor VPN estiver dentro de uma NAT e for atribuído apenas um endereço IP privado, você poderá conectar-se a esse servidor VPN pelo lado da Internet sem nenhuma configuração especial na NAT previamente.
S_4	&Status atual:
S_STATUS3	Nome do host DNS dinâmico atribuído:
B_HINT	Dica
S_STATUS4	Endereço IPv4 global:
S_STATUS5	Endereço IPv6 global:
S_5	Modificar as configurações:
S_STATUS6	&Altere o nome do host DNS dinâmico:
S_STATUS7	O nome do host possui apenas letras, números e traços '-'. Pelo menos três letras.\r\nVocê pode alterá-lo a qualquer momento depois.
IDOK	&Definir o hostname acima
B_RESTORE	&Restaurar
S_2	Se você não estiver conectado à internet via IPv6, "Endereço IPv6 global" deve mostrar um erro.\r\nAlguns países ou territórios podem proibir o serviço de DNS dinâmico.
IDCANCEL	S&air
B_DISABLE	&Desativar função de DNS dinâmico
B_PROXY	Conectar via servidor &proxy...
S_STATUS8	Chave DNS
B_HINT2	Dica
PREFIX	D_SM_SPECIALLISTENER
CAPTION	VPN over ICMP / DNS Function Settings
S_TITLE	Função de VPN sobre ICMP / DNS
S_1	Função de VPN sobre ICMP / DNS
S_2	You can establish a VPN only with ICMP or DNS packets even if there is a firewall or routers which blocks TCP/IP communications. You need to enable the following functions beforehand.
R_OVER_ICMP	Enable VPN over &ICMP Server Function
R_OVER_DNS	Enable VPN over &DNS Server Function (Uses UDP Port 53)
IDOK	&OK
IDCANCEL	Cancelar
S_3	Requires VPN Client / VPN Bridge internal version 4.0 or greater.
S_4	Warning: Use this function for emergency only. It is helpful when a firewall or router is misconfigured to blocks TCP/IP, but either ICMP or DNS is not blocked. It is not for long-term stable using.
PREFIX	D_SM_REDIRECT
CAPTION	HTTP URL Redirection Settings
S_1	The specified URL below will be mandatory replied to the client as a response for TCP connecting request packets which matches the conditions of this access list entry via this Virtual Hub.\r\n\r\nTo use this setting, you can enforce the web browser of the VPN Client computer to show the specified web site when that web browser tries to access the specific IP address.
S_2	Specify a URL which redirects to.
S_BOLD2	The &URL Redirect To:
S_3	Exemplo:
S_4	Simple URL Redirection:
S_5	Advanced URL Redirection:
B_HINT	&Usage of Advanced URL Redirection Function...
S_6	Legenda
S_BOLD	This function is for TCP/IP expert administrator. Read the following instructions and be careful to set up.
S_7	This redirection rule is not effective in the case that the destination session of a packet matches the destination username or groupname of an access list entries.
S_8	This redirection rule is ignored for non-TCP packets if it matches the condition.
S_9	This redirection rule always replies HTTP redirect messages. (Not limited for port 80.) If you want to apply to only port 80, set the destination port to 80 on the condition of the access list entry.
S_10	If as the result of redirection by this rule the client attempts to access the redirected URL and such a new request matches this rule again, the redirection results will be replied for such new requests. It will cause an infinite redirection loop.
IDOK	&OK
IDCANCEL	Cancelar
S_11	The advanced redirection function can provide the VPN Session information to the CGI which is redirected to.
PREFIX	D_SW_WELCOME
CAPTION	D_SW_WELCOME
S_WELCOME	O SoftEther VPN é um freeware desenvolvido na Universidade de Tsukuba, no Japão. Software VPN de alto desempenho com as últimas compatibilidade para muitos dispositivos. Windows, Mac, smartphones, tablets (iPhone, iPad, Android, Windows RT), Cisco e outros roteadores VPN são suportados. O SoftEther VPN também aceita clientes VPN OpenVPN e MS-SSTP.
S_TITLE	Software VPN de código aberto extremamente poderoso.
PREFIX	D_SW_MODE
CAPTION	D_SW_MODE
R_SYSTEM	&System Mode (Recommended)
R_USER	&Modo de usuário
S_1	Install the VPN software to this computer normally. The administrator privilege is required.
S_USER	Install the VPN software with the normal user privilege. No administrator privilege is required. Some functions such as Local Bridge will be disabled. Runs only the user "%s" is logged on Windows.
S_2	SoftEther VPN can be installed by one of two methods.\r\n\r\nPlease select the System Mode normally.\r\n\r\nIf you cannot use the administrator privilege for some reasons, you can select the User Mode to continue the installation.
PREFIX	D_SW_NOT_ADMIN
CAPTION	D_SW_NOT_ADMIN
S_INFO	The user "%s" which is logged on Windows does not have the administrator privilege.\r\n\r\nLog off Windows, log on by the user who has the administrator privilege and restart the Setup Wizard if you want to continue the setup.
S_INFO6	Click Finish to exit the Setup Wizard.
S_INFO2	If you cannot use the administrator privilege, you can choose the User Mode installation.\r\nTo install the software in the User Mode, click Back.
PREFIX	D_SW_COMPONENTS
CAPTION	D_SW_COMPONENTS
PREFIX	D_SW_EULA
CAPTION	D_SW_EULA
S_1	Por favor, leia atentamente o contrato de licença do usuário final.
B_AGREE	Eu concordo com o contrato de licença do usuário final.
PREFIX	D_SW_WARNING
CAPTION	D_SW_WARNING
S_1	O software SoftEther VPN possui habilidades de comunicação extremamente poderosas. Antes de usar, leia atentamente os avisos importantes.
PREFIX	D_SW_DIR
CAPTION	D_SW_DIR
S_INFO	Por favor, especifique o diretório para instalar o %s.
R_CUSTOM	&Especifique o diretório
S_DEST	&Diretório:
B_BROWSE	&Pesquisar...
R_SHOWCUSTOM	Opções avançadas de instalação para especialistas
R_FOR_SYSTEM	Instalar para &qualquer usuário
R_FOR_USER	Instalar apenas no ambiente do usuário "%s"
S_WARNING	Caution: Not recommended. After the user "%s" logs off Windows, %s will stop. Local Bridge function and L2TP/IPsec Function (supports for Mac and Smartphones) will be unavailabe.
PREFIX	D_SW_READY
CAPTION	D_SW_READY
S_INFO	Instalação do %s esta pronta.
S_INFO7	Clique em Avançar para instalar.
PREFIX	D_SW_PERFORM
CAPTION	D_SW_PERFORM
S_INFO	A instalação do %s está em andamento.\r\nPor favor, aguarde...
S_INFO8	O SoftEther VPN é um trabalho do projeto de pesquisa e desenvolvimento do governo japonês, subsidiado pelo Ministério da Economia, Comércio e Indústria do Japão, administrado pela Agência de Promoção da Informação.
PREFIX	D_SW_ERROR
CAPTION	D_SW_ERROR
S_INFO	An error occurred and the setup of %s is aborted.\r\n\r\nRestart the Setup Wizard if you want to retry.
PREFIX	D_SW_FINISH
CAPTION	D_SW_FINISH
S_INFO	O processo de instalação do %s foi concluído com êxito.
S_INFO8	O SoftEther VPN é um trabalho do projeto de pesquisa e desenvolvimento do governo japonês, subsidiado pelo Ministério da Economia, Comércio e Indústria do Japão, administrado pela Agência de Promoção da Informação.
PREFIX	D_SW_UNINST1
CAPTION	D_SW_UNINST1
S_WELCOME	O assistente de instalação pode desinstalar o %s do computador.\r\n\r\nClique em Próximo se desejar iniciar a desinstalação.
S_TITLE	%s Uninstall Wizard
PREFIX	D_SW_EASY1
CAPTION	D_SW_EASY1
S_WELCOME	Installing and setting up the VPN Clients to a lot of computers in the enterprise is a hard work.
S_TITLE	What is SoftEther VPN Client Easy Installer?
S_WELCOME2	Easy Installer Creator is a tool for enterprise administrators. You can create a VPN Client installer with embedding a specific VPN connection setting by using Easy Installer Creator. Personal users can also exploit this tool.
S_WELCOME3	A created Easy Installer can be distributed to employees in the enterprise by using file servers or e-mails. If a user runs the Easy Installer, VPN Client will be installed and the VPN connection setting will be imported, and then the VPN connection will be started automatically.
PREFIX	D_SW_EASY2
CAPTION	D_SW_EASY2
S_BOLD1	Specify a VPN connection setting file (.vpn file) to embed
S_1	Please specify a VPN connection setting file (a file which extension is .vpn) to embed on the Easy Installer. You can export a setting file by clicking Export VPN Connection Setting on the right-click menu of the target connection setting on the VPN Client Manager.
S_18	&Configuração de conexão:
B_BROWSE_SETTING	&Pesquisar...
B_DELETE_SENSITIVE	&Eliminar nome de usuário e senha do arquivo de configuração da conexão
S_BOLD2	Specify an EXE filename to be generated
S_3	This tool will output an EXE file (executable file) which implements an Easy Installer. Please specify the output filename to be generated.
S_19	Salvar &como:
B_BROWSE_OUT	P&esquisar...
B_EASYMODE	Set the VPN Client Manager to &Easy Mode when Installation
PREFIX	D_SW_WEB1
CAPTION	D_SW_WEB1
S_WELCOME	You can create a SoftEther VPN Client Web Installer and upload it on the Web server in the enterprise. A user opens that web page and can install the SoftEther VPN Client automatically. You can also setup the automatic import and kick-start of a built-in VPN connection setting.
S_TITLE	What is SoftEther VPN Web Installer?
S_WELCOME2	The generated Web Installer can be placed as HTML files on the intranet Web server. If an employee accesses to the URL of that HTML files, the SoftEther VPN Client Installer will be executed.
S_WELCOME3	Using ActiveX Control. Internet Explorer 5.0, greater on Windows 2000 or greater are supported. Other web browsers or older operating systems (for example Windows 98) are not supported.
PREFIX	D_SW_WEB2
CAPTION	D_SW_WEB2
S_BOLD1	Specify a VPN connection setting file (.vpn file) to embed
S_1	Please specify a VPN connection setting file (a file which extension is .vpn) to embed on the Web Installer. You can export a setting file by clicking Export VPN Connection Setting on the right-click menu of the target connection setting on the VPN Client Manager.
S_18	&Configuração de conexão:
B_BROWSE_SETTING	&Pesquisar...
B_DELETE_SENSITIVE	&Eliminar nome de usuário e senha do arquivo de configuração da conexão
S_BOLD2	Specify the output filename to be generated
S_3	This tool will output a ZIP file (archive file) which contains HTML files and CAB files that should be placed on the Web server. Please specify the output filename to be generated.
S_19	Salvar &como:
B_BROWSE_OUT	P&esquisar...
B_EASYMODE	Set the VPN Client Manager to &Easy Mode when Installation
PREFIX	D_UPDATE_NOTICE
CAPTION	Atualizações de %s
IDOK	&Show the Update Information...
B_CONFIG	&Configurar atualizações...
IDCANCEL	&Do Not Show this Message Again
S_INFO	The latest version of %s is released. You can download it and update now.
S_PRODUCT	Software:
S_CURRENT	Current Version:
S_CURRENT_STR	Ver %u.%02u.%04u%s
S_LATEST	Latest Version:
S_LATEST_STR	Ver %S%s
PREFIX	D_UPDATE_CONFIG
CAPTION	Configuration of Update Notification
S_INFO	Checks the new versions of %s periodically and popup a notification when a new version will be released.\r\n\r\nHTTPS packets will be used between this computer and the SoftEther Update server located in Tsukuba-city, Ibaraki-prefecture, Japan in order to check updates. No personal information will be sent.
S_TITLE	%s Update and Notify Settings
S_ENABLE	&Ativar virificação de atualizações
S_DISABLE	&Desativar virificação de atualizações
IDCANCEL	&Fechar
PREFIX	D_SM_VMBRIDGE
CAPTION	Instructions for Local Bridge on VM
S_TITLE	Using Local Bridge Function on VM
S_1	It has been detected that the VPN Server might be running on a VM (Virtual Machine) suchlike VMware or Hyper-V. Read the following instructions carefully. If you are not using a VM, please ignore this message.
S_2	Some VMs prohibit the "Promiscuous Mode" (MAC Address Spoofing) on the network adapters by default.\r\n\r\nIf the Promiscuous Mode (MAC Address Spoofing) is administratively disabled, the Local Bridge function between a Virtual Hub on the VPN Server and a physical network adapter on the physical computer does not work well. You should allow the Promiscuous Mode (MAC Address Spoofing) by using the configuration tool of the VM.\r\n\r\nFor details please refer the documents of your VM. If it is a shared-VM and administrated by other person, please request the administrator to permit the use of the Promiscuous (MAC Address Spoofing) Mode to your VM.
S_BOLD	Instruções
IDCANCEL	&OK
PREFIX	D_SM_AZURE
CAPTION	VPN Azure Service Settings
S_TITLE	Serviço de VPN Azure Cloud VPN (gratuito)
S_1	O VPN Azure facilita o estabelecimento de uma sessão VPN do seu PC doméstico para o PC do escritório. Enquanto uma conexão VPN é estabelecida, você pode acessar outros servidores na rede privada da sua empresa.
S_2	Você não precisa de um endereço IP global no PC do escritório (servidor VPN). Pode funcionar atrás de firewalls ou NATs. Nenhuma configuração de administrador de rede é necessária. Você pode usar o cliente SSTP-VPN interno do Windows em seu PC doméstico.
S_3	O VPN Azure é um serviço de VPN em nuvem operado pelo SoftEther VPN Project. O VPN Azure é gratuito e disponível para qualquer pessoa. Pressione o botão ao lado para ver detalhes e instruções de uso.
B_BOLD	Configuração VPN Azure
R_ENABLE	&Ativar VPN Azure
R_DISABLE	&Desativar VPN Azure
S_HOSTNAME_BORDER	Nome do host atual da VPN Azure
S_HOSTNAME_INFO	O nome do host da VPN do Azure é igual ao nome do host do DNS dinâmico, mas alterando o sufixo do domínio para "vpnazure.net".
B_CHANGE	Mudar &Hostname
B_WEB	Como usar o VPN Azure\r\n (Visite o site)
IDCANCEL	&OK
PREFIX	D_SM_PROXY
CAPTION	Conectar via servidor proxy
STATIC9	Você pode se conectar através de um servidor proxy.
STATIC10	&Tipo de proxy:
R_DIRECT_TCP	&Conexão TCP/IP direta (sem proxy)
R_HTTPS	Conectar via servidor proxy H&TTP
R_SOCKS	Conectar via servidor proxy S&OCKS4
R_SOCKS5	Conectar via servidor proxy S&OCKS5
B_PROXY_CONFIG	Configuração do servidor &proxy
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_VGC_LIST
CAPTION	VPN Gate Academic Experimental Project Plugin for SoftEther VPN Client
S_TITLE	VPN Gate Public VPN Relay Servers
S_INFO1	Gain freedom access to Internet by using VPN connection via Public VPN Servers provided by volunteers abound the world. Bypass your local malfunctioning firewall's packet blocking, and hide your IP address safely.
IDOK	&Connect to the VPN Server
B_PROXY	&Configurações de proxy:
S_VLAN	Adaptador de rede virtual:
B_WEB	VPN Gate Academic\r\nWeb Site
B_REFRESH	&Atualizar lista
S_REFRESH	Atualizando a lista...
S_RESEARCH	Academic project at University of Tsukuba, Japan.
S_INFO9	A VPN Server with higher Line Speed (measured by Mbps) and smaller Ping result are usually more comfortable to use. You might be able to browse websites which are normally unreachable from your area if you use VPN servers that are not in your area.
PREFIX	D_VGC_PROTOCOL
CAPTION	Select VPN Protocol to Connect
S_TITLE	The Public VPN Relay Server "%S" (%S) supports both TCP and UDP as VPN protocol.
S_INFO	Select preferred VPN Protocol to use in order to connect the VPN Server "%S" (%S). In general, the TCP protocol is easy to pass through the firewall. Try the UDP protocol only if the TCP has been failed.
R_TCP	Use &TCP Protocol (Ethernet over HTTPS VPN) (Recommended)
R_UDP	Use &UDP Protocol (Ethernet over UDP VPN)
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_VGS_CONFIG
CAPTION	VPN Gate Service Control Panel
R_ENABLE	&Enable the VPN Gate Relay Service and Join the VPN Gate Research as a Volunteer.
S_TITLE	Join the VPN Gate Academic Research Project?
S_INFO1	VPN Gate is an academic experiment for the research on the 'Distributed Public VPN Relay Server' technology, operated at the Graduate School on University of Tsukuba, Japan. VPN Gate Client users can connect to VPN Gate Services running on Public VPN Relay Servers, and enjoy unrestricted Internet access via the VPN Relay Server.
S_INFO9	When a VPN Gate Client user accesses to a server on Internet, the source IP address will be replaced to the IP address of the relaying Public VPN Server. Consequently, the VPN Gate Client user will be able to browse overseas web sites smoothly even if the user's local firewall is out of order by an unknown reason and unable to pass such an access.
S_WARNING	If you check the above checkbox and press OK, the VPN Gate Relay Service will be activated on this computer. As the result, any VPN Gate Client will be able to communicate towards the Internet via the VPN Gate Relay Service. It is secure even if your computer is on the private network (e.g. corporate network) because any accesses to private IP addresses will not be permitted to pass via the VPN Gate Relay Service.
B_OPTION	VPN Gate Service &Option Settings...
IDOK	&OK
IDCANCEL	Cancelar
B_WEB	&Browse http://www.vpngate.net/ ...
PREFIX	D_VGS_OPTION
CAPTION	Opções de serviço de porta VPN
S_TITLE	Opções de serviço de porta VPN
S_1	This computer will be a Public VPN Server. Please fill the operator's information of the server. The information will be published on the list at www.vpngate.net and other related services. The contact address will be also used to contact from VPN Gate Academic Project operators.
S_2	Operador:
S_3	&Operador do servidor:
S_19	(Até 64 letras)
S_20	&Abuse Report Address\r\n(e-mail addresses etc.):
S_21	(Até 64 letras)
S_22	The &Message to Users:\r\n(Up to 128 letters)
S_23	The message will be shown on the list of VPN Gate Servers. Enter an enjoyable message to let users feel pleasure.
S_24	Configurações VPN:
R_LOG	&Save VPN Packet Logs (Recommended)
R_2WEEKS	Auto Delete or Archive with Encoding for Packet Logs After &Two Weeks (Recommended)
R_PERMANENT	Make Packet Logs Occupy Free Disk Space &Permanently
R_L2TP	Enable &L2TP/IPsec VPN Server Function (Recommended)
S_25	Allows Mac OS X, iPhone, iPad and Android clients to make a VPN connection.
B_MESSAGE	Pop-up Your Advertisement Message on the VPN Client &Screen ...
IDOK	&OK
IDCANCEL	Cancelar
PREFIX	D_VGS_WARNING
CAPTION	Caution before Joining VPN Gate Academic Experiment
S1	The VPN Gate Academic Experiment Service is operated as a research project at the graduate school on University of Tsukuba, Japan. The service is governed under the Japanese laws. Other countries' laws are none of our concerns nor responsibilities.
S2	By nature, there are almost 200 countries in the World, with different laws. It is impossible to verify every countries' laws and regulations and make the software comply with all countries' laws in advance to release the software. If a user uses VPN Gate service in a specific country, and damaged by public servants of the authority, the developer of either the service or software will never be liable to recover or compensate such damages or criminal responsibilities.
S3	By using this software and service, the user must observe all concerned laws and rules with user's own responsibility. The user will be completely liable to any damages and responsibilities which are results of using this software and service, regardless of either inside or outside of Japan's territory.
S4	If you don't agree nor understand the above warnings, do not use any of VPN Gate Academic Experiment Service functions.
S5	Note: VPN Gate is a research project for just academic purpose only. VPN Gate was developed as a plug-in for SoftEther VPN and UT-VPN. However, all parts of VPN Gate were developed on this research project at University of Tsukuba. Any parts of VPN Gate are not developed by SoftEther VPN Project. The VPN Gate Research Project is not a subject to be led, operated, promoted nor guaranteed by SoftEther VPN Project.
R_NEVER	Do Not &Show This Message Again
B_WEB	Visite o &site do VPN Gate...
IDOK	&Concordar
IDCANCEL	&Discordo
S_BOLD	Caution! Do Not Use the VPN Gate Services in Countries where VPN Communications are Prohibited.
PREFIX	D_NM_PUSH
CAPTION	Edit the static routing table to push
S1	This Virtual DHCP Server can push the classless static routes (RFC 3442) with DHCP reply messages to VPN clients.
S2	Whether or not a VPN client can recognize the classless static routes (RFC 3442) depends on the target VPN client software. SoftEther VPN Client and OpenVPN Client are supporting the classless static routes. On L2TP/IPsec and MS-SSTP protocols, the compatibility depends on the implementation of the client software.
S3	You can realize the split tunneling if you clear the default gateway field on the Virtual DHCP Server options. On the client side, L2TP/IPsec and MS-SSTP clients need to be configured not to set up the default gateway for the split tunneling usage.
S4	You can also push the classless static routes (RFC 3442) by your existing external DHCP server. In that case, disable the Virtual DHCP Server function on SecureNAT, and you need not to set up the classless routes on this screen.
S5	Edit the static routing table to push
S6	Example: 192.168.5.0/255.255.255.0/192.168.4.254, 10.0.0.0/255.0.0.0/192.168.4.253\r\n\r\nSplit multiple entries (maximum: 64 entries) by comma or space characters.\r\nEach entry must be specified in the "IP network address/subnet mask/gateway IP address" format.
S7	See the RFC 3442 to understand the classless routes.
IDOK	&OK
IDCANCEL	Cancelar


###########################################################################
#                                                                         #
#String data of menus in software                                         #
#                                                                         #
###########################################################################


# Connection Manager menu
PREFIX	CM_MENU


# [Connect] menu
CMD_TOP_CONNECT	&Conectar
CMD_CONNECT	C&onectar\tEnter
CMD_STATUS	Ver &status...\tCtrl+S
CMD_DISCONNECT	D&esconectar\tCtrl+D
CMD_DISCONNECT_ALL	Desconectar &todos\tCtrl+I
CMD_NEW	&Nova configuração de conexão VPN...\tCtrl+N
CMD_CLONE	&Copiar\tCtrl+C
CMD_SHORTCUT	Criar atalho de conexão VPN...
CMD_EXPORT_ACCOUNT	E&xportar configuração de conexão VPN...
CMD_IMPORT_ACCOUNT	Im&portar configuração de conexão VPN...
CMD_STARTUP	Conec&tar na inicialização\tCtrl+T
CMD_NOSTARTUP	Não conectar na inicialização
CMD_RECENT	Servidores &VPN recentes
CMD_RENAME	Reno&mear\tF2
CMD_DELETE	&Excluir\tDel
CMD_PROPERTY	P&ropriedades...\tAlt+Enter
CMD_EXIT	&Fechar o gerenciador de conexões\tAlt+F4
CMD_QUIT	Sair do programa gerenciador de conexões\tAlt+Q


# [Edit] menu
CMD_TOP_EDIT	&Editar
CMD_SELECT_ALL	Selecionar &tudo\tCtrl+A
CMD_SWITCH_SELECT	Al&terar seleção


# [View] menu
CMD_TOP_VIEW	&Ver
CMD_STATUSBAR	&Mostrar barra de status
CMD_VISTASTYLE	Estilo do Windows Vista/7/8/10
CMD_SHOWPORT	Mostrar &portas na lista de conexões
CMD_TRAYICON	Mostrar ícones na &barra de tarefas
CMD_ICON	&Ícone
CMD_DETAIL	&Detalhes
CMD_GRID	Mostrar &grade
CMD_REFRESH	&Atualizar\tF5


# [VLAN] menu
CMD_TOP_VLAN	Adaptador &virtual
CMD_NEW_VLAN	&Novo adaptador de rede virtual...\tCtrl+L
CMD_ENABLE_VLAN	&Ativar adaptador de rede virtual\tCtrl+E
CMD_DISABLE_VLAN	&Desativar adaptador de rede virtual\tCtrl+B
CMD_DELETE_VLAN	&Excluir Adaptador de rede virtual\tDel
CMD_REINSTALL	&Reinstall Driver...\tCtrl+U
CMD_WINNET	Abrir conexões de rede do Windows...\tCtrl+W


# [Connect] menu
CMD_TOP_SECURE	&Smart Card
CMD_SECURE_MANAGER	&Gerenciador de Smart Card...\tCtrl+G
CMD_SECURE_SELECT	&Selecionar um Smart Card para usar...


# [Tools] menu
CMD_TOP_TOOL	&Ferramentas
CMD_PASSWORD	Definir &senha...\tCtrl+P
CMD_TRUST	&Gerenciar lista de certificados CA confiáveis\tCtrl+R
CMD_NETIF	&Status do dispositivo de rede...
CMD_TCPIP	&Utilitário de otimização de TCP...
CMD_MMCSS	Otimização para Windows e Vista/7/8/10...
CMD_TRAFFIC	Ferramenta de &teste de velocidade do tráfego de rede...\tCtrl+Q 
CMD_CM_SETTING	Alterar &modo de operação...
CMD_LANGUAGE	&Configurações de idioma...
CMD_OPTION	&Opções...\tCtrl+O


# [Voice] menu
CMD_TOP_VOICE	V&oz
CMD_VOIDE_NONE	Voice Gui&de Off 
CMD_VOICE_NORMAL	&Normal Voice Guide
CMD_VOICE_ODD	Extended V&oice Guide


# [Help] menu
CMD_TOP_HELP	&Ajuda
CMD_ABOUT	&Sobre...


###########################################################################
#                                                                         #
# Command prompt string data                                              #
#                                                                         #
###########################################################################
PREFIX	NULL


# Console system general 
CON_INFILE_ERROR	Error: Unable to open the specified input file "%s".
CON_OUTFILE_ERROR	Error: Unable to create the specified output file "%s".
CON_INFILE_START	The commands written in the file "%s" will be used instead of input from keyboard.
CON_OUTFILE_START	The message output to the console will be saved in the file "%s".
CON_USER_CANCEL	[EOF]
CON_UNKNOWN_CMD	"%S": Command not found. \nYou can use the HELP command to view a list of the available commands.
CON_AMBIGUOUS_CMD	"%S": The command-name is ambiguous.
CON_AMBIGUOUS_CMD_1	The specified command name matches the following multiple commands.
CON_AMBIGUOUS_CMD_2	Please re-specify the command name more strictly.
CON_INVALID_PARAM	The parameter "/%S" has been specified. It is not possible to specify this parameter when using the command "%S". Input "%S /HELP" to see the list of what parameters can be used. 
CON_AMBIGUOUS_PARAM	"%S": The parameter name is ambiguous.
CON_AMBIGUOUS_PARAM_1	The specified parameter name matches with the following parameters that can be specified as a parameter of command "%S".
CON_AMBIGUOUS_PARAM_2	Please re-specify the parameter name more strictly.


# Unknown command
CMD_UNKNOWM	There is no description for this command.
CMD_UNKNOWN_HELP	There is no detailed description for this command. If you would like to know more detail about this command, please refer to the manual or online documentation.
CMD_UNKNOWN_ARGS	There is no command execution example.
CMD_UNKNOWN_PARAM	There is no description for this parameter.


# Strings being used within console system
CMD_HELP_1	You can use the following %u commands: 
CMD_HELP_2	To reference the usage for each command, input "command name ?" to view a help.
CMD_EVAL_MIN_MAX	You must specify an integer in the range from %u to %u for the value. 
CMD_PROMPT	Entre um valor: 
CMD_EVAL_NOT_EMPTY	You cannot make a blank specification.
CMD_EVAL_SAFE	The string contains unusable characters.
CMD_EVAL_INT	You must specify an integer that is not less than 1.
CMD_HELP_TITLE	Help for command "%S"
CMD_HELP_DESCRIPTION	Objetivo:
CMD_HELP_USAGE	Uso:
CMD_HELP_HELP	Descrição:
CMD_HELP_ARGS	Parâmetros
CMD_PROMPT_PORT	Input the port number: 
CMD_EVAL_PORT	Port number is invalid. Specify a port number that is within the range of 1 to 65535.
CMD_CT_STD_COLUMN_1	Item
CMD_CT_STD_COLUMN_2	Valor
CMD_CT_STD_COLUMN_3	Descrição
CMD_PARSE_IP_SUBNET_ERROR_1_6	Specify in the format of "IPv6 address/subnet mask". \nSpecify the IPv6 address by separating the hexadecimal values using colons such as "2001:200:0:1::". For the subnet mask, either specify hexadecimal values separated by colons such as "ffff:ffff:ffff:ffff::", or you can specify the bit length of subnet mask using a decimal value such as 64. \nTo specify a standalone host, specify the subnet mask as either "ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff" or "128". \n(Example)\n2001:200:0:1::/64\n2001:200:0:1::/ffff:ffff:ffff:ffff::\n2001:200:0:1::5/12\n\n
CMD_PARSE_IP_SUBNET_ERROR_1	Specify in the format of "IPv4 address/subnet mask". \nSpecify the IPv4 address by separating the decimal values using dots such as "192.168.0.1". For the subnet mask, either specify decimal values separated by dots such as "255.255.255.0", or you can specify the bit length of subnet mask using a decimal value such as 24. \nTo specify a standalone host, specify the subnet mask as either "255.255.255.255" or "32". \n(Example)\n 192.168.0.1/24\n 192.168.0.1/255.255.255.0\n192.168.0.5/255.255.255.255\n\n
CMD_PARSE_IP_SUBNET_ERROR_2	The specified IP address is not a network address.
CMD_PARSE_IP_SUBNET_ERROR_3	The specified IP address is not a network prefix address.
CMD_EVAL_DATE_TIME_FAILED	The date and time specification is invalid. \nThe date and time must be in the same format as "2005/10/08 19:30:00" where 6 integers are specified, representing year/month/day hour:minute:second separated by forward slashes, a space and then colons. Specify 4 digits for the year.
CMD_PARSE_IP_MASK_ERROR_1_6	Specify in the format of "IPv6 address/mask". \nSpecify the IPv6 address by separating the hexadecimal values using colons such as "2001:200:0:1::". For the mask, either specify hexadecimal values separated by colons such as "ffff:ffff:ffff:ffff::", or you can specify the bit length of mask using a decimal value such as 64. \nTo specify a standalone host, specify the mask as either "ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff" or "128". \n(Example)\n2001:200:0:1::/64\n2001:200:0:1::/ffff:ffff:ffff:ffff::\n2001:200:0:1::5/12\n\n
CMD_PARSE_IP_MASK_ERROR_1	Specify in the format of "IPv4 address/mask". \nSpecify the IPv4 address by separating the decimal values using dots such as "192.168.0.1". For the mask, either specify decimal values separated by dots such as "255.255.255.0", or you can specify the bit length of mask using a decimal value such as 24. \nTo specify a standalone host, specify the mask as either "255.255.255.255" or "32". \n(Example)\n 192.168.0.1/24\n 192.168.0.1/255.255.255.0\n192.168.0.5/255.255.255.255\n\n


# Common messages
CMD_MSG_INVALID_HOSTNAME	Specified host name is invalid.
CMD_MSG_OK	The command completed successfully.
CMD_MSG_ALLOW	Permitir
CMD_MSG_DENY	Negar
CMD_MSG_INFINITE	Infinito
CMD_MSG_ENABLE	Ativar
CMD_MSG_DISABLE	Desativar
CMD_MSG_LOAD_CERT_FAILED	Unable to read the specified X.509 certificate file.
CMD_MSG_SAVE_CERT_FAILED	Failed to write the X.509 certificate file.
CMD_ACCOUNT_COLUMN_NAME	Nome da configuração da conexão VPN
CMD_ACCOUNT_COLUMN_HOSTNAME	Destination VPN Server Host Name
CMD_ACCOUNT_COLUMN_PORT	Destination VPN Server Port Number
CMD_ACCOUNT_COLUMN_HUBNAME	Destination VPN Server Virtual Hub Name
CMD_ACCOUNT_COLUMN_PROXY_TYPE	Proxy Server Type
CMD_ACCOUNT_COLUMN_PROXY_HOSTNAME	Proxy Server Host Name
CMD_ACCOUNT_COLUMN_PROXY_PORT	Proxy Server Port Number
CMD_ACCOUNT_COLUMN_PROXY_USERNAME	Proxy Server User Name
CMD_ACCOUNT_COLUMN_SERVER_CERT_USE	Verify Server Certificate
CMD_ACCOUNT_COLUMN_SERVER_CERT_NAME	Registered Server Individual Certificate
CMD_ACCOUNT_COLUMN_RETRY_ON_SERVER_CERT	Retry on Untrusted Server Certificate
CMD_ACCOUNT_COLUMN_ADD_DEFAULT_CA   Trust System Certificate Store
CMD_ACCOUNT_COLUMN_DEVICE_NAME	Device Name Used for Connection
CMD_ACCOUNT_COLUMN_AUTH_TYPE	Authentication Type
CMD_ACCOUNT_COLUMN_AUTH_USERNAME	Nome de usuário
CMD_ACCOUNT_COLUMN_AUTH_CERT_NAME	Client Certificate for Authentication Use
CMD_ACCOUNT_COLUMN_NUMTCP	Número de conexões TCP a serem usadas na comunicação VPN
CMD_ACCOUNT_COLUMN_TCP_INTERVAL	Interval between Establishing Each TCP Connection
CMD_ACCOUNT_COLUMN_TCP_TTL	Connection Life of Each TCP Connection
CMD_ACCOUNT_COLUMN_TCP_HALF	Use Half Duplex Mode
CMD_ACCOUNT_COLUMN_ENCRYPT	Encryption by SSL
CMD_ACCOUNT_COLUMN_COMPRESS	Data Compression
CMD_ACCOUNT_COLUMN_BRIDGE_ROUTER	Connect by Bridge / Router Mode
CMD_ACCOUNT_COLUMN_MONITOR	Connect by Monitoring Mode
CMD_ACCOUNT_COLUMN_NO_TRACKING	No Adjustment for Routing Table
CMD_ACCOUNT_COLUMN_QOS_DISABLE	Do not Use QoS Control Function
CMD_ACCOUNT_COLUMN_DISABLEUDP	Desativar aceleração UDP


# Debugging Information Collecting Tool
CMD_DEBUG_SOFTNAME	Debugging Information Collecting Tool
CMD_DEBUG_PRINT	Debugging Information Collecting Tool\r\n\r\n
CMD_DEBUG_NOT_2000	Windows 2000 or later is required.
CMD_DEBUG_NOT_ADMIN	You must login as Administrators on Windows to execute this command.
CMD_DEBUG_UAC_FAILED	Failed to obtain the Administrators privilege.
CMD_DEBUG_SAVE_TITLE	Specify Destination Path to Save File
CMD_DEBUG_OK	A debugging information file was saved as "%s".\r\n\r\nSend this file to your support staff.\r\nYou must verify the contents of this file before sending it to the support staff.\r\nRemove confidential information on this file with your responsibility and by yourself if there are some confidential information which you don't want to disclose it to the staff.\r\n\r\nIf you ignore the confidential information contained on the file, and you agree to send the entire file to the support staff, it means that you have agreed to disclose the entire contents of the file to the support staff.
CMD_DEBUG_NG	Failed to save the debugging information as "%s".


# TEST command
CMD_TEST	Executing test operation.
CMD_TEST_HELP	This is a test command. Executing test operation. With the test command, you can specify a number of arguments. You can omit the number of arguments.
CMD_TEST_ARGS	Test [/A1:a_str] [/A2:b_str] [/A3:int_value]
CMD_TEST_A1	Specifies parameter A1. This can be omitted.
CMD_TEST_A2	Specifies parameter A2. If this is omitted, a prompt will be displayed to input parameter A2 when the command is executed. You cannot make a blank specification.
CMD_TEST_A3	Specify a numeric value. You must specify an integer that is within the range of 1 to 100. Specifying an integer outside that range will cause an error message to be displayed.
CMD_TEST_EVAL_A2	You cannot make a blank specification for parameter A2.
CMD_IP_EVAL_FAILED	The IP address is incorrectly specified.
CMD_HOSTPORT_EVAL_FAILED	The host name and port number specification is invalid. \nPlease specify using the format of host name:port number, or IP address:port number.
CMD_PORTLIST_EVAL_FAILED	The port number list specification is invalid. \nThe list must have at least one port number set, and it is also possible to set multiple port numbers. When specifying multiple port numbers, separate them using a comma such as "443,992,8888".
CMD_PROTOCOL_EVAL_FAILED	The protocol is incorrectly specified. Specify either ip, tcp, udp, icmpv4, icmpv6 or a protocol number (0 to 255) for the protocol.
CMD_PORT_RANGE_EVAL_FAILED	The port number or the port number range was incorrectly specified. If specifying only one port number, an integer must be used to specify that port number. If specifying multiple ports, specify the beginning port number and the end port number joined together by a hyphen like "80-443".
CMD_TCP_CONNECTION_STATE_EVAL_FAILED	The TCP connection state specification is invalid. Specify either "Established" or "Unestablished" and specify TCP when selecting protocol.
CMD_MAC_ADDRESS_AND_MASK_EVAL_FAILED	The MAC address and mask specification is invalid. Use hexadecimal number with the separators, "-" or ":", and without the separators. An example is "00-AC-84-EA-33-BC/FF-FF-FF-FF-FF-FF".
CMD_EXEC_MSG_NAME	%S comando - %s
CMD_ID	ID
CMD_FILE_NOT_FOUND	Cannot find specified file "%s".
CMD_FILE_NAME_EMPTY	The file name is not specified.
CMD_SAVECERTPATH	Save X.509 certificate to file name: 
CMD_SAVECERT_FAILED	Failed to save the certificate file.
CMD_SAVEKEYPATH	Save private key to file name: 
CMD_SAVEKEY_FAILED	Failed to save the private key file.
CMD_SAVEFILE_FAILED	Failed to save the file.
CMD_LOADFILE_FAILED	Failed to open the file.
CMD_LOADCERTPATH	Read X.509 certificate from file name: 
CMD_LOADCERT_FAILED	Failed to read certificate file.
CMD_LOADKEYPATH	Read private key from file name: 
CMD_LOADKEY_FAILED	Failed to read private key file.
CMD_LOADKEY_ENCRYPTED_1	The specified private key file is protected by a passphrase.
CMD_LOADKEY_ENCRYPTED_2	Please enter the passphrase: 
CMD_LOADKEY_ENCRYPTED_3	The passphrase is incorrect.
CMD_KEYPAIR_FAILED	The X.509 certificate and private key combination has been incorrectly specified. \r\nA certificate and a private key that corresponds to that certificate is required.
CMD_CERT_NOT_EXISTS	The certificate is not registered.
CMD_NO_SETTINGS	-
CMD_DISCONNECTED_MSG	\n--- Error ---\n\nThe communication session with the host you were managing has been disconnected. From now on, if you run any commands an error will occur. \n\nTo reconnect to the host you were managing, first leave the prompt by inputting "EXIT" and then reconnect. \n\n


# VPNCMD ã‚³ãƒžãƒ³ãƒ‰
CMD_VPNCMD	SoftEther VPN Command Line Management Utility Developer Edition
CMD_VPNCMD_HELP	The 'vpncmd' program is a utility that allows you to manage SoftEther VPN software by using command lines. By using vpncmd, you can connect to a VPN Client, a VPN Server or VPN Bridge that is running on a local or remote computer and manage these services. Moreover, by using VPN Tools mode, you can call the Network Traffic Speed Test Tool and the certificate creation function. These can be used even when not connected to the VPN Server or VPN Client. \nWhen using vpncmd, if the file name is specified by using the /IN and /OUT parameter, the command can be executed in a batch according to a file in which the executable commands are enumerated and the execution results can be written to a file. Normally a command prompt will appear after vpncmd is launched but when an input file is specified by the /IN parameter, the program will automatically terminate after the execution of all lines in the input file is complete. Also, when a command to execute is specified by the /CMD parameter, the program will automatically terminate after the execution of that command is complete. You cannot specify the /IN parameter and the /CMD parameter at the same time. The termination code of the vpncmd program will be the error code of the last executed command (0 in the case of successful execution). \nUnder a Windows environment, when vpncmd is launched once or more by a user with administrator privileges, it is possible to simply input 'vpncmd' to a Windows command prompt or [Run...] window to launch vpncmd. To achieve the same result under a UNIX system, you can manually set, as appropriate, the PATH environment variable.
CMD_VPNCMD_ARGS	vpncmd [host:port] [/CLIENT|/SERVER|/TOOLS] [/HUB:hub] [/ADMINHUB:adminhub] [/PASSWORD:password] [/IN:infile] [/OUT:outfile] [/CMD commands...]
CMD_VPNCMD_[host:port]	By specifying parameters in the format "host name:port number", a connection will automatically be made to that host. If this is not specified, a prompt will appear to input the connection destination. When connecting to a VPN Client, you cannot specify a port number.
CMD_VPNCMD_CLIENT	This will connect to VPN Client to do management. You cannot specify it together with /SERVER.
CMD_VPNCMD_SERVER	This will connect to VPN Server or VPN Bridge to do management. You cannot specify it together with /CLIENT.
CMD_VPNCMD_TOOLS	This will enables use of VPN Tools commands. VPN Tools include the simple certificate creation tool (MakeCert command) and the Network Traffic Speed Test Tool (SpeedTest command).
CMD_VPNCMD_HUB	When connecting to the VPN Server by "Virtual Hub Admin Mode", this specifies the Virtual Hub name 'hub'. If you specify the host name but not the /HUB parameter, connection will be by "Server Admin Mode".
CMD_VPNCMD_ADMINHUB	This will specify the name of the Virtual Hub 'adminhub' that is automatically selected after connecting to the VPN Server. If the /HUB parameter was specified, the Virtual Hub will be selected automatically and this specification will not be necessary.
CMD_VPNCMD_PASSWORD	If the administrator password is required when connecting, specify the password 'password'. When the password is not specified, a prompt to input the password will be displayed.
CMD_VPNCMD_IN	This will specify the text file 'infile' that contains the list of commands that are automatically executed after the connection is completed. If the /IN parameter is specified, the vpncmd program will terminate automatically after the execution of all commands in the file are finished. If the file contains multiple-byte characters, the encoding must be Unicode (UTF-8). This cannot be specified together with /CMD (if /CMD is specified, /IN will be ignored).
CMD_VPNCMD_OUT	You can specify the text file 'outfile' to write all strings such as onscreen prompts, message, error and execution results. Note that if the specified file already exists, the contents of the existing file will be overwritten. Output strings will be recorded using Unicode (UTF-8) encoding.
CMD_VPNCMD_CMD	If the optional command 'commands...' is included after /CMD, that command will be executed after the connection is complete and the vpncmd program will terminate after that. This cannot be specified together with /IN (if specified together with /IN, /IN will be ignored). Specify the /CMD parameter after all other vpncmd parameters.
CMD_VPNCMD_CSV	You can specify this option to enable CSV outputs. Results of each command will be printed in the CSV format. It is useful for processing the results by other programs.
CMD_VPNCMD_CS_1	By using vpncmd program, the following can be achieved. \n\n1. Management of VPN Server or VPN Bridge \n2. Management of VPN Client\n3. Use of VPN Tools (certificate creation and Network Traffic Speed Test Tool)\n\n
CMD_VPNCMD_CS_2	Select 1, 2 or 3: 
CMD_VPNCMD_HOST_1	Specify the host name or IP address of the computer that the destination VPN Server or VPN Bridge is operating on. \nBy specifying according to the format 'host name:port number', you can also specify the port number. \n(When the port number is unspecified, 443 is used.)\nIf nothing is input and the Enter key is pressed, the connection will be made to the port number 443 of localhost (this computer).
CMD_VPNCMD_HOST_2	Specify the host name or IP address of the computer that the destination VPN Client is operating on. \nIf nothing is input and Enter is pressed, connection will be made to localhost (this computer).
CMD_VPNCMD_HOST_3	Hostname of IP Address of Destination: 
CMD_VPNCMD_HUB_1	If connecting to the server by Virtual Hub Admin Mode, please input the Virtual Hub name. \nIf connecting by server admin mode, please press Enter without inputting anything.
CMD_VPNCMD_HUB_2	Specify Virtual Hub Name: 
CMD_VPNCMD_ABOUT	SoftEther VPN Command Line Management Utility (vpncmd command)\nDeveloper Edition\n%S\n%S\nCopyright (c) all contributors on SoftEther VPN project in GitHub.\nCopyright (c) Daiyuu Nobori, SoftEther Project at University of Tsukuba, and SoftEther Corporation.\nAll rights reserved.\n
CMD_VPNCMD_PASSWORD_1	Access has been denied. Possibly the password is incorrect, or perhaps you are connecting by an incorrect admin mode. You can try inputting the password again. To cancel, press Ctrl+D.
CMD_VPNCMD_PASSWORD_2	Senha: 
CMD_VPNCMD_ERROR	Error occurred. (Error code: %u)\n%s
CMD_VPNCMD_SERVER_CONNECTED	Connection has been established with VPN Server "%S" (port %u).
CMD_VPNCMD_SERVER_CONNECTED_1	You have administrator privileges for the entire VPN Server.
CMD_VPNCMD_SERVER_CONNECTED_2	You have administrator privileges for Virtual Hub '%S' on the VPN Server.
CMD_VPNCMD_CLIENT_NO_REMODE	The destination VPN Client server does not allow administrating connections from remote computers. Launch the command line management utility or VPN Client Manager on the computer that VPN Client is running on and connect to localhost.
CMD_VPNCMD_PWPROMPT_0	Please enter the password. To cancel press the Ctrl+D key.
CMD_VPNCMD_PWPROMPT_1	Senha: 
CMD_VPNCMD_PWPROMPT_2	Confirmar saída: 
CMD_VPNCMD_PWPROMPT_3	The password and the password confirmation do not match. Please input the password and confirmation again.
CMD_VPNCMD_CLIENT_CONNECTED	Connected to VPN Client "%S".
CMD_VPNCMD_TOOLS_CONNECTED	VPN Tools has been launched. By inputting HELP, you can view a list of the commands that can be used.


#######################################################


#                                                     #


# Management commands for VPN Server are listed below #


#                                                     #


#######################################################


# About command
CMD_About	Display the version information
CMD_About_HELP	This displays the version information of this command line management utility. Included in the version information are the vpncmd version number, build number and build information.
CMD_About_ARGS	Sobre


# ServerInfoGet command
CMD_ServerInfoGet	Get server information
CMD_ServerInfoGet_Help	This allows you to obtain the server information of the currently connected VPN Server or VPN Bridge. Included in the server information are the version number, build number and build information. You can also obtain information on the current server operation mode and the information of operating system that the server is operating on.
CMD_ServerInfoGet_Args	ServerInfoGet


# ServerStatusGet command
CMD_ServerStatusGet	Get Current Server Status
CMD_ServerStatusGet_Help	This allows you to obtain in real-time the current status of the currently connected VPN Server or VPN Bridge. You can get statistical information on data communication and the number of different kinds of objects that exist on the server. You can get information on how much memory is being used on the current computer by the OS.
CMD_ServerStatusGet_Args	ServerStatusGet


# ListenerCreate command
CMD_ListenerCreate	Create New TCP Listener
CMD_ListenerCreate_Help	This allows you to create a new TCP Listener on the server. By creating the TCP Listener the server starts listening for a connection from clients at the specified TCP/IP port number. \nA TCP Listener that has been created can be deleted by the ListenerDelete command. \nYou can also get a list of TCP Listeners currently registered by using the ListenerList command. \nnTo execute this command, you must have VPN Server administrator privileges.
CMD_ListenerCreate_Args	ListenerCreate [port]
CMD_ListenerCreate_[port]	Using an integer, specify the newly added TCP/IP listener port number. You can also use a port number that is already being used by a different program; however the VPN Server will not be able to use it until that program ends the use of that port. Specify a port number that is within the range of 1 to 65535.
CMD_ListenerCreate_PortPrompt	Port number of newly added TCP/IP Listener: 


# ListenerDelete command
CMD_ListenerDelete	Delete TCP Listener
CMD_ListenerDelete_Help	This allows you to delete a TCP Listener that's registered on the server. When the TCP Listener is in a state of operation, the listener will automatically be deleted when its operation stops. \nYou can also get a list of TCP Listeners currently registered by using the ListenerList command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ListenerDelete_Args	ListenerDelete [port]
CMD_ListenerDelete_[port]	Using an integer, specify the TCP/IP listener port number you want to delete.
CMD_ListenerDelete_PortPrompt	Port number of TCP/IP Listener: 


# ListenerList command
CMD_ListenerList	Get List of TCP Listeners
CMD_ListenerList_Help	This allows you to get a list of TCP listeners registered on the current server. You can obtain information on whether the various TCP listeners have a status of operating or error. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ListenerList_Args	ListenerList
CMD_ListenerList_Column1	Número da porta TCP
CMD_ListenerList_Column2	Status


# ListenerEnable command
CMD_ListenerEnable	Begin TCP Listener Operation
CMD_ListenerEnable_Help	This starts the operation of stopped TCP Listeners registered on the current server. \nYou can also get a list of TCP Listeners currently registered by using the ListenerList command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ListenerEnable_Args	ListenerEnable [port]
CMD_ListenerEnable_[port]	Using an integer, specify the port number of the TCP/IP listener you want to start.
CMD_ListenerEnable_PortPrompt	Port number of TCP/IP Listener to start: 


# ListenerDisable command
CMD_ListenerDisable	Stop TCP Listener Operation
CMD_ListenerDisable_Help	This stops the operation of operating TCP Listeners registered on the current server. \nYou can also get a list of TCP Listeners currently registered by using the ListenerList command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ListenerDisable_Args	ListenerDisable [port]
CMD_ListenerDisable_[port]	Using an integer, specify the port number of the TCP/IP listener you want to stop.
CMD_ListenerDisable_PortPrompt	Port number of TCP/IP Listener to start: 


# PortsUDPSet command
CMD_PortsUDPSet			Sets the UDP ports that the server should listen on
CMD_PortsUDPSet_Help	This command can be used to specify a single or multiple UDP ports the server should listen on. \nYou can specify a port that is used by another process, however the server will not be able to use it until the port becomes free. \nSpecify a port number that is within the range of 1 to 65535. \nYou can list the ports that are currently set with the PortsUDPGet command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_PortsUDPSet_Args	PortsUDPSet [ports]
CMD_PortsUDPSet_[ports]	Multiple UDP ports can be specified by splitting them with a space or a comma, for example: "443, 992, 1194, 5555". \nSpecify "0" to disable the UDP listener. \n\nPorts: 


# PortsUDPGet command
CMD_PortsUDPGet			Lists the UDP ports that the server is listening on
CMD_PortsUDPGet_Help	This command can be used to retrieve the UDP ports the server is listening on. \nYou can set the ports with the PortsUDPSet command.
CMD_PortsUDPGet_Args	PortsUDPGet
CMD_PortsUDPGet_Ports	UDP ports


# ProtoOptionsSet command
CMD_ProtoOptionsSet						Sets an option's value for the specified protocol
CMD_ProtoOptionsSet_Help				This command can be used to change an option's value for a specific protocol. \nYou can retrieve the options using the ProtoOptionsGet command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ProtoOptionsSet_Args				ProtoOptionsSet [protocol] [/NAME:option_name] [/VALUE:string/true/false]
CMD_ProtoOptionsSet_[protocol]			Protocol name.
CMD_ProtoOptionsSet_NAME				Option name.
CMD_ProtoOptionsSet_VALUE				Option value. Make sure to write a value that is accepted by the specified protocol!
CMD_ProtoOptionsSet_Prompt_[protocol]	Protocol: 
CMD_ProtoOptionsSet_Prompt_NAME			Option: 
CMD_ProtoOptionsSet_Prompt_VALUE		Value: 


# ProtoOptionsGet command
CMD_ProtoOptionsGet						Lists the options for the specified protocol
CMD_ProtoOptionsGet_Help				This command can be used to retrieve the options for a specific protocol. \nDetailed info (e.g. value type) will be shown. \nYou can change an option's value with the ProtoOptionsSet command.
CMD_ProtoOptionsGet_Args				ProtoOptionsGet [protocol]
CMD_ProtoOptionsGet_[protocol]			Protocol name.
CMD_ProtoOptionsGet_Prompt_[protocol]	Protocol: 
CMD_ProtoOptionsGet_Column_Name			Name
CMD_ProtoOptionsGet_Column_Type			Type
CMD_ProtoOptionsGet_Column_Value		Value
CMD_ProtoOptionsGet_Column_Description	Description

# ProtoOptions
CMD_ProtoOptions_Description_OpenVPN_DefaultClientOption			When OpenVPN is compiled without OCC code, it doesn't send the options string to the server. The original OpenVPN server still works, because the configuration is static. SoftEther VPN is heuristic and wants to support as many different configurations as possible. This option allows to define the string that is sent to clients built without OCC code, so that they can successfully connect.
CMD_ProtoOptions_Description_OpenVPN_Obfuscation					This may help an OpenVPN client bypass firewalls that are aware of the protocol and block it. The same XOR mask has to be applied client-side, otherwise it will not be able to connect with certain obfuscation methods!
CMD_ProtoOptions_Description_OpenVPN_ObfuscationMask				Mask used to XOR the bytes in the packet (used for certain obfuscation modes).
CMD_ProtoOptions_Description_OpenVPN_PingSendInterval				Interval in milliseconds between each ping packet transmission.
CMD_ProtoOptions_Description_OpenVPN_PushDummyIPv4AddressOnL2Mode	There's a bug that manifests under certain circumstances on Linux. It causes the OpenVPN client to disconnect unless the TAP device is UP. This option tells the server to push a dummy IPv4 address (RFC7600) to the client, so that the TAP adapter is forced to be UP.
CMD_ProtoOptions_Description_OpenVPN_Timeout						Time in milliseconds after which the session is forcifully interrupted if no packets are received from the client in the meantime.


# ServerPasswordSet command
CMD_ServerPasswordSet	Set VPN Server Administrator Password
CMD_ServerPasswordSet_Help	This sets the VPN Server administrator password. You can specify the password as a parameter. If the password is not specified, a prompt will be displayed to input the password and password confirmation. If you include the password as a parameter, this password will be displayed momentarily on the screen, which poses a risk. We recommend that whenever possible, avoid specifying this parameter and input the password using the password prompt. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ServerPasswordSet_Args	ServerPasswordSet [password]
CMD_ServerPasswordSet_[password]	This specifies a new password setting.


# ClusterSettingGet command
CMD_ClusterSettingGet	Get Clustering Configuration of Current VPN Server
CMD_ClusterSettingGet_Help	You can use this to acquire the clustering configuration of the current VPN Server. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ClusterSettingGet_Args	ClusterSettingGet
CMD_ClusterSettingGet_Current	Current Configuration
CMD_ClusterSettingGet_None	(Sem configuração)
CMD_ClusterSettingGet_PublicIp	Public IP Address
CMD_ClusterSettingGet_PublicPorts	Lista de portas públicas
CMD_ClusterSettingGet_Controller	Destination Controller
CMD_ClusterSettingGet_ControllerOnly	Controller Function Only
CMD_ClusterSettingGet_Weight	Performance Standard in Cluster


# ClusterSettingStandalone command
CMD_ClusterSettingStandalone	Set VPN Server Type as Standalone
CMD_ClusterSettingStandalone_Help	Use this to set the VPN Server type as Standalone Server. Standalone server means a VPN Server that does not belong to any cluster in its current state. When VPN Server is installed, by default it will be in standalone server mode. Unless you have particular plans to configure a cluster, we recommend the VPN Server be operated in standalone mode. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, when this command is executed, VPN Server will automatically restart. \nThis command cannot be run on VPN Bridge.
CMD_ClusterSettingStandalone_Args	ClusterSettingStandalone


# ClusterSettingController command
CMD_ClusterSettingController	Set VPN Server Type as Cluster Controller
CMD_ClusterSettingController_Help	Use this to set the VPN Server type as Cluster Controller. A cluster controller is the central computer of all member servers of a cluster in the case where a clustering environment is made up of multiple VPN Servers. A cluster requires one computer to serve this role. The other cluster member servers that are configured in the same cluster begin operation as a cluster member by connecting to the cluster controller. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, when this command is executed, VPN Server will automatically restart. \nThis command cannot be run on VPN Bridge.
CMD_ClusterSettingController_Args	ClusterSettingController [/WEIGHT:weight] [/ONLY:yes|no]
CMD_ClusterSettingController_WEIGHT	This sets a value for the performance standard ratio of this VPN Server. This is the standard value for when load balancing is performed in the cluster. Normally it is 100. For example, making only one machine 200 while the other members have a status of 100, will regulate that machine to receive twice as many connections as the other members during load balancing. Specify 1 or higher for the value. If this parameter is left unspecified, 100 will be used.
CMD_ClusterSettingController_ONLY	By specifying "yes" here, the VPN Server will operate only as a controller on the cluster and it will always distribute general VPN Client connections to members other than itself. This function is used in high-load environments. If this parameter is left unspecified, "no" will be used.


# ClusterSettingMember command
CMD_ClusterSettingMember	Set VPN Server Type as Cluster Member
CMD_ClusterSettingMember_Help	Use this to set the VPN Server type as Cluster Member Server. A cluster member server is a member computer belonging to a clustering configuration made up of multiple VPN Servers with another existing cluster controller as the center. Multiple cluster members can be added to the cluster as required. \nBefore setting the VPN Server as a cluster member server, first ask the administrator of the cluster controller to be used for the controller's IP address and port number, the public IP address and public port number (when required) of this VPN Server and the password. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, when this command is executed, VPN Server will automatically restart. \nThis command cannot be run on VPN Bridge.
CMD_ClusterSettingMember_Args	ClusterSettingMember [server:port] [/IP:ip] [/PORTS:ports] [/PASSWORD:password] [/WEIGHT:weight]
CMD_ClusterSettingMember_[server:port]	Specify the host name or IP address, and port number of the destination cluster controller using the parameter with the format host name:port number.
CMD_ClusterSettingMember_IP	Specify the public IP address of this server. If you wish to leave public IP address unspecified, specify it like this: "/IP:none". When a public IP address is not specified, the IP address of the network interface used when connecting to the cluster controller will be automatically used.
CMD_ClusterSettingMember_PORTS	Use this to specify the list of public port numbers on this server. The list must have at least one public port number set, and it is also possible to set multiple public port numbers. When specifying multiple port numbers, separate them using a comma such as "/PORTS443,992,8888".
CMD_ClusterSettingMember_PASSWORD	Specify the password required to connect to the destination controller. It needs to be the same as an administrator password on the destination controller.
CMD_ClusterSettingMember_WEIGHT	This sets a value for the performance standard ratio of this VPN Server. This is the standard value for when load balancing is performed in the cluster. For example, making only one machine 200 while the other members have a status of 100, will regulate that machine to receive twice as many connections as the other members. Specify 1 or higher for the value. If this parameter is left unspecified, 100 will be used.
CMD_ClusterSettingMember_Prompt_IP_1	Specify a public IP address. \nIf you wish to leave this unspecified, press Enter without inputting anything.
CMD_ClusterSettingMember_Prompt_IP_2	Public IP Address: 
CMD_ClusterSettingMember_Prompt_PORT_1	Please specify a list of public port numbers. \nWhen specifying 2 or more port numbers, separate each entry with a comma, like: 444,992,888.
CMD_ClusterSettingMember_Prompt_PORT_2	Número da porta pública: 
CMD_ClusterSettingMember_Prompt_HOST_1	Destination Controller Host Name and Port Number: 


# ClusterMemberList command
CMD_ClusterMemberList	Get List of Cluster Members
CMD_ClusterMemberList_Help	Use this command when the VPN Server is operating as a cluster controller to get a list of the cluster member servers on the same cluster, including the cluster controller itself. \nFor each member, the following information is also listed. Type, Connection Start, Host Name, Points, Number of Session, Number of TCP Connections, Number of Operating Virtual Hubs, Using Client Connection License and Using Bridge Connection License. \nThis command cannot be run on VPN Bridge.
CMD_ClusterMemberList_Args	ClusterMemberList


# ClusterMemberInfoGet command
CMD_ClusterMemberInfoGet	Get Cluster Member Information
CMD_ClusterMemberInfoGet_Help	When the VPN Server is operating as a cluster controller, you can get information on cluster member servers on that cluster by specifying the IDs of the member servers. \nYou can get the following information about the specified cluster member server: Server Type, Time Connection has been Established, IP Address, Host Name, Points, Public Port List, Number of Operating Virtual Hubs, First Virtual Hub, Number of Sessions and Number of TCP Connections. \nThis command cannot be run on VPN Bridge.
CMD_ClusterMemberInfoGet_Args	ClusterMemberInfoGet [id]
CMD_ClusterMemberInfoGet_[id]	Specify the ID of the cluster member whose information you want to get. You can obtain the cluster member server ID by using the ClusterMemberList command.
CMD_ClusterMemberInfoGet_PROMPT_ID	Cluster Member ID to Get Info: 


# ClusterMemberCertGet command
CMD_ClusterMemberCertGet	Get Cluster Member Certificate
CMD_ClusterMemberCertGet_Help	When the VPN Server is operating as a cluster controller, you can get the public X.509 certificate of cluster member servers on that cluster by specifying the IDs of those member servers. You can save the certificate as an X.509 format file. \nThis command cannot be run on VPN Bridge.
CMD_ClusterMemberCertGet_Args	ClusterMemberCertGet [id] [/SAVECERT:cert]
CMD_ClusterMemberCertGet_[id]	Specify the ID of the cluster member whose certificate you want to get. You can obtain the cluster member server ID by using the ClusterMemberList command.
CMD_ClusterMemberCertGet_SAVECERT	Specify the file path name to save the certificate you obtained. You can save the certificate in X.509 format.
CMD_ClusterMemberCertGet_PROMPT_ID	Cluster Member ID to Get Certificate: 


# ClusterConnectionStatusGet command
CMD_ClusterConnectionStatusGet	Get Connection Status to Cluster Controller
CMD_ClusterConnectionStatusGet_Help	Use this command when the VPN Server is operating as a cluster controller to get the status of connection to the cluster controller. \nYou can get the following information: Controller IP Address, Port Number, Connection Status, Connection Start Time, First Connection Established Time, Current Connection Established Time, Number of Connection Attempts, Number of Successful Connections, Number of Failed Connections. \nThis command cannot be run on VPN Bridge.
CMD_ClusterConnectionStatusGet_Args	ClusterConnectionStatusGet


# Debug command
CMD_Debug	Execute a Debug Command
CMD_Debug_Help	Runs a debug command on the running VPN Server / Bridge process.\nThis command should be executed wjen the support staff requests to do so.\nMisuse of this command might cause a crash of VPN Server / Bridge running.
CMD_Debug_Args	Debug [id] [/ARG:arg]
CMD_Debug_[id]	Specify a debug command number.
CMD_Debug_ARG	Specify a string to pass to the debug command. If a string contains spaces, contains the whole command by " ".
CMD_Debug_Msg1	Sending the debug command...
CMD_Debug_Msg2	The debug command has executed.\nResults: \"%S\"


# Crash command
CMD_Crash	Raise a error on the VPN Server / Bridge to terminate the process forcefully.
CMD_Crash_Help	This command will raise a fatal error (memory access violation) on the VPN Server / Bridge running process in order to crash the process. As the result, VPN Server / Bridge will be terminated and restarted if it is running as a service mode. If the VPN Server is running as a user mode, the process will not automatically restarted.\nThis command is for a situation when the VPN Server / Bridge is under a non-recoverable error or the process is in an infinite loop. This command will disconnect all VPN Sessions on the VPN Server / Bridge. All unsaved settings in the memory of VPN Server / Bridge will be lost.\nBefore run this command, run the Flush command to try to save volatile data to the configuration file.\nTo execute this command, you must have VPN Server / VPN Bridge administrator privileges.
CMD_Crash_Args	Crash [yes]
CMD_Crash_[yes]	Input "yes" for confirmation.
CMD_Crash_Msg	Sending the Crush command to the VPN Server. The VPN Server will be let to crash immediately, so you can never get the result value of this command. After this moment, vpncmd will be disconnected from the VPN Server.
CMD_Crash_Confirm	Do you really want to crash the VPN Server?\nInput "yes" if it is ok: 
CMD_Crash_Aborted	The Crash command has been aborted.


# Flush command
CMD_Flush	Save All Volatile Data of VPN Server / Bridge to the Configuration File
CMD_Flush_Help	Normally, the VPN Server / VPN Bridge retains the volatile configuration data in memory. It is flushed to the disk as vpn_server.config or vpn_bridge.config periodically. The period is 300 seconds (5 minutes) by default. (The period can be altered by modifying the AutoSaveConfigSpan item in the configuration file.) The data will be saved on the timing of shutting down normally of the VPN Server / Bridge.\nExecute the Flush command to make the VPN Server / Bridge save the settings to the file immediately. The setting data will be stored on the disk drive of the server computer. Use the Flush command in a situation that you do not have an enough time to shut down the server process normally.\nTo execute this command, you must have VPN Server administrator privileges. \nTo execute this command, you must have VPN Server / VPN Bridge administrator privileges.
CMD_Flush_Args	Flush
CMD_Flush_Msg1	Writing volatile data from memory to the disk...\n
CMD_Flush_Msg2	Saving completed. The file size is %S bytes.\n


# ServerCertGet command
CMD_ServerCertGet	Get SSL Certificate of VPN Server
CMD_ServerCertGet_Help	Use this to get the SSL certificate that the VPN Server provides to the connected client. You can save the certificate as an X.509 format file.
CMD_ServerCertGet_Args	ServerCertGet [cert]
CMD_ServerCertGet_[cert]	Specify the file path name to save the certificate you obtained. You can save the certificate in X.509 format.


# ServerKeyGet command
CMD_ServerKeyGet	Get SSL Certificate Private Key of VPN Server
CMD_ServerKeyGet_Help	Use this to get the SSL certificate private key that the VPN Server provides to the connected client. You can save the private key as a Base 64 encoded file. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ServerKeyGet_Args	ServerKeyGet [key]
CMD_ServerKeyGet_[key]	Specify the file path name to save the private key you obtained. You can save the private key in a Base 64 encoded format.


# ServerCertSet command
CMD_ServerCertSet	Set SSL Certificate and Private Key of VPN Server
CMD_ServerCertSet_Help	You can set the SSL certificate that the VPN Server provides to the connected client and the private key for that certificate. The certificate must be in X.509 format and the private key must be Base 64 encoded format. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ServerCertSet_Args	ServerCertSet [/LOADCERT:cert] [/LOADKEY:key]
CMD_ServerCertSet_LOADCERT	Specify the X.509 format certificate file to use.
CMD_ServerCertSet_LOADKEY	Specify the Base 64 encoded private key file for the certificate to use.


# ServerCipherGet command
CMD_ServerCipherGet	Get the Encrypted Algorithm Used for VPN Communication.
CMD_ServerCipherGet_Help	Use this to get the current setting of the algorithm used for the electronic signature and encrypted for SSL connection to be used for communication between the VPN Server and the connected client and the list of algorithms that can be used on the VPN Server.
CMD_ServerCipherGet_Args	ServerCipherGet
CMD_ServerCipherGet_SERVER	Encrypted Algorithm Currently Used by VPN Server: 
CMD_ServerCipherGet_CIPHERS	List of Usable Encrypted Algorithm Names: 


# ServerCipherSet command
CMD_ServerCipherSet	Set the Encrypted Algorithm Used for VPN Communication.
CMD_ServerCipherSet_Help	Use this to set the algorithm used for the electronic signature and encrypted for SSL connections to be used for communication between the VPN Server and the connected client. \nBy specifying the algorithm name, the specified algorithm will be used later between the VPN Client and VPN Bridge connected to this server and the data will be encrypted. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ServerCipherSet_Args	ServerCipherSet [name]
CMD_ServerCipherSet_[name]	This specifies the encrypted and electronic signature algorithm to set. You can obtain the list of usable algorithms by using the ServerCipherGet command.
CMD_ServerCipherSet_PROMPT_NAME	Encrypted Algorithm Name to Specify: 


# KeepEnable command
CMD_KeepEnable	Enable the Keep Alive Internet Connection Function
CMD_KeepEnable_Help	This allows you to enable the Keep Alive Internet Connection Function. By using the Keep Alive Internet Connection Function for network connection environments where connections will automatically be disconnected when there are periods of no communication that are longer than a set period, it is possible to keep alive the Internet connection by sending packets to a nominated server on the Internet at set intervals. \nYou can set a destination host name etc, by using the KeepSet command. \nTo execute this command on a VPN Server or VPN Bridge, you must have administrator privileges.
CMD_KeepEnable_Args	KeepEnable


# KeepDisable command
CMD_KeepDisable	Disable the Keep Alive Internet Connection Function
CMD_KeepDisable_Help	This allows you to disable the Keep Alive Internet Connection Function.\nTo execute this command on a VPN Server or VPN Bridge, you must have administrator privileges.
CMD_KeepDisable_Args	KeepDisable


# KeepSet command
CMD_KeepSet	Set the Keep Alive Internet Connection Function
CMD_KeepSet_Help	Use this to set the destination host name etc. of the Keep Alive Internet Connection Function. For network connection environments where connections will automatically be disconnected where there are periods of no communication that are longer than a set period, by using the Keep Alive Internet Connection Function, it is possible to keep alive the Internet connection by sending packets to a nominated server on the Internet at set intervals. \nWhen using this command, you can specify the following: Host Name, Port Number, Packet Send Interval, and Protocol. \nPackets sent to keep alive the Internet connection will have random content and personal information that could identify a computer or user is not sent. \nYou can use the KeepEnable command or KeepDisable command to enable/disable the Keep Alive Internet Connection Function. KeepSet does not change the enabled/disabled status. \nTo execute this command on a VPN Server or VPN Bridge, you must have administrator privileges.
CMD_KeepSet_Args	KeepSet [/HOST:host:port] [/PROTOCOL:tcp|udp] [/INTERVAL:interval]
CMD_KeepSet_HOST	Specify the host name or IP address, and port number of the destination using the format "host name:port number".
CMD_KeepSet_PROTOCOL	Specify either tcp or udp.
CMD_KeepSet_INTERVAL	Specify, in seconds, the interval between the sending of packets.
CMD_KeepSet_PROMPT_HOST	Destination Host Name/IP Address and Port Number: 
CMD_KeepSet_PROMPT_PROTOCOL	TCP ou UDP: 
CMD_KeepSet_PROMPT_INTERVAL	Interval Between Packets Sends (Seconds): 
CMD_KeepSet_EVAL_TCP_UDP	Please specify "tcp" or "udp".


# KeepGet command
CMD_KeepGet	Get the Keep Alive Internet Connection Function
CMD_KeepGet_Help	Use this to get the current setting contents of the Keep Alive Internet Connection Function. In addition to the destination's Host Name, Port Number, Packet Send Interval and Protocol, you can obtain the current enabled/disabled status of the Keep Alive Internet Connection Function.
CMD_KeepGet_Args	KeepGet
CMD_KeepGet_COLUMN_1	Nome do host
CMD_KeepGet_COLUMN_2	Número da porta
CMD_KeepGet_COLUMN_3	Packet Send Interval (Sec)
CMD_KeepGet_COLUMN_4	Protocolo
CMD_KeepGet_COLUMN_5	Status atual


# SyslogEnable command
CMD_SyslogEnable	Set syslog Send Function
CMD_SyslogEnable_Help	Use this to set the usage of syslog send function and which syslog server to use. 
CMD_SyslogEnable_Args	SyslogEnable [1|2|3] [/HOST:host:port]
CMD_SyslogEnable_[1|2|3]	Specify, using an integer, 1, 2 or 3 for the setting to use the syslog send function. \n1: Send server log by syslog. \n2: Send server and Virtual Hub security logs by syslog. \n3: Send server, Virtual Hub security, and packet logs by syslog.
CMD_SyslogEnable_HOST	Specify the host name or IP address, and port number of the syslog server using the format [host name:port number]. If the port number is omitted, 514 will be used.
CMD_SyslogEnable_MINMAX	Specify, using an integer, 1, 2 or 3 for the setting to use the syslog send function.
CMD_SyslogEnable_Prompt_123	Setting to Use syslog Send Function (1-3): 
CMD_SyslogEnable_Prompt_HOST	Specify syslog Server: 


# SyslogDisable command
CMD_SyslogDisable	Disable syslog Send Function
CMD_SyslogDisable_Help	Use this to disable the syslog send function.
CMD_SyslogDisable_Args	SyslogDisable


# SyslogGet command
CMD_SyslogGet	Get syslog Send Function
CMD_SyslogGet_Help	This allows you to get the current setting contents of the syslog send function. You can get the usage setting of the syslog function and the host name and port number of the syslog server to use.
CMD_SyslogGet_Args	SyslogGet
CMD_SyslogGet_COLUMN_1	Set the Use of syslog Send Function
CMD_SyslogGet_COLUMN_2	syslog Server Host Name
CMD_SyslogGet_COLUMN_3	syslog Server Port Number


# ConnectionGet command
CMD_ConnectionList	Get List of TCP Connections Connecting to the VPN Server
CMD_ConnectionList_Help	Use this to get a list of TCP/IP connections that are currently connecting to the VPN Server. It does not display the TCP connections that have been established as VPN sessions. To get the list of TCP/IP connections that have been established as VPN sessions, you can use the SessionList command. \nYou can get the following: Connection Name, Connection Source, Connection Start and Type.\nTo execute this command, you must have VPN Server administrator privileges.
CMD_ConnectionList_Args	ConnectionList


# ConnectionList command
CMD_ConnectionGet	Get Information of TCP Connections Connecting to the VPN Server
CMD_ConnectionGet_Help	Use this to get detailed information of a specific TCP/IP connection that is connecting to the VPN Server. \nYou can get the following information: Connection Name, Connection Type, Source Hostname, Source IP Address, Source Port Number (TCP), Connection Start, Server Product Name, Server Version, Server Build Number, Client Product Name, Client Version, and Client Build Number. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ConnectionGet_Args	ConnectionGet [name]
CMD_ConnectionGet_[name]	This allows you to specify the name of the connection whose information you want to get. To get a list of connection names, you can use the ConnectionList command.
CMD_ConnectionGet_PROMPT_NAME	Connection Name to Get Info: 


# ConnectionDisconnect command
CMD_ConnectionDisconnect	Disconnect TCP Connections Connecting to the VPN Server
CMD_ConnectionDisconnect_Help	Use this to forcefully disconnect specific TCP/IP connections that are connecting to the VPN Server. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ConnectionDisconnect_Args	ConnectionDisconnect [name]
CMD_ConnectionDisconnect_[name]	Specify the name of the connection to disconnect. To get a list of connection names, you can use the ConnectionList command.
CMD_ConnectionDisconnect_PROMPT_NAME	Connection Name to Disconnect: 


# BridgeDeviceList command
CMD_BridgeDeviceList	Get List of Network Adapters Usable as Local Bridge
CMD_BridgeDeviceList_Help	Use this to get a list of Ethernet devices (network adapters) that can be used as a bridge destination device as part of a Local Bridge connection. If possible, network connection name is displayed. \nYou can use a device displayed here by using the BridgeCreate command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_BridgeDeviceList_Args	BridgeDeviceList


# BridgeList command
CMD_BridgeList	Get List of Local Bridge Connection
CMD_BridgeList_Help	Use this to get a list of the currently defined Local Bridge connections. \nYou can get the Local Bridge connection Virtual Hub name and the bridge destination Ethernet device (network adapter) name or tap device name, as well as the operating status. 
CMD_BridgeList_Args	BridgeList


# BridgeCreate command
CMD_BridgeCreate	Create Local Bridge Connection
CMD_BridgeCreate_Help	Use this to create a new Local Bridge connection on the VPN Server.\nBy using a Local Bridge, you can configure a Layer 2 bridge connection between a Virtual Hub operating on this VPN server and a physical Ethernet Device (Network Adapter). \nYou can create a tap device (virtual network interface) on the system and connect a bridge between Virtual Hubs (the tap device is only supported by Linux versions). \nIt is possible to establish a bridge to an operating network adapter of your choice for the bridge destination Ethernet device (network adapter), but in high load environments, we recommend you prepare a network adapter dedicated to serve as a bridge. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_BridgeCreate_Args	BridgeCreate [hubname] [/DEVICE:device_name] [/TAP:yes|no]
CMD_BridgeCreate_[hubname]	Specify the Virtual Hub to create bridge. To get a list of Virtual Hubs, you can use the HubList command. It is not essential that you specify a Virtual Hub that is currently operating. If you specify a Virtual Hub name that is not currently operating or that does not exist, the Local Bridge connection will become enabled when the actual operation of that Virtual Hub begins.
CMD_BridgeCreate_DEVICE	Specify the bridge destination Ethernet device (network adapter) or tap device name. You can get the list of Ethernet device names by using the BridgeDeviceList command.
CMD_BridgeCreate_TAP	Specify yes if you are using a tap device rather than a network adapter for the bridge destination (only supported for Linux versions). When this is omitted, it will be treated the same as when no is specified.
CMD_BridgeCreate_PROMPT_HUBNAME	Virtual Hub Name to Create Bridge: 
CMD_BridgeCreate_PROMPT_DEVICE	Bridge Destination Device Name: 
CMD_BridgeCreate_PROMPT_TAP	Use tap device? (yes/no): 


# BridgeDelete command
CMD_BridgeDelete	Delete Local Bridge Connection
CMD_BridgeDelete_Help	Use this to delete an existing Local Bridge connection. To get a list of current Local Bridge connections use the BridgeDeviceList command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_BridgeDelete_Args	BridgeDelete [hubname] [/DEVICE:device_name]
CMD_BridgeDelete_[hubname]	Specify the Virtual Hub of the Local Bridge to delete.
CMD_BridgeDelete_DEVICE	Specify the device name (network adapter or tap device name) of the Local Bridge to delete.
CMD_BridgeDelete_PROMPT_HUBNAME	Virtual Hub Name to Delete Bridge: 
CMD_BridgeDelete_PROMPT_DEVICE	Bridge Device Name to Delete: 


# Caps command
CMD_Caps	Get List of Server Functions/Capability
CMD_Caps_Help	Use this get a list of functions and capability of the VPN Server currently connected and being managed. \nThe function and capability of VPN Servers are different depending on the operating VPN server's edition and version. Sometimes commands may be included in the command line management utility that cannot operate because of the function and capability of the destination VPN Server. Using this command, you can find out the capability of the target VPN Server and report it. \nIf the version of the VPN Server is newer than the command line management utility and there are functions that the command line management utility does not recognize, you can display the contents strings (variable names) as they are.
CMD_Caps_Args	Caps


# Reboot command
CMD_Reboot	Reboot VPN Server Service
CMD_Reboot_Help	Use this to restart the VPN Server service. \nWhen you restart the VPN Server, all currently connected sessions and TCP connections will be disconnected and no new connections will be accepted until the restart process has completed. \nBy using this command, only the VPN Server service program will be restarted and the physical computer that VPN Server is operating on does not restart. This management session will also be disconnected, so you will need to reconnect to continue management. \nAlso, by specifying the /RESTCONFIG:yes parameter, the contents of the configuration file (.config) held by the current VPN Server will be initialized. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_Reboot_Args	Reboot [/RESETCONFIG:yes|no]
CMD_Reboot_RESETCONFIG	By specifying yes, the contents of the configuration file (.config) held by the current VPN Server will be initialized. Please carefully consider the implications when setting this parameter.


# ConfigGet command
CMD_ConfigGet	Get the current configuration of the VPN Server
CMD_ConfigGet_Help	Use this to get a text file (.config file) that contains the current configuration contents of the VPN server. You can get the status on the VPN Server at the instant this command is executed. \nWhen part of the contents of the configuration file does not specify a parameter, it will be displayed on screen as it is. By specifying a save destination file name by parameter, the contents will be saved by that file name. \nYou can edit the configuration file by using a regular text editor. To write an edited configuration to the VPN Server, use the ConfigSet command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ConfigGet_Args	ConfigGet [path]
CMD_ConfigGet_[path]	When you want to save the contents of the configuration file to a file, use this to specify the file name. If left unspecified, the configuration contents will be displayed on screen. If the configuration file contains multiple-byte characters, the encoding must be saved as Unicode (UTF-8).
CMD_ConfigGet_FILENAME	Config name: "%S", Size: %u
CMD_ConfigGet_FILE_SAVE_FAILED	Creation of specified file failed.


# ConfigSet command
CMD_ConfigSet	Write Configuration File to VPN Server
CMD_ConfigSet_Help	Use this to write the configuration file to the VPN Server. By executing this command, the contents of the specified configuration file will be applied to the VPN Server and the VPN Server program will automatically restart and upon restart, operate according to the new configuration contents. \nBecause it is difficult for an administrator to write all the contents of a configuration file, we recommend you use the ConfigGet command to get the current contents of the VPN Server configuration and save it to file. You can then edit these contents in a regular text editor and then use the ConfigSet command to rewrite the contents to the VPN Server. \nThis command is for people with a detailed knowledge of the VPN Server and if an incorrectly configured configuration file is written to the VPN Server, it not only could cause errors, it could also result in the lost of the current setting data. Take special care when carrying out this action. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_ConfigSet_Args	ConfigSet [path]
CMD_ConfigSet_[path]	Specify the file name of the write destination configuration file. If the write destination file contains multiple-byte characters, the encoding must be Unicode (UTF-8).
CMD_ConfigSet_PROMPT_PATH	Config file path name to upload to server: 
CMD_ConfigSet_FILE_LOAD_FAILED	Reading from specified file failed.


# RouterList command
CMD_RouterList	Get List of Virtual Layer 3 Switches
CMD_RouterList_Help	Use this to get the list of Virtual Layer 3 Switches defined on the VPN Server. You can get the following information on the Virtual Layer 3 Switches: Switch Name, Operating Status, Number of Interfaces, and Number of Routing Tables. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge.
CMD_RouterList_Args	RouterList


# RouterAdd command
CMD_RouterAdd	Define New Virtual Layer 3 Switch
CMD_RouterAdd_Help	Use this to define a new Virtual Layer 3 Switch on the VPN Server. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge. \n\n[Explanation on Virtual Layer 3 Switch Function]\nYou can define Virtual Layer 3 Switches between multiple Virtual Hubs operating on this VPN Server and configure routing between different IP networks. \n\n[Caution about the Virtual Layer 3 Switch Function]\nThe Virtual Layer 3 Switch functions are provided for network administrators and other people who know a lot about networks and IP routing. If you are using the regular VPN functions, you do not need to use the Virtual Layer 3 Switch functions. \nIf the Virtual Layer 3 Switch functions are to be used, the person who configures them must have sufficient knowledge of IP routing and be perfectly capable of not impacting the network.
CMD_RouterAdd_Args	RouterAdd [name]
CMD_RouterAdd_[name]	Use this to specify the name of the newly created Virtual Layer 3 Switch name. You cannot add a name that is identical to an existing Virtual Layer 3 Switch.
CMD_RouterAdd_PROMPT_NAME	Name of Virtual Layer 3 Switch to Create: 


# RouterDelete command
CMD_RouterDelete	Delete Virtual Layer 3 Switch
CMD_RouterDelete_Help	Use this to delete an existing Virtual Layer 3 Switch that is defined on the VPN Server. When the specified Virtual Layer 3 Switch is operating, it will be automatically deleted after operation stops. \nTo get a list of existing Virtual Layer 3 Switches, use the RouterList command. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge.
CMD_RouterDelete_Args	RouterDelete [name]
CMD_RouterDelete_[name]	Use this to specify the name of the Virtual Layer 3 Switch to be deleted.
CMD_RouterDelete_PROMPT_NAME	Name of Virtual Layer 3 Switch to Delete: 


# RouterStart command
CMD_RouterStart	Start Virtual Layer 3 Switch Operation
CMD_RouterStart_Help	Use this to start the operation of an existing Virtual Layer 3 Switch defined on the VPN Server whose operation is currently stopped. \nTo get a list of existing Virtual Layer 3 Switches, use the RouterList command. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge. \n\n[Explanation on Virtual Layer 3 Switch Function]\nYou can define Virtual Layer 3 Switches between multiple Virtual Hubs operating on this VPN Server and configure routing between different IP networks. \n\n[Caution about the Virtual Layer 3 Switch Function]\nThe Virtual Layer 3 Switch functions are provided for network administrators and other people who know a lot about networks and IP routing. If you are using the regular VPN functions, you do not need to use the Virtual Layer 3 Switch functions. \nIf the Virtual Layer 3 Switch functions are to be used, the person who configures them must have sufficient knowledge of IP routing and be perfectly capable of not impacting the network.
CMD_RouterStart_Args	RouterStart [name]
CMD_RouterStart_[name]	Use this to specify the name of the Virtual Layer 3 Switch to start.
CMD_RouterStart_PROMPT_NAME	Name of Virtual Layer 3 Switch to Start: 


# RouterStop command
CMD_RouterStop	Stop Virtual Layer 3 Switch Operation
CMD_RouterStop_Help	Use this to stop the operation of an existing Virtual Layer 3 Switch defined on the VPN Server whose operation is currently operating. \nTo get a list of existing Virtual Layer 3 Switches, use the RouterList command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_RouterStop_Args	RouterStop [name]
CMD_RouterStop_[name]	Use this to specify the name of the Virtual Layer 3 Switch to stop.
CMD_RouterStop_PROMPT_NAME	Name of Virtual Layer 3 Switch to Stop: 


# RouterIfList command
CMD_RouterIfList	Get List of Interfaces Registered on the Virtual Layer 3 Switch
CMD_RouterIfList_Help	Use this to get a list of virtual interfaces when virtual interfaces have been defined on a specified Virtual Layer 3 Switch. \nYou can define multiple virtual interfaces and routing tables for a single Virtual Layer 3 Switch. \nA virtual interface is associated to a virtual Hub and operates as a single IP host on the Virtual Hub when that Virtual Hub is operating. When multiple virtual interfaces that respectively belong to a different IP network of a different Virtual Hub are defined, IP routing will be automatically performed between these interfaces. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge.
CMD_RouterIfList_Args	RouterIfList [name]
CMD_RouterIfList_[name]	Use this to specify the name of the Virtual Layer 3 Switch.
CMD_RouterIfList_PROMPT_NAME	Nome do Virtual Layer 3 Switch: 


# RouterIfAdd command
CMD_RouterIfAdd	Add Virtual Interface to Virtual Layer 3 Switch
CMD_RouterIfAdd_Help	Use this to add to a specified Virtual Layer 3 Switch, a virtual interface that connects to a Virtual Hub operating on the same VPN Server. \nYou can define multiple virtual interfaces and routing tables for a single Virtual Layer 3 Switch. \nA virtual interface is associated to a virtual Hub and operates as a single IP host on the Virtual Hub when that Virtual Hub is operating. When multiple virtual interfaces that respectively belong to a different IP network of a different Virtual Hub are defined, IP routing will be automatically performed between these interfaces. \nYou must define the IP network space that the virtual interface belongs to and the IP address of the interface itself. \nAlso, you must specify the name of the Virtual Hub that the interface will connect to. \nYou can specify a Virtual Hub that currently doesn't exist for the Virtual Hub name. \nThe virtual interface must have one IP address in the Virtual Hub. You also must specify the subnet mask of an IP network that the IP address belongs to. \nRouting via the Virtual Layer 3 Switches of IP spaces of multiple virtual Hubs operates based on the IP address is specified here. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge. \nTo execute this command, the target Virtual Layer 3 Switch must be stopped. If it is not stopped, first use the RouterStop command to stop it and then execute this command.
CMD_RouterIfAdd_Args	RouterIfAdd [name] [/HUB:hub] [/IP:ip/mask]
CMD_RouterIfAdd_[name]	Use this to specify the name of the Virtual Layer 3 Switch.
CMD_RouterIfAdd_HUB	Use this to specify the name of the Virtual Hub to be the connection destination of the virtual interface to be newly added. To get a list of Virtual Hubs, you can use the HubList command. It is not essential that you specify a Virtual Hub that is currently operating. If you specify a Virtual Hub name that is not currently operating or that does not exist, the Virtual Layer 3 Switch will become enabled when the actual operation of that Virtual Hub begins.
CMD_RouterIfAdd_IP	Using the format: "IP address/subnet mask", specify the IP address and subnet mask held by the virtual interface to be newly added. Specify the IP address by separating the decimal values using dots such as 192.168.0.1 For the subnet mask, either specify decimal values separated by dots such as 255.255.255.0, or you can specify the bit length from the header using a decimal value such as 24. 
CMD_RouterIfAdd_PROMPT_NAME	Nome do Virtual Layer 3 Switch: 
CMD_RouterIfAdd_PROMPT_HUB	Destination Virtual Hub Name of Virtual Interface: 
CMD_RouterIfAdd_PROMPT_IP	IP Address/Subnet Mask: 


# RouterIfDel command
CMD_RouterIfDel	Delete Virtual Interface of Virtual Layer 3 Switch
CMD_RouterIfDel_Help	Use this to delete a virtual interface already defined in the specified Virtual Layer 3 Switch. \nYou can get a list of the virtual interfaces currently defined, by using the RouterIfList command. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge. \nTo execute this command, the target Virtual Layer 3 Switch must be stopped. If it is not stopped, first use the RouterStop command to stop it and then execute this command.
CMD_RouterIfDel_Args	RouterIfDel [name] [/HUB:hub]
CMD_RouterIfDel_[name]	Use this to specify the name of the Virtual Layer 3 Switch.
CMD_RouterIfDel_HUB	Use this to specify the name of the Virtual Hub to be the connection destination of the virtual interface to be deleted.


# RouterTableList command
CMD_RouterTableList	Get List of Routing Tables of Virtual Layer 3 Switch 
CMD_RouterTableList_Help	Use this to get a list of routing tables when routing tables have been defined on a specified Virtual Layer 3 Switch. \nIf the destination IP address of the IP packet does not belong to any IP network that belongs to a virtual interface, the IP routing engine of the Virtual Layer 3 Switch will reference this routing table and execute routing. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge.
CMD_RouterTableList_Args	RouterTableList [name]
CMD_RouterTableList_[name]	Use this to specify the name of the Virtual Layer 3 Switch.
CMD_RouterTableList_PROMPT_NAME	Nome do Virtual Layer 3 Switch: 


# RouterTableAdd command
CMD_RouterTableAdd	Add Routing Table Entry for Virtual Layer 3 Switch
CMD_RouterTableAdd_Help	Here you can add a new routing table entry to the routing table of the specified Virtual Layer 3 Switch. \nIf the destination IP address of the IP packet does not belong to any IP network that belongs to a virtual interface, the IP routing engine of the Virtual Layer 3 Switch will reference the routing table and execute routing. \nYou must specify the contents of the routing table entry to be added to the Virtual Layer 3 Switch. You must specify any IP address that belongs to the same IP network in the virtual interface of this Virtual Layer 3 Switch as the gateway address. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge. \nTo execute this command, the target Virtual Layer 3 Switch must be stopped. If it is not stopped, first use the RouterStop command to stop it and then execute this command.
CMD_RouterTableAdd_Args	RouterTableAdd [name] [/NETWORK:ip/mask] [/GATEWAY:gwip] [/METRIC:metric]
CMD_RouterTableAdd_[name]	Use this to specify the name of the Virtual Layer 3 Switch.
CMD_RouterTableAdd_NETWORK	Using the format: "IP address/subnet mask", specify the network address and subnet mask of the routing table entry to be newly added. Specify the network address by separating the decimal values using dots such as "192.168.0.1". For the subnet mask, either specify decimal values separated by dots such as 255.255.255.0, or you can specify the bit length from the header using a decimal value such as 24. If you specify 0.0.0.0/0.0.0.0, the default route will be used. 
CMD_RouterTableAdd_GATEWAY	Especifique o endereço IP do gateway.
CMD_RouterTableAdd_METRIC	Specify a metric value. Specify an integer (1 or higher).
CMD_RouterTableAdd_PROMPT_NAME	Nome do Virtual Layer 3 Switch: 
CMD_RouterTableAdd_PROMPT_NETWORK	Network Address/Subnet Mask: 
CMD_RouterTableAdd_PROMPT_GATEWAY	Gateway Address: 
CMD_RouterTableAdd_PROMPT_METRIC	Valor métrica: 


# RouterTableDel command
CMD_RouterTableDel	Delete Routing Table Entry of Virtual Layer 3 Switch
CMD_RouterTableDel_Help	Use this to delete a routing table entry that is defined in the specified Virtual Layer 3 Switch. \nYou can get a list of the already defined routing table entries by using the RouterTableList command. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Bridge. \nTo execute this command, the target Virtual Layer 3 Switch must be stopped. If it is not stopped, first use the RouterStop command to stop it and then execute this command.
CMD_RouterTableDel_Args	RouterTableDel [name] [/NETWORK:ip/mask] [/GATEWAY:gwip] [/METRIC:metric]
CMD_RouterTableDel_[name]	Use this to specify the name of the Virtual Layer 3 Switch.
CMD_RouterTableDel_NETWORK	Using the format: "IP address/subnet mask", specify the network address of the routing table entry to be deleted.
CMD_RouterTableDel_GATEWAY	Especifique o endereço IP do gateway.
CMD_RouterTableDel_METRIC	Specify a metric value. Specify an integer (1 or higher).


# LogFileList command
CMD_LogFileList	Get List of Log Files
CMD_LogFileList_Help	Use this to display a list of log files outputted by the VPN Server that have been saved on the VPN Server computer. By specifying a log file file name displayed here and calling it using the LogFileGet command you can download the contents of the log file. \nIf you are connected to the VPN Server in server admin mode, you can display or download the packet logs and security logs of all Virtual Hubs and the server log of the VPN Server. \nWhen connected in Virtual Hub Admin Mode, you are able to view or download only the packet log and security log of the Virtual Hub that is the target of management.
CMD_LogFileList_Args	LogFileList
CMD_LogFileList_START	Getting list of log files. This may take a while. Please wait...
CMD_LogFileList_NUM_LOGS	In total there are %u log files.


# LogFileGet command
CMD_LogFileGet	Download Log file
CMD_LogFileGet_Help	Use this to download the log file that is saved on the VPN Server computer. To download the log file first display the list of log files using the LogFileList command and then download the log file using the LogFileGet command. If you are connected to the VPN Server in server admin mode, you can display or download the packet logs and security logs of all Virtual Hubs and the server log of the VPN Server. When connected in Virtual Hub Admin Mode, you are able to view or download only the packet log and security log of the Virtual Hub that is the target of management. \nIf you have specified the file name as a parameter, the downloaded log file will be saved to the file of that file name. If the destination file is not specified, the log file will be displayed onscreen. \nThe size of the log file can get very big, so pay careful attention to this issue.
CMD_LogFileGet_Args	LogFileGet [name] [/SERVER:server] [/SAVEPATH:savepath]
CMD_LogFileGet_[name]	Specify the name of the log file to be downloaded. To get a list of downloadable log files, use the LogFileList command.
CMD_LogFileGet_SERVER	Use this to specify the server name when making a download request to a cluster controller. Specify the server that will be displayed by the LogFileGet command.
CMD_LogFileGet_SAVEPATH	Use this to specify the destination file name for when saving the downloaded log file. When this is left unspecified, the file will be displayed onscreen.
CMD_LogFileGet_PROMPT_NAME	Name of log file to download: 
CMD_LogFileGet_START	Downloading log file. This may take a while. Please wait...
CMD_LogFileGet_FAILED	The download failed.
CMD_LogFileGet_SAVE_FAILED	Unable to write to the specified file.
CMD_LogFileGet_FILESIZE	File size of log file: %u


# WgkAdd command
CMD_WgkAdd	Add a WireGuard key
CMD_WgkAdd_Help	This command can be used to add a WireGuard key to the allowed key list. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_WgkAdd_Args	WgkAdd [key] [/HUB:hub] [/USER:user]
CMD_WgkAdd_[key]	WireGuard key. Make sure it is the public one!
CMD_WgkAdd_HUB	Hub the key will be associated to.
CMD_WgkAdd_USER	User the key will be associated to, in the specified hub.
CMD_WgkAdd_Prompt_[key]	Key: 
CMD_WgkAdd_Prompt_HUB	Hub: 
CMD_WgkAdd_Prompt_USER	User: 


# WgkDelete command
CMD_WgkDelete	Delete a WireGuard key
CMD_WgkDelete_Help	This command can be used to delete a WireGuard key from the allowed key list. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_WgkDelete_Args	WgkDelete [key]
CMD_WgkDelete_[key]	WireGuard key.
CMD_WgkDelete_Prompt_[key]	Key: 


# WgkEnum command
CMD_WgkEnum	List the WireGuard keys
CMD_WgkEnum_Help	This command retrieves the WireGuard keys that are allowed to connect to the server, along with the associated Virtual Hub and user. \nYou can add a key with the WgkAdd command. \nYou can delete a key with the WgkDelete command. \nTo execute this command, you must have VPN Server administrator privileges.
CMD_WgkEnum_Args	WgkEnum
CMD_WgkEnum_Column_Key	Key
CMD_WgkEnum_Column_Hub	Hub
CMD_WgkEnum_Column_User	User


# HubCreate command
CMD_HubCreate	Create New Virtual Hub
CMD_HubCreate_Help	Use this to create a new Virtual Hub on the VPN Server. \nThe created Virtual Hub will begin operation immediately. \nWhen the VPN Server is operating on a cluster, this command is only valid for the cluster controller. Also, the new Virtual Hub will operate as a dynamic Virtual Hub. You can change it to a static Virtual Hub by using the HubSetStatic command. To get a list of Virtual Hubs that are already on the VPN Server, use the HubList command. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Servers that are operating as a VPN Bridge or cluster member. \nWhen issuing the command to a cluster controller on a cluster to create a Virtual Hub, use either the HubCreateStatic command or the HubCreateDynamic command (issuing the HubCreate command to a cluster controller has the same operational effect as issuing the HubCreateDynamic command).
CMD_HubCreate_Args	HubCreate [name] [/PASSWORD:password]
CMD_HubCreate_[name]	Specify the name of the Virtual Hub to create.
CMD_HubCreate_PASSWORD	Specify an administrator password when the administrator password is going to be set for the Virtual Hub to be created. If this is not specified, a prompt will appear to input the password.
CMD_HubCreate_PROMPT_NAME	Name of Virtual Hub to be created: 


# HubCreateDynamic command
CMD_HubCreateDynamic	Create New Dynamic Virtual Hub (For Clustering)
CMD_HubCreateDynamic_Help	Use this to create a new dynamic Virtual Hub on the VPN Server. \nThe created Virtual Hub will begin operation immediately. \nWhen the VPN Server is operating on a cluster, this command is only valid for the cluster controller. Also, the new Virtual Hub will operate as a dynamic Virtual Hub. You can change it to a static Virtual Hub by using the HubSetStatic command. To get a list of Virtual Hubs that are already on the VPN Server, use the HubList command. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Servers that are operating as a VPN Bridge, cluster member or standalone server.
CMD_HubCreateDynamic_Args	HubCreateDynamic [name] [/PASSWORD:password]
CMD_HubCreateDynamic_[name]	Specify the name of the Virtual Hub to create.
CMD_HubCreateDynamic_PASSWORD	Specify an administrator password when the administrator password is going to be set for the Virtual Hub to be created. If this is not specified, a prompt will appear to input the password.


# HubCreateStatic command
CMD_HubCreateStatic	Create New Static Virtual Hub (For Clustering)
CMD_HubCreateStatic_Help	Use this to create a new static Virtual Hub on the VPN Server. \nThe created Virtual Hub will begin operation immediately. \nWhen the VPN Server is operating on a cluster, this command is only valid for the cluster controller. Also, the new Virtual Hub will operate as a dynamic Virtual Hub. You can change it to a static Virtual Hub by using the HubSetStatic command. To get a list of Virtual Hubs that are already on the VPN Server, use the HubList command. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Servers that are operating as a VPN Bridge, cluster member or standalone server.
CMD_HubCreateStatic_Args	HubCreateStatic [name] [/PASSWORD:password]
CMD_HubCreateStatic_[name]	Specify the name of the Virtual Hub to create.
CMD_HubCreateStatic_PASSWORD	Specify an administrator password when the administrator password is going to be set for the Virtual Hub to be created. If this is not specified, a prompt will appear to input the password.


# HubDelete command
CMD_HubDelete	Delete Virtual Hub
CMD_HubDelete_Help	Use this to delete an existing Virtual Hub on the VPN Server. \nIf you delete the Virtual Hub, all sessions that are currently connected to the Virtual Hub will be disconnected and new sessions will be unable to connect to the Virtual Hub. \nAlso, this will also delete all the Hub settings, user objects, group objects, certificates and Cascade Connections. \nOnce you delete the Virtual Hub, it cannot be recovered. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Servers that are operating as a VPN Bridge or cluster member.
CMD_HubDelete_Args	HubDelete [name]
CMD_HubDelete_[name]	Specify the name of the Virtual Hub to delete.
CMD_HubDelete_PROMPT_NAME	Name of Virtual Hub to delete: 


# HubSetStatic command
CMD_HubSetStatic	Change Virtual Hub Type to Static Virtual Hub
CMD_HubSetStatic_Help	Use this when a VPN Server is operating on a cluster and you want to change the type of the Virtual Hub to a static Virtual Hub. When the type of the Virtual Hub is changed, all sessions that are currently connected to the Virtual Hub will be disconnected. \nWhen there is a Virtual Hub operating as a static virtual Hub, a Virtual Hub with that name will be created on all the cluster member servers. A user who attempts to connect this Virtual Hub will be connected to one of the cluster members hosting this Virtual Hub as determined by an algorithm based on each server's load status. \nA static Virtual Hub, for example, could be used for a remote access VPN that allows thousands or tens of thousands of users to connect at the same time for the purpose of remotely accessing an internal company LAN from the Internet for business. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Servers that are operating as a VPN Bridge, cluster member or standalone server. \nThis command cannot be used for VPN Servers that are newer than Build 5190.
CMD_HubSetStatic_Args	HubSetStatic [name]
CMD_HubSetStatic_[name]	Specify the name of the Virtual Hub to be set as the static Virtual Hub.
CMD_HubChange_PROMPT_NAME	Name of Virtual Hub to change setting: 


# HubSetDynamic command
CMD_HubSetDynamic	Change Virtual Hub Type to Dynamic Virtual Hub
CMD_HubSetDynamic_Help	Use this when a VPN Server is operating on a cluster and you want to change the type of the Virtual Hub to a dynamic Virtual Hub. When the type of the Virtual Hub is changed, all sessions that are currently connected to the Virtual Hub will be disconnected. \nWhen there is not even one client connected to a dynamic Virtual Hub defined on the cluster, then that Virtual Hub does not exist on any cluster member. When the first client to attempt to connect to the dynamic Virtual Hub does so, the server with the lowest load on the cluster starts hosting that Virtual Hub. When the second and subsequent clients attempt to connect to the same virtual Hub, they are automatically connected to the server hosting the Virtual Hub. When all the clients are disconnected from a particular dynamic Virtual Hub, the Virtual Hub will return to the original state of not existing on any of the servers. \nThere is a broad range of applications for dynamic Virtual Hubs, such as a Virtual Hub defined for each business section within a company so that employees can connect to the Virtual Hub of their own department to do their work in a centralized management environment that is deployed on a single cluster. \nTo execute this command, you must have VPN Server administrator privileges. \nAlso, this command does not operate on VPN Servers that are operating as a VPN Bridge, cluster member or standalone server. \nThis command cannot be used for VPN Servers that are newer than Build 5190.
CMD_HubSetDynamic_Args	HubSetDynamic [name]
CMD_HubSetDynamic_[name]	Specify the name of the Virtual Hub to be set as the dynamic Virtual Hub.


# HubList command
CMD_HubList	Get List of Virtual Hubs
CMD_HubList_Help	Use this to get a list of existing Virtual Hubs on the VPN Server. For each Virtual Hub, you can get the following information: Virtual Hub Name, Status, Type, Number of Users, Number of Groups, Number of Sessions, Number of MAC Tables, Number of IP Tables, Number of Logins, Last Login, and Last Communication.\nNote that when connecting in Virtual Hub Admin Mode, if in the options of a Virtual Hub that you do not have administrator privileges for, the option Don't Enumerate this Virtual Hub for Anonymous Users is enabled then that Virtual Hub will not be enumerated. If you are connected in Server Admin Mode, then the list of all Virtual Hubs will be displayed. \nWhen connecting to and managing a non-cluster-controller cluster member of a clustering environment, only the Virtual Hub currently being hosted by that VPN Server will be displayed. When connecting to a cluster controller for administration purposes, all the Virtual Hubs will be displayed.
CMD_HubList_Args	ListaHub


# Hub command
CMD_Hub	Select Virtual Hub to Manage
CMD_Hub_Help	Use this to select the Virtual Hub to be the target of administration. For an administration utility with the status of being connected to a VPN Server, before executing a command to set or manage a Virtual Hub, you must use the Hub command to select the Virtual Hub to manage. \nWhen in the status of being connected to a VPN Server in Virtual Hub Admin Mode, you can select a single Virtual Hub to be the target of administration but you cannot select other Virtual Hubs. When having the status of being connected to the VPN Server in Server Admin Mode, you can make all Virtual Hubs the target of administration. \nTo get a list of Virtual Hubs that currently exist on the VPN Server, use the HubList command. \nFor the VPN Bridge, you can only select the Virtual Hub that has the name "BRIDGE".
CMD_Hub_Args	Hub [name]
CMD_Hub_[name]	Specify the name of the Virtual Hub to manage. If this parameter is left unspecified, the Select Virtual Hub to Manage will be cancelled.
CMD_Hub_Unselected	The Virtual Hub selection has been unselected.
CMD_Hub_Selected	The Virtual Hub "%S" has been selected.
CMD_Hub_Select_Failed	When attempting to select Virtual Hub "%S" that has been specified by /ADMINHUB, the following error occurred.
CMD_Hub_Not_Selected	Before executing this command, first select the Virtual Hub to manage using the Hub command.


# Online command
CMD_Online	Switch Virtual Hub to Online
CMD_Online_Help	Use this when the Virtual Hub currently being managed is offline to switch it to online. A Virtual Hub with an offline status cannot receive VPN connections from clients. By switching the Virtual Hub to online, that Virtual Hub becomes able to receive connections from users and provide services. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_Online_Args	Online


# Offline command
CMD_Offline	Switch Virtual Hub to Offline
CMD_Offline_Help	Use this when the Virtual Hub currently being managed is online to switch it to offline. If there are sessions currently connected to the Virtual Hub, all sessions will be disconnected. A Virtual Hub with an offline status cannot receive VPN connections from clients. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_Offline_Args	Offline


# SetStaticNetwork command
CMD_SetStaticNetwork				Set Virtual Hub static IPv4 network parameters
CMD_SetStaticNetwork_Help			Set the static IPv4 network parameters for the Virtual Hub. They are used when DHCP is not available (e.g. WireGuard sessions). \nYou can get the current settings by using the OptionsGet command.
CMD_SetStaticNetwork_Args			SetStaticNetwork [/GATEWAY:gateway] [/SUBNET:subnet]
CMD_SetStaticNetwork_GATEWAY		Specify the IP address of the gateway that will be used for internet communication.
CMD_SetStaticNetwork_SUBNET			Specify the subnet mask, required to determine the size of the local VPN network.
CMD_SetStaticNetwork_Prompt_GATEWAY	Gateway: 
CMD_SetStaticNetwork_Prompt_SUBNET	Subnet mask: 


# SetMaxSession command
CMD_SetMaxSession	Set the Max Number of Concurrently Connected Sessions for Virtual Hub
CMD_SetMaxSession_Help	Use this to set the maximum number of sessions that can be concurrently connected to the Virtual Hub that is currently being managed. When there are more sessions than the maximum number of concurrently connected sessions that are being connected from the VPN Client or VPN Bridge, when the maximum number of sessions is reached, clients will no longer be able to connect. This limit on the maximum number of concurrently connected sessions does not include sessions generated in the Virtual Hub by Local Bridges, Virtual NAT, and Cascade Connections. \nYou can get the current setting for the max number of concurrently connected sessions by using the OptionsGet command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SetMaxSession_Args	SetMaxSession [max_session]
CMD_SetMaxSession_[max_session]	Using an integer, specify the maximum number of concurrently connected sessions to set. Specifying 0 results in a setting of unlimited.
CMD_SetMaxSession_Prompt	Max Number of Sessions: 


# SetHubPassword command
CMD_SetHubPassword	Set Virtual Hub Administrator Password
CMD_SetHubPassword_Help	Use this to set the Administrator Password for the Virtual Hub that is currently being managed. When a Virtual Hub administrator password has been set, you are able to connect to that Virtual Hub from a VPN Server connection utility in Virtual Hub Admin Mode, by specifying the password. It is also possible to make a VPN connection from a VPN client or VPN Bridge by specifying "Administrator" for the user name and the password for the Virtual Hub administrator password. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SetHubPassword_Args	SetHubPassword [password]
CMD_SetHubPassword_[password]	Specify the password you wish to set. If a password is not specified by parameter, a prompt will appear to input the password.


# SetEnumAllow command
CMD_SetEnumAllow	Allow Enumeration by Virtual Hub Anonymous Users
CMD_SetEnumAllow_Help	Use this to change the options setting of the Virtual Hub you are currently managing to allow anonymous users to enumerate this Virtual Hub. By setting this option, it makes it possible for VPN Client users to enumerate this Virtual Hub simply by inputting this VPN Server address. Also, by using the SetEnumDeny command, you can deny anonymous users the ability to enumerate. At the time a Virtual Hub is created, enumeration will be allowed. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SetEnumAllow_Args	SetEnumAllow


# SetEnumDeny command
CMD_SetEnumDeny	Deny Enumeration by Virtual Hub Anonymous Users
CMD_SetEnumDeny_Help	Use this to change the options setting of the Virtual Hub you are currently managing to prevent anonymous users from enumerating this Virtual Hub. By setting this option, the VPN Client user will be unable to enumerate this Virtual Hub even if they send a Virtual Hub enumeration request to the VPN Server. Also, by using the SetEnumAllow command, you can allow anonymous users to enumerate. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SetEnumDeny_Args	SetEnumDeny


# OptionsGet command
CMD_OptionsGet	Get Options Setting of Virtual Hubs
CMD_OptionsGet_Help	Use this to get a list of the Options setting of the Virtual Hub currently being managed. You can get the following: Allow/Deny Virtual Hub Enumeration, Maximum Concurrent Connections, Online/Offline Status, and Virtual Hub Type in Clustering Environment. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_OptionsGet_Args	OptionsGet
CMD_OptionsGet_TITLE	Options Setting List of Virtual Hub "%S"
CMD_OptionsGet_ENUM	Enumeration of Virtual Hub for Anonymous User
CMD_OptionsGet_MAXSESSIONS	Max Number of Sessions
CMD_OptionsGet_STATUS	Status
CMD_OptionsGet_TYPE	Virtual Hub Type
CMD_OptionsGet_GATEWAY	Default gateway
CMD_OptionsGet_SUBNET	Default subnet


# RadiusServerSet command
CMD_RadiusServerSet	Set RADIUS Server to use for User Authentication
CMD_RadiusServerSet_Help	To accept users to the currently managed Virtual Hub in RADIUS server authentication mode, you can specify an external RADIUS server that confirms the user name and password. (You can specify multiple hostname by splitting with comma or semicolon.) \nThe RADIUS server must be set to receive requests from IP addresses of this VPN Server. Also, authentication by Password Authentication Protocol (PAP) must be enabled. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_RadiusServerSet_Args	RadiusServerSet [server_name:port] [/SECRET:secret] [/RETRY_INTERVAL:interval]
CMD_RadiusServerSet_[server_name:port]	Using the format "host name:port number", specify the host name or IP address, and the UDP port number of the RADIUS server being used. If the port number is omitted, 1812 will be used. You can specify multiple hostname by splitting with comma or semicolon.
CMD_RadiusServerSet_SECRET	Specify the shared secret (password) used for communication with the RADIUS Server
CMD_RadiusServerSet_RETRY_INTERVAL	Specify the retry interval between retries in milliseconds.
CMD_RadiusServerSet_Prompt_Host	Host Number and Port Number of RADIUS Server to Use: 
CMD_RadiusServerSet_Prompt_Secret	Shared Secret: 
CMD_RadiusServerSet_Prompt_RetryInterval	Retry Interval (milliseconds): 
CMD_RadiusServerSet_EVAL_NUMINTERVAL	The retry interval must be in from 500 to 10000 milliseconds.


# RadiusServerDelete command
CMD_RadiusServerDelete	Delete Setting to Use RADIUS Server for User Authentication
CMD_RadiusServerDelete_Help	Use this to delete the setting related to using a RADIUS server when a user connects to the currently managed Virtual Hub in RADIUS Server Authentication Mode and disable the RADIUS authentication. To get the settings related to the current RADIUS server use the RadiusServerGet command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_RadiusServerDelete_Args	RadiusServerDelete


# RadiusServerGet command
CMD_RadiusServerGet	Get Setting of RADIUS Server Used for User Authentication
CMD_RadiusServerGet_Help	Use this to get the current settings for the RADIUS server used when a user connects to the currently managed Virtual Hub using RADIUS Server Authentication Mode. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_RadiusServerGet_Args	RadiusServerGet
CMD_RadiusServerGet_STATUS	Use RADIUS Server
CMD_RadiusServerGet_HOST	RADIUS Server Host Name or IP Address: 
CMD_RadiusServerGet_PORT	RADIUS Server Port Number
CMD_RadiusServerGet_SECRET	Segredo compartilhado 
CMD_RadiusServerGet_RetryInterval	Retry Interval (in milliseconds)


# StatusGet command
CMD_StatusGet	Get Current Status of Virtual Hub
CMD_StatusGet_Help	Use this to get the current status of the Virtual Hub currently being managed. You can get the following information: Virtual Hub Type, Number of Sessions, Number of Each Type of Object, Number of Logins, Last Login, Last Communication, and Communication Statistical Data.
CMD_StatusGet_Args	StatusGet


# LogGet command
CMD_LogGet	Get Log Save Setting of Virtual Hub
CMD_LogGet_Help	Use this to get the log save setting for the Virtual Hub that is currently being managed. You can get the setting information such as the save setting related to security logs and packet logs and information on what has been saved.
CMD_LogGet_Args	LogGet
CMD_Log_SecurityLog	Save Security Log
CMD_Log_PacketLog	Save Packet Log
CMD_Log_SwitchType	Log File Switch Cycle
CMD_Log_0	TCP Connection Log
CMD_Log_1	TCP Packet Log
CMD_Log_2	Log DHCP
CMD_Log_3	Log UDP
CMD_Log_4	Log ICMP
CMD_Log_5	IP Log
CMD_Log_6	ARP Log
CMD_Log_7	Log Ethernet


# LogEnable command
CMD_LogEnable	Enable Security Log or Packet Log
CMD_LogEnable_Help	Use this to enable a security log or packet log of the Virtual Hub currently being managed. \nTo get the current setting, you can use the LogGet command.
CMD_LogEnable_Args	LogEnable [security|packet]
CMD_LogEnable_[security|packet]	Select the type of log to enable. Specify either "security" or "packet".
CMD_LogEnable_Prompt	Select Security or Packet: 
CMD_LogEnable_Prompt_Error	Invalid specification.


# LogDisable command
CMD_LogDisable	Disable Security Log or Packet Log
CMD_LogDisable_Help	Use this to disable a security log or packet log of the Virtual Hub currently being managed. \nTo get the current setting, you can use the LogGet command.
CMD_LogDisable_Args	LogDisable [security|packet]
CMD_LogDisable_[security|packet]	Select the type of log to disable. Specify either "security" or "packet".


#  LogSwitchSet command
CMD_LogSwitchSet	Set Log File Switch Cycle
CMD_LogSwitchSet_Help	Use this to set the log file switch cycle for the security log or packet log that the currently managed Virtual Hub saves. The log file switch cycle can be changed to switch in every second, every minute, every hour, every day, every month ,or not switch. \nTo get the current setting, you can use the LogGet command.
CMD_LogSwitchSet_Args	LogSwitchSet [security|packet] [/SWITCH:sec|min|hour|day|month|none]
CMD_LogSwitchSet_[security|packet]	Select the type of log to change setting. Specify either "security" or "packet".
CMD_LogSwitchSet_SWITCH	Select the switch cycle to set. Specify sec, min, hour, day, month or none.
CMD_LogSwitchSet_Prompt	Specify sec, min, hour, day, month or none: 


# LogPacketSaveType command
CMD_LogPacketSaveType	Set Save Contents and Type of Packet to Save to Packet Log
CMD_LogPacketSaveType_Help	Use this to set the save contents of the packet log for each type of packet to be saved by the currently managed Virtual Hub. There are the following packet types: TCP Connection Log, TCP Packet Log, DHCP Packet Log, UDP Packet Log, ICMP Packet Log, IP Packet Log, ARP Packet Log, and Ethernet Packet Log.\nTo get the current setting, you can use the LogGet command.
CMD_LogPacketSaveType_Args	LogPacketSaveType [/TYPE:tcpconn|tcpdata|dhcp|udp|icmp|ip|arp|ether] [/SAVE:none|header|full]
CMD_LogPacketSaveType_TYPE	Specify tcpconn, tcpdata, dhcp, udp, icmp, ip, arp, or ether to specify the type of packet whose save contents are going to be changed.
CMD_LogPacketSaveType_SAVE	Specify the save contents of the packet log. \nSpecify either none: save nothing\nheader: header information only\nfull: all packet contents
CMD_LogPacketSaveType_Prompt_TYPE	Specify tcpconn, tcpdata, dhcp, udp, icmp, ip, arp, or ether: 
CMD_LogPacketSaveType_Prompt_SAVE	Specify none, header, or full: 


# CAList command
CMD_CAList	Get List of Trusted CA Certificates
CMD_CAList_Help	Here you can manage the certificate authority certificates that are trusted by this currently managed Virtual Hub. The list of certificate authority certificates that are registered is used to verify certificates when a VPN Client is connected in signed certificate authentication mode. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_CAList_Args	ListaCA
CMD_CAList_COLUMN_ID	ID


# CAAdd command
CMD_CAAdd	Adicionar certificado CA confiável
CMD_CAAdd_Help	Use this to add a new certificate to a list of CA certificates trusted by the currently managed Virtual Hub. The list of certificate authority certificates that are registered is used to verify certificates when a VPN Client is connected in signed certificate authentication mode. \nTo get a list of the current certificates you can use the CAList command. \nThe certificate you add must be saved in the X.509 file format. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_CAAdd_Args	CAAdd [path]
CMD_CAAdd_[path]	Specify the file name of the X.509 certificate to register.
CMD_CAAdd_PROMPT_PATH	Name of X.509 Certificate File to Register: 


# CADelete command
CMD_CADelete	Excluir certificado de CA confiável
CMD_CADelete_Help	Use this to delete an existing certificate from the list of CA certificates trusted by the currently managed Virtual Hub. \nTo get a list of the current certificates you can use the CAList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_CADelete_Args	CADelete [id]
CMD_CADelete_[id]	Specify the ID of the certificate to delete.
CMD_CADelete_PROMPT_ID	ID of Certificate to Delete: 


# CAGet command
CMD_CAGet	Adicionar certificado CA confiável
CMD_CAGet_Help	Use this to get an existing certificate from the list of CA certificates trusted by the currently managed Virtual Hub and save it as a file in X.509 format. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_CAGet_Args	CAGet [id] [/SAVECERT:path]
CMD_CAGet_[id]	Specify the ID of the certificate to get.
CMD_CAGet_SAVECERT	Specify the file name to save the certificate you obtained.
CMD_CAGet_PROMPT_ID	ID of Certificate to Get: 
CMD_CAGet_PROMPT_SAVECERT	Name of File to Save: 


# CascadeList command
CMD_CascadeList	Get List of Cascade Connections
CMD_CascadeList_Help	Use this to get a list of Cascade Connections that are registered on the currently managed Virtual Hub. \nBy using a Cascade Connection, you can connect this Virtual Hub by Layer 2 Cascade Connection to another Virtual Hub that is operating on the same or a different computer. \n\n[Warning About Cascade Connections]\nBy connecting using a Cascade Connection you can create a Layer 2 bridge between multiple Virtual Hubs but if the connection is incorrectly configured, a loopback Cascade Connection could inadvertently be created. When using a Cascade Connection function please design the network topology with care. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeList_Args	CascadeList


# CascadeCreate command
CMD_CascadeCreate	Create New Cascade Connection
CMD_CascadeCreate_Help	Use this to create a new Cascade Connection on the currently managed Virtual Hub. \nBy using a Cascade Connection, you can connect this Virtual Hub by Cascade Connection to another Virtual Hub that is operating on the same or a different computer. \nTo create a Cascade Connection, you must specify the name of the Cascade Connection, destination server and destination Virtual Hub and user name. When a new Cascade Connection is created, the type of user authentication is initially set as Anonymous Authentication and the proxy server setting and the verification options of the server certificate is not set. To change these settings and other advanced settings after a Cascade Connection has been created, use the other commands that begin with the name "Cascade". \n\n[Warning About Cascade Connections]\nBy connecting using a Cascade Connection you can create a Layer 2 bridge between multiple Virtual Hubs but if the connection is incorrectly configured, a loopback Cascade Connection could inadvertently be created. When using a Cascade Connection function please design the network topology with care. \n\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeCreate_Args	CascadeCreate [name] [/SERVER:hostname:port] [/HUB:hubname] [/USERNAME:username]
CMD_CascadeCreate_[name]	Specify the name of the Cascade Connection to create.
CMD_CascadeCreate_SERVER	Specify the host name and port number of the destination VPN Server using the format [host name:port number]. You can also specify by IP address.
CMD_CascadeCreate_HUB	Specify the Virtual Hub on the destination VPN Server.
CMD_CascadeCreate_USERNAME	Specify the user name to use for user authentication when connecting to the destination VPN Server.
CMD_CascadeCreate_Prompt_Name	Cascade Connection Name: 
CMD_CascadeCreate_Prompt_Server	Destination VPN Server Host Name and Port Number: 
CMD_CascadeCreate_Prompt_Hub	Nome do hub virtual de destino: 
CMD_CascadeCreate_Prompt_Username	Nome de usuário da conexão: 


# CascadeSet command
CMD_CascadeSet	Set the Destination for Cascade Connection
CMD_CascadeSet_Help	Use this to set the destination VPN Server host name and port number, Virtual Hub name and the user name that will use the connection for the Cascade Connection registered on the currently managed virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeSet_Args	CascadeSet [name] [/SERVER:hostname:port] [/HUB:hubname]
CMD_CascadeSet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeSet_SERVER	Specify the host name and port number of the destination VPN Server using the format [host name:port number]. You can also specify by IP address.
CMD_CascadeSet_HUB	Specify the Virtual Hub on the destination VPN Server.


# CascadeGet command
CMD_CascadeGet	Get the Cascade Connection Setting
CMD_CascadeGet_Help	Use this to get the Connection Setting of a Cascade Connection that is registered on the currently managed Virtual Hub. \nTo change the Connection Setting contents of the Cascade Connection, use the other commands that begin with the name "Cascade" after creating the Cascade Connection. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeGet_Args	CascadeGet [name]
CMD_CascadeGet_[name]	Specify the name of the Cascade Connection whose setting you want to get.
CMD_CascadeGet_Policy	[Cascade Session Security Policy Setting Value]


# CascadeDelete command
CMD_CascadeDelete	Delete Cascade Connection Setting
CMD_CascadeDelete_Help	Use this to delete a Cascade Connection that is registered on the currently managed Virtual Hub. If the specified Cascade Connection has a status of online, the connections will be automatically disconnected and then the Cascade Connection will be deleted. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeDelete_Args	CascadeDelete [name]
CMD_CascadeDelete_[name]	Specify the name of the Cascade Connection to delete.


# CascadeUsernameSet command
CMD_CascadeUsernameSet	Set User Name to Use Connection of Cascade Connection
CMD_CascadeUsernameSet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to the VPN Server, use this to specify the user name required for user authentication. \nIn some cases it is necessary to specify the type of user authentication and specify the required parameters. To change this information you can use commands such as CascadeAnonymousSet, CascadePasswordSet, and CascadeCertSet. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeUsernameSet_Args	CascadeUsernameSet [name] [/USERNAME:username]
CMD_CascadeUsernameSet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeUsernameSet_USERNAME	Specify the user name required for user authentication when the Cascade Connection connects to the VPN Server.
CMD_CascadeUsername_Notice	The auth type for this Connection Setting is currently set as password authentication. After changing the user name, you must use the CascadePasswordSet command to reset the password.


# CascadeAnonymousSet command
CMD_CascadeAnonymousSet	Set User Authentication Type of Cascade Connection to Anonymous Authentication
CMD_CascadeAnonymousSet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to the VPN Server, set the user authe type to [anonymous authentication]. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeAnonymousSet_Args	CascadeAnonymousSet [name]
CMD_CascadeAnonymousSet_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadePasswordSet command
CMD_CascadePasswordSet	Set User Authentication Type of Cascade Connection to Password Authentication
CMD_CascadePasswordSet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to the VPN Server, use this to set the user auth type to Password Authentication. Specify Standard Password Authentication and RADIUS or NT Domain Authentication as the password authentication type. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadePasswordSet_Args	CascadePasswordSet [name] [/PASSWORD:password] [/TYPE:standard|radius]
CMD_CascadePasswordSet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadePasswordSet_PASSWORD	Specify the password to use for password authentication. If this is not specified, a prompt will appear to input the password.
CMD_CascadePasswordSet_TYPE	Specify either "standard" (Standard Password Authentication) or "radius" (RADIUS or NT Domain Authentication) as the password authentication type.
CMD_CascadePasswordSet_Prompt_Type	Especificar padrão ou radius: 
CMD_CascadePasswordSet_Type_Invalid	The standard or radius specification is invalid.


# CascadeCertSet command
CMD_CascadeCertSet	Set User Authentication Type of Cascade Connection to Client Certificate Authentication
CMD_CascadeCertSet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to the VPN Server, use this to set the user auth type to Client Certificate Authentication. For this certificate, you must specify a certificate file in the X.509 format and a private key file that is Base 64 encoded. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeCertSet_Args	CascadeCertSet [name] [/LOADCERT:cert] [/LOADKEY:key]
CMD_CascadeCertSet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeCertSet_LOADCERT	Specify the X.509 format certificate file to provide for certificate authentication.
CMD_CascadeCertSet_LOADKEY	Specify the Base-64-encoded private key file name for the certificate.


# CascadeCertGet command
CMD_CascadeCertGet	Get Client Certificate to Use for Cascade Connection
CMD_CascadeCertGet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection uses client certificate authentication, use this to get the certificate that is provided as the client certificate and save the certificate file in X.509 format. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeCertGet_Args	CascadeCertGet [name] [/SAVECERT:cert]
CMD_CascadeCertGet_[name]	Specify the name of the Cascade Connection whose setting you want to get.
CMD_CascadeCertGet_SAVECERT	Specify the file name to save the certificate you obtained in X.509 format.
CMD_CascadeCertSet_Not_Auth_Cert	The specified Cascade Connection is not in client certificate authentication mode.
CMD_CascadeCertSet_Cert_Not_Exists	The certificate is not stored in the Connection Setting of the specified Cascade Connection.


# CascadeEncryptEnable command
CMD_CascadeEncryptEnable	Enable Encryption when Communicating by Cascade Connection
CMD_CascadeEncryptEnable_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers to be encrypted by SSL. \nNormally communication between VPN Servers is encrypted by SSL to prevent eavesdropping of information and fraud. You can also disable encryption. When encryption is disabled, the communication throughput improves but the communication data flows over the network in plain text. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeEncryptEnable_Args	CascadeEncryptEnable [name]
CMD_CascadeEncryptEnable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeEncryptDisable command
CMD_CascadeEncryptDisable	Disable Encryption when Communicating by Cascade Connection
CMD_CascadeEncryptDisable_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers not to be encrypted. \nNormally communication between VPN Servers is encrypted by SSL to prevent eavesdropping of information and fraud. You can also disable encryption. When encryption is disabled, the communication throughput improves but the communication data flows over the network in plain text. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeEncryptDisable_Args	CascadeEncryptDisable [name]
CMD_CascadeEncryptDisable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeCompressEnable command
CMD_CascadeCompressEnable	Enable Data Compression when Communicating by Cascade Connection
CMD_CascadeCompressEnable_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers to be compressed. \nIt is possible to achieve a maximum of 80% compression. Compression however places higher loads on the CPU of both the client and server machines. When the line speed is about 10 Mbps or greater, compression can lower throughput, but sometimes it can have the opposite effect. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeCompressEnable_Args	CascadeCompressEnable [name]
CMD_CascadeCompressEnable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeCompressDisable command
CMD_CascadeCompressDisable	Disable Data Compression when Communicating by Cascade Connection
CMD_CascadeCompressDisable_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers to be not compressed. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeCompressDisable_Args	CascadeCompressDisable [name]
CMD_CascadeCompressDisable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeHttpHeader* commands
CMD_CascadeHttpHeader_Prompt_Name	Value name (part before the colon): 
CMD_CascadeHttpHeader_Prompt_Data	Dados do valor (parte após os dois pontos): 


# CascadeHttpHeaderAdd command
CMD_CascadeHttpHeaderAdd	Add a custom value in the HTTP header sent to the proxy server
CMD_CascadeHttpHeaderAdd_Help	Use this to add a custom value in the HTTP header sent to the proxy server. A custom HTTP header can be used to bypass certain restrictions imposed on the network or to avoid speed limitations applied by the QoS.
CMD_CascadeHttpHeaderAdd_Args	CascadeHttpHeaderAdd [name] [/NAME:name] [/DATA:data]
CMD_CascadeHttpHeaderAdd_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeHttpHeaderAdd_NAME	Specify the name of the custom value (the part before the colon character).
CMD_CascadeHttpHeaderAdd_DATA	Specify the data of the custom value (the part after the colon character).


# CascadeHttpHeaderDelete command
CMD_CascadeHttpHeaderDelete	Delete a custom value in the HTTP header sent to the proxy server
CMD_CascadeHttpHeaderDelete_Help	Use this to delete a custom value in the HTTP header sent to the proxy server. A custom HTTP header can be used to bypass certain restrictions imposed on the network or to avoid speed limitations applied by the QoS.
CMD_CascadeHttpHeaderDelete_Args	CascadeHttpHeaderDelete [name] [/NAME:name]
CMD_CascadeHttpHeaderDelete_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeHttpHeaderDelete_NAME	Specify the name of the custom value (the part before the colon character).


# CascadeHttpHeaderGet command
CMD_CascadeHttpHeaderGet	Get the list of custom values in the HTTP header sent to the proxy server
CMD_CascadeHttpHeaderGet_Help	Use this to get the list of custom values in the HTTP header sent to the proxy server. A custom HTTP header can be used to bypass certain restrictions imposed on the network or to avoid speed limitations applied by the QoS.
CMD_CascadeHttpHeaderGet_Args	CascadeHttpHeaderGet [name]
CMD_CascadeHttpHeaderGet_[name]	Specify the name of the Cascade Connection whose setting you want to get.


# CascadeProxyNone command
CMD_CascadeProxyNone	Specify Direct TCP/IP Connection as the Connection Method of Cascade Connection
CMD_CascadeProxyNone_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to a VPN Server, use this to set Direct TCP/IP Connection as the connection method to use, in which case the connection route will not be via a proxy server. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeProxyNone_Args	CascadeProxyNone [name]
CMD_CascadeProxyNone_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeProxyHttp command
CMD_CascadeProxyHttp	Set Connection Method of Cascade Connection to be via an HTTP Proxy Server
CMD_CascadeProxyHttp_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to a VPN Server, use this to set Connect via HTTP Proxy Server as the method of connection to use, which requires the specification of the host name and port number of the HTTP Proxy server to communicate via as well as a user name and password (when required). \nThe HTTP server that communication will travel via must be compatible with the CONNECT method to use HTTPS communication. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeProxyHttp_Args	CascadeProxyHttp [name] [/SERVER:hostname:port] [/USERNAME:username] [/PASSWORD:password]
CMD_CascadeProxyHttp_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeProxyHttp_SERVER	Specify the host name or IP address, and port number of the on-route HTTP proxy server using the format [host name:port number].
CMD_CascadeProxyHttp_USERNAME	When user authentication is required to connect to the on-route HTTP proxy server, specify the user name. Also, specify the /PASSWORD parameter at the same time. If the parameters /USERNAME and /PASSWORD are not specified, the user authentication data will not be set.
CMD_CascadeProxyHttp_PASSWORD	When user authentication is required to connect to the on-route HTTP proxy server, specify the password. Specify this together with the /USERNAME parameter.
CMD_CascadeProxyHttp_Prompt_Server	Proxy Server Host Name and Port Number: 


# CascadeProxySocks command
CMD_CascadeProxySocks	Set Connection Method of Cascade Connection to be via a SOCKS4 Proxy Server
CMD_CascadeProxySocks_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to a VPN Server, use this to set Connect via SOCKS4 Proxy Server as the method of connection to use, which requires the specification of the host name and port number of the SOCKS4 Proxy server to communicate via as well as a user name and password (when required). \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeProxySocks_Args	CascadeProxySocks [name] [/SERVER:hostname:port] [/USERNAME:username] [/PASSWORD:password]
CMD_CascadeProxySocks_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeProxySocks_SERVER	Specify the host name or IP address, and port number of the on-route SOCKS4 proxy server using the format "host name:port number".
CMD_CascadeProxySocks_USERNAME	When user authentication is required to connect to the on-route SOCKS4 proxy server, specify the user name. Also, specify the /PASSWORD parameter at the same time. If the parameters /USERNAME and /PASSWORD are not specified, the user authentication data will not be set.
CMD_CascadeProxySocks_PASSWORD	When user authentication is required to connect to the on-route SOCKS4 proxy server, specify the password. Specify this together with the /USERNAME parameter.


# CascadeProxySocks5 command
CMD_CascadeProxySocks5	Set Connection Method of Cascade Connection to be via a SOCKS5 Proxy Server
CMD_CascadeProxySocks5_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to a VPN Server, use this to set Connect via SOCKS5 Proxy Server as the method of connection to use, which requires the specification of the host name and port number of the SOCKS Proxy server to communicate via as well as a user name and password (when required). \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeProxySocks5_Args	CascadeProxySocks5 [name] [/SERVER:hostname:port] [/USERNAME:username] [/PASSWORD:password]
CMD_CascadeProxySocks5_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeProxySocks5_SERVER	Specify the host name or IP address, and port number of the on-route SOCKS5 proxy server using the format "host name:port number".
CMD_CascadeProxySocks5_USERNAME	When user authentication is required to connect to the on-route SOCKS5 proxy server, specify the user name. Also, specify the /PASSWORD parameter at the same time. If the parameters /USERNAME and /PASSWORD are not specified, the user authentication data will not be set.
CMD_CascadeProxySocks5_PASSWORD	When user authentication is required to connect to the on-route SOCKS5 proxy server, specify the password. Specify this together with the /USERNAME parameter.


# CascadeServerCertEnable command
CMD_CascadeServerCertEnable	Enable Cascade Connection Server Certificate Verification Option
CMD_CascadeServerCertEnable_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to a VPN Server, use this to enable the option to check whether the SSL certificate provided by the destination VPN Server can be trusted. \nIf this option is enabled you must either use the CascadeServerCertSet command to save the connection destination server SSL certificate beforehand in the Cascade Connection Settings beforehand, or use the CAAdd command etc. to register a root certificate containing the signed server SSL certificate in the list of Virtual Hub trusted CA certificates. \nIf the certificate of the connected VPN Server cannot be trusted under the condition where the option to verify server certificates was enabled for the Cascade Connection, the connection will be promptly cancelled and continual reattempts at connection will be made. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeServerCertEnable_Args	CascadeServerCertEnable [name]
CMD_CascadeServerCertEnable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeServerCertDisable command
CMD_CascadeServerCertDisable	Disable Cascade Connection Server Certificate Verification Option
CMD_CascadeServerCertDisable_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to a VPN Server, use this to disable the option to check whether the SSL certificate provided by the destination VPN Server can be trusted. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeServerCertDisable_Args	CascadeServerCertDisable [name]
CMD_CascadeServerCertDisable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeDefaultCAEnable command
CMD_CascadeDefaultCAEnable	        Enable Trust System Certificate Store Option
CMD_CascadeDefaultCAEnable_Help	    When server certificate verification is enabled, use this to enable trusting certificates from the system trust store. \nIf server certificate verification is disabled, this option does nothing.
CMD_CascadeDefaultCAEnable_Args	    CascadeDefaultCAEnable [name]
CMD_CascadeDefaultCAEnable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeDefaultCADisable command
CMD_CascadeDefaultCADisable         Disable Trust System Certificate Store Option
CMD_CascadeDefaultCADisable_Help    When server certificate verification is enabled, use this to disable trusting certificates from the system trust store. \nIf server certificate verification is disabled, this option does nothing.
CMD_CascadeDefaultCADisable_Args	CascadeDefaultCADisable [name]
CMD_CascadeDefaultCADisable_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeServerCertSet command
CMD_CascadeServerCertSet	Set the Server Individual Certificate for Cascade Connection
CMD_CascadeServerCertSet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to a VPN Server, use this to register beforehand the same certificate as the SSL certificate provided by the destination VPN Server. \nIf the option to verify server certificates for Cascade Connections is enabled, you must either use this command to save the connection destination server SSL certificate beforehand in the Cascade Connection Settings beforehand, or use the CAAdd command etc. to register a root certificate containing the signed server SSL certificate in the list of Virtual Hub trusted CA certificates. \nIf the certificate of the connected VPN Server cannot be trusted under the condition where the option to verify server certificates was enabled for the Cascade Connection, the connection will be promptly cancelled and continual reattempts at connection will be made. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeServerCertSet_Args	CascadeServerCertSet [name] [/LOADCERT:cert]
CMD_CascadeServerCertSet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeServerCertSet_LOADCERT	Specify X.509 format certificate file name that the server individual certificate you wish to set is saved under.


# CascadeServerCertDelete command
CMD_CascadeServerCertDelete	Delete the Server Individual Certificate for Cascade Connection
CMD_CascadeServerCertDelete_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and a server individual certificate is registered for that Cascade Connection, use this to delete that server individual certificate. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeServerCertDelete_Args	CascadeServerCertDelete [name]
CMD_CascadeServerCertDelete_[name]	Specify the name of the Cascade Connection whose setting you want to change.


# CascadeServerCertGet command
CMD_CascadeServerCertGet	Get the Server Individual Certificate for Cascade Connection
CMD_CascadeServerCertGet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and a server individual certificate is registered for that Cascade Connection, use this to get that certificate and save it as an X.509 format certificate file. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeServerCertGet_Args	CascadeServerCertGet [name] [/SAVECERT:path]
CMD_CascadeServerCertGet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeServerCertGet_SAVECERT	Specify the certificate file name to save the server individual certificate in X.509 format.


# CascadeDetailSet command
CMD_CascadeDetailSet	Set Advanced Settings for Cascade Connection
CMD_CascadeDetailSet_Help	Use this to customize the VPN protocol communication settings used when a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection connects to the VPN Server. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeDetailSet_Args	CascadeDetailSet [name] [/MAXTCP:max_connection] [/INTERVAL:interval] [/TTL:disconnect_span] [/HALF:yes|no] [/NOQOS:yes|no]
CMD_CascadeDetailSet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadeDetailSet_MAXTCP	Specify, using an integer in the range 1 to 32, the number of TCP connections to be used for VPN communication. By using data transmission by multiple TCP connections for VPN communication sessions with VPN Servers it is sometimes possible to increase communication speed. \nNote: We recommend about 8 lines when the connection lines to the server are fast, and 1 line when using a slow connection such as dialup.
CMD_CascadeDetailSet_INTERVAL	When communicating by VPN by establishing multiple TCP connections, specify in seconds, the establishing interval for each TCP connection. The standard value is 1 second.
CMD_CascadeDetailSet_TTL	When specifying connection life of each TCP connection specify in seconds the keep-alive time from establishing a TCP connection until disconnection. If 0 is specified, keep-alive will not be set.
CMD_CascadeDetailSet_HALF	Specify "yes" when enabling half duplex mode. When using two or more TCP connections for VPN communication, it is possible to use Half Duplex Mode. By enabling half duplex mode it is possible to automatically fix data transmission direction as half and half for each TCP connection. In the case where a VPN using 8 TCP connections is established, for example, when half-duplex is enabled, communication can be fixes so that 4 TCP connections are dedicated to the upload direction and the other 4 connections are dedicated to the download direction.
CMD_CascadeDetailSet_NOQOS	Specify "yes" when disabling VoIP / QoS functions. Normally "no" is specified.
CMD_CascadeDetailSet_Eval_MaxTcp	Specify an integer in the range 1 to 32 for the number of TCP connections.
CMD_CascadeDetailSet_Eval_Interval	Set at least 1 second for the interval to establish a TCP connection.
CMD_CascadeDetailSet_Prompt_MaxTcp	Número de conexões TCP a serem usadas na comunicação VPN: 
CMD_CascadeDetailSet_Prompt_Interval	Interval between Establishing Each TCP Connection: 
CMD_CascadeDetailSet_Prompt_TTL	Connection Life of Each TCP Connection (0 for no keep-alive): 
CMD_CascadeDetailSet_Prompt_HALF	Enable half-duplex mode (yes/no): 


# CascadePolicySet command
CMD_CascadePolicySet	Set Cascade Connection Session Security Policy
CMD_CascadePolicySet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection is established, use this to change the security policy contents that are applied to the session generated by the Virtual Hub. \nWhen a Virtual Hub makes a Cascade Connection to another VPN Server, a Cascade Session will be newly generated on the Virtual Hub that is the Cascade Connection source. You can use this command to set the security policy contents that will set this Cascade session. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadePolicySet_Args	[name] [/NAME:policy_name] [/VALUE:num|yes|no]
CMD_CascadePolicySet_[name]	Specify the name of the Cascade Connection whose setting you want to change.
CMD_CascadePolicySet_NAME	Specify the name of policy whose values you want to change. You can use the PolicyList command to display a list of policy names and values that can be set.
CMD_CascadePolicySet_VALUE	Specify a new policy value. If the policy is an integer value, specify an integer. Specify yes or no for Boolean types. You can view the type and value that can be set by using the PolicyList command.
CMD_CascadePolicySet_PROMPT_POLNAME	Name of Policy Whose Value you want to Change: 
CMD_CascadePolicySet_PROMPT_POLVALUE	Value to newly set: 
CMD_CascadePolicySet_Invalid_Name	The specified policy name "%S" is invalid. \nCheck the list of policy names that can be set using the PolicyList command.
CMD_CascadePolicySet_Invalid_Name_For_Cascade	The specified policy name "%S" cannot be used for a Cascade Connection security policy setting.
CMD_CascadePolicySet_Invalid_Range	Specify policy "%S" within the range of %s.


# PolicyList command
CMD_PolicyList	Display List of Security Policy Types and Settable Values
CMD_PolicyList_Help	Use this to display a list of item names, descriptions, and settable values in the security policies that can be set for VPN Server users and groups and Cascade Connections. \nBy running the PolicyList command without specifying any parameters, a list of all supported security policy names and descriptions will be displayed. \nBy specifying the name using the PolicyList command parameter, a detailed description related to this value and the type and range of the settable value will be displayed.
CMD_PolicyList_Args	PolicyList [name]
CMD_PolicyList_[name]	This allows you to specify the policy name whose description you want to display. If you don't specify a name, a list of all supported security names and descriptions will be displayed.
CMD_PolicyList_Invalid_Name	The specified policy name is invalid.
CMD_PolicyList_Column_1	Nome da política
CMD_PolicyList_Column_2	Simple description of policy
CMD_PolicyList_Column_3	Valor de configuração:
CMD_PolicyList_Help_1	[Nome da política]
CMD_PolicyList_Help_2	[Simple Description of Policy]
CMD_PolicyList_Help_3	[Range of Settable Values]
CMD_PolicyList_Help_4	[Default Value]
CMD_PolicyList_Help_5	[Detailed Description of Policy]
CMD_PolicyList_Range_Bool	sim ou não
CMD_PolicyList_Range_Int_1	Range from %s to %s (0 cannot be specified)
CMD_PolicyList_Range_Int_2	Range from %s to %s (if 0 is specified, nothing is set)


# CascadeStatusGet command
CMD_CascadeStatusGet	Get Current Cascade Connection Status
CMD_CascadeStatusGet_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified and that Cascade Connection is currently online, use this to get its connection status and other information. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeStatusGet_Args	CascadeStatusGet [name]
CMD_CascadeStatusGet_[name]	Specify the name of the Cascade Connection whose information you want to get.


# CascadeRename command
CMD_CascadeRename	Change Name of Cascade Connection
CMD_CascadeRename_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified, use this to change the name of that Cascade Connection. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeRename_Args	CascadeRename [name] [/NEW:new_name]
CMD_CascadeRename_[name]	Specify the current name of the Cascade Connection whose name you want to change.
CMD_CascadeRename_NEW	Specify the new name after the change. 
CMD_CascadeRename_PROMPT_OLD	Nome atual: 
CMD_CascadeRename_PROMPT_NEW	Novo Nome: 


# CascadeOnline command
CMD_CascadeOnline	Switch Cascade Connection to Online Status
CMD_CascadeOnline_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified, use this to switch that Cascade Connection to online status. The Cascade Connection that is switched to online status begins the process of connecting to the destination VPN Server in accordance with the Connection Setting. The Cascade Connection that is switched to online status will establish normal connection to the VPN Server or continue to attempt connection until it is switched to offline status. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeOnline_Args	CascadeOnline [name]
CMD_CascadeOnline_[name]	Specify the name of the Cascade Connection to switch to online status.


# CascadeOffline command
CMD_CascadeOffline	Switch Cascade Connection to Offline Status
CMD_CascadeOffline_Help	When a Cascade Connection registered on the currently managed Virtual Hub is specified, use this to switch that Cascade Connection to offline status. The Cascade Connection that is switched to offline will not connect to the VPN Server until next time it is switched to the online status using the CascadeOnline command \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CascadeOffline_Args	CascadeOffline [name]
CMD_CascadeOffline_[name]	Specify the name of the Cascade Connection to switch to offline status.


# AccessAdd command
CMD_AccessAdd	Add Access List Rules (IPv4)
CMD_AccessAdd_Help	Use this to add a new rule to the access list of the currently managed Virtual Hub. \nThe access list is a set of packet file rules that are applied to packets that flow through the Virtual Hub. You can register multiple rules in an access list and you can also define an priority for each rule. All packets are checked for the conditions specified by the rules registered in the access list and based on the operation that is stipulated by the first matching rule, they either pass or are discarded. Packets that do not match any rule are implicitly allowed to pass. You can also use the AccessAddEx command to generate delays, jitters and packet losses. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessAdd_Args	AccessAdd [pass|discard] [/MEMO:memo] [/PRIORITY:priority] [/SRCUSERNAME:username] [/DESTUSERNAME:username] [/SRCMAC:mac/mask] [/DESTMAC:mac/mask] [/SRCIP:ip/mask] [/DESTIP:ip/mask] [/PROTOCOL:tcp|udp|icmpv4|icmpv6|ip|num] [/SRCPORT:start-end] [/DESTPORT:start-end] [/TCPSTATE: established|unestablished]
CMD_AccessAdd_[pass|discard]	When a packet matches this rule condition, this operation is decided. When pass is specified, the packet is allowed to pass, and when discard is specified, the packet is discarded.
CMD_AccessAdd_MEMO	Specify a description (memo) for this rule.
CMD_AccessAdd_PRIORITY	Specify an integer of 1 or higher to indicate the priority of the rule. Higher priority is given to rules with the lower priority values.
CMD_AccessAdd_SRCIP	Specify a source IPv4 address as a rule condition. Specify the IPv4 address in the format of "IP Address/Mask" by separating the decimal values using dots such as "192.168.0.1". For the mask, either specify decimal values separated by dots such as "255.255.255.0", or you can specify the bit length from the header using a decimal value such as "24". If you specify "0.0.0.0/0.0.0.0", this means all hosts.
CMD_AccessAdd_DESTIP	Specify a destination IPv4 address as a rule condition in the format of "IP Address/Mask". Use the same method of specification as for the /SRCIP parameter.
CMD_AccessAdd_PROTOCOL	Specify a protocol type as a rule condition. Input the IP protocol number using decimal values or specify one of the keywords "tcp" (TCP/IP protocol, no.6), "udp" (UDP/IP protocol, no.17), "icmpv4" (ICMPv4 protocol, no.1), "icmpv6" (ICMPv6 protocol, no.58) or "ip" (all protocols, no.0). Specify 0 to make the rule apply to all IP protocols.
CMD_AccessAdd_SRCPORT	If the specified protocol is TCP/IP or UDP/IP, specify the source port number as the rule condition. Protocols other than this will be ignored. When this parameter is not specified, the rules will apply to all port numbers. When specifying, do so using the following method "1-1024" (1 to 1024), "23" (only 23).
CMD_AccessAdd_DESTPORT	If the specified protocol is TCP/IP or UDP/IP, specify the destination port number as the rule condition. Protocols other than this will be ignored. Use the same method of specification as for the /SRCPORT parameter.
CMD_AccessAdd_SRCUSERNAME	You can apply this rule to only the packets sent by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAdd_DESTUSERNAME	You can apply this rule to only the packets received by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAdd_SRCMAC	Specify destination MAC address as a rule. Specify MAC address with "-" or ":" separators and hexadecimal number like "00-AC-84-EA-33-BC/FF-FF-FF-FF-FF-00". The separators are skippable. 
CMD_AccessAdd_DESTMAC	Specify destination MAC address as a rule. Use the same method of specification as for the /SRCMAC parameter.
CMD_AccessAdd_TCPSTATE	Specify TCP connection state as a rule. Use Established or Unestablished.
CMD_AccessAdd_Prompt_TYPE	Aprovar ou descartar: 
CMD_AccessAdd_Prompt_MEMO	Descrição da regra (lembrete): 
CMD_AccessAdd_Prompt_PRIORITY	Prioridade da regra: 
CMD_AccessAdd_Eval_PRIORITY	Specify an integer of 1 or higher for the priority.
CMD_AccessAdd_Prompt_SRCIP	Source IP Address ("0.0.0.0/0" specifies all): 
CMD_AccessAdd_Prompt_DESTIP	Destination IP Address ("0.0.0.0/0" specifies all): 
CMD_AccessAdd_Prompt_PROTOCOL	Protocol No. or Protocol Name (tcp/udp/icmpv4/icmpv6/ip): 
CMD_AccessAdd_Prompt_SRCPORT	Source Port Number Range (tcp/udp only): 
CMD_AccessAdd_Prompt_DESTPORT	Destination Port Number Range (tcp/udp only): 
CMD_AccessAdd_Prompt_SRCUSERNAME	Source User Name (all when unspecified): 
CMD_AccessAdd_Prompt_DESTUSERNAME	Destination User Name (all when unspecified): 
CMD_AccessAdd_Prompt_SRCMAC	Source MAC Address and Mask (all when unspecified): 
CMD_AccessAdd_Prompt_DESTMAC	Destination MAC Address and Mask (all when unspecified): 
CMD_AccessAdd_Prompt_TCPSTATE	TCP Connection State (Established/Unestablished): 


# AccessAddEx command
CMD_AccessAddEx	Add Extended Access List Rules (IPv4: Delay, Jitter and Packet Loss Generating)
CMD_AccessAddEx_Help	Use this to add a new rule to the access list of the currently managed Virtual Hub. You can set to generate delays, jitters and packet losses when a packet is passing via the Virtual Hub. \nThe access list is a set of packet file rules that are applied to packets that flow through the Virtual Hub. You can register multiple rules in an access list and you can also define an priority for each rule. All packets are checked for the conditions specified by the rules registered in the access list and based on the operation that is stipulated by the first matching rule, they either pass or are discarded. Packets that do not match any rule are implicitly allowed to pass. You can also use the AccessAddEx command to generate delays, jitters and packet losses. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessAddEx_Args	AccessAddEx [pass|discard] [/MEMO:memo] [/PRIORITY:priority] [/SRCUSERNAME:username] [/DESTUSERNAME:username] [/SRCMAC:mac/mask] [/DESTMAC:mac/mask] [/SRCIP:ip/mask] [/DESTIP:ip/mask] [/PROTOCOL:tcp|udp|icmpv4|icmpv6|ip|num] [/SRCPORT:start-end] [/DESTPORT:start-end] [/TCPSTATE: established|unestablished] [/DELAY:delay_millisec] [/JITTER:jitter_percent] [/LOSS:loss_percent] [/REDIRECTURL:url]
CMD_AccessAddEx_[pass|discard]	When a packet matches this rule condition, this operation is decided. When pass is specified, the packet is allowed to pass, and when discard is specified, the packet is discarded. The setting of delays, jitters and packet losses is applied if the action is pass.
CMD_AccessAddEx_MEMO	Specify a description (memo) for this rule.
CMD_AccessAddEx_PRIORITY	Specify an integer of 1 or higher to indicate the priority of the rule. Higher priority is given to rules with the lower priority values.
CMD_AccessAddEx_SRCIP	Specify a source IPv4 address as a rule condition. Specify the IPv4 address in the format of "IP Address/Mask" by separating the decimal values using dots such as "192.168.0.1". For the mask, either specify decimal values separated by dots such as "255.255.255.0", or you can specify the bit length from the header using a decimal value such as "24". If you specify "0.0.0.0/0.0.0.0", this means all hosts.
CMD_AccessAddEx_DESTIP	Specify a destination IPv4 address as a rule condition in the format of "IP Address/Mask". Use the same method of specification as for the /SRCIP parameter.
CMD_AccessAddEx_PROTOCOL	Specify a protocol type as a rule condition. Input the IP protocol number using decimal values or specify one of the keywords "tcp" (TCP/IP protocol, no.6), "udp" (UDP/IP protocol, no.17), "icmpv4" (ICMPv4 protocol, no.1), "icmpv6" (ICMPv6 protocol, no.58) or "ip" (all protocols, no.0). Specify 0 to make the rule apply to all IP protocols.
CMD_AccessAddEx_SRCPORT	If the specified protocol is TCP/IP or UDP/IP, specify the source port number as the rule condition. Protocols other than this will be ignored. When this parameter is not specified, the rules will apply to all port numbers. When specifying, do so using the following method "1-1024" (1 to 1024), "23" (only 23).
CMD_AccessAddEx_DESTPORT	If the specified protocol is TCP/IP or UDP/IP, specify the destination port number as the rule condition. Protocols other than this will be ignored. Use the same method of specification as for the /SRCPORT parameter.
CMD_AccessAddEx_SRCUSERNAME	You can apply this rule to only the packets sent by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAddEx_DESTUSERNAME	You can apply this rule to only the packets received by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAddEx_SRCMAC	Specify destination MAC address as a rule. Specify MAC address with "-" or ":" separators and hexadecimal number like "00-AC-84-EA-33-BC/FF-FF-FF-FF-FF-00". The separators are skippable. 
CMD_AccessAddEx_DESTMAC	Specify destination MAC address as a rule. Use the same method of specification as for the /SRCMAC parameter.
CMD_AccessAddEx_TCPSTATE	Specify TCP connection state as a rule. Use Established or Unestablished.
CMD_AccessAddEx_DELAY	Set this value to generate delays when packets is passing. Specify the delay period in milliseconds. Specify 0 means no delays to generate. The delays must be 10000 milliseconds at most.
CMD_AccessAddEx_JITTER	Set this value to generate jitters when packets is passing. Specify the ratio of fluctuation of jitters within 0% to 100% range. Specify 0 means no jitters to generate.
CMD_AccessAddEx_LOSS	Set this value to generate packet losses when packets is passing. Specify the ratio of packet losses within 0% to 100% range. Specify 0 means no packet losses to generate.
CMD_AccessAddEx_REDIRECTURL	The specified URL will be mandatory replied to the client as a response for TCP connecting request packets which matches the conditions of this access list entry via this Virtual Hub. To use this setting, you can enforce the web browser of the VPN Client computer to show the specified web site when that web browser tries to access the specific IP address.
CMD_AccessAddEx_Prompt_DELAY	Delays to Generate (in milliseconds: 0 - 10000): 
CMD_AccessAddEx_Prompt_JITTER	Fluctuation of Jitters to Generate (Percent: 0 - 100): 
CMD_AccessAddEx_Prompt_LOSS	Ratio of Packet Losses (Percent: 0 - 100): 
CMD_AccessAddEx_Eval_DELAY	Os atrasos devem ser 10.000 no máximo.
CMD_AccessAddEx_Eval_JITTER	Fluctuation of Jitters must be 100 at maximum.
CMD_AccessAddEx_Eval_LOSS	Ratio of Packet Losses must be 100 at maximum.


# AccessAdd6 command
CMD_AccessAdd6	Add Access List Rules (IPv6)
CMD_AccessAdd6_Help	Use this to add a new rule to the access list of the currently managed Virtual Hub. \nThe access list is a set of packet file rules that are applied to packets that flow through the Virtual Hub. You can register multiple rules in an access list and you can also define an priority for each rule. All packets are checked for the conditions specified by the rules registered in the access list and based on the operation that is stipulated by the first matching rule, they either pass or are discarded. Packets that do not match any rule are implicitly allowed to pass. You can also use the AccessAddEx6 command to generate delays, jitters and packet losses. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessAdd6_Args	AccessAdd6 [pass|discard] [/MEMO:memo] [/PRIORITY:priority] [/SRCUSERNAME:username] [/DESTUSERNAME:username] [/SRCMAC:mac/mask] [/DESTMAC:mac/mask] [/SRCIP:ip/mask] [/DESTIP:ip/mask] [/PROTOCOL:tcp|udp|icmpv4|icmpv6|ip|num] [/SRCPORT:start-end] [/DESTPORT:start-end] [/TCPSTATE: established|unestablished]
CMD_AccessAdd6_[pass|discard]	When a packet matches this rule condition, this operation is decided. When pass is specified, the packet is allowed to pass, and when discard is specified, the packet is discarded.
CMD_AccessAdd6_MEMO	Specify a description (memo) for this rule.
CMD_AccessAdd6_PRIORITY	Specify an integer of 1 or higher to indicate the priority of the rule. Higher priority is given to rules with the lower priority values.
CMD_AccessAdd6_SRCIP	Specify a source IPv6 address as a rule condition. Specify the IPv6 address in the format of "IP Address/Mask" by separating the hexadecimal values using colons such as "2001:200:0:1::". For the mask, either specify hexadecimal values separated by colons such as ffff:ffff:ffff:ffff::, or you can specify the bit length from the header using a decimal value such as "64". If you specify "::/0", this means all hosts.
CMD_AccessAdd6_DESTIP	Specify a destination IPv6 address as a rule condition in the format of "IP Address/Mask". Use the same method of specification as for the /SRCIP parameter.
CMD_AccessAdd6_PROTOCOL	Specify a protocol type as a rule condition. Input the IP protocol number using decimal values or specify one of the keywords "tcp" (TCP/IP protocol, no.6), "udp" (UDP/IP protocol, no.17), "icmpv4" (ICMPv4 protocol, no.1), "icmpv6" (ICMPv6 protocol, no.58) or "ip" (all protocols, no.0). Specify 0 to make the rule apply to all IP protocols.
CMD_AccessAdd6_SRCPORT	If the specified protocol is TCP/IP or UDP/IP, specify the source port number as the rule condition. Protocols other than this will be ignored. When this parameter is not specified, the rules will apply to all port numbers. When specifying, do so using the following method "1-1024" (1 to 1024), "23" (only 23).
CMD_AccessAdd6_DESTPORT	If the specified protocol is TCP/IP or UDP/IP, specify the destination port number as the rule condition. Protocols other than this will be ignored. Use the same method of specification as for the /SRCPORT parameter.
CMD_AccessAdd6_SRCUSERNAME	You can apply this rule to only the packets sent by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAdd6_DESTUSERNAME	You can apply this rule to only the packets received by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAdd6_SRCMAC	Specify destination MAC address as a rule. Specify MAC address with "-" or ":" separators and hexadecimal number like "00-AC-84-EA-33-BC/FF-FF-FF-FF-FF-00". The separators can be skipped.
CMD_AccessAdd6_DESTMAC	Specify destination MAC address as a rule. Use the same method of specification as for the /SRCMAC parameter.
CMD_AccessAdd6_TCPSTATE	Specify TCP connection state as a rule. Use Established or Unestablished.
CMD_AccessAdd6_Prompt_TYPE	Aprovar ou descartar: 
CMD_AccessAdd6_Prompt_MEMO	Descrição da regra (lembrete): 
CMD_AccessAdd6_Prompt_PRIORITY	Prioridade da regra: 
CMD_AccessAdd6_Eval_PRIORITY	Specify an integer of 1 or higher for the priority.
CMD_AccessAdd6_Prompt_SRCIP	Source IP Address ("::/0" specifies all): 
CMD_AccessAdd6_Prompt_DESTIP	Destination IP Address ("::/0" specifies all): 
CMD_AccessAdd6_Prompt_PROTOCOL	Protocol No. or Protocol Name (tcp/udp/icmpv4/icmpv6/ip): 
CMD_AccessAdd6_Prompt_SRCPORT	Source Port Number Range (tcp/udp only): 
CMD_AccessAdd6_Prompt_DESTPORT	Destination Port Number Range (tcp/udp only): 
CMD_AccessAdd6_Prompt_SRCUSERNAME	Source User Name (all when unspecified): 
CMD_AccessAdd6_Prompt_DESTUSERNAME	Destination User Name (all when unspecified): 
CMD_AccessAdd6_Prompt_SRCMAC	Source MAC Address and Mask (all when unspecified): 
CMD_AccessAdd6_Prompt_DESTMAC	Destination MAC Address and Mask (all when unspecified): 
CMD_AccessAdd6_Prompt_TCPSTATE	TCP Connection State (Established/Unestablished): 


# AccessAddEx6 command
CMD_AccessAddEx6	Add Extended Access List Rules (IPv6: Delay, Jitter and Packet Loss Generating)
CMD_AccessAddEx6_Help	Use this to add a new rule to the access list of the currently managed Virtual Hub. You can set to generate delays, jitters and packet losses when a packet is passing via the Virtual Hub. \nThe access list is a set of packet file rules that are applied to packets that flow through the Virtual Hub. You can register multiple rules in an access list and you can also define a priority for each rule. All packets are checked for the conditions specified by the rules registered in the access list and based on the operation that is stipulated by the first matching rule, they either pass or are discarded. Packets that do not match any rule are implicitly allowed to pass. You can also use the AccessAddEx6 command to generate delays, jitters and packet losses. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessAddEx6_Args	AccessAddEx6 [pass|discard] [/MEMO:memo] [/PRIORITY:priority] [/SRCUSERNAME:username] [/DESTUSERNAME:username] [/SRCMAC:mac/mask] [/DESTMAC:mac/mask] [/SRCIP:ip/mask] [/DESTIP:ip/mask] [/PROTOCOL:tcp|udp|icmpv4|icmpv6|ip|num] [/SRCPORT:start-end] [/DESTPORT:start-end] [/TCPSTATE: established|unestablished] [/DELAY:delay_millisec] [/JITTER:jitter_percent] [/LOSS:loss_percent] [/REDIRECTURL:url]
CMD_AccessAddEx6_[pass|discard]	When a packet matches this rule condition, this operation is decided. When pass is specified, the packet is allowed to pass, and when discard is specified, the packet is discarded. The setting of delays, jitters and packet losses is applied if the action is pass.
CMD_AccessAddEx6_MEMO	Specify a description (memo) for this rule.
CMD_AccessAddEx6_PRIORITY	Specify an integer of 1 or higher to indicate the priority of the rule. Higher priority is given to rules with the lower priority values.
CMD_AccessAddEx6_SRCIP	Specify a source IPv6 address as a rule condition. Specify the IPv6 address in the format of "IP Address/Mask" by separating the hexadecimal values using colons such as "2001:200:0:1::". For the mask, either specify hexadecimal values separated by colons such as "ffff:ffff:ffff:ffff::", or you can specify the bit length from the header using a decimal value such as 64. If you specify "::/0", this means all hosts.
CMD_AccessAddEx6_DESTIP	Specify a destination IPv6 address as a rule condition in the format of "IP Address/Mask". Use the same method of specification as for the /SRCIP parameter.
CMD_AccessAddEx6_PROTOCOL	Specify a protocol type as a rule condition. Input the IP protocol number using decimal values or specify one of the keywords "tcp" (TCP/IP protocol, no.6), "udp" (UDP/IP protocol, no.17), "icmpv4" (ICMPv4 protocol, no.1), "icmpv6" (ICMPv6 protocol, no.58) or "ip" (all protocols, no.0). Specify 0 to make the rule apply to all IP protocols.
CMD_AccessAddEx6_SRCPORT	If the specified protocol is TCP/IP or UDP/IP, specify the source port number as the rule condition. Protocols other than this will be ignored. When this parameter is not specified, the rules will apply to all port numbers. When specifying, do so using the following method "1-1024" (1 to 1024), "23" (only 23).
CMD_AccessAddEx6_DESTPORT	If the specified protocol is TCP/IP or UDP/IP, specify the destination port number as the rule condition. Protocols other than this will be ignored. Use the same method of specification as for the /SRCPORT parameter.
CMD_AccessAddEx6_SRCUSERNAME	You can apply this rule to only the packets sent by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAddEx6_DESTUSERNAME	You can apply this rule to only the packets received by a user session of a user name that has been specified as a rule condition. In this case, specify the user name.
CMD_AccessAddEx6_SRCMAC	Specify destination MAC address as a rule. Specify MAC address with "-" or ":" separators and hexadecimal number like "00-AC-84-EA-33-BC/FF-FF-FF-FF-FF-00". The separators can be skipped.
CMD_AccessAddEx6_DESTMAC	Specify destination MAC address as a rule. Use the same method of specification as for the /SRCMAC parameter.
CMD_AccessAddEx6_TCPSTATE	Specify TCP connection state as a rule. Use Established or Unestablished.
CMD_AccessAddEx6_DELAY	Set this value to generate delays when packets is passing. Specify the delay period in milliseconds. Specify 0 means no delays to generate. The delays must be 10000 milliseconds at most.
CMD_AccessAddEx6_JITTER	Set this value to generate jitters when packets is passing. Specify the ratio of fluctuation of jitters within 0% to 100% range. Specify 0 means no jitters to generate.
CMD_AccessAddEx6_LOSS	Set this value to generate packet losses when packets is passing. Specify the ratio of packet losses within 0% to 100% range. Specify 0 means no packet losses to generate.
CMD_AccessAddEx6_REDIRECTURL	The specified URL will be mandatory replied to the client as a response for TCP connecting request packets which matches the conditions of this access list entry via this Virtual Hub. To use this setting, you can enforce the web browser of the VPN Client computer to show the specified web site when that web browser tries to access the specific IP address.
CMD_AccessAddEx6_Prompt_DELAY	Delays to Generate (in milliseconds: 0 - 10000): 
CMD_AccessAddEx6_Prompt_JITTER	Fluctuation of Jitters to Generate (Percent: 0 - 100): 
CMD_AccessAddEx6_Prompt_LOSS	Ratio of Packet Losses (Percent: 0 - 100): 
CMD_AccessAddEx6_Eval_DELAY	Os atrasos devem ser 10.000 no máximo.
CMD_AccessAddEx6_Eval_JITTER	Fluctuation of Jitters must be 100 at maximum.
CMD_AccessAddEx6_Eval_LOSS	Ratio of Packet Losses must be 100 at maximum.


# AccessList command
CMD_AccessList	Get Access List Rule List 
CMD_AccessList_Help	Use this to get a list of packet filter rules that are registered on access list of the currently managed Virtual Hub. \nThe access list is a set of packet file rules that are applied to packets that flow through the Virtual Hub. You can register multiple rules in an access list and you can also define a priority for each rule. All packets are checked for the conditions specified by the rules registered in the access list and based on the operation that is stipulated by the first matching rule, they either pass or are discarded. Packets that do not match any rule are implicitly allowed to pass. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessList_Args	ListaAcess


# AccessDelete command
CMD_AccessDelete	Delete Rule from Access List
CMD_AccessDelete_Help	Use this to specify a packet filter rule registered on the access list of the currently managed Virtual Hub and delete it. \nTo delete a rule, you must specify that rule's ID. You can display the ID by using the AccessList command. \nIf you wish not to delete the rule but to only temporarily disable it, use the AccessDisable command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessDelete_Args	AccessDelete [id]
CMD_AccessDelete_[id]	Specify either the ID or the Unique ID of the rule to delete.
CMD_Access_Prompt_ID	Access List Rule ID or Unique ID: 


# AccessEnable command
CMD_AccessEnable	Enable Access List Rule
CMD_AccessEnable_Help	Use this to specify a packet filter rule registered on the access list of the currently managed Virtual Hub and enable it. The enabled rule will be used by packet filtering. \nTo enable a rule, you must specify that rule's ID. You can display the ID by using the AccessList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessEnable_Args	AccessEnable [id]
CMD_AccessEnable_[id]	Specify the ID of the rule to enable.


# AccessDisable command
CMD_AccessDisable	Disable Access List Rule
CMD_AccessDisable_Help	Use this to specify a packet filter rule registered on the access list of the currently managed Virtual Hub and disable it. The disabled rule will be used by packet filtering. \nTo disable a rule, you must specify that rule's ID. You can display the ID by using the AccessList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_AccessDisable_Args	AccessDisable [id]
CMD_AccessDisable_[id]	Specify the ID of the rule to disable.


# UserList command
CMD_UserList	Get List of Users
CMD_UserList_Help	Use this to get a list of users that are registered on the security account database of the currently managed Virtual Hub. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserList_Args	ListaUser


# UserCreate command
CMD_UserCreate	Criar usuário 
CMD_UserCreate_Help	Use this to create a new user in the security account database of the currently managed Virtual Hub. \nBy creating a user, the VPN Client can connect to the Virtual Hub by using the authentication information of that user. \nWhen a user is created using the UserCreate command and the auth type of that user is registered as Password Authentication, a random string will be assigned as the password. Therefore, that user will not be able to connect to the Virtual Hub in that state. After creating the user, you must always use the UserPasswordSet command to specify the user password, or alternatively use the UserAnonymousSet command, UserCertSet command, UserSignedSet command, UserRadiusSet command or UserNTLMSet command to change the user's auth type. \nNote that a user whose user name has been created as "*" (a single asterisk character) will automatically be registered as a RADIUS authentication user. For cases where there are users with "*" as the name, when a user, whose user name that has been provided when a client connected to a VPN Server does not match existing user names, is able to be authenticated by a RADIUS server or NT domain controller by inputting a user name and password, the authentication settings and security policy settings will follow the setting for the user "*". \nTo change the user information of a user that has been created, use the UserSet command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserCreate_Args	UserCreate [name] [/GROUP:group] [/REALNAME:realname] [/NOTE:note]
CMD_UserCreate_[name]	Specify the user name of the user to be newly created.
CMD_UserCreate_GROUP	When assigning a user in a group, specify the group name. When not assigning a user to any group, specify /GROUP:none. 
CMD_UserCreate_REALNAME	Specify the user's full name. If you are not specifying this, specify /REALNAME:none.
CMD_UserCreate_NOTE	Specify a description of the user. If you are not specifying this, specify /NOTE:none
CMD_UserCreate_Prompt_NAME	Nome de usuário: 
CMD_UserCreate_Prompt_GROUP	Assigned Group Name: 
CMD_UserCreate_Prompt_REALNAME	User Full Name: 
CMD_UserCreate_Prompt_NOTE	User Description: 


# UserSet command
CMD_UserSet	Change User Information
CMD_UserSet_Help	Use this to change user information that is registered on the security account database of the currently managed Virtual Hub. \nThe user information that can be changed using this command are the three items that are specified when a new user is created using the UserCreate command: Group Name, Full Name, and Description. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserSet_Args	UserSet [name] [/GROUP:group] [/REALNAME:realname] [/NOTE:note]
CMD_UserSet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserSet_GROUP	When assigning a user in a group, specify the group name. When not assigning a user to any group, specify /GROUP:none. 
CMD_UserSet_REALNAME	Specify the user's full name. If you are not specifying this, specify /REALNAME:none
CMD_UserSet_NOTE	Specify a description of the user. If you are not specifying this, specify /NOTE:none.


# UserDelete command
CMD_UserDelete	Excluir usuário
CMD_UserDelete_Help	Use this to delete a user that is registered on the security account database of the currently managed Virtual Hub. By deleting the user, that user will no long be able to connect to the Virtual Hub. \nYou can use the UserPolicySet command to instead of deleting a user, set the user to be temporarily denied from logging in. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserDelete_Args	UserDelete [name]
CMD_UserDelete_[name]	Specify the name of the user to delete.


# UserGet command
CMD_UserGet	Get User Information
CMD_UserGet_Help	Use this to get user registration information that is registered on the security account database of the currently managed Virtual Hub. \nThe information that you can get using this command are User Name, Full Name, Group Name, Expiration Date, Security Policy, and Auth Type, as well as parameters that are specified as auth type attributes and the statistical data of that user. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserGet_Args	UserGet [name]
CMD_UserGet_[name]	Specify the user name of the user whose information you want to get.
CMD_UserGet_Column_Name	Nome de usuário
CMD_UserGet_Column_RealName	Nome completo
CMD_UserGet_Column_Note	Descrição
CMD_UserGet_Column_Group	Nome do grupo
CMD_UserGet_Column_Expires	Data de validade
CMD_UserGet_Column_AuthType	Tipo Auth
CMD_UserGet_Column_UserCert	Registered User Individual Certificate
CMD_UserGet_Column_RadiusAlias	External Authentication Server Authentication User Name
CMD_UserGet_Column_RootCert_CN	Limit of Certificate CN Value
CMD_UserGet_Column_RootCert_SERIAL	Limit of Certificate Serial Number
CMD_UserGet_Policy	Security Policy Set for this User


# UserAnonymousSet command
CMD_UserAnonymousSet	Set Anonymous Authentication for User Auth Type
CMD_UserAnonymousSet_Help	Use this to set Anonymous Authentication as the auth type for a user that is registered on the security account database of the currently managed Virtual Hub. A VPN Client that has connected to a Virtual Hub using a user name of a user set to anonymous authentication can connect to a Virtual Hub without undergoing user authentication and without conditions. The anonymous authentication function is ideally suited to public VPN Servers that are setup to allow anyone to connect via the Internet etc. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserAnonymousSet_Args	UserAnonymousSet [name]
CMD_UserAnonymousSet_[name]	Specify the user name of the user whose setting you want to change.


# UserPasswordSet command
CMD_UserPasswordSet	Set Password Authentication for User Auth Type and Set Password
CMD_UserPasswordSet_Help	Use this to set Password Authentication as the auth type for a user that is registered on the security account database of the currently managed Virtual Hub. Password Authentication requires a user-defined password to be set for the user object in the security account database of the Virtual Hub and when a user attempts to connect to the Virtual Hub using this user name, they will be prompted to input a password and if it is the matching password, connection will be allowed. \nThe user password is actually saved in hash code which means even if the VPN Server setting file is analyzed, the original password cannot be deciphered. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserPasswordSet_Args	UserPasswordSet [name] [/PASSWORD:password]
CMD_UserPasswordSet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserPasswordSet_PASSWORD	Specify the password to be set for the user. If this parameter is not specified a prompt will appear to input the password.


# UserCertSet command
CMD_UserCertSet	Set Individual Certificate Authentication for User Auth Type and Set Certificate
CMD_UserCertSet_Help	Use this to set Individual Certificate Authentication as the Auth Type for a user that is registered on the security account database of the currently managed Virtual Hub. Individual Certificate Authentication requires one X.509 format certificate to be set for the user object in the security account database of the Virtual Hub and when a user attempts to connect to the Virtual Hub using this user name, an RSA algorithm is used to verify if the provided certificate matches the registered certificate and whether the client holds a private key that corresponds to that certificate and if so, connection is allowed. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserCertSet_Args	UserCertSet [name] [/LOADCERT:cert]
CMD_UserCertSet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserCertSet_LOADCERT	Specify the certificate to set for the user by specifying an X.509 format certificate file.


# UserCertGet command
CMD_UserCertGet	Get Certificate Registered for Individual Certificate Authentication User
CMD_UserCertGet_Help	Use this to get an X.509 format certificate registered for a user of Individual Certificate Authentication who is registered in the security account database of the currently managed Virtual Hub and save it to file. \nIf the specified user is not set as Individual Certificate Authentication an error will occur. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserCertGet_Args	UserCertGet [name] [/SAVECERT:cert]
CMD_UserCertGet_[name]	Specify the user name of the user whose information you want to get.
CMD_UserCertGet_SAVECERT	Specify the file name to save, in X.509 format, the user certificate you obtained.
CMD_UserCertGet_Not_Cert	Either the user is not set as individual certificate authentication or a unique certificate is not set.


# UserSignedSet command
CMD_UserSignedSet	Set Signed Certificate Authentication for User Auth Type
CMD_UserSignedSet_Help	Use this to set Signed Certificate Authentication as the auth type for a user that is registered on the security account database of the currently managed Virtual Hub. When a user connects to a Virtual Hub using a user name that is set for signed certificate authentication, an RSA algorithm is used to verify whether the certificate provided by the user is signed by any of the certificates in the list of trusted CA certificates of that Virtual Hub and whether the client holds a private key that corresponds with that certificate, and if so, connection is allowed. \nIt is also possible to set the connection to be allowed only when a certificate common name (CN) and serial number that is expected for each user is registered and the contents of the certificate after the abovementioned verification is passed matches the set value. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserSignedSet_Args	UserSignedSet [name] [/CN:cn] [/SERIAL:serial]
CMD_UserSignedSet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserSignedSet_CN	When this parameter is set, after it has been verified that the certificate that the user provided has been signed by the trusted certificate authority, connection will only be allowed when the value of the common name (CN) of this certificate is compared with the value set by this parameter and the values match. When "none" is specified, this check is not made.
CMD_UserSignedSet_SERIAL	When this parameter is set, after it has been verified that the certificate that the user provided has been signed by the trusted certificate authority, connection will only be allowed when the value of the serial number of this certificate is compared with the value set by this parameter and the values match. When "none" is specified, this check is not made.
CMD_UserSignedSet_Prompt_CN	Limit of Common Name (CN) Value: 
CMD_UserSignedSet_Prompt_SERIAL	Limit of Serial Number Value: 


# UserRadiusSet command
CMD_UserRadiusSet	Set RADIUS Authentication for User Auth Type
CMD_UserRadiusSet_Help	Use this to set RADIUS Authentication as the auth type for a user that is registered on the security account database of the currently managed Virtual Hub. When a user connects to a Virtual Hub using a user name that is set for RADIUS authentication, the user name and the user input password is sent to the RADIUS server where the RADIUS SERVER checks the user name and password, then if the verification is successful, that user is allowed VPN connection. \nIn order to user RADIUS authentication, the RADIUS server used for this verification must be set in the Virtual Hub beforehand by using the RadiusServerSet command. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserRadiusSet_Args	UserRadiusSet [name] [/ALIAS:alias_name]
CMD_UserRadiusSet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserRadiusSet_ALIAS	When this parameter is set, it is possible to make the user name sent to the RADIUS server different to the user name on the Virtual Hub. When this is not set, please specify /ALIAS:none (the user name on the Virtual Hub will be used). If the user name is "*", the /ALIAS parameter will be ignored. To read an explanation of the "*" user, please input UserCreate/HELP to display this information.
CMD_UserRadiusSet_Prompt_ALIAS	Alias Name for Authentication (Optional): 


# UserNTLMSet command
CMD_UserNTLMSet	Set NT Domain Authentication for User Auth Type
CMD_UserNTLMSet_Help	Use this to set NT Domain Authentication as the auth type for a user that is registered on the security account database of the currently managed Virtual Hub. When a user connects to a Virtual Hub using a user name that is set for NT Domain authentication, the user name and the user input password is sent to the Windows NT / 2000 / Server 2003 / Server 2008 / Server 2008 R2 / Server 2012 Domain Controller or Active Directory Server where the server checks the user name and password, then if the verification is successful, that user is allowed VPN connection. \nTo use NT Domain authentication, the VPN Server must be operating on a Windows NT 4.0, Windows 2000, Windows XP, Windows Vista, Windows Server 2008, Windows Server 2008 R2 or Windows Server 2012 operating system that is connected to that domain. For details please contact the VPN Server's administrator. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserNTLMSet_Args	UserNTLMSet [name] [/ALIAS:alias_name]
CMD_UserNTLMSet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserNTLMSet_ALIAS	When this parameter is set, it is possible to make the user name sent to the NT Domain or Active Directory server different to the user name on the Virtual Hub. When this is not set, please specify /ALIAS:none (the user name on the Virtual Hub will be used). If the user name is "*", the /ALIAS parameter will be ignored. To read an explanation of the "*" user, please input UserCreate/HELP to display this information.


# UserPolicyRemove command
CMD_UserPolicyRemove	Delete User Security Policy
CMD_UserPolicyRemove_Help	Use this to delete the security policy setting that is set for a user that is registered on the security account database of the currently managed Virtual Hub. A user who has had their security policy setting deleted will be assigned the security policy setting of the group that user is assigned to. In the cases where the user is not assigned to a group or when a security policy setting has not been set for the group, the default values (Allow Access: Enabled, Maximum Number of TCP Connections: 32, Time-out Period: 20 seconds) will be applied. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserPolicyRemove_Args	UserPolicyRemove [name]
CMD_UserPolicyRemove_[name]	Specify the user name of the user whose setting you want to change.


# UserPolicySet command
CMD_UserPolicySet	Set User Security Policy
CMD_UserPolicySet_Help	Use this to set the security policy contents that are set for a user that is registered on the security account database of the currently managed Virtual Hub. \nWhen a user has not been set a security policy, use this to change the specified values after a new default security policy has been set. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserPolicySet_Args	UserPolicySet [name] [/NAME:policy_name] [/VALUE:num|yes|no]
CMD_UserPolicySet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserPolicySet_NAME	Specify the name of policy whose values you want to change. You can use the PolicyList command to display a list of policy names and values that can be set.
CMD_UserPolicySet_VALUE	Specify a new policy value. If the policy is an integer value, specify an integer. Specify yes or no for Boolean types. You can view the type and value that can be set by using the PolicyList command.


# UserExpiresSet command
CMD_UserExpiresSet	Set User's Expiration Date
CMD_UserExpiresSet_Help	Use this to set the user's expiration date that is registered on the security account database of the currently managed Virtual Hub. A user whose expiration date has expired cannot connect to the Virtual Hub. \nTo get the list of currently registered users, use the UserList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_UserExpiresSet_Args	UserExpiresSet [name] [/EXPIRES:expires]
CMD_UserExpiresSet_[name]	Specify the user name of the user whose setting you want to change.
CMD_UserExpiresSet_EXPIRES	Specify the user expiration date and time. The date and time must be in the same format as "2005/10/08 19:30:00" where 6 integers are specified, representing year/month/day hour:minute:second separated by forward slashes, a space and then colons. Specify 4 digits for the year. If you put a space in a value, the entire value must be enclosed by "". For this specification, local time (standard time for the computer on which the command line management utility is running) can be specified. By specifying /EXPIRES:none, you can remove the expiration date restriction.
CMD_UserExpiresSet_Prompt_EXPIRES	User Expiration Date (no expiration if nothing specified): 


# GroupList command
CMD_GroupList	Get List of Groups
CMD_GroupList_Help	Use this to get a list of groups that are registered on the security account database of the currently managed Virtual Hub. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupList_Args	ListaGroup


# GroupCreate command
CMD_GroupCreate	Criar grupo
CMD_GroupCreate_Help	Use this to create a new group in the security account database of the currently managed Virtual Hub. \nYou can register multiple users in a group. To register users in a group use the GroupJoin command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupCreate_Args	GroupCreate [name] [/REALNAME:realname] [/NOTE:note]
CMD_GroupCreate_[name]	Specify the name of the group to create.
CMD_GroupCreate_REALNAME	Specify the group's full name. For example, if the group corresponds to an actual section or department name, specify that name. If you are not specifying this, specify /REALNAME:none
CMD_GroupCreate_NOTE	Specify a description of the group. If you are not specifying this, specify /NOTE:none
CMD_GroupCreate_Prompt_NAME	Nome do grupo: 
CMD_GroupCreate_Prompt_REALNAME	Group Full Name: 
CMD_GroupCreate_Prompt_NOTE	Group Description: 


# GroupSet command
CMD_GroupSet	Set Group Information
CMD_GroupSet_Help	Use this to set group information that is registered on the security account database of the currently managed Virtual Hub. \nTo get the list of currently registered groups, use the GroupList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupSet_Args	GroupSet [name] [/REALNAME:realname] [/NOTE:note]
CMD_GroupSet_[name]	Specify the group name of the group whose setting you want to change.
CMD_GroupSet_REALNAME	Specify the group's Full name. For example, if the group corresponds to an actual section or department name, specify that name. If you are not specifying this, specify /REALNAME:none
CMD_GroupSet_NOTE	Specify a description of the group. If you are not specifying this, specify /NOTE:none.


# GroupDelete command
CMD_GroupDelete	Excluir grupo
CMD_GroupDelete_Help	Use this to delete a group that is registered on the security account database of the currently managed Virtual Hub. \nWhen you delete a group all users assigned to that group will become unassigned. \nTo get the list of currently registered groups, use the GroupList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupDelete_Args	GroupDelete [name]
CMD_GroupDelete_[name]	Specify the name of the group to delete.


# GroupGet command
CMD_GroupGet	Get Group Information and List of Assigned Users
CMD_GroupGet_Help	Use this to get the information of a group that is registered on the security account database of the currently managed Virtual Hub as well as a list of users assigned to that group. \nTo get the list of currently registered groups, use the GroupList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupGet_Args	GroupGet [name]
CMD_GroupGet_[name]	Specify the group name of the group whose information you want to get.
CMD_GroupGet_Column_NAME	Nome do grupo
CMD_GroupGet_Column_REALNAME	Nome completo
CMD_GroupGet_Column_NOTE	Descrição
CMD_GroupGet_Column_POLICY	This is the security policy that is set for this group.
CMD_GroupGet_Column_MEMBERS	This is a list of user names of users who are assigned to this group.


# GroupJoin command
CMD_GroupJoin	Add User to Group
CMD_GroupJoin_Help	Use this to add a user in the security account database of the currently managed Virtual Hub to a group that is registered on that security account database. \nTo get a list of users and groups that are currently registered, use the UserList command and the GroupList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupJoin_Args	GroupJoin [name] [/USERNAME:username]
CMD_GroupJoin_[name]	Specify the group name of the group to which you want to add a user.
CMD_GroupJoin_USERNAME	Specify the user name of the user you want to add to the group specified by "name".
CMD_GroupJoin_Prompt_USERNAME	Name of User to Join Group: 


# GroupUnjoin command
CMD_GroupUnjoin	Delete User from Group
CMD_GroupUnjoin_Help	Use this to delete a specified user from the group that is registered on the security account database of the currently managed Virtual Hub. By deleting a user from the group, that user becomes unassigned. \nTo get a list of users that are currently assigned to a group, use the GroupGet command. \nTo get the list of currently registered groups, use the GroupList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupUnjoin_Args	GroupUnjoin [name]
CMD_GroupUnjoin_[name]	Specify the name of the user to delete from the group.
CMD_GroupUnjoin_Prompt_name	Name of User to Delete from Group: 


# GroupPolicyRemove command
CMD_GroupPolicyRemove	Delete Group Security Policy
CMD_GroupPolicyRemove_Help	Use this to delete the security policy setting that is set for a group that is registered on the security account database of the currently managed Virtual Hub. Users who do not have a security policy set for the user themselves or for the group they are assigned to, will have the default values (Allow Access: Enabled, Maximum Number of TCP Connections: 32, Time-out Period: 20 seconds) applied to them. \nTo get the list of currently registered groups, use the GroupList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupPolicyRemove_Args	GroupPolicyRemove [name]
CMD_GroupPolicyRemove_[name]	Specify the group name of the group whose setting you want to change.


# GroupPolicySet command
CMD_GroupPolicySet	Set Group Security Policy
CMD_GroupPolicySet_Help	Use this to set the security policy contents that are set for a group that is registered on the security account database of the currently managed Virtual Hub. \nWhen a group has not been set a security policy, use this to change the specified values after a new default security policy has been set. \nTo get the list of currently registered groups, use the GroupList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a member server on a cluster.
CMD_GroupPolicySet_Args	GroupPolicySet [name] [/NAME:policy_name] [/VALUE:num|yes|no]
CMD_GroupPolicySet_[name]	Specify the group name of the group whose setting you want to change.
CMD_GroupPolicySet_NAME	Specify the name of policy whose values you want to change. You can use the PolicyList command to display a list of policy names and values that can be set.
CMD_GroupPolicySet_VALUE	Specify a new policy value. If the policy is an integer value, specify an integer. Specify yes or no for Boolean types. You can view the type and value that can be set by using the PolicyList command.


# SessionList command
CMD_SessionList	Get List of Connected Sessions
CMD_SessionList_Help	Use this to get a list of the sessions connected to the Virtual Hub currently being managed. In the list of sessions, the following information will be displayed for each connection: Session Name, Session Site, User Name, Source Host Name, TCP Connection, Transfer Bytes and Transfer Packets. \nIf the currently connected VPN Server is a cluster controller and the currently managed Virtual Hub is a static Virtual Hub, you can get an all-linked-together list of all sessions connected to that Virtual Hub on all cluster members. \nIn all other cases, only the list of sessions that are actually connected to the currently managed VPN Server will be obtained.
CMD_SessionList_Args	SessionList


# SessionGet command
CMD_SessionGet	Get Session Information
CMD_SessionGet_Help	Use this to specify a session currently connected to the currently managed Virtual Hub and get the session information. The session information includes the following: source host name and user name, version information, time information, number of TCP connections, communication parameters, session key, statistical information on data transferred, and other client and server information. \nTo get the list of currently connected sessions, use the SessionList command.
CMD_SessionGet_Args	SessionGet [name]
CMD_SessionGet_[name]	Specify the session name of the session whose information you want to get.
CMD_SessionGet_Prompt_NAME	Nome da sessão: 


# SessionDisconnect command
CMD_SessionDisconnect	Disconnect Session
CMD_SessionDisconnect_Help	Use this to specify a session currently connected to the currently managed Virtual Hub and forcefully disconnect that session using manager privileges. \nNote that when communication is disconnected by settings on the source client side and the automatically reconnect option is enabled, it is possible that the client will reconnect. \nTo get the list of currently connected sessions, use the SessionList command.
CMD_SessionDisconnect_Args	SessionDisconnect [name]
CMD_SessionDisconnect_[name]	Specify the session name of the session to disconnect.


# MacTable command
CMD_MacTable	Get the MAC Address Table Database
CMD_MacTable_Help	Use this to get the MAC address table database that is held by the currently managed Virtual Hub. \nThe MAC address table database is a table that the Virtual Hub requires to perform the action of switching Ethernet frames and the Virtual Hub decides the sorting destination session of each Ethernet frame based on the MAC address table database. The MAC address database is built by the Virtual Hub automatically analyzing the contents of the communication throughput. \nBy specifying the session name you can get the MAC address table entry that has been associated with that session.
CMD_MacTable_Args	MacTable [session_name]
CMD_MacTable_[session_name]	By specifying the session name as a parameter, you can display only the MAC address table entry that is associated with that session. When this is left unspecified, all the entries will be displayed.


# MacDelete command
CMD_MacDelete	Delete MAC Address Table Entry
CMD_MacDelete_Help	Use this command to operate the MAC address table database held by the currently managed Virtual Hub and delete a specified MAC address table entry from the database. \nTo get the contents of the current MAC address table database use the MacTable command.
CMD_MacDelete_Args	MacDelete [id]
CMD_MacDelete_[id]	Specify the ID of the MAC address table entry to delete.
CMD_MacDelete_Prompt	ID a ser excluído: 


# IpTable command
CMD_IpTable	Get the IP Address Table Database
CMD_IpTable_Help	Use this to get the IP address table database that is held by the currently managed Virtual Hub. \nThe IP address table database is a table that is automatically generated by analyzing the contents of communication so that the Virtual Hub can always know which session is using which IP address and it is frequently used by the engine that applies the Virtual Hub security policy. \nBy specifying the session name you can get the IP address table entry that has been associated with that session.
CMD_IpTable_Args	IpTable [session_name]
CMD_IpTable_[session_name]	By specifying the session name as a parameter, you can display only the IP address table entry that is associated with that session. When this is left unspecified, all the entries will be displayed.


# IpDelete command
CMD_IpDelete	Delete IP Address Table Entry
CMD_IpDelete_Help	Use this command to operate the IP address table database held by the currently managed Virtual Hub and delete a specified IP address table entry from the database. \nTo get the contents of the current IP address table database use the IpTable command.
CMD_IpDelete_Args	IpDelete [id]
CMD_IpDelete_[id]	Specify the ID of the IP address table entry to delete.


# SecureNatEnable command
CMD_SecureNatEnable	Enable the Virtual NAT and DHCP Server Function (SecureNat Function)
CMD_SecureNatEnable_Help	Use this to enable the Virtual NAT and DHCP Server function (SecureNat Function) on the currently managed Virtual Hub and begin its operation. Before executing this command, you must first check the setting contents of the current Virtual NAT function and DHCP Server function using the SecureNatHostGet command, NatGet command and DhcpGet command. \nBy enabling the SecureNAT function, you can virtually operate a NAT router (IP masquerade) and the DHCP Server function on a virtual network on the Virtual Hub. \n\n[Warning about SecureNAT Function]\nThe SecureNAT function is recommended only for system administrators and people with a detailed knowledge of networks. \nIf you use the SecureNAT function correctly, it is possible to achieve a safe form of remote access via a VPN. However when used in the wrong way, it can put the entire network in danger. Anyone who does not have a thorough knowledge of networks and anyone who does not have the network administrator's permission must not enable the SecureNAT function. For a detailed explanation of the SecureNAT function, please refer to the VPN Server's manual and online documentation. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SecureNatEnable_Args	SecureNatEnable


# SecureNatDisable command
CMD_SecureNatDisable	Disable the Virtual NAT and DHCP Server Function (SecureNat Function)
CMD_SecureNatDisable_Help	Use this to disable the Virtual NAT and DHCP Server function (SecureNat Function) on the currently managed Virtual Hub. By executing this command the Virtual NAT function immediately stops operating and the Virtual DHCP Server function deletes the DHCP lease database and stops the service. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SecureNatDisable_Args	SecureNatDisable


# SecureNatStatusGet command
CMD_SecureNatStatusGet	Get the Operating Status of the Virtual NAT and DHCP Server Function (SecureNat Function)
CMD_SecureNatStatusGet_Help	Use this to get the operating status of the Virtual NAT and DHCP Server function (SecureNat Function) when it is operating on the currently managed Virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SecureNatStatusGet_Args	SecureNatStatusGet


# SecureNatHostGet command
CMD_SecureNatHostGet	Get Network Interface Setting of Virtual Host of SecureNAT Function
CMD_SecureNatHostGet_Help	Use this to get the virtual host network interface setting from the setting items of the Virtual NAT and DHCP Server function (SecureNAT function) on the currently managed Virtual Hub. \nThe SecureNAT function holds one virtual network adapter on the L2 segment inside the Virtual Hub and it has been assigned a MAC address and an IP address. By doing this, another host connected to the same L2 segment is able to communicate with the SecureNAT virtual host as if it is an actual IP host existing on the network. \n\n[Warning about SecureNAT Function]\nThe SecureNAT function is recommended only for system administrators and people with a detailed knowledge of networks. \nIf you use the SecureNAT function correctly, it is possible to achieve a safe form of remote access via a VPN. However when used in the wrong way, it can put the entire network in danger. Anyone who does not have a thorough knowledge of networks and anyone who does not have the network administrators permission must not enable the SecureNAT function. For a detailed explanation of the SecureNAT function, please refer to the VPN Server's manual and online documentation. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SecureNatHostGet_Args	SecureNatHostGet
CMD_SecureNatHostGet_Column_MAC	Endereço MAC
CMD_SecureNatHostGet_Column_IP	Endereço IP
CMD_SecureNatHostGet_Column_MASK	Máscara de sub-rede
CMD_SecureNatHostGet_Column_LOG	Save NAT and DHCP Operation Log


# SecureNatHostSet command
CMD_SecureNatHostSet	Change Network Interface Setting of Virtual Host of SecureNAT Function
CMD_SecureNatHostSet_Help	Use this to change and save the virtual host network interface setting in the setting items of the Virtual NAT and DHCP Server function (SecureNAT function) on the currently managed Virtual Hub. \nThe SecureNAT function holds one virtual network adapter on the L2 segment inside the Virtual Hub and it has been assigned a MAC address and an IP address. By doing this, another host connected to the same L2 segment is able to communicate with the SecureNAT virtual host as if it is an actual IP host existing on the network. \n\n[Warning about SecureNAT Function]\nThe SecureNAT function is recommended only for system administrators and people with a detailed knowledge of networks. \nIf you use the SecureNAT function correctly, it is possible to achieve a safe form of remote access via a VPN. However when used in the wrong way, it can put the entire network in danger. Anyone who does not have a thorough knowledge of networks and anyone who does not have the network administrators permission must not enable the SecureNAT function. For a detailed explanation of the SecureNAT function, please refer to the VPN Server's manual and online documentation. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_SecureNatHostSet_Args	SecureNatHostSet [/MAC:mac] [/IP:ip] [/MASK:mask]
CMD_SecureNatHostSet_MAC	Specify the MAC address to assign for the virtual interface. Specify a MAC address using a string like "00-AC-01-23-45-67". When /MAC:none is specified, no changes will be made to the current setting.
CMD_SecureNatHostSet_IP	Specify the IP address to assign for the virtual interface. When /IP:none is specified, no changes will be made to the current setting.
CMD_SecureNatHostSet_MASK	Specify the subnet mask to assign for the virtual interface. When /MASK:none is specified, no changes will be made to the current setting.
CMD_SecureNatHostSet_Prompt_MAC	Endereço MAC: 
CMD_SecureNatHostSet_Prompt_IP	Endereço IP: 
CMD_SecureNatHostSet_Prompt_MASK	Máscara de sub-rede: 


# NatGet command
CMD_NatGet	Get Virtual NAT Function Setting of SecureNAT Function
CMD_NatGet_Help	Use this to get the virtual NAT setting from the setting items of the Virtual NAT and DHCP Server function (SecureNAT function) on the currently managed Virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_NatGet_Args	NatGet
CMD_NatGet_Column_USE	Use Virtual NAT Function
CMD_NetGet_Column_MTU	Valor MTU
CMD_NatGet_Column_TCP	TCP Session Timeout (Seconds) 
CMD_NatGet_Column_UDP	UDP Session Timeout (Seconds) 


# NatEnable command
CMD_NatEnable	Enable Virtual NAT Function of SecureNAT Function
CMD_NatEnable_Help	Use this to enable the Virtual NAT function on the currently managed Virtual Hub. \nIf the SecureNAT function is still not operating even after this command has been used to enable the Virtual NAT function, Virtual NAT is not operating. To start the operation of the SecureNAT Function, use the SecureNatEnable command. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_NatEnable_Args	NatEnable


# NatDisable command
CMD_NatDisable	Disable Virtual NAT Function of SecureNAT Function
CMD_NatDisable_Help	Use this to disable the Virtual NAT function on the currently managed Virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_NatDisable_Args	NatDisable


# NatSet command
CMD_NatSet	Change Virtual NAT Function Setting of SecureNAT Function
CMD_NatSet_Help	Use this to change the Virtual NAT setting of the currently managed Virtual Hub. The contents of the Virtual NAT setting includes: MTU value, TCP session timeout and UDP session timeout \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_NatSet_Args	NatSet [/MTU:mtu] [/TCPTIMEOUT:tcp_timeout] [/UDPTIMEOUT:udp_timeout] [/LOG:yes|no]
CMD_NatSet_MTU	Set the MTU (Maximum transferable unit size) using an integer to specify the byte length unit. This value is the maximum payload length excluding the MAC header of the Ethernet frame that the Virtual NAT sends and the default is 1500 bytes.
CMD_NatSet_TCPTIMEOUT	This sets how many seconds a condition of non-communication continues in a TCP session that the Virtual NAT is relaying before a timeout occurs and the session is discarded.
CMD_NatSet_UDPTIMEOUT	This sets how many seconds a condition of non-communication continues in a UDP session that the Virtual NAT is relaying before a timeout occurs and the session is discarded.
CMD_NatSet_LOG	Specify whether or not to save the Virtual NAT operation in the Virtual Hub security log. Specify "yes" to save it, and "no" to not save it.
CMD_NatSet_Prompt_MTU	Valor MTU: 
CMD_NatSet_Prompt_TCPTIMEOUT	TCP Session Timeout (Seconds): 
CMD_NatSet_Prompt_UDPTIMEOUT	UDP Session Timeout (Seconds): 
CMD_NatSet_Prompt_LOG	Save Log (yes / no): 
CMD_NatSet_Eval_MTU	Specify a value in the range %d to %d for the MTU value.
CMD_NatSet_Eval_TCP	Specify the number of seconds in the range %d to %d for the TCP session timeout.
CMD_NatSet_Eval_UDP	Specify the number of seconds in the range %d to %d for the UDP session timeout.


# NatTable command
CMD_NatTable	Get Virtual NAT Function Session Table of SecureNAT Function
CMD_NatTable_Help	Use this to get the table of TCP and UDP sessions currently communicating via the Virtual NAT (NAT table) in cases when the Virtual NAT function is operating on the currently managed Virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_NatTable_Args	TabelaNat


# DhcpGet command
CMD_DhcpGet	Get Virtual DHCP Server Function Setting of SecureNAT Function
CMD_DhcpGet_Help	Use this to get the virtual DHCP Server setting from the setting items of the Virtual NAT and DHCP Server function (SecureNAT function) on the currently managed Virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_DhcpGet_Args	DhcpGet
CMD_DhcpGet_Column_Log	Record Log of NAT and DHCP Operation
CMD_DhcpGet_Column_USE	Use Virtual DHCP Function
CMD_DhcpGet_Column_IP1	Start Distribution Address Band
CMD_DhcpGet_Column_IP2	End Distribution Address Band
CMD_DhcpGet_Column_MASK	Máscara de sub-rede
CMD_DhcpGet_Column_LEASE	Lease Limit (Seconds) 
CMD_DhcpGet_Column_GW	Default Gateway Address
CMD_DhcpGet_Column_DNS	DNS Server Address 1
CMD_DhcpGet_Column_DNS2	DNS Server Address 2
CMD_DhcpGet_Column_DOMAIN	Nome do domínio
CMD_DhcpGet_Column_PUSHROUTE	Static Routing Table to Push


# DhcpEnable command
CMD_DhcpEnable	Enable Virtual DHCP Server Function of SecureNAT Function
CMD_DhcpEnable_Help	Use this to enable the Virtual DHCP Server function on the currently managed Virtual Hub. \nIf the SecureNAT function is still not operating even after this command has been used to enable the Virtual DHCP function, Virtual DHCP Server is not operating. To start the operation of the SecureNAT Function, use the SecureNatEnable command. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_DhcpEnable_Args	DhcpEnable


# DhcpDisable command
CMD_DhcpDisable	Disable Virtual DHCP Server Function of SecureNAT Function
CMD_DhcpDisable_Help	Use this to disable the Virtual DHCP Server function on the currently managed Virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_DhcpDisable_Args	DhcpDisable


# DhcpSet command
CMD_DhcpSet	Change Virtual DHCP Server Function Setting of SecureNAT Function
CMD_DhcpSet_Help	Use this to change the Virtual DHCP Server setting of the currently managed Virtual Hub. The Virtual DHCP Server settings include the following items: distribution address band, subnet mask, lease limit, and option values assigned to clients. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_DhcpSet_Args	DhcpSet [/START:start_ip] [/END:end_ip] [/MASK:subnetmask] [/EXPIRE:sec] [/GW:gwip] [/DNS:dns] [/DNS2:dns2][/DOMAIN:domain] [/LOG:yes|no] [/PUSHROUTE:"routing_table"]
CMD_DhcpSet_START	Specify the start point of the address band to be distributed to the client. (Example: 192.168.30.10)
CMD_DhcpSet_END	Specify the end point of the address band to be distributed to the client. (Example: 192.168.30.200)
CMD_DhcpSet_MASK	Specify the subnet mask to be specified for the client. (Example: 255.255.255.0)
CMD_DhcpSet_EXPIRE	Specify the expiration date in second units for leasing an IP address to a client.
CMD_DhcpSet_GW	Specify the IP address of the default gateway to be notified to the client. You can specify a SecureNAT Virtual Host IP address for this when the SecureNAT Function's Virtual NAT Function has been enabled and is being used also. If you specify 0 or none, then the client will not be notified of the default gateway.
CMD_DhcpSet_DNS	Specify the IP address of the primary DNS Server to be notified to the client. You can specify a SecureNAT Virtual Host IP address for this when the SecureNAT Function's Virtual NAT Function has been enabled and is being used also. If you specify 0 or none, then the client will not be notified of the DNS Server address.
CMD_DhcpSet_DNS2	Specify the IP address of the secondary DNS Server to be notified to the client. You can specify a SecureNAT Virtual Host IP address for this when the SecureNAT Function's Virtual NAT Function has been enabled and is being used also. If you specify 0 or none, then the client will not be notified of the DNS Server address.
CMD_DhcpSet_DOMAIN	Specify the domain name to be notified to the client. If you specify none, then the client will not be notified of the domain name.
CMD_DhcpSet_LOG	Specify whether or not to save the Virtual DHCP Server operation in the Virtual Hub security log. Specify "yes" to save it. This value is interlinked with the Virtual NAT Function log save setting.
CMD_DhcpSet_PUSHROUTE	Specify the static routing table to push.\nExample: "192.168.5.0/255.255.255.0/192.168.4.254, 10.0.0.0/255.0.0.0/192.168.4.253"\nSplit multiple entries (maximum: 64 entries) by comma or space characters. Each entry must be specified in the "IP network address/subnet mask/gateway IP address" format.\nThis Virtual DHCP Server can push the classless static routes (RFC 3442) with DHCP reply messages to VPN clients.\nWhether or not a VPN client can recognize the classless static routes (RFC 3442) depends on the target VPN client software. SoftEther VPN Client and OpenVPN Client are supporting the classless static routes. On L2TP/IPsec and MS-SSTP protocols, the compatibility depends on the implementation of the client software. You can realize the split tunneling if you clear the default gateway field on the Virtual DHCP Server options. On the client side, L2TP/IPsec and MS-SSTP clients need to be configured not to set up the default gateway for the split tunneling usage.\nYou can also push the classless static routes (RFC 3442) by your existing external DHCP server. In that case, disable the Virtual DHCP Server function on SecureNAT, and you need not to set up the classless routes on this command.\nSee the RFC 3442 to understand the classless routes.
CMD_DhcpSet_Prompt_START	Start Point for Distributed Address Band: 
CMD_DhcpSet_Prompt_END	End Point for Distributed Address Band: 
CMD_DhcpSet_Prompt_MASK	Máscara de sub-rede: 
CMD_DhcpSet_Prompt_EXPIRE	Lease Limit (Seconds): 
CMD_DhcpSet_Prompt_GW	Default Gateway ('none' to not set this): 
CMD_DhcpSet_Prompt_DNS	DNS Server 1 ('none' to not set this): 
CMD_DhcpSet_Prompt_DNS2	DNS Server 2 ('none' to not set this): 
CMD_DhcpSet_Prompt_DOMAIN	Nome do domínio: 


# DhcpTable command
CMD_DhcpTable	Get Virtual DHCP Server Function Lease Table of SecureNAT Function
CMD_DhcpTable_Help	Use this to get the lease table of IP addresses, held by the Virtual DHCP Server, that are assigned to clients in cases when the Virtual NAT function is operating on the currently managed Virtual Hub. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_DhcpTable_Args	TabelaDhcp


# AdminOptionList command
CMD_AdminOptionList	Get List of Virtual Hub Administration Options
CMD_AdminOptionList_Help	Use this to get a list of Virtual Hub administration options that are set on the currently managed Virtual Hub. \nThe purpose of the Virtual Hub administration options is for the VPN Server Administrator to set limits for the setting ranges when the administration of the Virtual Hub is to be trusted to each Virtual Hub administrator. \nOnly an administrator with administration privileges for this entire VPN Server is able to add, edit and delete the Virtual Hub administration options. The Virtual Hub administrators are unable to make changes to the administration options, however they are able to view them. \nThere is an exception however. If allow_hub_admin_change_option is set to "1", even Virtual Hub administrators are able to edit the administration options. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster member.
CMD_AdminOptionList_Args	AdminOptionList


# AdminOptionSet command
CMD_AdminOptionSet	Set Values of Virtual Hub Administration Options
CMD_AdminOptionSet_Help	Use this to change the values of Virtual Hub administration options that are set on the currently managed Virtual Hub. \nThe purpose of the Virtual Hub administration options is for the VPN Server Administrator to set limits for the setting ranges when the administration of the Virtual Hub is to be trusted to each Virtual Hub administrator. \nOnly an administrator with administration privileges for this entire VPN Server is able to add, edit and delete the Virtual Hub administration options. The Virtual Hub administrators are unable to make changes to the administration options, however they are able to view them. \nThere is an exception however. If allow_hub_admin_change_option is set to "1", even Virtual Hub administrators are able to edit the administration options. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster member.
CMD_AdminOptionSet_Args	AdminOptionSet [name] [/VALUE:value]
CMD_AdminOptionSet_[name]	Specify the name of the administration option whose value you want to change. You can get a list of names by using the AdminOptionList command.
CMD_AdminOptionSet_VALUE	Specify an integer for the setting value.
CMD_AdminOptionSet_Prompt_name	Name of Administration Option to Change Value: 
CMD_AdminOptionSet_Prompt_VALUE	Valor de configuração (inteiro): 


# ExtOptionList command
CMD_ExtOptionList	Get List of Virtual Hub Extended Options
CMD_ExtOptionList_Help	Use this to get a Virtual Hub Extended Options List that is set on the currently managed Virtual Hub.\nVirtual Hub Extended Option enables you to configure more detail settings of the Virtual Hub.\nBy default, both VPN Server's global administrators and individual Virtual Hub's administrators can modify the Virtual Hub Extended Options.\nHowever, if the deny_hub_admin_change_ext_option is set to 1 on the Virtual Hub Admin Options, the individual Virtual Hub's administrators cannot modify the Virtual Hub Extended Options.\nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster member.
CMD_ExtOptionList_Args	ExtOptionList


# ExtOptionSet command
CMD_ExtOptionSet	Set a Value of Virtual Hub Extended Options
CMD_ExtOptionSet_Help	Use this to set a value in the Virtual Hub Extended Options List that is set on the currently managed Virtual Hub.\nVirtual Hub Extended Option enables you to configure more detail settings of the Virtual Hub.\nBy default, both VPN Server's global administrators and individual Virtual Hub's administrators can modify the Virtual Hub Extended Options.\nHowever, if the deny_hub_admin_change_ext_option is set to 1 on the Virtual Hub Admin Options, the individual Virtual Hub's administrators cannot modify the Virtual Hub Extended Options.\nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster member.
CMD_ExtOptionSet_Args	ExtOptionSet [name] [/VALUE:value]
CMD_ExtOptionSet_[name]	Specify the name of the Virtual Hub Extended Options whose value you want to change. You can get a list of names by using the ExtOptionList command.
CMD_ExtOptionSet_VALUE	Specify an integer for the setting value.
CMD_ExtOptionSet_Prompt_name	Name of Extended Option to Change Value: 
CMD_ExtOptionSet_Prompt_VALUE	Valor de configuração (inteiro): 


# CrlList command
CMD_CrlList	Get List of Certificates Revocation List
CMD_CrlList_Help	Use this to get a Certificates Revocation List that is set on the currently managed Virtual Hub. \nBy registering certificates in the Certificates Revocation List, the clients who provide these certificates will be unable to connect to this Virtual Hub using certificate authentication mode. \nNormally with this function, in cases where the security of a private key has been compromised or where a person holding a certificate has been stripped of their privileges, by registering that certificate as invalid on the Virtual Hub, it is possible to deny user authentication when that certificate is used by a client to connect to the Virtual Hub. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CrlList_Args	ListaCrl


# CrlAdd command
CMD_CrlAdd	Add a Revoked Certificate
CMD_CrlAdd_Help	Use this to add a new revoked certificate definition in the Certificate Revocation List that is set on the currently managed Virtual Hub. \nSpecify the contents to be registered in the Certificate Revocation List by using the parameters of this command. When a user connects to a Virtual Hub in certificate authentication mode and that certificate matches 1 or more of the contents registered in the certificates revocation list, the user is denied connection. \nA certificate that matches all the conditions that are defined by the parameters specified by this command will be judged as invalid. \nThe items that can be set are as follows: Name (CN), Organization (O), Organization Unit (OU), Country (C), State (ST), Locale (L), Serial Number (hexadecimal), MD5 Digest Value (hexadecimal, 128 bit), and SHA-1 Digest Value (hexadecimal, 160 bit). For the specification of a digest value (hash value) a certificate is optionally specified depending on the circumstances. Normally when a MD5 or SHA-1 digest value is input, it is not necessary to input the other items. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CrlAdd_Args	CrlAdd [/SERIAL:serial] [/MD5:md5] [/SHA1:sha1] [/CN:cn] [/O:o] [/OU:ou] [/C:c] [/ST:st] [/L:l]
CMD_CrlAdd_SERIAL	Use this parameter to specify the value for the certificate serial number (hexadecimal) when it is set as a condition.
CMD_CrlAdd_MD5	Use this parameter to specify the value for the certificate MD5 digest value (hexadecimal, 128 bits) when it is set as a condition. If this parameter specification is other than a hexadecimal value of 32 characters (16 bytes), it will be ignored.
CMD_CrlAdd_SHA1	Use this parameter to specify the value for the certificate SHA1 digest value (hexadecimal, 160 bits) when it is set as a condition. If this parameter specification is other than a hexadecimal value of 40 characters (16 bytes), it will be ignored.
CMD_CrlAdd_CN	Use this parameter to specify the name (CN) of the certificate when it is set as a condition. 
CMD_CrlAdd_O	Use this parameter to specify the organization (O) of the certificate when it is set as a condition. 
CMD_CrlAdd_OU	Use this parameter to specify the organization unit (OU) of the certificate when it is set as a condition. 
CMD_CrlAdd_C	Use this parameter to specify the country (C) of the certificate when it is set as a condition. 
CMD_CrlAdd_ST	Use this parameter to specify the state (ST) of the certificate when it is set as a condition. 
CMD_CrlAdd_L	Use this parameter to specify the locale (L) of the certificate when it is set as a condition. 


# CrlDel command
CMD_CrlDel	Delete a Revoked Certificate
CMD_CrlDel_Help	Use this to specify and delete a revoked certificate definition from the certificate revocation list that is set on the currently managed Virtual Hub. \nTo get the list of currently registered revoked certificate definitions, use the CrlList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CrlDel_Args	CrlDel [id]
CMD_CrlDel_[id]	Specify the ID of the revoked certificate definition you want to delete.
CMD_CrlDel_Prompt_ID	ID a ser excluído: 


# CrlGet command
CMD_CrlGet	Get a Revoked Certificate
CMD_CrlGet_Help	Use this to specify and get the contents of a revoked certificate definition from the Certificates Revocation List that is set on the currently managed Virtual Hub. \nTo get the list of currently registered revoked certificate definitions, use the CrlList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_CrlGet_Args	CrlGet [id]
CMD_CrlGet_[id]	Specify the ID of the revoked certificate definition you want to get.
CMD_CrlGet_Prompt_ID	ID para obter: 
CMD_CrlGet_CN	Common Name (CN)
CMD_CrlGet_O	Organization (O)
CMD_CrlGet_OU	Organization Unit (OU)
CMD_CrlGet_C	País (C)
CMD_CrlGet_ST	Estado (ST)
CMD_CrlGet_L	Local (L)
CMD_CrlGet_SERI	Serial Number (Hexadecimal)
CMD_CrlGet_MD5_HASH	MD5 Digest Value (Hexadecimal, 128 bit)
CMD_CrlGet_SHA1_HASH	SHA-1 Digest Value (Hexadecimal, 160 bit)


# AcList command
CMD_AcList	Get List of Rule Items of Source IP Address Limit List
CMD_AcList_Help	Use this to get a list of Source IP Address Limit List rules that is set on the currently managed Virtual Hub. \nYou can allow or deny VPN connections to this Virtual Hub according to the client computer's source IP address. You can define multiple rules and set a priority for each rule. The search proceeds from the rule with the highest order or priority and based on the action of the rule that the IP address first matches, the connection from the client is either allowed or denied. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_AcList_Args	ListaAc


# AcAdd command
CMD_AcAdd	Add Rule to Source IP Address Limit List (IPv4)
CMD_AcAdd_Help	Use this to add a new rule to the Source IP Address Limit List that is set on the currently managed Virtual Hub. \nThe items set here will be used to decide whether to allow or deny connection from a VPN Client when this client attempts connection to the Virtual Hub. \nYou can specify a client IP address, or IP address or mask to match the rule as the contents of the rule item. By specifying an IP address only, there will only be one specified computer that will match the rule, but by specifying an IP net mask address or subnet mask address, all the computers in the range of that subnet will match the rule. \nYou can specify the priority for the rule. You can specify an integer of 1 or greater for the priority and the smaller the number, the higher the priority. \nTo get a list of the currently registered Source IP Address Limit List, use the AcList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_AcAdd_Args	AcAdd [allow|deny] [/PRIORITY:priority] [/IP:ip/mask]
CMD_AcAdd_[allow|deny]	Set whether to "allow" or "deny" the connection from a client that matches the rule.
CMD_AcAdd_PRIORITY	Specify an integer of 1 or higher to indicate the priority of the rule. The smaller the value the higher the priority.
CMD_AcAdd_IP	Using the format: "IP Address/Mask", specify the range of client IPv4 addresses. Specify the IPv4 address by separating the decimal values using dots such as "192.168.0.1". For the mask, either specify decimal values separated by dots such as "255.255.255.0", or you can specify the bit length from the header using a decimal value such as "24". To specify a single IPv4 host, specify the mask as "32" or "255.255.255.255".
CMD_AcAdd_Prompt_AD	permitir ou negar: 
CMD_AcAdd_Prompt_PRIORITY	Prioridade: 
CMD_AcAdd_Prompt_IP	IPv4 Address/Mask: 
CMD_AcAdd_Eval_PRIORITY	Specify 1 or higher for the priority.


# AcAdd6 command
CMD_AcAdd6	Add Rule to Source IP Address Limit List (IPv6)
CMD_AcAdd6_Help	Use this to add a new rule to the Source IP Address Limit List that is set on the currently managed Virtual Hub. \nThe items set here will be used to decide whether to allow or deny connection from a VPN Client when this client attempts connection to the Virtual Hub. \nYou can specify a client IP address, or IP address or mask to match the rule as the contents of the rule item. By specifying an IP address only, there will only be one specified computer that will match the rule, but by specifying an IP net mask address or subnet mask address, all the computers in the range of that subnet will match the rule. \nYou can specify the priority for the rule. You can specify an integer of 1 or greater for the priority and the smaller the number, the higher the priority. \nTo get a list of the currently registered Source IP Address Limit List, use the AcList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_AcAdd6_Args	AcAdd6 [allow|deny] [/PRIORITY:priority] [/IP:ip/mask]
CMD_AcAdd6_[allow|deny]	Set whether to "allow" or "deny" the connection from a client that matches the rule.
CMD_AcAdd6_PRIORITY	Specify an integer of 1 or higher to indicate the priority of the rule. The smaller the value the higher the priority.
CMD_AcAdd6_IP	Using the format: "IP Address/Mask", specify the range of client IPv6 addresses. Specify the IPv6 address by separating the hexadecimal values using colons such as "2001:200:0:1::". For the mask, either specify hexadecimal values separated by colons such as "ffff:ffff:ffff:ffff::", or you can specify the bit length from the header using a decimal value such as "64". To specify a single IPv6 host, specify the mask as "128" or "ffff:ffff:ffff:ffff:ffff:ffff:ffff:ffff".
CMD_AcAdd6_Prompt_AD	permitir ou negar: 
CMD_AcAdd6_Prompt_PRIORITY	Prioridade: 
CMD_AcAdd6_Prompt_IP	IPv6 Address/Mask: 
CMD_AcAdd6_Eval_PRIORITY	Specify 1 or higher for the priority.


# AcDel command
CMD_AcDel	Delete Rule from Source IP Address Limit List
CMD_AcDel_Help	Use this to delete a rule from the Source IP Address Limit List that is set on the currently managed Virtual Hub. \nTo get a list of the currently registered IP access control list, use the AcList command. \nThis command cannot be run on VPN Bridge. \nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_AcDel_Args	AcDel [id]
CMD_AcDel_[id]	Specify the ID of the rule in the Source IP Address Limit List that you want to delete.
CMD_AcDel_Prompt_ID	ID of Rule to Delete: 


# LicenseAdd command
CMD_LicenseAdd	Adicionar registro de chave de licença
CMD_LicenseAdd_Help	Use this to register a new license key on the SoftEther VPN Server. \nTo use SoftEther VPN Server you must acquire a valid license and register the license key. The license keys are 36 alphanumeric characters in length plus hyphens. They are key codes that certify the ownership of a license. \nWhen a license certificate is received together with this software, the license key is printed on this license certificate. If the license for this software has been purchased online, the license key is provided by email and on the website window at the time the license is purchased. The license key may also be written down by some other method. If you don't know where the license key is written down, ask the vendor who sold you the license. \n\nTo get the list of currently registered licenses, use the LicenseList command. \nTo display the license status of the current VPN Server, use the LicenseStatus command. \nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_LicenseAdd_Args	LicenseAdd [key]
CMD_LicenseAdd_[key]	Specify the license key to register. Specify 36 digits of alphanumeric characters and group the digits in groups of 6 separating them by hyphen. 
CMD_LicenseAdd_Prompt_Key	Chave de licença: 


# LicenseDel command
CMD_LicenseDel	Delete Registered License
CMD_LicenseDel_Help	Use this to delete a specified license from the license list that is currently registered on the SoftEther VPN Server. \n\nTo get the list of currently registered licenses, use the LicenseList command. \nTo display the license status of the current VPN Server, use the LicenseStatus command. \nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_LicenseDel_Args	LicenseDel [id]
CMD_LicenseDel_[id]	Specify the license number to delete.
CMD_LicenseDel_Prompt_ID	License Number to Delete: 


# LicenseList command
CMD_LicenseList	Get List of Registered Licenses
CMD_LicenseList_Help	Use this to display a list of license information currently registered on the SoftEther VPN Server including: license key, license type name, status, expiration date, license ID, license type ID, server ID and serial ID. \n\nTo display the license status of the current VPN Server, use the LicenseStatus command. \nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_LicenseList_Args	Início da concessão


# LicenseStatus command
CMD_LicenseStatus	Get License Status of Current VPN Server
CMD_LicenseStatus_Help	Use this to get and display the license status of the current SoftEther VPN Server. \nThe following current information on the SoftEther VPN Server will be displayed: product edition, server ID, product license expiration date, number of usable Client Connection Licenses and number of Bridge Connection Licenses. \n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_LicenseStatus_Args	LicenseStatus


# Commands added after SoftEther VPN 4.0


# IPsecEnable command
CMD_IPsecEnable	Enable or Disable IPsec VPN Server Function
CMD_IPsecEnable_Help	Enable or Disable IPsec VPN Server Function on SoftEther VPN Server.\nIf you enable this function, Virtual Hubs on the VPN Server will be able to accept Remote-Access VPN connections from L2TP-compatible PCs, Mac OS X and Smartphones, and also can accept EtherIP Site-to-Site VPN Connection. VPN Connections from Smartphones suchlike iPhone, iPad and Android, and also from native VPN Clients on Mac OS X and Windows can be accepted.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_IPsecEnable_Args	IPsecEnable [/L2TP:yes|no] [/L2TPRAW:yes|no] [/ETHERIP:yes|no] [/PSK:pre-shared-key] [/DEFAULTHUB:default_hub]
CMD_IPsecEnable_L2TP	Enable or Disable the L2TP over IPsec Server Function. To accept VPN connections from iPhone, iPad, Android, Windows or Mac OS X, enable this option.
CMD_IPsecEnable_L2TPRAW	Enable or Disable the L2TP Server Function (Raw L2TP with No Encryptions). To accept special VPN clients, enable this option.
CMD_IPsecEnable_ETHERIP	Enable or Disable the EtherIP / L2TPv3 over IPsec Server Function (for site-to-site VPN Server function). Router Products which are compatible with EtherIP over IPsec can connect to Virtual Hubs on the VPN Server and establish Layer-2 (Ethernet) Bridging.
CMD_IPsecEnable_PSK	Specify the IPsec Pre-Shared Key. An IPsec Pre-Shared Key is also called as "PSK" or "secret". Specify it equal or less than 8 letters, and distribute it to every users who will connect to the VPN Server. Please note: Google Android 4.0 has a bug which a Pre-Shared Key with 10 or more letters causes a unexpected behavior. For that reason, the letters of a Pre-Shared Key should be 9 or less characters.
CMD_IPsecEnable_DEFAULTHUB	Specify the default Virtual HUB in a case of omitting the name of HUB on the Username. Users should specify their username such as "Username@Target Virtual HUB Name" to connect this L2TP Server. If the designation of the Virtual Hub is omitted, the above HUB will be used as the target.
CMD_IPsecEnable_Prompt_L2TP	Enable L2TP over IPsec Server Function (yes / no): 
CMD_IPsecEnable_Prompt_L2TPRAW	Enable Raw L2TP Server Function (yes / no): 
CMD_IPsecEnable_Prompt_ETHERIP	Enable EtherIP / L2TPv3 over IPsec Server Function (yes / no): 
CMD_IPsecEnable_Prompt_PSK	Pre Shared Key for IPsec (Recommended: 9 letters at maximum): 
CMD_IPsecEnable_Prompt_DEFAULTHUB	Default Virtual HUB in a case of omitting the HUB on the Username: 


# IPsecGet command
CMD_IPsecGet	Get the Current IPsec VPN Server Settings
CMD_IPsecGet_Help	Get and view the current IPsec VPN Server settings on the SoftEther VPN Server.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_IPsecGet_Args	IPsecGet
CMD_IPsecGet_PRINT_L2TP	L2TP over IPsec Server Function Enabled
CMD_IPsecGet_PRINT_L2TPRAW	Raw L2TP Server Function Enabled
CMD_IPsecGet_PRINT_ETHERIP	EtherIP / L2TPv3 over IPsec Server Function Enabled
CMD_IPsecGet_PRINT_PSK	IPsec Pre-Shared Key String
CMD_IPsecGet_PRINT_DEFAULTHUB	Name of Default Virtual Hub


# EtherIpClientAdd command
CMD_EtherIpClientAdd	Add New EtherIP / L2TPv3 over IPsec Client Setting to Accept EtherIP / L2TPv3 Client Devices
CMD_EtherIpClientAdd_Help	Add a new setting entry to enable the EtherIP / L2TPv3 over IPsec Server Function to accept client devices.\nIn order to accept connections from routers by the EtherIP / L2TPv3 over IPsec Server Function, you have to define the relation table between an IPsec Phase 1 string which is presented by client devices of EtherIP / L2TPv3 over IPsec compatible router, and the designation of the destination Virtual Hub.\nAfter you add a definition entry by EtherIpClientAdd command, the defined connection setting to the Virtual Hub will be applied on the login-attempting session from an EtherIP / L2TPv3 over IPsec client device.\nThe username and password in an entry must be registered on the Virtual Hub. An EtherIP / L2TPv3 client will be regarded as it connected the Virtual HUB with the identification of the above user information.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_EtherIpClientAdd_Args	EtherIpClientAdd [ID] [/HUB:hubname] [/USERNAME:username] [/PASSWORD:password]
CMD_EtherIpClientAdd_[ID]	Specify an ISAKMP Phase 1 ID. The ID must be exactly same as a ID in the configuration of the EtherIP / L2TPv3 Client. You can specify IP address as well as characters as ID, if the EtherIP Client uses IP address as Phase 1 ID. If you specify '*' (asterisk), it will be a wildcard to match any clients which doesn't match other explicit rules.
CMD_EtherIpClientAdd_HUB	Specify the name of the Virtual Hub to connect.
CMD_EtherIpClientAdd_USERNAME	Specify the username to login to the destination Virtual Hub.
CMD_EtherIpClientAdd_PASSWORD	Specify the password to login to the destination Virtual Hub.
CMD_EtherIpClientAdd_Prompt_ID	ISAKMP Phase 1 ID ('*' is a wildcard): 
CMD_EtherIpClientAdd_Prompt_HUB	Virtual Hub Name: 
CMD_EtherIpClientAdd_Prompt_USERNAME	Username to Login Virtual Hub: 
CMD_EtherIpClientAdd_Prompt_PASSWORD	Password to Login Virtual Hub: 


# EtherIpClientDelete command
CMD_EtherIpClientDelete	Delete an EtherIP / L2TPv3 over IPsec Client Setting
CMD_EtherIpClientDelete_Help	This command deletes an entry to accept VPN clients by EtherIP / L2TPv3 over IPsec Function. \n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_EtherIpClientDelete_Args	EtherIpClientDelete [ID]
CMD_EtherIpClientDelete_[ID]	Specify the ISAKMP Phase 1 ID to delete.
CMD_EtherIpClientDelete_Prompt_ID	ISAKMP Phase 1 ID: 


# EtherIpClientList command
CMD_EtherIpClientList	Get the Current List of EtherIP / L2TPv3 Client Device Entry Definitions
CMD_EtherIpClientList_Help	This command gets and shows the list of entries to accept VPN clients by EtherIP / L2TPv3 over IPsec Function.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_EtherIpClientList_Args	EtherIpClientList


# OpenVpnMakeConfig command
CMD_OpenVpnMakeConfig	Generate a Sample Setting File for OpenVPN Client
CMD_OpenVpnMakeConfig_Help	Originally, the OpenVPN Client requires a user to write a very difficult configuration file manually. This tool helps you to make a useful configuration sample. What you need to generate the configuration file for the OpenVPN Client is to run this command.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_OpenVpnMakeConfig_Args	OpenVpnMakeConfig [ZIP_FileName]
CMD_OpenVpnMakeConfig_[ZIP_FileName]	Specify the output setting files to be saved as ZIP compression format. If no file extension is specified, the ".zip" extension will be appended to the filename.
CMD_OpenVpnMakeConfig_Prompt_ZIP	Output Filename of Setting Files (ZIP compressed file): 
CMD_OpenVpnMakeConfig_OK	The sample setting file was saved as "%s". You can unzip this file to extract setting files.\n
CMD_OpenVpnMakeConfig_ERROR	The sample setting files were unable to be saved as "%s". The filename might be invalid.\n


# ServerCertRegenerate command
CMD_ServerCertRegenerate	Generate New Self-Signed Certificate with Specified CN (Common Name) and Register on VPN Server
CMD_ServerCertRegenerate_Help	You can use this command to replace the current certificate on the VPN Server to a new self-signed certificate which has the CN (Common Name) value in the fields.\n\nThis command is convenient if you are planning to use Microsoft SSTP VPN Clone Server Function. Because of the value of CN (Common Name) on the SSL certificate of VPN Server must match to the hostname specified on the SSTP VPN client.\n\nThis command will delete the existing SSL certificate of the VPN Server. It is recommended to backup the current SSL certificate and private key by using the ServerKeyGet command beforehand.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_ServerCertRegenerate_Args	ServerCertRegenerate [CN]
CMD_ServerCertRegenerate_[CN]	Specify a Common Name (CN) which the new certificate will have.
CMD_ServerCertRegenerate_Prompt_CN	Value of Common Name (CN): 


# VpnOverIcmpDnsEnable command
CMD_VpnOverIcmpDnsEnable	Enable / Disable the VPN over ICMP / VPN over DNS Server Function
CMD_VpnOverIcmpDnsEnable_Help	You can establish a VPN only with ICMP or DNS packets even if there is a firewall or routers which blocks TCP/IP communications. You have to enable the following functions beforehand.\n\nWarning: Use this function for emergency only. It is helpful when a firewall or router is misconfigured to blocks TCP/IP, but either ICMP or DNS is not blocked. It is not for long-term stable using.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_VpnOverIcmpDnsEnable_Args	VpnOverIcmpDnsEnable [/ICMP:yes|no] [/DNS:yes|no]
CMD_VpnOverIcmpDnsEnable_ICMP	Specify yes to enable the VPN over ICMP Server. Specify no to disable.
CMD_VpnOverIcmpDnsEnable_DNS	Specify yes to enable the VPN over DNS Server. Specify no to disable.
CMD_VpnOverIcmpDnsEnable_Prompt_ICMP	Enable VPN over ICMP Server (yes / no): 
CMD_VpnOverIcmpDnsEnable_Prompt_DNS	Enable VPN over DNS Server (yes / no): 


# VpnOverIcmpDnsGet command
CMD_VpnOverIcmpDnsGet	Get Current Setting of the VPN over ICMP / VPN over DNS Function
CMD_VpnOverIcmpDnsGet_Help	Get and show the current VPN over ICMP / VPN over DNS Function status.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_VpnOverIcmpDnsGet_Args	VpnOverIcmpDnsGet
CMD_VpnOverIcmpDnsGet_PRINT_ICMP	VPN over ICMP Server Enabled
CMD_VpnOverIcmpDnsGet_PRINT_DNS	VPN over DNS Server Enabled


# DynamicDnsGetStatus command
CMD_DynamicDnsGetStatus	Show the Current Status of Dynamic DNS Function
CMD_DynamicDnsGetStatus_Help	Get and show the current status of the Dynamic DNS function.\n\nThe Dynamic DNS assigns a unique and permanent DNS hostname for this VPN Server. You can use that hostname to specify this VPN Server on the settings for VPN Client and VPN Bridge. You need not to register and keep a domain name.\nAlso, if your ISP assigns you a dynamic (not-fixed) IP address, the corresponding IP address of your Dynamic DNS hostname will be automatically changed. It enables you to keep running the VPN Server by using only a dynamic IP address.\r\nTherefore, you need not any longer to keep static global IP addresses with expenses monthly costs.\n[Caution]\nTo disable the Dynamic DNS Function, modify the configuration file of VPN Server.\r\n\r\nThe "declare root" directive has the "declare DDnsClient" directive. In this directive, you can switch "bool Disable" from false to true, and reboot the VPN Server, then the Dynamic DNS Function will be disabled.\r\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_DynamicDnsGetStatus_Args	DynamicDnsGetStatus
CMD_DynamicDnsGetStatus_PRINT_FQDN	Nome do host DNS dinâmico atribuído (completo):
CMD_DynamicDnsGetStatus_PRINT_HOSTNAME	Nome do host DNS dinâmico atribuído (hostname):
CMD_DynamicDnsGetStatus_PRINT_SUFFIX	Sufixo DNS
CMD_DynamicDnsGetStatus_PRINT_IPv4	Global IPv4 Address
CMD_DynamicDnsGetStatus_PRINT_IPv6	Global IPv6 Address


# DynamicDnsSetHostname command
CMD_DynamicDnsSetHostname	Defina o nome do host DNS dinâmico
CMD_DynamicDnsSetHostname_Help	You can use this command to change the hostname assigned by the Dynamic DNS function. The currently assigned hostname can be showen by the DynamicDnsGetStatus command.\n\nThe Dynamic DNS assigns a unique and permanent DNS hostname for this VPN Server. You can use that hostname to specify this VPN Server on the settings for VPN Client and VPN Bridge. You need not to register and keep a domain name.\nAlso, if your ISP assigns you a dynamic (not-fixed) IP address, the corresponding IP address of your Dynamic DNS hostname will be automatically changed. It enables you to keep running the VPN Server by using only a dynamic IP address.\r\nTherefore, you need not any longer to keep static global IP addresses with expenses monthly costs.\n[Caution]\nTo disable the Dynamic DNS Function, modify the configuration file of VPN Server.\r\n\r\nThe "declare root" directive has the "declare DDnsClient" directive. In this directive, you can switch "bool Disable" from false to true, and reboot the VPN Server, then the Dynamic DNS Function will be disabled.\r\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.
CMD_DynamicDnsSetHostname_Args	DynamicDnsSetHostname [hostname]
CMD_DynamicDnsSetHostname_[hostname]	Specify the new hostname with 3 letters at least and 31 letters at most. Only alphabets and numerics can be used.
CMD_DynamicDnsSetHostname_Prompt_hostname	Dynamic DNS Hostname (3 - 31 letters): 


# VpnAzureGetStatus command
CMD_VpnAzureGetStatus	Show the current status of VPN Azure function
CMD_VpnAzureGetStatus_Help	Get and show the current status of the VPN Azure function.\n\nVPN Azure makes it easier to establish a VPN Session from your home PC to your office PC. While a VPN connection is established, you can access to any other servers on the private network of your company.\nYou don't need a global IP address on the office PC (VPN Server). It can work behind firewalls or NATs. No network administrator's configuration required. You can use the built-in SSTP-VPN Client of Windows in your home PC.\nVPN Azure is a cloud VPN service operated by SoftEther VPN Project. VPN Azure is free of charge and available to anyone. Visit http://www.vpnazure.net/ to see details and how-to-use instructions.\n\nThe VPN Azure hostname is same to the hostname of the Dynamic DNS setting, but altering the domain suffix to "vpnazure.net". To change the hostname use the DynamicDnsSetHostname command.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_VpnAzureGetStatus_Args	VpnAzureGetStatus
CMD_VpnAzureGetStatus_PRINT_ENABLED	VPN Azure Function is Enabled
CMD_VpnAzureGetStatus_PRINT_CONNECTED	Connection to VPN Azure Cloud Server is Established
CMD_VpnAzureGetStatus_PRINT_HOSTNAME	Hostname of this VPN Server on VPN Azure Service


# VpnAzureSetEnable command
CMD_VpnAzureSetEnable	Enable / Disable VPN Azure Function
CMD_VpnAzureSetEnable_Help	Enable or disable the VPN Azure function.\n\nVPN Azure makes it easier to establish a VPN Session from your home PC to your office PC. While a VPN connection is established, you can access to any other servers on the private network of your company.\nYou don't need a global IP address on the office PC (VPN Server). It can work behind firewalls or NATs. No network administrator's configuration required. You can use the built-in SSTP-VPN Client of Windows in your home PC.\nVPN Azure is a cloud VPN service operated by SoftEther VPN Project. VPN Azure is free of charge and available to anyone. Visit http://www.vpnazure.net/ to see details and how-to-use instructions.\n\nThe VPN Azure hostname is same to the hostname of the Dynamic DNS setting, but altering the domain suffix to "vpnazure.net". To change the hostname use the DynamicDnsSetHostname command.\n\nTo execute this command, you must have VPN Server administrator privileges. \nThis command cannot be run on VPN Bridge.\nYou cannot execute this command for Virtual Hubs of VPN Servers operating as a cluster.
CMD_VpnAzureSetEnable_Args	VpnAzureSetEnable [yes|no]
CMD_VpnAzureSetEnable_[yes|no]	Specify 'yes' to enable VPN Azure. 'no' to disable it.
CMD_VpnAzureSetEnable_PROMPT	Enable VPN Azure (yes / no): 


#######################################################


#                                                     #


# Management commands for VPN Client are listed below #


#                                                     #


#######################################################


# VersionGet command
CMD_VersionGet	Get Version Information of VPN Client Service
CMD_VersionGet_Help	Use this to get the version information of the currently managed VPN Client Service program.
CMD_VersionGet_Args	VersionGet
CMD_VersionGet_1	Nome do produto
CMD_VersionGet_2	Version Information
CMD_VersionGet_3	Build Information
CMD_VersionGet_4	ID processo
CMD_VersionGet_5	Tipo de OS


# PasswordSet command
CMD_PasswordSet	Set the password to connect to the VPN Client service.
CMD_PasswordSet_Help	You can make it mandatory to input a password for occasions when the Command Line Management Utility and the VPN Client Manager connect to a VPN Client service to control it. You can use this command to set the password that must be input. \nYou can also make it mandatory for this password to be input when doing remote operations (from a computer that is not localhost)
CMD_PasswordSet_Args	PasswordSet [password] [/REMOTEONLY:yes|no]
CMD_PasswordSet_[password]	Specify the password you wish to set. You can delete the password setting by specifying "none".
CMD_PasswordSet_REMOTEONLY	Specify "yes" to only require the password to be input when operation is done remotely (from a computer that is not localhost). This stops the password being required when the connection is from localhost. When this parameter is omitted, it will be regarded as "no".


# PasswordGet command
CMD_PasswordGet	Get Password Setting to Connect to VPN Client Service
CMD_PasswordGet_Help	Use this to get the setting that determines whether to input a password for occasions when the Command Line Management Utility and the VPN Client Manager connect to a VPN Client service to control it. \nIn the case when a password is requested, it also gets the setting that determines whether this password is only requested when operation is performed remotely (from a computer that is not localhost).
CMD_PasswordGet_Args	PasswordGet
CMD_PasswordGet_1	Definir senha
CMD_PasswordGet_2	Request Password for Remote Operation Only


# CertList command
CMD_CertList	Get List of Trusted CA Certificates
CMD_CertList_Help	Aqui você pode gerenciar a lista de certificados de autoridade de certificação que serão confiáveis ao VPN Cliente. Você pode usar a lista de certificados CA registrados para verificar os certificados do servidor ao conectar-se aos servidores VPN.
CMD_CertList_Args	ListaCert


# CertAdd command
CMD_CertAdd	Adicionar certificado CA confiável
CMD_CertAdd_Help	Use this to add a new certificate to a list of CA certificates trusted by the VPN Client. You can use the registered CA certificate list to verify server certificates when connecting to VPN Servers. \nTo get a list of the current certificates you can use the CertList command. \nThe certificate you add must be saved in the X.509 file format.
CMD_CertAdd_Args	CertAdd [path]
CMD_CertAdd_[path]	Specify the file name of the X.509 certificate to register.


# CertDelete command
CMD_CertDelete	Excluir certificado de CA confiável
CMD_CertDelete_Help	Use this to delete an existing certificate from a list of CA certificates trusted by the VPN Client. \nTo get a list of the current certificates you can use the CertList command.
CMD_CertDelete_Args	CertDelete [id]
CMD_CertDelete_[id]	Specify the ID of the certificate to delete.


# CertGet command
CMD_CertGet	Obter certificado de CA confiável
CMD_CertGet_Help	Use this to get an existing certificate from the list of CA certificates trusted by the VPN Client and save it as a file in X.509 format. 
CMD_CertGet_Args	CertGet [id] [/SAVECERT:path]
CMD_CertGet_[id]	Specify the ID of the certificate to get.
CMD_CertGet_SAVECERT	Specify the file name to save the certificate you obtained.


# SecureList command
CMD_SecureList	Get List of Usable Smart Card Types
CMD_SecureList_Help	Use this to display a list of smart cards that are supported by VPN Client. \nThe types of smart cards listed in this list have had their drivers installed on the current computer and are supported by VPN software. \r\nIf there is a type of smart card that is currently being used that does not appear in the list, it may be possible to enable use by updating the VPN software to a newer version.
CMD_SecureList_Args	SecureList


# SecureSelect command
CMD_SecureSelect	Select the Smart Card Type to Use
CMD_SecureSelect_Help	Use this to select the type of the smart card to be used by the VPN Client. \nTo get the list of usable smart card types, use the SecureList command. 
CMD_SecureSelect_Args	SecureSelect [id]
CMD_SecureSelect_[id]	Specify the ID of the smart card type.
CMD_SecureSelect_PROMPT_ID	ID of Smart Card Type to Use 


# SecureGet command
CMD_SecureGet	Get ID of Smart Card Type to Use
CMD_SecureGet_Help	Use this to get the ID of the smart card type that is set to be used for the current VPN Client. By viewing the results of the SecureList command based on this ID, you can get the type of the currently selected smart card. \nIf there is no smart card that is currently selected, 0 will be displayed for the ID.
CMD_SecureGet_Args	SecureGet
CMD_SecureGet_Print	The currently selected smart card ID is %u.
CMD_SecureGet_NoPrint	Currently, a smart card is not selected.


# NicCreate command
CMD_NicCreate	Criar um novo adapatador de rede virtual
CMD_NicCreate_Help	Use this to add a new Virtual Network Adapter to the system. You can give the virtual network adapter a name of your choice. \nYou can set a name that consists of alphanumeric characters for the virtual network adapter. For Windows 2000 or newer systems, this name can be up to 31 characters, but for Windows 98, 98SE and ME it can be up to 4 characters. \nIf the NicCreate command was called, a new virtual network adapter device driver will be installed on the operating system that the VPN Client is operating on. \nIn this case, depending on the operating system, a dialog box may appear to confirm if it is OK to install the device driver.
CMD_NicCreate_Args	NicCreate [name]
CMD_NicCreate_[name]	Especifique o nome do adaptador de rede virtual.
CMD_NicCreate_PROMPT_NAME	Nome do adaptador de rede virtual: 


# NicDelete command
CMD_NicDelete	Excluir adaptador de rede virtual
CMD_NicDelete_Help	Use this to delete an existing virtual network adapter from the system. \nWhen you delete a virtual network adapter from the system, all the connections which are using that virtual network adapter will be disconnected. \nAlso, the Connection Settings that are set to use a virtual network adapter that has been deleted will have their settings automatically changed to use another virtual network adapter. \nThis command can be used when VPN Client is operating on Windows 2000 or newer operating systems.
CMD_NicDelete_Args	NicDelete [name]
CMD_NicDelete_[name]	Especifique o nome do adaptador de rede virtual.


# NicUpgrade command
CMD_NicUpgrade	Upgrade Virtual Network Adapter Device Driver
CMD_NicUpgrade_Help	If the device driver version of the existing virtual network adapter is old, then this upgrades to the latest device driver that was bundled with the currently operating VPN client. Even if a upgrade is not performed, the device driver will be reinstalled. \nIn this case, depending on the operating system, a dialog box may appear to confirm if it is OK to install the device driver. \nThis command can be used when VPN Client is operating on Windows 2000 or newer operating systems.
CMD_NicUpgrade_Args	NicUpgrade [name]
CMD_NicUpgrade_[name]	Especifique o nome do adaptador de rede virtual.


# NicGetSetting command
CMD_NicGetSetting	Obter a configuração do adaptador de rede virtual
CMD_NicGetSetting_Help	Use this to get the MAC address setting of the existing virtual network adapter. \nThis command can be used when VPN Client is operating on Windows 2000 or newer operating systems.
CMD_NicGetSetting_Args	NicGetSetting [name]
CMD_NicGetSetting_[name]	Especifique o nome do adaptador de rede virtual.
CMD_NicGetSetting_1	Nome do dispositivo
CMD_NicGetSetting_2	Status
CMD_NicGetSetting_3	Endereço MAC
CMD_NicGetSetting_4	Versão
CMD_NicGetSetting_5	Nome do arquivo do driver
CMD_NicGetSetting_6	GUID


# NicSetSetting command
CMD_NicSetSetting	Mudar a configuração do adaptador de rede virtual
CMD_NicSetSetting_Help	Use this to change the MAC address setting of the existing virtual network adapter. When this command is executed, the currently operating virtual network adapter device drivers will be restarted. \nThis command can be used when VPN Client is operating on Windows 2000 or newer operating systems.
CMD_NicSetSetting_Args	NicSetSetting [name] [/MAC:mac]
CMD_NicSetSetting_[name]	Especifique o nome do adaptador de rede virtual.
CMD_NicSetSetting_MAC	Specify the MAC address you wish to set. \nSpecify a 6-byte hexadecimal string for the MAC address. \nExample: 00:AC:01:23:45:67 or 00-AC-01-23-45-67
CMD_NicSetSetting_PROMPT_MAC	MAC Address to Set: 


# NicEnable command
CMD_NicEnable	Ativar adaptador de rede virtual
CMD_NicEnable_Help	Use this to enable an existing, disabled virtual network adapter. \nThis command can be used when VPN Client is operating on Windows 2000 or newer operating systems.
CMD_NicEnable_Args	NicEnable [name]
CMD_NicEnable_[name]	Especifique o nome do adaptador de rede virtual.


# NicDisable command
CMD_NicDisable	Desativar adaptador de rede virtual
CMD_NicDisable_Help	Use this to disable an existing, enabled virtual network adapter. \nThis command can be used when VPN Client is operating on Windows 2000 or newer operating systems.
CMD_NicDisable_Args	NicDisable [name]
CMD_NicDisable_[name]	Especifique o nome do adaptador de rede virtual.


# NicList command
CMD_NicList	Obter lista de adaptadores de rede virtuais
CMD_NicList_Help	This allows you to get a list of virtual network adapters registered on the current system.
CMD_NicList_Args	ListaNic


# AccountList command
CMD_AccountList	Get List of VPN Connection Settings
CMD_AccountList_Help	Use this to get a list of VPN Connection Settings registered on the VPN Client.
CMD_AccountList_Args	AccountList


# AccountCreate command
CMD_AccountCreate	Criar nova configuração de conexão VPN...
CMD_AccountCreate_Help	Use this to create a new VPN Connection Setting on the VPN Client. \nTo create a VPN Connection Setting, in addition to specifying the VPN Connection Setting name and destination server as initial parameters and the destination virtual Hub, and user name, you must also specify the name of the virtual network adapter to use. When a new VPN Connection Setting is created, the type of user authentication is initially set as Anonymous Authentication and the proxy server setting and the verification options of the server certificate is not set. To change these settings and other advanced settings after the VPN Connection Setting has been created, use the other commands that begin with the name "Account".
CMD_AccountCreate_Args	AccountCreate [name] [/SERVER:hostname:port] [/HUB:hubname] [/USERNAME:username] [/NICNAME:nicname]
CMD_AccountCreate_[name]	Specify the name of the VPN Connection Setting to create.
CMD_AccountCreate_SERVER	Specify the host name and port number of the destination VPN Server using the format [host name:port number]. You can also specify by IP address.
CMD_AccountCreate_HUB	Specify the Virtual Hub on the destination VPN Server.
CMD_AccountCreate_USERNAME	Specify the user name to use for user authentication when connecting to the destination VPN Server.
CMD_AccountCreate_NICNAME	Especificque o adaptador de rede virtual a ser usado na conexão.
CMD_AccountCreate_Prompt_Name	Name of VPN Connection Setting: 
CMD_AccountCreate_Prompt_Server	Destination VPN Server Host Name and Port Number: 
CMD_AccountCreate_Prompt_Hub	Nome do hub virtual de destino: 
CMD_AccountCreate_Prompt_Username	Nome de usuário da conexão: 
CMD_AccountCreate_Prompt_Nicname	Used Virtual Network Adapter Name: 


# AccountSet command
CMD_AccountSet	Set the VPN Connection Setting Connection Destination
CMD_AccountSet_Help	Use this to set, for the VPN Connection Setting registered on the VPN Client, the destination VPN Server host name and port number, Virtual Hub name, user name used for connection and virtual network adapter name to use.
CMD_AccountSet_Args	AccountSet [name] [/SERVER:hostname:port] [/HUB:hubname]
CMD_AccountSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountSet_SERVER	Specify the host name and port number of the destination VPN Server using the format "host name:port number". You can also specify by IP address.
CMD_AccountSet_HUB	Specify the Virtual Hub on the destination VPN Server.


# AccountGet command
CMD_AccountGet	Get Setting of VPN Connection Setting 
CMD_AccountGet_Help	Use this to get the VPN Connection Setting contents of a VPN Connection Setting registered on the VPN Client. \nTo change the VPN Connection Setting contents of the VPN Connection Setting, use the other commands that begin with the name "Account" after creating the VPN Connection Setting.
CMD_AccountGet_Args	AccountGet [name]
CMD_AccountGet_[name]	Specify the name of the VPN Connection Setting whose setting you want to get.


# AccountDelete command
CMD_AccountDelete	Excluir configuração de conexão VPN
CMD_AccountDelete_Help	Use this to delete VPN Connection Setting that is registered on the VPN Client. If the specified VPN Connection Setting has a status of online, the connections will be automatically disconnected and then the VPN Connection Setting will be deleted.
CMD_AccountDelete_Args	AccountDelete [name]
CMD_AccountDelete_[name]	Specify the name of the VPN Connection Setting to delete.


# AccountUsernameSet command
CMD_AccountUsernameSet	Set User Name of User to Use Connection of VPN Connection Setting
CMD_AccountUsernameSet_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to the VPN Server, use this to specify the user name required for user authentication. \nIn some cases it is necessary to specify the type of user authentication and specify the required parameters. To change this information you can use commands such as AccountAnonymousSet, AccountPasswordSet, AccountCertSet and AccountSecureCertSet.
CMD_AccountUsernameSet_Args	AccountUsernameSet [name] [/USERNAME:username]
CMD_AccountUsernameSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountUsernameSet_USERNAME	Specify the user name required for user authentication when the VPN Connection Setting connects to the VPN Server.
CMD_AccountUsername_Notice	The auth type for this VPN Connection Setting is currently set as password authentication. After changing the user name, you must use the AccountPasswordSet command to reset the password.


# AccountAnonymousSet command
CMD_AccountAnonymousSet	Set User Authentication Type of VPN Connection Setting to Anonymous Authentication
CMD_AccountAnonymousSet_Help	Use this to set the user auth type to [Anonymous Authentication] for when a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to the VPN Server.
CMD_AccountAnonymousSet_Args	AccountAnonymousSet [name]
CMD_AccountAnonymousSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountPasswordSet command
CMD_AccountPasswordSet	Set User Authentication Type of VPN Connection Setting to Password Authentication
CMD_AccountPasswordSet_Help	Use this to set the user auth type to Password Authentication for when a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to the VPN Server. Specify Standard Password Authentication and RADIUS or NT Domain Authentication as the password authentication type.
CMD_AccountPasswordSet_Args	AccountPasswordSet [name] [/PASSWORD:password] [/TYPE:standard|radius]
CMD_AccountPasswordSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountPasswordSet_PASSWORD	Specify the password to use for password authentication. If this is not specified, a prompt will appear to input the password.
CMD_AccountPasswordSet_TYPE	Specify either "standard" (Standard Password Authentication) or "radius" (RADIUS or NT Domain Authentication) as the password authentication type.
CMD_AccountPasswordSet_Prompt_Type	Especificar padrão ou radius: 
CMD_AccountPasswordSet_Type_Invalid	The standard or radius specification is invalid.


# AccountCertSet command
CMD_AccountCertSet	Set User Authentication Type of VPN Connection Setting to Client Certificate Authentication
CMD_AccountCertSet_Help	Use this to set the user auth type to Client Certificate Authentication for when a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to the VPN Server. For this certificate, you must specify a certificate file in the X.509 format and a private key file that is Base 64 encoded.
CMD_AccountCertSet_Args	AccountCertSet [name] [/LOADCERT:cert] [/LOADKEY:key]
CMD_AccountCertSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountCertSet_LOADCERT	Specify the X.509 format certificate file to provide for certificate authentication.
CMD_AccountCertSet_LOADKEY	Specify the Base-64-encoded private key file name for the certificate.


# AccountCertGet command
CMD_AccountCertGet	Get Client Certificate to Use for Cascade Connection
CMD_AccountCertGet_Help	When a VPN Connection Setting registered on VPN Client is specified and that VPN Connection Setting uses client certificate authentication, use this to get the certificate that is provided as the client certificate and save the certificate file in X.509 format.
CMD_AccountCertGet_Args	AccountCertGet [name] [/SAVECERT:cert]
CMD_AccountCertGet_[name]	Specify the name of the VPN Connection Setting whose setting you want to get.
CMD_AccountCertGet_SAVECERT	Specify the file name to save the certificate you obtained in X.509 format.


# AccountEncryptEnable command
CMD_AccountEncryptEnable	Enable Encryption when Communicating by VPN Connection Setting
CMD_AccountEncryptEnable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers to be encrypted by SSL. \nNormally communication between VPN Servers is encrypted by SSL to prevent eavesdropping of information and fraud. You can also disable encryption. When encryption is disabled, the communication throughput improves but the communication data flows over the network in plain text.
CMD_AccountEncryptEnable_Args	AccountEncryptEnable [name]
CMD_AccountEncryptEnable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountEncryptDisable command
CMD_AccountEncryptDisable	Disable Encryption when Communicating by VPN Connection Setting
CMD_AccountEncryptDisable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers not to be encrypted. \nNormally communication between VPN Servers is encrypted by SSL to prevent eavesdropping of information and fraud. You can also disable encryption. When encryption is disabled, the communication throughput improves but the communication data flows over the network in plain text.
CMD_AccountEncryptDisable_Args	AccountEncryptDisable [name]
CMD_AccountEncryptDisable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountCompressEnable command
CMD_AccountCompressEnable	Enable Data Compression when Communicating by VPN Connection Setting
CMD_AccountCompressEnable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers to be compressed. \nIt is possible to achieve a maximum of 80% compression. Compression however places higher loads on the CPU of both the client and server machines. When the line speed is about 10 Mbps or greater, compression can lower throughput, but sometimes it can have the opposite effect.
CMD_AccountCompressEnable_Args	AccountCompressEnable [name]
CMD_AccountCompressEnable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountCompressDisable command
CMD_AccountCompressDisable	Disable Data Compression when Communicating by VPN Connection Setting
CMD_AccountCompressDisable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting is used for communication between VPN Servers via a VPN connection, use this to set the communication contents between the VPN Servers not to be compressed.
CMD_AccountCompressDisable_Args	AccountCompressDisable [name]
CMD_AccountCompressDisable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountHttpHeader* commands
CMD_AccountHttpHeader_Prompt_Name	Value name (part before the colon): 
CMD_AccountHttpHeader_Prompt_Data	Dados do valor (parte após os dois pontos): 


# AccountHttpHeaderAdd command
CMD_AccountHttpHeaderAdd	Add a custom value in the HTTP header sent to the proxy server
CMD_AccountHttpHeaderAdd_Help	Use this to add a custom value in the HTTP header sent to the proxy server. A custom HTTP header can be used to bypass certain restrictions imposed on the network or to avoid speed limitations applied by the QoS.
CMD_AccountHttpHeaderAdd_Args	AccountHttpHeaderAdd [name] [/NAME:name] [/DATA:data]
CMD_AccountHttpHeaderAdd_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountHttpHeaderAdd_NAME	Specify the name of the custom value (the part before the colon character).
CMD_AccountHttpHeaderAdd_DATA	Specify the data of the custom value (the part after the colon character).


# AccountHttpHeaderDelete command
CMD_AccountHttpHeaderDelete	Delete a custom value in the HTTP header sent to the proxy server
CMD_AccountHttpHeaderDelete_Help	Use this to delete a custom value in the HTTP header sent to the proxy server. A custom HTTP header can be used to bypass certain restrictions imposed on the network or to avoid speed limitations applied by the QoS.
CMD_AccountHttpHeaderDelete_Args	AccountHttpHeaderDelete [name] [/NAME:name]
CMD_AccountHttpHeaderDelete_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountHttpHeaderDelete_NAME	Specify the name of the custom value (the part before the colon character).


# AccountHttpHeaderGet command
CMD_AccountHttpHeaderGet	Get the list of custom values in the HTTP header sent to the proxy server
CMD_AccountHttpHeaderGet_Help	Use this to get the list of custom values in the HTTP header sent to the proxy server. A custom HTTP header can be used to bypass certain restrictions imposed on the network or to avoid speed limitations applied by the QoS.
CMD_AccountHttpHeaderGet_Args	AccountHttpHeaderGet [name]
CMD_AccountHttpHeaderGet_[name]	Specify the name of the VPN Connection Setting whose setting you want to get.


# AccountProxyNone command
CMD_AccountProxyNone	Specify Direct TCP/IP Connection as the Connection Method of VPN Connection Setting
CMD_AccountProxyNone_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to set Direct TCP/IP Connection as the connection method to use, in which case the connection route will not be via a proxy server.
CMD_AccountProxyNone_Args	AccountProxyNone [name]
CMD_AccountProxyNone_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountProxyHttp command
CMD_AccountProxyHttp	Set Connection Method of VPN Connection Setting to be via an HTTP Proxy Server
CMD_AccountProxyHttp_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to set Connect via HTTP Proxy Server as the method of connection to use, which requires the specification of the host name and port number of the HTTP Proxy server to communicate via as well as a user name and password (when required). \nThe HTTP proxy server that communication will travel via must be compatible with the CONNECT method to use HTTPS communication.
CMD_AccountProxyHttp_Args	AccountProxyHttp [name] [/SERVER:hostname:port] [/USERNAME:username] [/PASSWORD:password]
CMD_AccountProxyHttp_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountProxyHttp_SERVER	Specify the host name or IP address, and port number of the on-route HTTP proxy server using the format [host name:port number].
CMD_AccountProxyHttp_USERNAME	When user authentication is required to connect to the on-route HTTP proxy server, specify the user name. Also, specify the /PASSWORD parameter at the same time. If the parameters /USERNAME and /PASSWORD are not specified, the user authentication data will not be set.
CMD_AccountProxyHttp_PASSWORD	When user authentication is required to connect to the on-route HTTP proxy server, specify the password. Specify this together with the /USERNAME parameter.
CMD_AccountProxyHttp_Prompt_Server	Proxy Server Host Name and Port Number: 


# AccountProxySocks command
CMD_AccountProxySocks	Set Connection Method of VPN Connection Setting to be via a SOCKS4 Proxy Server
CMD_AccountProxySocks_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to set Connect via SOCKS4 Proxy Server as the method of connection to use, which requires the specification of the host name and port number of the SOCKS4 Proxy server to communicate via as well as a user name and password (when required).
CMD_AccountProxySocks_Args	AccountProxySocks [name] [/SERVER:hostname:port] [/USERNAME:username] [/PASSWORD:password]
CMD_AccountProxySocks_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountProxySocks_SERVER	Specify the host name or IP address, and port number of the on-route SOCKS4 proxy server using the format [host name:port number].
CMD_AccountProxySocks_USERNAME	When user authentication is required to connect to the on-route SOCKS4 proxy server, specify the user name. Also, specify the /PASSWORD parameter at the same time. If the parameters /USERNAME and /PASSWORD are not specified, the user authentication data will not be set.
CMD_AccountProxySocks_PASSWORD	When user authentication is required to connect to the on-route SOCKS4 proxy server, specify the password. Specify this together with the /USERNAME parameter.


# AccountProxySocks5 command
CMD_AccountProxySocks5	Set Connection Method of VPN Connection Setting to be via a SOCKS5 Proxy Server
CMD_AccountProxySocks5_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to set Connect via SOCKS5 Proxy Server as the method of connection to use, which requires the specification of the host name and port number of the SOCKS5 Proxy server to communicate via as well as a user name and password (when required).
CMD_AccountProxySocks5_Args	AccountProxySocks5 [name] [/SERVER:hostname:port] [/USERNAME:username] [/PASSWORD:password]
CMD_AccountProxySocks5_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountProxySocks5_SERVER	Specify the host name or IP address, and port number of the on-route SOCKS5 proxy server using the format [host name:port number].
CMD_AccountProxySocks5_USERNAME	When user authentication is required to connect to the on-route SOCKS5 proxy server, specify the user name. Also, specify the /PASSWORD parameter at the same time. If the parameters /USERNAME and /PASSWORD are not specified, the user authentication data will not be set.
CMD_AccountProxySocks5_PASSWORD	When user authentication is required to connect to the on-route SOCKS5 proxy server, specify the password. Specify this together with the /USERNAME parameter.


# AccountServerCertEnable command
CMD_AccountServerCertEnable	Enable VPN Connection Setting Server Certificate Verification Option
CMD_AccountServerCertEnable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to enable the option to check whether the SSL certificate provided by the destination VPN Server can be trusted. \nIf this option is enabled, we recommend that you either use the AccountServerCertSet command to save the connection destination server SSL certificate beforehand in the VPN Connection Setting settings beforehand, or use the CertAdd command etc. to register a root certificate containing the signed server SSL certificate in the list of Virtual Hub trusted CA certificates. If it is not registered, a confirmation message sometimes is displayed on the initial connection. \nIf the certificate of the connected VPN Server cannot be trusted under the condition where the option to verify server certificates has been enabled for the VPN Connection Setting, the connection will be promptly cancelled and continual reattempts at connection will be made.
CMD_AccountServerCertEnable_Args	AccountServerCertEnable [name]
CMD_AccountServerCertEnable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountServerCertDisable command
CMD_AccountServerCertDisable	Disable VPN Connection Setting Server Certificate Verification Option
CMD_AccountServerCertDisable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to disable the option to check whether the SSL certificate provided by the destination VPN Server can be trusted.
CMD_AccountServerCertDisable_Args	AccountServerCertDisable [name]
CMD_AccountServerCertDisable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountRetryOnServerCertEnable command
CMD_AccountRetryOnServerCertEnable	Enable VPN connection retry if server certificate is invalid
CMD_AccountRetryOnServerCertEnable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to enable the option to retry connection if Server certificate cannot be trusted.
CMD_AccountRetryOnServerCertEnable_Args	AccountRetryOnServerCertEnable [name]
CMD_AccountRetryOnServerCertEnable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountRetryOnServerCertDisable command
CMD_AccountRetryOnServerCertDisable	Disable VPN connection retry if server certificate is invalid
CMD_AccountRetryOnServerCertDisable_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to disable the option to retry connection if Server certificate cannot be trusted.
CMD_AccountRetryOnServerCertDisable_Args	AccountRetryOnServerCertDisable [name]
CMD_AccountRetryOnServerCertDisable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountDefaultCAEnable command
CMD_AccountDefaultCAEnable	        Enable Trust System Certificate Store Option
CMD_AccountDefaultCAEnable_Help	    When server certificate verification is enabled, use this to enable trusting certificates from the system trust store. \nIf server certificate verification is disabled, this option does nothing.
CMD_AccountDefaultCAEnable_Args	    AccountDefaultCAEnable [name]
CMD_AccountDefaultCAEnable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountDefaultCADisable command
CMD_AccountDefaultCADisable         Disable Trust System Certificate Store Option
CMD_AccountDefaultCADisable_Help    When server certificate verification is enabled, use this to disable trusting certificates from the system trust store. \nIf server certificate verification is disabled, this option does nothing.
CMD_AccountDefaultCADisable_Args	AccountDefaultCADisable [name]
CMD_AccountDefaultCADisable_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountServerCertSet command
CMD_AccountServerCertSet	Set Server Individual Certificate for VPN Connection Setting
CMD_AccountServerCertSet_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to a VPN Server, use this to register the same certificate as the SSL certificate provided by the destination VPN Server. \nIf the option to verify server certificates for VPN Connection Settings is enabled, you must either use this command to save the connection destination server SSL certificate beforehand in the VPN Connection Setting settings beforehand, or use the CAAdd command etc. to register a root certificate containing the signed server SSL certificate in the list of Virtual Hub trusted CA certificates. \nIf the certificate of the connected VPN Server cannot be trusted under the condition where the option to verify server certificates has been enabled for the VPN Connection Setting, the connection will be promptly cancelled and continual reattempts at connection will be made.
CMD_AccountServerCertSet_Args	AccountServerCertSet [name] [/LOADCERT:cert]
CMD_AccountServerCertSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountServerCertSet_LOADCERT	Specify X.509 format certificate file name that the server individual certificate which you wish to set is saved under.


# AccountServerCertDelete command
CMD_AccountServerCertDelete	Delete Server Individual Certificate for VPN Connection Setting
CMD_AccountServerCertDelete_Help	When a VPN Connection Setting registered on the VPN Client is specified and a server individual certificate is registered for that VPN Connection Setting, use this to delete that certificate.
CMD_AccountServerCertDelete_Args	AccountServerCertDelete [name]
CMD_AccountServerCertDelete_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountServerCertGet command
CMD_AccountServerCertGet	Get Server Individual Certificate for VPN Connection Setting
CMD_AccountServerCertGet_Help	When a VPN Connection Setting is specified and a server Individual certificate is registered for that VPN Connection Setting, use this to get that certificate and save it as an X.509 format certificate file. 
CMD_AccountServerCertGet_Args	AccountServerCertGet [name] [/SAVECERT:path]
CMD_AccountServerCertGet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountServerCertGet_SAVECERT	Specify the certificate file name to save the server individual certificate in X.509 format.


# AccountDetailSet command
CMD_AccountDetailSet	Set Advanced Settings for VPN Connection Setting
CMD_AccountDetailSet_Help	Use this to customize the VPN protocol communication settings used when a VPN Connection Setting registered on a VPN Client is specified and that VPN Connection Setting connects to the VPN Server.
CMD_AccountDetailSet_Args	AccountDetailSet [name] [/MAXTCP:max_connection] [/INTERVAL:additional_interval] [/TTL:disconnect_span] [/HALF:yes|no] [/BRIDGE:yes|no] [/MONITOR:yes|no] [/NOTRACK:yes|no] [/NOQOS:yes|no]
CMD_AccountDetailSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountDetailSet_MAXTCP	Specify, using an integer in the range 1 to 32, the number of TCP connections to be used for VPN communication. By using data transmission by multiple TCP connections for VPN communication sessions with VPN Servers it is sometimes possible to increase communication speed. \nNote: We recommend about 8 lines when the connection lines to the server are fast, and 1 line when using a slow connection such as dialup.
CMD_AccountDetailSet_INTERVAL	When communicating by VPN by establishing multiple TCP connections, specify in seconds, the establishing interval for each TCP connection. The standard value is 1 second.
CMD_AccountDetailSet_TTL	When specifying connection life of each TCP connection specify in seconds the keep-alive time from establishing a TCP connection until disconnection. If 0 is specified, keep-alive will not be set.
CMD_AccountDetailSet_HALF	Specify "yes" when enabling half duplex mode. When using two or more TCP connections for VPN communication, it is possible to use Half Duplex Mode. By enabling half duplex mode it is possible to automatically fix data transmission direction as half and half for each TCP connection. In the case where a VPN using 8 TCP connections is established, for example, when half-duplex is enabled, communication can be fixes so that 4 TCP connections are dedicated to the upload direction and the other 4 connections are dedicated to the download direction.
CMD_AccountDetailSet_BRIDGE	Specify "yes" when connecting to the VPN Server using Bridge / Router Mode. When using Bridge / Router Mode to connect, it is possible to provide bridging or routing to another network on the side of the virtual network adapter of the VPN Client. However, if the security policy of the user who is being used for connection denies the use of bridges or routing, then connection will fail.
CMD_AccountDetailSet_MONITOR	Specify "yes" when connecting to the VPN Server using Monitoring Mode. When a connection is made using Monitoring Mode, you can receive all packets that flow through the Virtual Hub. However, if the security policy of the user who is being used for connection does not allow Monitoring Mode, then connection will fail.
CMD_AccountDetailSet_NOTRACK	Especificar "sim" desativará os ajustes da tabela de roteamento. Normalmente "não" é especificado.
CMD_AccountDetailSet_NOQOS	Specify "yes" when disabling VoIP / QoS functions. Normally "no" is specified.
CMD_AccountDetailSet_DISABLEUDP	Specify "yes" when disabling UDP acceleration function. Normally "no" is specified.
CMD_AccountDetailSet_Eval_MaxTcp	Specify an integer in the range 1 to 32 for the number of TCP connections.
CMD_AccountDetailSet_Eval_Interval	Set at least 1 second for the interval to establish a TCP connection.
CMD_AccountDetailSet_Prompt_MaxTcp	Número de conexões TCP a serem usadas na comunicação VPN: 
CMD_AccountDetailSet_Prompt_Interval	Interval between Establishing Each TCP Connection: 
CMD_AccountDetailSet_Prompt_TTL	Connection Life of Each TCP Connection (0 for no keep-alive): 
CMD_AccountDetailSet_Prompt_HALF	Enable Half-Duplex Mode (yes/no): 
CMD_AccountDetailSet_Prompt_BRIDGE	Enable Bridge / Router Mode (yes/no): 
CMD_AccountDetailSet_Prompt_MONITOR	Enable Monitoring Mode (yes/no): 
CMD_AccountDetailSet_Prompt_NOTRACK	Disable Adjustment of Routing Table (yes/no): 
CMD_AccountDetailSet_Prompt_NOQOS	 Disable QoS Control Function (yes/no): 
CMD_AccountDetailSet_Prompt_DISABLEUDP	 Desativar função de aceleração UDP (sim/não): 


# AccountRename command
CMD_AccountRename	Change VPN Connection Setting Name
CMD_AccountRename_Help	Use this to specify a VPN Connection Setting registered on the VPN Client and change its name.
CMD_AccountRename_Args	AccountRename [name] [/NEW:new_name]
CMD_AccountRename_[name]	Specify the current name of the VPN Connection Setting whose name you want to change.
CMD_AccountRename_NEW	Specify the new name after the change.
CMD_AccountRename_PROMPT_OLD	Nome atual: 
CMD_AccountRename_PROMPT_NEW	Novo Nome: 


# AccountConnect command
CMD_AccountConnect	Start Connection to VPN Server using VPN Connection Setting
CMD_AccountConnect_Help	Use this to specify a VPN Connection Setting registered on the VPN Client and start a connection to the VPN Server using that VPN Connection Setting. A VPN Connection Setting that has a connecting status or a connected status will continue to be connected to the VPN Server, or continue to attempt to connect to the VPN Server until the AccountDisconnect command is used to disconnect the connection (Note however, if the AccountRetrySet command is used to specify the number of retries, connection attempts will be aborted when the specified value is reached.)
CMD_AccountConnect_Args	AccountConnect [name]
CMD_AccountConnect_[name]	Specify the name of the VPN Connection Setting whose connection you want to start.


# AccountDisconnect command
CMD_AccountDisconnect	Disconnect VPN Connection Setting During Connection
CMD_AccountDisconnect_Help	Use this to specify a VPN Connection Setting that is registered on the VPN Client and that is either in the condition of connecting or is connected, and immediately disconnect it.
CMD_AccountDisconnect_Args	AccountDisconnect [name]
CMD_AccountDisconnect_[name]	Specify the name of the VPN Connection Setting to disconnect.


# AccountStatusGet command
CMD_AccountStatusGet	Get Current VPN Connection Setting Status
CMD_AccountStatusGet_Help	When a VPN Connection Setting that is registered on the VPN Client is specified and that VPN Connection Setting is currently connected, use this to get its connection status and other information.
CMD_AccountStatusGet_Args	AccountStatusGet [name]
CMD_AccountStatusGet_[name]	Specify the name of the VPN Connection Setting whose information you want to get.


# AccountNicSet command
CMD_AccountNicSet	Set Virtual Network Adapter for VPN Connection Setting to Use
CMD_AccountNicSet_Help	Use this to change the Virtual Network Adapter name that the existing VPN Connection Settings registered on the VPN Client will use for the connection to a VPN Server.
CMD_AccountNicSet_Args	AccountNicSet [name] [/NICNAME:nicname]
CMD_AccountNicSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountNicSet_NICNAME	Especifique o nome do adaptador de rede virtual a ser usado ao conectar-se ao servidor VPN.


# AccountStatusShow command
CMD_AccountStatusShow	Set Connection Status and Error Screen to Display when Connecting to VPN Server
CMD_AccountStatusShow_Help	When a communication setting is registered on the VPN Client and that communication setting is being used to connect to the VPN Server, use this to set the connection status and error screen to be displayed on the computer display.
CMD_AccountStatusShow_Args	AccountStatusShow [name]
CMD_AccountStatusShow_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountStatusHide command
CMD_AccountStatusHide	Set Connection Status and Error Screen to be Hidden when Connecting to VPN Server
CMD_AccountStatusHide_Help	When a communication setting is registered on the VPN Client and that communication setting is being used to connect to the VPN Server, use this to set the connection status and error screen to not be displayed on the computer display.
CMD_AccountStatusHide_Args	AccountStatusHide [name]
CMD_AccountStatusHide_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountSecureCertSet command
CMD_AccountSecureCertSet	Set User Authentication Type of VPN Connection Setting to Smart Card Authentication
CMD_AccountSecureCertSet_Help	Use this to set the user auth type to Smart Card Authentication for when a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting connects to the VPN Server. Also, you must specify the names of the certificate object and the private key object stored on the smart card.
CMD_AccountSecureCertSet_Args	AccountSecureCertSet [name] [/CERTNAME:cert] [/KEYNAME:key]
CMD_AccountSecureCertSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountSecureCertSet_CERTNAME	Specify the name of the certificate object stored on the smart card.
CMD_AccountSecureCertSet_KEYNAME	Specify the name of the private key object stored on the smart card. The private key must be compatible with the certificate specified by /CERTNAME.
CMD_AccountSecureCertSet_PROMPT_CERTNAME	Name of Certificate Object on Smart Card: 
CMD_AccountSecureCertSet_PROMPT_KEYNAME	Name of Private Key Object on Smart Card: 


# PcAccountOpensslEngineCertSet
CMD_AccountOpensslCertSet_PROMPT_KEYNAME Specify the openssl engine specific key name: 
CMD_AccountOpensslCertSet_PROMPT_ENGINENAME Specify the openssl engine name: 


# AccountRetrySet command
CMD_AccountRetrySet	Set Interval between Connection Retries for Connection Failures or Disconnections of VPN Connection Setting
CMD_AccountRetrySet_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting attempts to connect to a VPN Server, use this to specify the interval to wait between connection attempts and the limit of how many times to retry connecting when communication with the VPN Server has been disconnected or when the connection process failed. \nIf the user authentication type is Smart Card Authentication, no connection retry will be performed regardless of the Number of Connection Attempts setting.
CMD_AccountRetrySet_Args	AccountRetrySet [name] [/NUM:num_retry] [/INTERVAL:retry_interval]
CMD_AccountRetrySet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.
CMD_AccountRetrySet_NUM	Specify the number of times to make consecutive retries. By specifying "999", there will be limitless attempts to reconnection (always connect). By specifying "0", not attempt at reconnection will be made.
CMD_AccountRetrySet_INTERVAL	When attempting a reconnection, this sets how many seconds to wait after the previous disconnection or connection failure before starting the reconnection process.
CMD_AccountRetrySet_PROMPT_NUM	Reconnection Count ("999" is unlimited): 
CMD_AccountRetrySet_PROMPT_INTERVAL	Reconnection Interval (Seconds): 
CMD_AccountRetrySet_EVAL_INTERVAL	Specify 5 seconds or more for the retries interval.


# AccountStartupSet command
CMD_AccountStartupSet	Set VPN Connection Setting as Startup Connection
CMD_AccountStartupSet_Help	Use this to specify a VPN Connection Setting registered on the VPN Client and set it as the startup connection. The VPN Connection Setting that is set as the startup connection will automatically start the connection process when the VPN Client service starts.
CMD_AccountStartupSet_Args	AccountStartupSet [name]
CMD_AccountStartupSet_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountStartupRemove command
CMD_AccountStartupRemove	Remove Startup Connection of VPN Connection Setting 
CMD_AccountStartupRemove_Help	When a VPN Connection Setting registered on the VPN Client is specified and that VPN Connection Setting is currently set as a startup connection, use this to delete the startup connection.
CMD_AccountStartupRemove_Args	AccountStartupRemove [name]
CMD_AccountStartupRemove_[name]	Specify the name of the VPN Connection Setting whose setting you want to change.


# AccountExport command
CMD_AccountExport	Exportar configuração de conexão VPN
CMD_AccountExport_Help	Use this to specify a VPN Connection Setting registered on the VPN Client and export its contents as a text file. By exporting a VPN Connection Setting file, and then later, importing it, you can duplicate the contents of a VPN Connection Setting. Also, because it gets saved as a text file, you can edit the contents using a conventional text editor. \nThe export destination file is saved as a UTF-8 format text file. Also, it is convenient to save the file name with the file extension .vpn as this file extension is associated to the Windows Edition VPN Client Manager.
CMD_AccountExport_Args	AccountExport [name] [/SAVEPATH:savepath]
CMD_AccountExport_[name]	Specify the name of the VPN Connection Setting to export.
CMD_AccountExport_SAVEPATH	Specify a file name for the save destination.
CMD_AccountExport_PROMPT_SAVEPATH	Save Destination File Name (recommended extension: vpn): 


# AccountImport command
CMD_AccountImport	Importar configuração de conexão VPN
CMD_AccountImport_Help	Use this to import the VPN Connection Setting file that has been exported by the AccountExport command and add it to the VPN Client.
CMD_AccountImport_Args	AccountImport [path]
CMD_AccountImport_[path]	Specify the file name of the import source.
CMD_AccountImport_PROMPT_PATH	Import Source File Name: 
CMD_AccountImport_FAILED_PARSE	Unable to correctly parse the specified file. Please check it if the file was exported correctly.
CMD_AccountImport_OK	The VPN Connection Setting "%s" has been imported.


# RemoteEnable command
CMD_RemoteEnable	Allow Remote Management of VPN Client Service
CMD_RemoteEnable_Help	Use this to allow management of a VPN Client service from a remote computer that is not localhost, via a remote connection by Command Line Management Utility or VPN Client Manager.
CMD_RemoteEnable_Args	RemoteEnable


# RemoteDisable command
CMD_RemoteDisable	Deny Remote Management of VPN Client Service
CMD_RemoteDisable_Help	Use this to deny management of a VPN Client service from a remote computer that is not localhost, via a remote connection by Command Line Management Utility or VPN Client Manager.
CMD_RemoteDisable_Args	RemoteDisable


###################################################


#                                                 #


# Commands for VPN Tools are listed below         #


#                                                 #


###################################################


# GenX25519 command
CMD_GenX25519				Create new X25519 keypair
CMD_GenX25519_Help			Use this to create a new X25519 keypair, which can be used for WireGuard. \nBoth the private and public key will be shown. \nThe public key can be shared and is used to identify a peer. \nAlso, it can always be retrieved from the private key using the GetPublicX25519 command. \nThe private key should be kept in a secure place and never be shared. \nIt cannot be recovered once lost.
CMD_GenX25519_ARGS			GenX25519
CMD_GenX25519_PRIVATE_KEY	Private key: 
CMD_GenX25519_PUBLIC_KEY	Public key: 


# GetPublicX25519 command
CMD_GetPublicX25519				Retrieve public X25519 key from a private one
CMD_GetPublicX25519_Help		Use this if you have a private X25519 key and want to get its corresponding public key.
CMD_GetPublicX25519_ARGS    	GetPublicX25519 [private]
CMD_GetPublicX25519_[private]	The private X25519 key you want to get the corresponding public key of.
CMD_GetPublicX25519_PRIVATE_KEY	Private key: 
CMD_GetPublicX25519_PUBLIC_KEY	Public key: 


# MakeCert command
CMD_MakeCert	Create New X.509 Certificate and Private Key (1024 bit)
CMD_MakeCert_Help	Use this to create a new X.509 certificate and private key and save it as a file. \nThe algorithm used to create the public key and private key of the certificate is RSA 1024 bit. \nYou can choose to create a root certificate (self-signed certificate) or a certificate signed by another certificate. To create a certificate that is signed by another certificate, you require a private key file (base 64 encoded) that is compatible with the certificate that uses the signature (X.509 format file). \n\nWhen creating a certificate, you can specify the following: Name (CN), Organization (O), Organization Unit (OU), Country (C), State (ST), Locale (L), Serial Number, and Expiration Date. \nThe created certificate will be saved as an X.509 format file and the private key file will be saved in a Base 64 encoded RSA 1024 bit format file. \n\nThe MakeCert command is a tool that provides the most rudimentary function for creating certificates. If you want to create a more substantial certificate, we recommend that you use either free software such as OpenSSL, or commercial CA (certificate authority) software. \n\nNote: This command can be called from the SoftEther VPN Command Line Management Utility. You can also execute this command while connected to the current VPN Server or VPN Client in Administration Mode but, what actually performs the RSA computation, generates the certificate data and saves it to file is the computer on which the command is running, and all this is executed in a context that has absolutely no relationship to the computer that is the destination of the Administration Mode connection.
CMD_MakeCert_Args	MakeCert [/CN:cn] [/O:o] [/OU:ou] [/C:c] [/ST:st] [/L:l] [/SERIAL:serial] [/EXPIRES:expires] [/SIGNCERT:signcert] [/SIGNKEY:signkey] [/SAVECERT:savecert] [/SAVEKEY:savekey]
CMD_MakeCert_CN	Specify the Name (CN) item of the certificate to create. You can specify "none".
CMD_MakeCert_O	Specify the Organization (O) item of the certificate to create. You can specify "none".
CMD_MakeCert_OU	Specify the Organization Unit (OU) item of the certificate to create. You can specify "none".
CMD_MakeCert_C	Specify the Country (C) item of the certificate to create. You can specify "none".
CMD_MakeCert_ST	Specify the State (ST) item of the certificate to create. You can specify "none".
CMD_MakeCert_L	Specify the Locale (L) item of the certificate to create. You can specify "none".
CMD_MakeCert_SERIAL	Specify the Serial Number item of the certificate to create. Specify using hexadecimal values. You can specify "none".
CMD_MakeCert_EXPIRES	Specify the Expiration Date item of the certificate to create. If you specify "none" or "0", 3650 days (approx. 10 years) will be used. You can specify a maximum of 10950 days (about 30 years).
CMD_MakeCert_SIGNCERT	For cases when the certificate to be created is signed by an existing certificate, specify the X.509 format certificate file name to be used to sign the signature. When this parameter is omitted, such signature signing is not performed and the new certificate is created as a root certificate.
CMD_MakeCert_SIGNKEY	Specify a private key (RSA, base-64 encoded) that is compatible with the certificate specified by /SIGNCERT.
CMD_MakeCert_SAVECERT	Specify the file name to save the certificate you created. The certificate is saved as an X.509 file that includes a public key that is RSA format 1024 bit.
CMD_MakeCert_SAVEKEY	Specify the file name to save private key that is compatible with the certificate you created. The private key will be saved as an RSA-format 1024-bit private key file.
CMD_MakeCert_PROMPT_CN	Name of Certificate to Create (CN): 
CMD_MakeCert_PROMPT_O	Organization of Certificate to Create (O): 
CMD_MakeCert_PROMPT_OU	Organization Unit of Certificate to Create (OU): 
CMD_MakeCert_PROMPT_C	Country of Certificate to Create (C): 
CMD_MakeCert_PROMPT_ST	State of Certificate to Create (ST): 
CMD_MakeCert_PROMPT_L	Locale of Certificate to Create (L): 
CMD_MakeCert_PROMPT_SERIAL	Serial Number of Certificate to Create (Hexadecimal): 
CMD_MakeCert_PROMPT_EXPIRES	Expiration Date of Certificate to Create (Days): 
CMD_MakeCert_PROMPT_SAVECERT	File Name to Save Certificate to Create: 
CMD_MakeCert_PROMPT_SAVEKEY	File Name to Save Private Key to Create: 
CMD_MakeCert_EVAL_EXPIRES	Specify the Expiration Date within the range %u to %u.
CMD_MakeCert_ERROR_SIGNKEY	Either it is not possible to read the certificate or private key specified by /SIGNCERT and /SIGNKEY, or they were an invalid combination.
CMD_MakeCert_ERROR_GEN_FAILED	Creation of certificate and private key failed.


# MakeCert2048 command
CMD_MakeCert2048	Create New X.509 Certificate and Private Key (2048 bit)
CMD_MakeCert2048_Help	Use this to create a new X.509 certificate and private key and save it as a file. \nThe algorithm used to create the public key and private key of the certificate is RSA 2048 bit. \nYou can choose to create a root certificate (self-signed certificate) or a certificate signed by another certificate. To create a certificate that is signed by another certificate, you require a private key file (base 64 encoded) that is compatible with the certificate that uses the signature (X.509 format file). \n\nWhen creating a certificate, you can specify the following: Name (CN), Organization (O), Organization Unit (OU), Country (C), State (ST), Locale (L), Serial Number, and Expiration Date. \nThe created certificate will be saved as an X.509 format file and the private key file will be saved in a Base 64 encoded RSA 2048 bit format file. \n\nThe MakeCert command is a tool that provides the most rudimentary function for creating certificates. If you want to create a more substantial certificate, we recommend that you use either free software such as OpenSSL, or commercial CA (certificate authority) software. \n\nNote: This command can be called from the SoftEther VPN Command Line Management Utility. You can also execute this command while connected to the current VPN Server or VPN Client in Administration Mode but, what actually performs the RSA computation, generates the certificate data and saves it to file is the computer on which the command is running, and all this is executed in a context that has absolutely no relationship to the computer that is the destination of the Administration Mode connection.
CMD_MakeCert2048_Args	MakeCert2048 [/CN:cn] [/O:o] [/OU:ou] [/C:c] [/ST:st] [/L:l] [/SERIAL:serial] [/EXPIRES:expires] [/SIGNCERT:signcert] [/SIGNKEY:signkey] [/SAVECERT:savecert] [/SAVEKEY:savekey]
CMD_MakeCert2048_CN	Specify the Name (CN) item of the certificate to create. You can specify "none".
CMD_MakeCert2048_O	Specify the Organization (O) item of the certificate to create. You can specify "none".
CMD_MakeCert2048_OU	Specify the Organization Unit (OU) item of the certificate to create. You can specify "none".
CMD_MakeCert2048_C	Specify the Country (C) item of the certificate to create. You can specify "none".
CMD_MakeCert2048_ST	Specify the State (ST) item of the certificate to create. You can specify "none".
CMD_MakeCert2048_L	Specify the Locale (L) item of the certificate to create. You can specify "none".
CMD_MakeCert2048_SERIAL	Specify the Serial Number item of the certificate to create. Specify using hexadecimal values. You can specify "none".
CMD_MakeCert2048_EXPIRES	Specify the Expiration Date item of the certificate to create. If you specify "none" or "0", 3650 days (approx. 10 years) will be used. You can specify a maximum of 10950 days (about 30 years).
CMD_MakeCert2048_SIGNCERT	For cases when the certificate to be created is signed by an existing certificate, specify the X.509 format certificate file name to be used to sign the signature. When this parameter is omitted, such signature signing is not performed and the new certificate is created as a root certificate.
CMD_MakeCert2048_SIGNKEY	Specify a private key (RSA, base-64 encoded) that is compatible with the certificate specified by /SIGNCERT.
CMD_MakeCert2048_SAVECERT	Specify the file name to save the certificate you created. The certificate is saved as an X.509 file that includes a public key that is RSA format 2048 bit.
CMD_MakeCert2048_SAVEKEY	Specify the file name to save private key that is compatible with the certificate you created. The private key will be saved as an RSA-format 2048-bit private key file.


# TrafficClient command
CMD_TrafficClient	Run Network Traffic Speed Test Tool in Client Mode
CMD_TrafficClient_Help	Use this to execute the communication throughput measurement tool's client program. \nTwo commands, TrafficClient and TrafficServer, are used for the communication throughput measurement tool to enable the measurement of communication throughput that can be transferred between two computers connected by IP network. The TrafficServer command is used first on another computer which puts the communication throughput measurement tool server in a listening condition. Then the TrafficClient command is used to connect to that server by specifying its host name or IP address and port number, which makes it possible to measure the communication speed. \nMeasurement of the communication speed is carried out by concurrently establishing multiple TCP connections and calculating the actual number of bits of data that can be transferred within a specified time based on the respective results of transferring the maximum stream data on each connection and then using that to calculate the average value (bps) of communication throughput. Normally when there is one TCP connection, it is common to only be able to achieve communication speeds slower than the actual net throughput because of limitations related to the TCP algorithm. We therefore recommend the establishment of multiple concurrent TCP connections when measuring communication results. Because the throughput that is measured using this measurement method is calculated from the bit length of the data that arrives on the receiver side as a stream by TCP, the packet loss that occurs during transfer and the packets with corrupted data are not included in the packets that actually arrive, which means it is possible to calculate a genuine value that is close to the maximum possible communication bandwidth of the network. \nUsing the measurement results, i.e. the stream size transferred by TCP, the approximate value of data volume that actually passed through the network is calculated and this is divided by time to calculate the bits per sec (bps). The calculation assumes the type of the physical network is Ethernet (IEEE802.3) and the MAC frame payload size is 1,500 bytes (TCP MSS is 1,460 bytes). By specifying the /RAW option, the calculation will not make corrections for the TCP/IP header and MAC header data volume. \n\nNote: This command can be called from the SoftEther VPN Command Line Management Utility. You can also execute this command while connected to the current VPN Server or VPN Client in Administration Mode but, what actually conducts communication and measures the throughput is the computer on which the command is running, and all this is executed in a context that has absolutely no relationship to the computer that is the destination of the Administration Mode connection.
CMD_TrafficClient_Args	TrafficClient [host:port] [/NUMTCP:numtcp] [/TYPE:download|upload|full] [/SPAN:span] [/DOUBLE:yes|no] [/RAW:yes|no]
CMD_TrafficClient_[host:port]	Specify the host name or IP address and port number that the communication throughput measurement tool server (TrafficServer) is listening for. If the port number is omitted, 9821 will be used.
CMD_TrafficClient_NUMTCP	Specify the number of TCP connections to be concurrently established between the client and the server for data transfer. If omitted, 32 will be used.
CMD_TrafficClient_TYPE	Specify the direction of data flow when throughput measurement is performed. Specify one of the following options: "download", "upload" or "full". By specifying "download" the data will be transmitted from the server side to the client side. By specifying "upload" the data will be transmitted from the client side to the server side. By specifying "full", the data will be transferred in both directions. When "full" is specified, the NUMTCP value must be an even number of two or more (half the number will be used for concurrent TCP connections in the download direction and the other half will be used in the upload direction). If this parameter is omitted, "full" will be used.
CMD_TrafficClient_SPAN	Specify, using seconds, the time span to conduct data transfer for the measurement of throughput. If this parameter is omitted, "15" will be used.
CMD_TrafficClient_DOUBLE	When "yes" is specified, the throughput of the measured result will be doubled and then displayed. This option is used for cases when a network device etc. is somewhere on the data route and the total throughput capability that is input and output by this network device is being measured.
CMD_TrafficClient_RAW	By specifying "yes", the calculation will not make corrections for the TCP/IP header and MAC header data volume.
CMD_TrafficClient_EVAL_NUMTCP	Specify a value of 32 or less for the number of TCP connections.
CMD_TrafficClient_PROMPT_HOST	Measurement Server Name and Port Number (9821 if omitted): 
CMD_TrafficClient_ERROR_NUMTCP	When the data direction is "full" (both directions), you must specify an even value for the number of TCP connections (/NUMTCP).
CMD_TrafficClient_ERROR_HOSTPORT	The host name or port number is incorrectly specified.


# TrafficServer command
CMD_TrafficServer	Run Network Traffic Speed Test Tool in Server Mode
CMD_TrafficServer_Help	Use this to execute the communication throughput measurement tool's server program. \nTwo commands, TrafficClient and TrafficServer, are used for the communication throughput measurement tool to enable the measurement of communication throughput that can be transferred between two computers connected by IP network. \nTo set the TCP port of this computer to the Listen status to listen for the connection from the TrafficClient of another computer, specify the port number and start the server program using the TrafficServer command. \nYou can display more detailed information on the communication throughput measurement tool by inputting "TrafficClient ?". \n\nNote: This command can be called from the SoftEther VPN Command Line Management Utility. You can also execute this command while connected to the current VPN Server or VPN Client in Administration Mode but, what actually conducts communication and measures the throughput is the computer on which the command is running, and all this is executed in a context that has absolutely no relationship to the computer that is the destination of the Administration Mode connection.
CMD_TrafficServer_Args	TrafficServer [port] [/NOHUP:yes|no]
CMD_TrafficServer_[port]	Specify, using an integer, the port number at which to listen for the connection. If the specified port has been already being used by another program, or if the port cannot be opened, an error will occur.
CMD_TrafficServer_NOHUP	When "yes" is specified, the server process never stops without regard to any input from the console. It is convenient when you want to run the TrafficServer endlessly.


# Internal message strings concerning TrafficClient / TrafficServer
TT_LISTEN_FAILED	Unable to set TCP port %u to Listen status. The port may be being used by another application or this application did not have the authority to open the port.
TTS_LISTEN_STOP	The port for listening has been closed.
TTS_ENTER_TO_EXIT	\n----------------------------------------\nThe Network Traffic Speed Test Tool in Server Mode started. \n\nPress the Enter key to stop the server program. \n----------------------------------------\n\n
TTS_INIT	Starting the server program...
TTS_LISTEN_STARTED	The server program has been started. Now the IPv4 TCP port %u is set to Listen status and listening for connection from the client.
TTS_LISTEN_STARTED_V6	The IPv6 TCP Port %u is listening to accept clients.
TTS_LISTEN_FAILED_V6	Failed to open the IPv6 TCP Port %u. Another application might be using the same IPv6 TCP Port, or the IPv6 stack is not installed on the operating system.
TTS_STOP_INIT	Stopping the server program...
TTS_STOP_FINISHED	The stopping of the server program is complete.
TTS_ACCEPTED	Connection %u: Connected from Client %S Port %u.
TTS_DISCONNECTED	Connection %u (%S) has been disconnected.
TTS_DISCONNECT	Connection %u (%S) has been disconnected.
TTC_INIT	Starting the client program...
TTC_FREE	The client program has been terminated.
TTC_CONNECT_START	The connection to server %S (port %u) will start. %u TCP connections will be connected.
TTC_CONNECT_FAILED	The connection of TCP connection number %u failed.
TTC_CONNECT_NOT_SERVER	Because a program other than TrafficServer is operating on the destination TCP port, traffic cannot be measured.
TTC_CONNECT_OK	TCP connection number %u has been connected.
TTC_CONNECT_OK_2	\        Data transfer direction: %s
TTC_ERROR_ABORTED	The TCP connection initialization with the server failed. Measurement will stop.
TTC_SUMMARY_BAR	-------------------------------------------------------
TTC_SUMMARY_TITLE	Network Traffic Speed Test Tool Client Setting Parameters
TTC_SUMMARY_HOST	Destination Host Name
TTC_SUMMARY_PORT	Destination TCP Port Number
TTC_SUMMARY_NUMTCP	Number of TCP Connections to Establish
TTC_SUMMARY_TYPE	Data Transfer Direction
TTC_SUMMARY_SPAN	Data Transmission Time
TTC_SUMMARY_ETHER	Correção de dados para quadros Ethernet
TTC_SUMMARY_DOUBLE	Measurement of Total Speed of Relay Device Input Output
TTC_TYPE_DOWNLOAD	Download (Server to Client)
TTC_TYPE_UPLOAD	Upload (Client to Server)
TTC_TYPE_FULL	Full (Server < -- > Client)
TTC_SPAN_STR	%.1f segundos
TTC_COMM_START	\nAll connections were established and so data transfer started. \nMeasurement Start Time: %s\nScheduled Finish Time: %s\n\nMeasuring in progress. Please wait... \n(Do not use any other applications while measuring is in progress.)\n\n
TTC_COMM_END	Because %.1f seconds or more have passed, the data communication will end. \n\n
TTC_COMM_USER_CANCEL	Because of cancellation by user, the data communication will end. \n\n
TTC_COMM_DISCONNECTED	The TCP connection %u has been disconnected.
TTC_STOPPING	Stopping the operation of the communication throughput measurement tool client...
TTC_ENTER_TO_EXIT	\n----------------------------------------\nThe Network Traffic Speed Test Tool in Client Mode started. \n\nPress the Enter key to stop the client program. \n----------------------------------------\n\n
TTC_RES_TITLE	\n\nNetwork Traffic Speed Test Tool\n\n
TTC_RES_COLUMN_1	Nome do item
TTC_RES_COLUMN_2	Visão normal
TTC_RES_COLUMN_3	Simplified View
TTC_RES_SPAN	Time Span for Measurement
TTC_RES_ETHER	Correção de dados para quadros Ethernet
TTC_RES_BYTES_DOWNLOAD	Communication Data Volume in Download Direction
TTC_RES_BYTES_UPLOAD	Communication Data Volume in Upload Direction
TTC_RES_BYTES_TOTAL	Total Communication Data Volume
TTC_RES_DOUBLE	Relay Device Input Output Total Throughput Computation
TTC_RES_BPS_DOWNLOAD	Average Throughput in Download Direction
TTC_RES_BPS_UPLOAD	Average Throughput in Upload Direction
TTC_RES_BPS_TOTAL	Total Average Throughput


# Check command
CMD_Check	Check whether SoftEther VPN Operation is Possible
CMD_Check_Help	Use this to check if the current computer that is running vpncmd is a suitable operation platform for SoftEther VPN Server / Bridge. \nIf this check passes on a system, it is most likely that SoftEther VPN software will operate correctly on that system. \nAlso, if this check does not pass on a system, then this indicates that some type of trouble may arise if SoftEther VPN software is used on that system.
CMD_Check_Args	Verificar


# Concerning System Checker


# (This contains some strange character strings which are used to check character code conversion.)
CHECK_TITLE	---------------------------------------------------\nSoftEther VPN Operation Environment Check Tool\nDeveloper Edition\n\nCopyright (c) SoftEther VPN Project.\nAll Rights Reserved.\n\n
CHECK_NOTE	If this operation environment check tool is run on a system and that system passes, it is most likely that SoftEther VPN software can operate on that system. This check may take a while. Please wait...\n\n
CHECK_EXEC_TAG	Checking '%s'... \n
CHECK_PASS	Senha
CHECK_FAIL	Falha
CHECK_RESULT_1	All checks passed. It is most likely that SoftEther VPN Server / Bridge can operate normally on this system.
CHECK_RESULT_2	Some checks failed. Please check the operation environment of this system. If SoftEther VPN Server / Bridge were to be executed on this system, troubles may occur.
CHECK_TEST_123456789	123456789
CHECK_PROC_KERNEL	Kernel System
CHECK_PROC_MEMORY	Memory Operation System
CHECK_PROC_STRINGS	ANSI / Unicode string processing system
CHECK_PROC_FILESYSTEM	Sistema de arquivos
CHECK_PROC_THREAD	Thread processing system
CHECK_PROC_NETWORK	Network system


######################################################


#                                                    #


# Setup Wizard (SW) Strings                          #


#                                                    #


######################################################
SW_TITLE	Assistente de configuração da Edição de Desenvolvedor do SoftEther VPN (Versão %S)
SW_EXIT_CONFIRM	O processo de instalação do SoftEther VPN ainda não foi concluído.\r\n\r\nDeseja sair da instalação?
SW_UNINSTALL_CONFIRM	Starting the uninstall process of %s.\r\n\r\nDo you want to continue?
SW_COMPONENT_VPNSERVER_TITLE	SoftEther VPN Servidor
SW_COMPONENT_VPNSERVER_DESCRIPTION	Instale-o num servidor central de VPN. As ferramentas de gerenciamento também serão instaladas.
SW_COMPONENT_VPNCLIENT_TITLE	SoftEther VPN Cliente
SW_COMPONENT_VPNCLIENT_DESCRIPTION	Instale-o em computadores cliente VPN. Um computador cliente VPN poderá se conectar ao servidor VPN central. As ferramentas de gerenciamento também serão instaladas.
SW_COMPONENT_VPNBRIDGE_TITLE	SoftEther VPN Bridge
SW_COMPONENT_VPNBRIDGE_DESCRIPTION	Instale-o nos computadores de cada lugar. Cada VPN Bridge estabelecerá uma conexão VPN com o servidor VPN central. As ferramentas de gerenciamento também serão instaladas.
SW_COMPONENT_VPNSMGR_TITLE	Gerenciador de servidores SoftEther VPN (apenas ferramentas administrativas)
SW_COMPONENT_VPNSMGR_DESCRIPTION	Somente o gerenciador de servidores VPN será instalado. O serviço do servidor VPN não será instalado. Você pode usar o gerenciador de servidores VPN para conectar e gerenciar servidores VPN remotos e Bridges VPN em outros computadores que podem ser executados no Windows, Linux, Mac OS X, Solaris e FreeBSD.
SW_COMPONENT_VPNCMGR_TITLE	Gerenciador de clientes SoftEther VPN (apenas ferramentas administrativas)
SW_COMPONENT_VPNCMGR_DESCRIPTION	Apenas o Gerenciador de clientes VPN será instalado. O serviço do programa VPN Cliente não será instalado. Você pode usar o Gerenciador de clientes VPN para conectar e gerenciar clientes VPN remotos em outros computadores que podem ser executados no Windows e Linux.
SW_WELCOME_TITLE	Bem-vindo ao Assistente de configuração da Edição de Desenvolvedor do SoftEther VPN
SW_MODE_TITLE	Select a Setup Mode
SW_NOT_ADMIN_TITLE	Not Enough Privileges
SW_COMPONENTS_TITLE	Selecione o componente de software que deseja instalar
SW_EULA_TITLE	Contrato de licença do usuário final
SW_WARNING_TITLE	Avisos importantes
SW_DIR_TITLE	Diretório para instalar
SW_READY_TITLE	Pronto para instalar
SW_PERFORM_TITLE	A instalação está em andamento
SW_ERROR_TITLE	Resultados da instalação
SW_FINISH_TITLE	A instalação terminou
SW_UNINST1_TITLE	Desinstalador
SW_LANG1_TITLE	SoftEther VPN: Configure the Display Language
SW_EASY1_TITLE	Welcome to SoftEther VPN Client Easy Installer Creator
SW_EASY2_TITLE	Especificar arquivos
SW_WEB1_TITLE	Welcome to SoftEther VPN Client Web Installer Creator
SW_WEB2_TITLE	Especificar arquivos
SW_UNINSTALLINFO_URL	http://selinks.org/
SW_UNINSTALLINFO_PUBLISHER	Projeto SoftEther VPN
SW_KB3033929_REQUIRED	In Windows 7 and Windows Server 2008 R2, some SoftEther VPN functions require the Microsoft's Windows Update module KB3033929 installed.\r\n\r\nIf KB3033929 is not installed in your Windows, please install it from Windows Update or Microsoft website before installing SoftEther VPN.
SW_COMPONENTS_ABOUT_TAG	Sobre o %s
SW_COMPONENTS_REQUIRE_ADMIN	Installation Requires Administrators Privileges
SW_COMPONENTS_REQUIRE_ADMIN_TEXT	You have to restart the setup wizard by a user who has Administrators privileges to install %s in the System Mode. To install in the System Mode, click Back.
SW_DIR_SELECT	Por favor, especifique o diretório para instalar
SW_DIR_MORE_THAN_110	The directory name is too long.\r\nSpecify 110 letters at most.
SW_DIR_WRITE_ERROR	Unable to create the specified directory "%s" or failed to write a file on the directory.\r\n\r\nSpecify another directory.
SW_DIR_DST_IS_SAME_TO_SRC	The specified directory "%s" is same as the source directory.
SW_DIR_IS_NOT_HDD	The specified directory "%s" is not a local hard disk drive.\r\n\r\nTo install %s in the System Mode, you have to specify a directory on a local hard disk drive.
SW_DIR_IS_NOT_FULLPATH	The directory "%s" is not a format of full path.\r\n\r\nPlease specify the full path of the directory.
SW_DIR_DST_IS_OTHER_PRODUCT	The specified directory has another component already installed.\r\n\r\nPlease specify another directory.
SW_DIR_DST_IS_NEWER	Newer version of the software has been installed on the specified directory.\r\n\r\nYou need not to install this version.
SW_DIR_DST_IS_NEWER_2	Newer version of the software has been installed on the specified directory.\r\n\r\nThis installer will import and apply the VPN Connection Settings which is built-in on the Easy Installer. No program files will be overwritten.
SW_DIR_DST_IS_BROKEN	Unable to read a file "%s" which is on the specified directory.\r\n\r\nPlease specify another directory.
SW_DIR_DST_IS_SYSTEM_MODE	The same software is already installed on the specified directory as the System Mode.\r\n\r\nPlease specify another directory.
SW_DIR_DST_IS_USER_MODE	The same software is already installed on the specified directory as the User Mode.\r\n\r\nPlease specify another directory.
SW_SYSTEM_MODE_ALREADY_INSTALLED	The software "%s" is already installed on this computer as the System Mode.\r\n\r\nBoth the System Mode and the User Mode installation of the same software on the same computer will conflict.\r\n\r\nDo you really want to continue the installation as the User Mode?

SW_SETUPLOG_CORRUPTED	The "setuplog.dat" file is broken.
SW_MSI_UNINSTALL_FAILED	The older version of %s (Product Code: "%S") is installed. Windows Installer failed to uninstall this older version.\r\n\r\nPlease uninstall this older version manually and restart this installer again.
SW_MSI_UNINSTALL_REBOOT_REQUIRED	Windows Installer has uninstalled the older version of %s. The reboot of computer is required.\r\n\r\nPress Finish button and reboot the computer MANUALLY, and restart this installer after the reboot.
SW_NOTICE_VPNSERVER_IS_INSTALLED	SoftEther VPN Bridge is selected as a component to install. However, this computer has already had SoftEther VPN Server installed.\r\n\r\nUsually, you don't need to install both SoftEther VPN Server and SoftEther VPN Bridge on the same computer.\r\nIf you install both software, conflicts such as port number duplication will occur.\r\nIf you want to replace the SoftEther VPN Server to SoftEther VPN Bridge, you should exit this installer, uninstall SoftEther VPN Server and restart this installer after that.\r\n\r\nDo you really want to continue the SoftEther VPN Bridge installation?
SW_NOTICE_VPNBRIDGE_IS_INSTALLED	SoftEther VPN Server is selected as a component to install. However, this computer has already had SoftEther VPN Bridge installed.\r\n\r\nUsually, you don't need to install both SoftEther VPN Bridge and SoftEther VPN Server on the same computer.\r\nIf you install both software, conflicts such as port number duplication will occur.\r\nIf you want to replace the SoftEther VPN Server to SoftEther VPN Server, you should exit this installer, uninstall SoftEther VPN Bridge and restart this installer after that.\r\n\r\nDo you really want to continue the SoftEther VPN Server installation?
SW_OS_FAILED	This operating system doesn't support %s.
SW_LANG_NOT_CHANGED	The language settings of %s were not changed.
SW_LANG_LIST_LOAD_FAILED	Loading the available language list failed.
SW_LANG_OK	The display language of %s has been changed successfully.\r\nIf %s programs are currently running, exit a program and restart it to apply the new display language. If the display language still doesn't effect, reboot Windows.\r\n
SW_LANG_OK_SERVICE	\r\nThe language of log files which the service program records will be changed to the new language after a reboot.
SW_LANG_OK_VPNCMGR	\r\nThe display setting of VPN Client Manager will be changed after exit and reboot VPN Client Manager. (Including complete termination from the task tray.)
SW_CHILD_PROCESS_ERROR	Failed to execute a child process.
SW_EXE_FILTER	Windows Executable Files (*.EXE)|*.exe|All Files (*.*)|*.*
SW_PERFORM_MSG_EASY_INFO	Compiling the VPN Client Easy Installer...
SW_EASY_FINISHED_MSG	The VPN Client Easy Installer is created successfully.\r\nThe installer is saved as the following filename.\r\n\r\n%s\r\n\r\nYou can distribute the above file in the enterprise.
SW_EASY_ERROR_MSG	Failed to create a VPN Client Easy Installer.
SW_OTHER_INSTANCE_EXISTS	Another SoftEther VPN Setup Wizard is running.\r\n\r\nYou can continue this wizard after another wizard exits.
SW_PERFORM_MSG_WEB_INFO	Compiling the VPN Client Web Installer...
SW_WEB_ERROR_MSG	Failed to create a VPN Client Web Installer.
SW_INSTALLER_CACHE_IS_NOT_SIGNED	The currently installed SoftEther VPN Client of this computer has not been installed from the digital-signed package signed by an Authenticode digital certificate of SoftEther VPN Project.\r\nIt might be installed from a customized installer (for example, an installer created by Easy Installer Creator.)\r\n\r\nIf you continue to create a Web Installer, a warning message will be appeared on the user's screen when its loading.\r\nTo avoid showing the warning message, you should cancel this creating wizard, download the latest version of SoftEther VPN Client from the SoftEther VPN Project's web site, re-install it and restart the Web Installer Creator wizard.\r\n\r\nDo you really to continue to create a Web Installer?
SW_FILE_NOT_FOUNT	The file "%s" not found.
SW_WEB_FINISHED	The Web Installer is created and saved as "%s".\r\n\r\nPlease extract inner files from the ZIP file, upload them into the Web server, and edit a HTML file and an inf file to replace URLs appropriately.\r\n\r\nThe explanation to deploy the Web Installer is described on the ZIP file.
SW_VG_CONFIRM_MSG	Do you really want to install and activate the VPN Gate P2P Relay Function plug-in module with SoftEther VPN Client?\r\n\r\nThis plug-in will realize the stability of communication to bypass the government censorship firewall. However, the communication of VPN Gate usually consumes some network bandwidth. VPN Gate is not recommended to be used in the mobile connections. \r\n\r\nPlease note that there are some countries and regions which have the regulation to forbid the encrypted communications to bypass government censorship firewalls. In such a case, you must not use the VPN Gate functions on your computer. VPN Gate is intended to be used mainly in Japan. VPN Gate is a research project for just academic purpose only. VPN Gate is governed under the Japanese laws. Other countries' laws are none of our concerns nor responsibilities. By using this software and service, you must observe all concerned laws and rules with your own responsibility. You will be completely liable to any damages and responsibilities which are results of using this software and service, regardless of either inside or outside of Japan's territory.
SW_PERFORM_MSG_INIT_TASKS	Preparando as tarefas...
SW_PERFORM_MSG_COPY_PREPARE	Preparando a cópia de arquivos...
SW_PERFORM_MSG_WRITE_ERROR	Failed to write the destination file "%s".\r\n\r\nThere might be another person who has been keeping this file open.\r\nIf programs or services of %s are running, please terminate them and click Retry.
SW_PERFORM_MSG_COPY_FILE	Copying "%s" ...
SW_PERFORM_MSG_SET_SECURITY	Setting a security on "%s" ...
SW_PERFORM_MSG_PLUGIN	Installing the plugins...
SW_PERFORM_MSG_STOP_SVC	Stopping the "%s" service ...
SW_PERFORM_MSG_WAIT_FOR_FILE_UNLOCK	The file "%s" is locked by a running program. Waiting to unlock...
SW_PERFORM_MSG_INSTALL_SVC	Installing the %s service...
SW_PERFORM_MSG_START_SVC	Starting the %s service...
SW_PERFORM_MSG_CREATE_LINKS	Criando atalhos...
SW_PERFORM_MSG_DELETE_LINKS	Deleting shortcut files...
SW_PERFORM_MSG_DELETE_OLD_LINKS	Deleting old shortcut files...
SW_PERFORM_MSG_REGISTER_UNINSTALL	Registering uninstall information on the Control Panel...
SW_PERFORM_MSG_IMPORTING_ACCOUNT	Importing the Built-in VPN Connection Setting in the Easy Installer...
SW_PERFORM_MSG_DELETE_SETUP_INFO	Deleting the install information and logs...
SW_PERFORM_MSG_WRITE_LOG	Writing a setup log...
SW_PERFORM_MSG_COPY_ERROR	Copying to the file "%s" failed.
SW_PERFORM_MSG_CREATE_LINK_ERROR	Creating the shortcut file "%s" failed.\r\n\r\nDo you want to retry?
SW_PERFORM_MSG_WRITE_LOG_ERROR	Creating the setup log file "%s".\r\n\r\nDo you want to retry?
SW_PERFORM_MSG_STOP_SVC_ERROR	Stopping the "%s" service (internal name: "%S") failed.
SW_PERFORM_MSG_START_SVC_ERROR	Starting the "%s" service (internal name: "%S") failed.
SW_PERFORM_MSG_SVC_UNINSTALL_FAILED	Uninstall of the "%s" service (internal name: "%S") failed.
SW_PERFORM_MSG_SVC_INSTALL_FAILED	Install of the "%s" service (internal name: "%S") failed.
SW_PERFORM_MSG_SVC_USERMODE_EXEC_FAILED	Starting the user-mode service "%s" failed.
SW_PERFORM_MSG_UPDATING	Updating system settings...
SW_PERFORM_MSG_DELETE_NIC	Removendo os adaptadores de rede virtuais...
SW_PERFORM_MSG_FINISHED	Setup progress finished.
SW_PERFORM_MSG_UNINSTALL_MSI	Windows Installer is uninstalling the older version of %s...
SW_PERFORM_MSG_UPDATE_LANG_CONFIG	Changing the language settings...
SW_PERFORM_MSG_INIT_UNINST	Preparando a desinstalação...
SW_PERFORM_MSG_DELETE_PREPARE	Preparando para excluir arquivos...
SW_PERFORM_MSG_DELETE_ERROR	Unable to delete the file "%s".\r\n\r\nThere might be another program who is keeping this file open.\r\nIf programs or services of %s are running, please terminate them and click Retry.
SW_PERFORM_MSG_UNINSTALL_SVC	Uninstalling the "%s" service ...
SW_PERFORM_MSG_DELETE	Deleting the "%s" service ...
SW_PERFORM_MSG_EASY_INIT	Building the Easy Installer...
SW_PERFORM_MSG_WEB_INIT	Building the Web Installer...
SW_PERFORM_MSG_INSTALL_SELOW	Creating a restore point of the system and installing essential components. It may take a while...
SW_TAG_USERNAME	\ (User-mode)
SW_DIRNAME_CONFIG_TOOLS	Configuration Tools
SW_DIRNAME_ADMIN_TOOLS	Administrative Tools
SW_DIRNAME_LANGUAGE_TOOLS	Configurações de idioma
SW_RUN_TEXT_VPNSMGR	Iniciar o gerenciador de servidores VPN SoftEther.
SW_RUN_TEXT_VPNCMGR	Iniciar o gerenciador de clientes VPN SoftEther.
SW_NIC_UNINSTALL	Virtual Network Adapters of SoftEther VPN Client have been created on the system.\r\nDo you want to delete these Virtual Network Adapters?


# Do not translate this section !!!
SW_TAG_USERNAME_ENGLISH						\ (User-Mode)
SW_LINK_NAME_VPNSERVER_SVC					SoftEther VPN Server Developer User-mode Service
SW_LINK_NAME_VPNBRIDGE_SVC					SoftEther VPN Bridge Developer User-mode Service
SW_LONG_VPNSERVER							SoftEther VPN Server Developer Edition
SW_LONG_VPNCLIENT							SoftEther VPN Client Developer Edition
SW_LONG_VPNBRIDGE							SoftEther VPN Bridge Developer Edition
SW_LONG_VPNSMGR								SoftEther VPN Server Manager Developer Edition
SW_LONG_VPNCMGR								SoftEther VPN Client Manager Developer Edition
SW_LANG_SET_FAILED							Failed to write the new language setting on lang.config file.


# --- end of "Do not translate this section" ---


# Shortcuts Filenames
SW_LINK_NAME_VPNSMGR_SHORT	SoftEther VPN Server Manager (Dev)
SW_LINK_NAME_VPNSMGR_SHORT_UM	SE-VPN Server Manager (Dev User)
SW_LINK_NAME_VPNSMGR_SHORT_TOOLSONLY	SE-VPN Server Manager (Dev Tools)
SW_LINK_NAME_VPNSMGR_SHORT_TOOLSONLY_UM	SE-VPN Server Manager (Dev Tools User)
SW_LINK_NAME_VPNSMGR_FULL	Edição de desenvolvedor do gerenciador SoftEther VPN Servidor
SW_LINK_NAME_VPNSMGR_COMMENT	You can manage SoftEther VPN Server or SoftEther VPN Bridge on a remote computer.
SW_LINK_NAME_VPNCMGR_SHORT	Gerenciador do SoftEther VPN Cliente (Des)
SW_LINK_NAME_VPNCMGR_FULL	Edição de desenvolvedor do gerenciador SoftEther VPN Cliente
SW_LINK_NAME_VPNCMGR_COMMENT	You can connect to a VPN Server by using SoftEther VPN Client.
SW_LINK_NAME_VPNCMGRTOOLS_SHORT	SoftEther VPN Client Remote Manager (Dev)
SW_LINK_NAME_VPNCMGRTOOLS_SHORT_UM	SE-VPN Client Remote Manager (Dev User)
SW_LINK_NAME_VPNCMGRTOOLS_FULL	SoftEther VPN Client Remote Manager Developer Edition
SW_LINK_NAME_VPNCMGR2_FULL	Manage Remote Computer's SoftEther VPN Client
SW_LINK_NAME_VPNCMGR2_COMMENT	You can establish a remote connection to and manage a SoftEther VPN Client on a remote computer.
SW_LINK_NAME_VPNCMGRTRAY_FULL	SoftEther VPN Client Manager Developer Edition Startup
SW_LINK_NAME_VPNCMGRTRAY_COMMENT	Registers an icon of SoftEther VPN Client Developer Edition on the taskbar's notification area.
SW_LINK_NAME_EASYINSTALLER	Easy Installer Creator
SW_LINK_NAME_EASYINSTALLER_COMMENT	A tool for enterprise system administrators to create a SoftEther VPN Client Easy Installer which has a function to kick-start a VPN connection to the specific destination automatically.
SW_LINK_NAME_WEBINSTALLER	Web Installer Creator
SW_LINK_NAME_WEBINSTALLER_COMMENT	A tool for enterprise system administrators to create a SoftEther VPN Client Web Installer (ActiveX Installer) which has a function to kick-start a VPN connection to the specific destination automatically.
SW_LINK_NAME_VPNCMD	SoftEther VPN Command Line Utility (vpncmd)
SW_LINK_NAME_VPNCMD_COMMENT	Manage SoftEther VPN Server, SoftEther VPN Bridge and SoftEther VPN Client on the command-line interface in vpncmd.
SW_LINK_NAME_TRAFFIC	Ferramenta de teste de velocidade do tráfego de rede
SW_LINK_NAME_TRAFFIC_COMMENT	Performs transmitting packets between two computers connected with TCP/IP, with large amount of throughput as possible, in order to measure the actual network traffic speed available.
SW_LINK_NAME_TCP	Utilitário de otimização de TCP
SW_LINK_NAME_TCP_COMMENT	TCP Optimization Utility can adjust the parameters of TCP/IP of Windows in order to increase the network communication throughput of this computer.
SW_LINK_NAME_SERVICES	Services Running on this Computer
SW_LINK_NAME_SERVICES_COMMENT	Starts, stops, and configures Windows services. You can start and stop SoftEther VPN services.
SW_LINK_NAME_VPNSERVER_SVC_COMMENT	Starts SoftEther VPN Server Service in the User Mode.
SW_LINK_NAME_VPNBRIDGE_SVC_COMMENT	Starts SoftEther VPN Bridge Service in the User Mode.
SW_LINK_NAME_UNINSTALL	Desinstalar %s
SW_LINK_NAME_UNINSTALL_COMMENT	Uninstall %s on this computer.
SW_LINK_NAME_LANGUAGE	Configure Display Language
SW_LINK_NAME_LANGUAGE_COMMENT	Change the display language setting of %s.
SW_LINK_NAME_DEBUG	Debugging Information Collecting Tool
SW_LINK_NAME_DEBUG_COMMENT	Collects debugging information of SoftEther VPN. Use this tool only if your support staff asks you to do so.
